TDI Format 1.5	Offset	Rxx::R	Rxx::Theta	Rxx::X	Rxx::Y	Rxy::R	Rxy::Theta	Rxy::X	Rxy::Y	temperature: T1	temperature: T2	temperature: T3	temperature: T4	temperature: dT/dt	iterator	multi[0]:iterator	multi[0]:y	multi[0]:temperature: setpoint	multi[0]:temperature: T1	multi[0]:temperature: T2	multi[0]:temperature: T3	multi[0]:temperature: T4	multi[0]:temperature: heater	multi[0]:temperature: gas	multi[0]:temperature: dT/dt	multi[0]:temperature: current temperature	multi[0]:temperature: error	multi[1]:iterator	multi[1]:y	multi[1]:Control:Magnet Output
2nd Parameter Class{String}=Multi-Parameter	0E+0	1.795471397E-3	4.2E-2	1.795471397E-3	1.180117377E-6	1.622134069E-6	-1.261404E+2	-9.588461291E-7	-1.312352568E-6	1.75133E+2	1.70745E+2	9.41619E+1	7.35612E+1	8.3100833E-2	8.1E+1	4E+0	1.75E+2	1.75E+2	1.75133E+2	1.70742E+2	9.42335E+1	7.35612E+1	4.2E+0	1.75E+2	8.42891261E-2	1.75134E+2	-1.34E-1	0E+0	0E+0	-0E+0
2nd Parameter Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	0E+0	1.7968149E-3	4.2E-2	1.7968149E-3	1.180117377E-6	6.890000393E-6	-1.08996E+1	6.764610561E-6	-1.304449942E-6	1.75134E+2	1.70822E+2	9.38754E+1	7.35612E+1	7.109311968E-2	8.2E+1	4E+0	1.75E+2	8E+1	1.75133E+2	1.70745E+2	9.41619E+1	7.35612E+1	4.2E+0	1.75E+2	8.3100833E-2	7.2727E+1	-1.34E-1	1E+0	5E-1	5E-1
Analysis Class{String}=Basic Plot	0E+0	1.799855459E-3	4.2E-2	1.799855459E-3	1.180117377E-6	1.454651585E-5	-5.0688E+0	1.448915535E-5	-1.286537796E-6	1.75135E+2	1.70901E+2	9.38754E+1	7.35612E+1	6.592666358E-2	8.3E+1	4E+0	1.75E+2	8E+1	1.75134E+2	1.70822E+2	9.38754E+1	7.35612E+1	4.2E+0	1.75E+2	7.109311968E-2	7.2727E+1	-1.34E-1	2E+0	1E+0	9.999E-1
Analysis Class Path{Path}=C\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV\\\\plugins\\\\Plotting\\\\Plotting_Base_class\\\\Plotting_Base.lvclass	0E+0	1.804598731E-3	4.08E-2	1.804598731E-3	1.146399697E-6	2.2252113E-5	-3.3384E+0	2.22141838E-5	-1.297074253E-6	1.75134E+2	1.70981E+2	9.41619E+1	7.35612E+1	6.892055273E-2	8.4E+1	4E+0	1.75E+2	8E+1	1.75135E+2	1.70901E+2	9.38754E+1	7.35612E+1	4.2E+0	1.75E+2	6.592666358E-2	7.2727E+1	-1.34E-1	3E+0	1.5E+0	1.4999E+0
Analysis.# pre-routines{I32}=5	0E+0	1.804598731E-3	4.2E-2	1.804598731E-3	1.180117377E-6	2.223890425E-5	-3.3192E+0	2.220046592E-5	-1.288644974E-6	1.75137E+2	1.70988E+2	9.41261E+1	7.35612E+1	7.251895219E-2	8.5E+1	4E+0	1.75E+2	8E+1	1.75134E+2	1.70981E+2	9.41619E+1	7.35612E+1	4.2E+0	1.75E+2	6.892055273E-2	7.2727E+1	-1.34E-1	4E+0	1.5E+0	1.5E+0
Analysis:Pre[0]:T Control Measure{1D Array (I32)}=[1,2,3,4,7]	0E+0	1.80271217E-3	4.08E-2	1.80271217E-3	1.146399697E-6	1.839193223E-5	-4.05E+0	1.834554603E-5	-1.300235303E-6	1.75135E+2	1.71027E+2	9.36605E+1	7.35612E+1	6.369787455E-2	8.6E+1	4E+0	1.75E+2	8E+1	1.75137E+2	1.70988E+2	9.41261E+1	7.35612E+1	4.2E+0	1.75E+2	7.251895219E-2	7.2727E+1	-1.34E-1	5E+0	1.25E+0	1.2502E+0
Autosave Tabs{Enum U32 ((XY Measurement Save,Parameter Plot Save 2))}=Parameter Plot Save 2	0E+0	1.801029256E-3	4.2E-2	1.801029256E-3	1.180117377E-6	1.455073021E-5	-5.1312E+0	1.449226662E-5	-1.3028697E-6	1.75135E+2	1.71062E+2	9.36246E+1	7.35612E+1	5.836297944E-2	8.7E+1	4E+0	1.75E+2	8E+1	1.75135E+2	1.71027E+2	9.36605E+1	7.35612E+1	4.2E+0	1.75E+2	6.369787455E-2	7.2727E+1	-1.34E-1	6E+0	1E+0	1.0001E+0
Control:Magnet Output{Double Float}=-0.007000	0E+0	1.799719694E-3	4.2E-2	1.799719694E-3	1.180117377E-6	1.070428711E-5	-7.0032E+0	1.062473476E-5	-1.306557686E-6	1.75134E+2	1.71107E+2	9.37679E+1	7.35612E+1	5.964675546E-2	8.8E+1	4E+0	1.75E+2	8E+1	1.75135E+2	1.71062E+2	9.36246E+1	7.35612E+1	4.2E+0	1.75E+2	5.836297944E-2	7.2727E+1	-1.34E-1	7E+0	7.5E-1	7.501E-1
Control:Magnet Rate{Double Float}=0.500000	0E+0	1.799006931E-3	4.2E-2	1.799006931E-3	1.180117377E-6	6.88367603E-6	-1.09152E+1	6.758817943E-6	-1.304976878E-6	1.75131E+2	1.71152E+2	9.41619E+1	7.35612E+1	6.595426798E-2	8.9E+1	4E+0	1.75E+2	8E+1	1.75134E+2	1.71107E+2	9.37679E+1	7.35612E+1	4.2E+0	1.75E+2	5.964675546E-2	7.2727E+1	-1.34E-1	8E+0	5E-1	5.001E-1
Display Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	0E+0	1.798667519E-3	4.2E-2	1.798667519E-3	1.180117377E-6	3.17262125E-6	-2.42748E+1	2.891820662E-6	-1.30603075E-6	1.75133E+2	1.71192E+2	9.3947E+1	7.35612E+1	5.955781043E-2	9E+1	4E+0	1.75E+2	8E+1	1.75131E+2	1.71152E+2	9.41619E+1	7.35612E+1	4.2E+0	1.75E+2	6.595426798E-2	7.2727E+1	-1.34E-1	9E+0	2.5E-1	2.502E-1
Elapsed Time{Double Float}=12790.950867	0E+0	1.798667519E-3	4.2E-2	1.798667519E-3	1.180117377E-6	1.649006955E-6	-1.269456E+2	-9.941437682E-7	-1.320782129E-6	1.75128E+2	1.71239E+2	9.38754E+1	7.35612E+1	6.883595884E-2	9.1E+1	4E+0	1.75E+2	8E+1	1.75133E+2	1.71192E+2	9.3947E+1	7.35612E+1	4.2E+0	1.75E+2	5.955781043E-2	7.2727E+1	-1.34E-1	1E+1	0E+0	0E+0
File:Autodel{Boolean}=True	0E+0	1.799176636E-3	4.2E-2	1.799176636E-3	1.180117377E-6	5.052900206E-6	-1.648128E+2	-4.879045275E-6	-1.324469832E-6	1.75128E+2	1.71276E+2	9.38395E+1	7.35612E+1	6.549406052E-2	9.2E+1	4E+0	1.75E+2	8E+1	1.75128E+2	1.71239E+2	9.38754E+1	7.35612E+1	4.2E+0	1.75E+2	6.883595884E-2	7.2727E+1	-1.34E-1	1.1E+1	-2.5E-1	-2.498E-1
File:Autosave{Boolean}=False	0E+0	1.800180728E-3	4.2E-2	1.800180728E-3	1.180117377E-6	8.8308586E-6	-1.712652E+2	-8.731815568E-6	-1.342383393E-6	1.75123E+2	1.71312E+2	9.38754E+1	7.35612E+1	5.732691661E-2	9.3E+1	4E+0	1.75E+2	8E+1	1.75128E+2	1.71276E+2	9.38395E+1	7.35612E+1	4.2E+0	1.75E+2	6.549406052E-2	7.2727E+1	-1.34E-1	1.2E+1	-5E-1	-4.999E-1
File:Export Config{Boolean}=True	0E+0	1.801368667E-3	4.2E-2	1.801368667E-3	1.180117377E-6	1.266520735E-5	-1.739328E+2	-1.25972459E-5	-1.340275649E-6	1.75121E+2	1.71353E+2	9.41977E+1	7.35612E+1	5.646742135E-2	9.4E+1	4E+0	1.75E+2	8E+1	1.75123E+2	1.71312E+2	9.38754E+1	7.35612E+1	4.2E+0	1.75E+2	5.732691661E-2	7.2727E+1	-1.34E-1	1.3E+1	-7.5E-1	-7.5E-1
File:Final Autosave{Boolean}=True	0E+0	1.803255228E-3	4.2E-2	1.803255228E-3	1.180117377E-6	1.650687041E-5	-1.753044E+2	-1.645474249E-5	-1.352396308E-6	1.75119E+2	1.71392E+2	9.39112E+1	7.35612E+1	5.442586541E-2	9.5E+1	4E+0	1.75E+2	8E+1	1.75121E+2	1.71353E+2	9.41977E+1	7.35612E+1	4.2E+0	1.75E+2	5.646742135E-2	7.2727E+1	-1.34E-1	1.4E+1	-1E+0	-9.999E-1
Filter:Enable{Enum U16 ((None,Analog,Digital,Analog&Digitial))}=None	0E+0	1.805413318E-3	3.6E-2	1.805413318E-3	1.180117377E-6	2.036756029E-5	-1.761792E+2	-2.032487933E-5	-1.358718125E-6	1.75116E+2	1.71448E+2	9.36246E+1	7.35612E+1	7.651688159E-2	9.6E+1	4E+0	1.75E+2	8E+1	1.75119E+2	1.71392E+2	9.39112E+1	7.35612E+1	4.2E+0	1.75E+2	5.442586541E-2	7.2727E+1	-1.34E-1	1.5E+1	-1.25E+0	-1.2499E+0
Filter:Points{I32}=1	0E+0	1.80794476E-3	3.72E-2	1.80794476E-3	1.180117377E-6	2.421195844E-5	-1.767708E+2	-2.417609399E-5	-1.365041357E-6	1.75121E+2	1.71482E+2	9.37679E+1	7.35612E+1	6.36575073E-2	9.7E+1	4E+0	1.75E+2	8E+1	1.75116E+2	1.71448E+2	9.36246E+1	7.35612E+1	4.2E+0	1.75E+2	7.651688159E-2	7.2727E+1	-1.34E-1	1.6E+1	-1.5E+0	-1.4999E+0
Filter:Type{U16}=1	0E+0	1.808012643E-3	3.6E-2	1.808012643E-3	1.180117377E-6	2.42167102E-5	-1.767324E+2	-2.417929011E-5	-1.381373261E-6	1.75122E+2	1.71481E+2	9.38037E+1	7.35612E+1	5.827749148E-2	9.8E+1	4E+0	1.75E+2	8E+1	1.75121E+2	1.71482E+2	9.37679E+1	7.35612E+1	4.2E+0	1.75E+2	6.36575073E-2	7.2727E+1	-1.34E-1	1.7E+1	-1.5E+0	-1.5E+0
Filter:Type.__text__{String}=Repeat	0E+0	1.804239521E-3	4.2E-2	1.804239521E-3	1.180117377E-6	1.650265605E-5	-1.753428E+2	-1.645052814E-5	-1.34185674E-6	1.75114E+2	1.7155E+2	9.41977E+1	7.35612E+1	5.493235216E-2	9.9E+1	4E+0	1.75E+2	8E+1	1.75122E+2	1.71481E+2	9.38037E+1	7.35612E+1	4.2E+0	1.75E+2	5.827749148E-2	7.2727E+1	-1.34E-1	1.8E+1	-1E+0	-1E+0
Filter:Window{Double Float}=1.000000	0E+0	1.80204749E-3	4.2E-2	1.80204749E-3	1.180117377E-6	8.839287313E-6	-1.712484E+2	-8.739715365E-6	-1.346598881E-6	1.75114E+2	1.71639E+2	9.38037E+1	7.35612E+1	8.558826894E-2	1E+2	4E+0	1.75E+2	8E+1	1.75114E+2	1.7155E+2	9.41977E+1	7.35612E+1	4.2E+0	1.75E+2	5.493235216E-2	7.2727E+1	-1.34E-1	1.9E+1	-5E-1	-5E-1
Iterator{I32}=0	
Magnet: Control Mode{Boolean}=False	
Magnet: Final Switch Heater{Enum U8 ((False,True,Mixed))}=	
Magnet: Power Supply{Enum U16 ((IPS120,LS625,PS110,Hg iPS,SMS Series,Cryomagnetics 4G,DMG Little CryoFree,DMG Big CryoFree))}=Hg iPS	
Magnet: Rate{Double Float}=0.500000	
Magnet: Setpoint{Double Float}=0.000000	
Magnet: Units{Enum U16 ((Field,Current))}=Field	
Magnet: VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
Main Screen Path{Path}=C:\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV\\\\1Code.vi	
Measurement Timestamp{Timestamp}=<12:04:48.365 19/05/2023>T	
Measurement Title{String}=	
Measurment Select{U16}=4	
Measurment Select.__text__{String}=6221-Lockin-DAQ	
Notes{String}=I+1E I-3A\\nrxx+2B Rxx-2C\\nRxy+2D Rxy-2E	
Offset{Double Float}=0.000000	
Option: 2182 Autozero{Boolean}=True	
Option: 2182 Front Autozero{Boolean}=True	
Option: 2182 Hold{Boolean}=False	
Option: 2182 Hold Count{I32}=10	
Option: 2182 Hold Window{Double Float}=1.000000	
Option: 2182 Line Sync{Boolean}=False	
Option: 2182 Reference Reading{Double Float}=0.000000	
Option: 2182 Relative Mode{Boolean}=False	
Option: 2182 Trigger Delay{Cluster (Boolean,Double Float)}={'Auto':True,'Time(s)':0.000000}	
Option: 2182 Trigger Source{Enum U16 ((Immediate,Timer,Manual,Bus,Trigger link))}=Bus	
Option: 2182 Trigger Timer{Double Float}=0.000000	
Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	
Option: 560 Enabled{Boolean}=False	
Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	
Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	
Option: 6221 Adjust Mode{Enum U16 ((Offset,Frequency,Amplitude))}=Offset	
Option: 6221 Amplitude{Double Float}=1.000000E-6	
Option: 6221 Compliance{Double Float}=10.000000	
Option: 6221 Duty Cycle{Double Float}=50.000000	
Option: 6221 External Trigger{Boolean}=False	
Option: 6221 External Trigger Ignore Multiple{Boolean}=False	
Option: 6221 Frequency{Double Float}=119.770000	
Option: 6221 Function{U16}=1	
Option: 6221 Function.__text__{String}=Sine	
Option: 6221 Idle Level{Double Float}=0.000000	
Option: 6221 Input trigger Line{U8}=5	
Option: 6221 Offset{Double Float}=0.000000	
Option: 6221 Output Trigger Line{U8}=4	
Option: 6221 Pass Through{Boolean}=True	
Option: 6221 Phase Marker{Boolean}=True	
Option: 6221 Phase Marker Phase{Double Float}=0.000000	
Option: 6221 Range Level{Double Float}=2.000000E-12	
Option: 6221 Ranging{U16}=1	
Option: 6221 Ranging.__text__{String}=Best	
Option: 6221 Update Clock{Double Float}=0.000000	
Option: 6221 VISA{Visa Refnum (Void)}=GPIB0::13::INSTR	
Option: Confirm Config{Boolean}=False	
Option: Control Panel Ref{LVObjVI Refnum (Void)}=	
Option: DAQ Global Channel{Boolean}=False	
Option: DAQ Input Rate{Double Float}=10000.000000	
Option: DAQ Input Samples{I32}=200	
Option: DAQ Measurement Channels{1D Array (Cluster (UserDefinedRefnumTag Refnum (Void),\tkDAQmxPhysChanTagType Tag,\tkDAQmxScaleTagType Tag,Boolean,Double Float,String))}=[]	
Option: Differential{I32}=10106	
Option: Differential.__text__{String}=Differential	
Option: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values))}=Function Generator	
Option: Lockin Standoff Time{Double Float}=0.000000	
Option: Paranoid Save Data{Boolean}=True	
Option: Plot Autoback Path{Path}=C:\\\\TEMP\\\\XY Multiparam\\\\Backup.txt	
Option: SR830  Ref Phase{Double Float}=0.000000	
Option: SR830  Synch Filter{Boolean}=False	
Option: SR830  Time Constant{I16}=8	
Option: SR830  Time Constant.__text__{String}=100 ms	
Option: SR830 2x Line Filter{Boolean}=True	
Option: SR830 Adjust Gains{Boolean}=False	
Option: SR830 Auto Gain Lower.__text__{String}=2 nV/fA	
Option: SR830 Auto Gain Upper.__text__{String}=1 V/uA	
Option: SR830 Auto Offset 1{Boolean}=False	
Option: SR830 Auto Offset 2{Boolean}=False	
Option: SR830 Autophase{Boolean}=False	
Option: SR830 DC Coupling?{Boolean}=False	
Option: SR830 Display 1{U16}=0	
Option: SR830 Display 1.__text__{String}=X	
Option: SR830 Display 2{U16}=0	
Option: SR830 Display 2.__text__{String}=Y	
Option: SR830 Dynamic Reserve{I16}=1	
Option: SR830 Dynamic Reserve.__text__{String}=Normal	
Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Option: SR830 Filter Slope{I32}=1	
Option: SR830 Filter Slope.__text__{String}=12 dB/oct	
Option: SR830 Gain{I32}=-1	
Option: SR830 Gain.__text__{String}=Auto Gain	
Option: SR830 Ground Shield?{Boolean}=False	
Option: SR830 Harmonic{I32}=1	
Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A	
Option: SR830 Line Filter{Boolean}=True	
Option: SR830 No Reset{Boolean}=False	
Option: SR830 Offset 1{Double Float}=0.000000	
Option: SR830 Offset 2{Double Float}=0.000000	
Option: SR830 Output Channel 1{Boolean}=False	
Option: SR830 Output Channel 2{Boolean}=False	
Option: SR830 Ratio 1{U16}=0	
Option: SR830 Ratio 1.__text__{String}=None	
Option: SR830 Ratio 2{U16}=0	
Option: SR830 Ratio 2.__text__{String}=None	
Option: SR830 Ref Amplitude{Double Float}=0.100000	
Option: SR830 Ref Frequency{Double Float}=1013.000000	
Option: SR830 Ref Source{Boolean}=False	
Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta]	
Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Option: SR830 VISA{Visa Refnum (Void)}=	
Option: Sense Autorange{Boolean}=False	
Option: Sense Range Level{Double Float}=0.100000	
Option: Sense Rate{Double Float}=1.000000	
Option:560 Comport{Visa Refnum (Void)}=COM1	
Option:560 Filter High Pass{U16}=0	
Option:560 Filter High Pass.__text__{String}=0.03	
Option:560 Filter Lowpass{U16}=0	
Option:560 Filter Lowpass.__text__{String}=0.03	
Option:560 Filter Mode{U16}=0	
Option:560 Filter Mode.__text__{String}=6 dB high pass	
Option:560 Invert{Boolean}=False	
Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Option:570 Enabled{Boolean}=False	
Option:570 Filter High Pass{U16}=0	
Option:570 Filter High Pass.__text__{String}=0.03	
Option:570 Filter Lowpass{U16}=0	
Option:570 Filter Lowpass.__text__{String}=0.03	
Option:570 Filter Mode{U16}=0	
Option:570 Filter Mode.__text__{String}=6 dB high pass	
Option:570 Gain Mode{U16}=0	
Option:570 Gain Mode.__text__{String}=Low Noise	
Option:570 Input Offset{U16}=0	
Option:570 Input Offset On{Boolean}=False	
Option:570 Input Offset.__text__{String}=1pA	
Option:570 Sensitivity{U16}=0	
Option:570 Sensitivity.__text__{String}=1pA/V	
Option:Debug On{Boolean}=False	
Option:GPIB 2182{Visa Refnum (Void)}=	
Option:Parallel Config Voltage Measurers{Boolean}=True	
Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Option:SR830 Settle Time{Double Float}=5.000000	
Option:Sense Digits{I32}=8	
Output Names{1D Array (String)}=['Offset','Rxx::R','Rxx::Theta','Rxx::X','Rxx::Y','Rxy::R','Rxy::Theta','Rxy::X','Rxy::Y','temperature: T1','temperature: T2','temperature: T3','temperature: T4','temperature: dT/dt','iterator','multi[0]:iterator','multi[0]:y','multi[0]:temperature: setpoint','multi[0]:temperature: T1','multi[0]:temperature: T2','multi[0]:temperature: T3','multi[0]:temperature: T4','multi[0]:temperature: heater','multi[0]:temperature: gas','multi[0]:temperature: dT/dt','multi[0]:temperature: current temperature','multi[0]:temperature: error','multi[1]:iterator','multi[1]:y','multi[1]:Control:Magnet Output']	
Parameter Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Parameter Select{U16}=6	
Parameter Select.__text__{String}=Multi-Parameter	
Paths{U32}=0	
Plot: Column Renames{1D Array (Cluster (String,String))}=[]	
Plot: No dups{Boolean}=False	
Plot: StdDevs{Boolean}=False	
Plotting Class{String}=Parameter Plot	
Plotting Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	
Plotting Select{U16}=1	
Plotting Select.__text__{String}=Parameter Plot	
Project Code{String}=Topological_Insulators	
Ref: Temperature Window{LVObjVI Refnum (Void)}=	
Ref:Control Subpanel{LVObjUnknown Refnum (Void)}=	
Ref:Main Screen{LVObjVI Refnum (Void)}=	
Ref:Plotting Subpanel{LVObjUnknown Refnum (Void)}=	
Ref:Toolbar{LVObjUnknown Refnum (Void)}=	
Ref:XY Subpanel{LVObjUnknown Refnum (Void)}=	
Rxx::R{Double Float}=0.001802	
Rxx::Theta{Double Float}=0.042000	
Rxx::X{Double Float}=0.001802	
Rxx::Y{Double Float}=1.180117E-6	
Rxx:Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	
Rxx:Option: 560 Enabled{Boolean}=False	
Rxx:Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	
Rxx:Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	
Rxx:Option: Lockin Standoff Time{Double Float}=0.000000	
Rxx:Option: Lockin Type{Enum U16 ((SRS 830,EG&G 5302))}=SRS 830	
Rxx:Option: SR803 Full Scale Reading{Double Float}=0.000000	
Rxx:Option: SR830  Ref Phase{Double Float}=0.000000	
Rxx:Option: SR830  Synch Filter{Boolean}=False	
Rxx:Option: SR830  Time Constant{I16}=8	
Rxx:Option: SR830 2x Line Filter{Boolean}=False	
Rxx:Option: SR830 Adjust Gains{Boolean}=False	
Rxx:Option: SR830 Auto Gain Lower{I32}=0	
Rxx:Option: SR830 Auto Gain Upper{I32}=26	
Rxx:Option: SR830 Auto Offset 1{Boolean}=False	
Rxx:Option: SR830 Auto Offset 2{Boolean}=False	
Rxx:Option: SR830 Autophase{Boolean}=False	
Rxx:Option: SR830 DC Coupling?{Boolean}=False	
Rxx:Option: SR830 Display 1{U16}=0	
Rxx:Option: SR830 Display 2{U16}=0	
Rxx:Option: SR830 Dynamic Reserve{I16}=2	
Rxx:Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Rxx:Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Rxx:Option: SR830 Filter Slope{I32}=3	
Rxx:Option: SR830 Gain{I32}=18	
Rxx:Option: SR830 Ground Shield?{Boolean}=False	
Rxx:Option: SR830 Harmonic{I32}=1	
Rxx:Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A-B	
Rxx:Option: SR830 Line Filter{Boolean}=False	
Rxx:Option: SR830 No Reset{Boolean}=False	
Rxx:Option: SR830 Offset 1{Double Float}=0.000000	
Rxx:Option: SR830 Offset 2{Double Float}=0.000000	
Rxx:Option: SR830 Output Channel 1{Boolean}=False	
Rxx:Option: SR830 Output Channel 2{Boolean}=False	
Rxx:Option: SR830 Ratio 1{U16}=0	
Rxx:Option: SR830 Ratio 2{U16}=0	
Rxx:Option: SR830 Ref Amplitude{Double Float}=0.100000	
Rxx:Option: SR830 Ref Frequency{Double Float}=1013.000000	
Rxx:Option: SR830 Ref Source{Boolean}=False	
Rxx:Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta,X,Y]	
Rxx:Option: SR830 Time Constant value{Double Float}=0.000000	
Rxx:Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Rxx:Option: SR830 VISA{Visa Refnum (Void)}=GPIB0::5::INSTR	
Rxx:Option:560 Comport{Visa Refnum (Void)}=COM1	
Rxx:Option:560 Filter High Pass{U16}=0	
Rxx:Option:560 Filter Lowpass{U16}=0	
Rxx:Option:560 Filter Mode{U16}=0	
Rxx:Option:560 Invert{Boolean}=False	
Rxx:Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Rxx:Option:570 Enabled{Boolean}=False	
Rxx:Option:570 Filter High Pass{U16}=0	
Rxx:Option:570 Filter Lowpass{U16}=0	
Rxx:Option:570 Filter Mode{U16}=0	
Rxx:Option:570 Gain Mode{U16}=0	
Rxx:Option:570 Input Offset{U16}=0	
Rxx:Option:570 Input Offset On{Boolean}=False	
Rxx:Option:570 Sensitivity{U16}=0	
Rxx:Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Rxx:Option:SR830 Autogain Lower Threshold{Double Float}=0.100000	
Rxx:Option:SR830 Autogain Standoff{Double Float}=3.000000	
Rxx:Option:SR830 Autogain Upper Threshold{Double Float}=0.900000	
Rxx:Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Rxx:Option:SR830 Settle Time{Double Float}=0.000000	
Rxy::R{Double Float}=8.839287E-6	
Rxy::Theta{Double Float}=-171.248400	
Rxy::X{Double Float}=-8.739715E-6	
Rxy::Y{Double Float}=-1.346599E-6	
Rxy:Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	
Rxy:Option: 560 Enabled{Boolean}=False	
Rxy:Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	
Rxy:Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	
Rxy:Option: Lockin Standoff Time{Double Float}=0.000000	
Rxy:Option: Lockin Type{Enum U16 ((SRS 830,EG&G 5302))}=SRS 830	
Rxy:Option: SR803 Full Scale Reading{Double Float}=0.000000	
Rxy:Option: SR830  Ref Phase{Double Float}=0.000000	
Rxy:Option: SR830  Synch Filter{Boolean}=False	
Rxy:Option: SR830  Time Constant{I16}=8	
Rxy:Option: SR830 2x Line Filter{Boolean}=False	
Rxy:Option: SR830 Adjust Gains{Boolean}=False	
Rxy:Option: SR830 Auto Gain Lower{I32}=0	
Rxy:Option: SR830 Auto Gain Upper{I32}=26	
Rxy:Option: SR830 Auto Offset 1{Boolean}=False	
Rxy:Option: SR830 Auto Offset 2{Boolean}=False	
Rxy:Option: SR830 Autophase{Boolean}=False	
Rxy:Option: SR830 DC Coupling?{Boolean}=False	
Rxy:Option: SR830 Display 1{U16}=0	
Rxy:Option: SR830 Display 2{U16}=1	
Rxy:Option: SR830 Dynamic Reserve{I16}=2	
Rxy:Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Rxy:Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Rxy:Option: SR830 Filter Slope{I32}=3	
Rxy:Option: SR830 Gain{I32}=13	
Rxy:Option: SR830 Ground Shield?{Boolean}=False	
Rxy:Option: SR830 Harmonic{I32}=1	
Rxy:Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A-B	
Rxy:Option: SR830 Line Filter{Boolean}=False	
Rxy:Option: SR830 No Reset{Boolean}=False	
Rxy:Option: SR830 Offset 1{Double Float}=0.000000	
Rxy:Option: SR830 Offset 2{Double Float}=0.000000	
Rxy:Option: SR830 Output Channel 1{Boolean}=False	
Rxy:Option: SR830 Output Channel 2{Boolean}=False	
Rxy:Option: SR830 Ratio 1{U16}=0	
Rxy:Option: SR830 Ratio 2{U16}=0	
Rxy:Option: SR830 Ref Amplitude{Double Float}=0.100000	
Rxy:Option: SR830 Ref Frequency{Double Float}=1013.000000	
Rxy:Option: SR830 Ref Source{Boolean}=False	
Rxy:Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta,X,Y]	
Rxy:Option: SR830 Time Constant value{Double Float}=0.000000	
Rxy:Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Rxy:Option: SR830 VISA{Visa Refnum (Void)}=GPIB0::6::INSTR	
Rxy:Option:560 Comport{Visa Refnum (Void)}=COM1	
Rxy:Option:560 Filter High Pass{U16}=0	
Rxy:Option:560 Filter Lowpass{U16}=0	
Rxy:Option:560 Filter Mode{U16}=0	
Rxy:Option:560 Invert{Boolean}=False	
Rxy:Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Rxy:Option:570 Enabled{Boolean}=False	
Rxy:Option:570 Filter High Pass{U16}=0	
Rxy:Option:570 Filter Lowpass{U16}=0	
Rxy:Option:570 Filter Mode{U16}=0	
Rxy:Option:570 Gain Mode{U16}=0	
Rxy:Option:570 Input Offset{U16}=0	
Rxy:Option:570 Input Offset On{Boolean}=False	
Rxy:Option:570 Sensitivity{U16}=0	
Rxy:Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Rxy:Option:SR830 Autogain Lower Threshold{Double Float}=0.100000	
Rxy:Option:SR830 Autogain Standoff{Double Float}=3.000000	
Rxy:Option:SR830 Autogain Upper Threshold{Double Float}=0.900000	
Rxy:Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Rxy:Option:SR830 Settle Time{Double Float}=0.000000	
Sample ID{String}=MBE202221214_PA_D1 700C Cracker MobvT	
Save:Filename{String}=${X-Y Class} ${2nd Parameter Class} ${iterator}{%04d} ${y}{%04.2g}.txt	
Save:Final Filename{String}=${X-Y Class} ${2nd Parameter Class} .txt	
Save:Final path{Path}=C:\\\\Data\\\\${Project Code}\\\\${User}\\\\${Sample ID}\\\\${Measurement Timestamp}{%Y%m%d}\\\\${X-Y Class}	
Save:Path{Path}=C:\\\\Data\\\\${Project Code}\\\\${User}\\\\${Sample ID}\\\\${Measurement Timestamp}{%Y%m%d}\\\\${X-Y Class}	
Startup path{Path}=C:\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV	
Sub Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Sweep Step{I32}=3	
T Control Measure.__text__{1D Array (String)}=['temperature: T1','temperature: T2','temperature: T3','temperature: T4','temperature: dT/dt']	
Timestamp{Timestamp}=<12:05:57.572 19/05/2023>T	
Toolbar{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Unaved Data{Boolean}=True	
Unsaved Data{Boolean}=False	
User{String}=Craig	
X-Y Class{String}=6221-Lockin-DAQ	
X-Y Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	
d(Offset){Double Float}=0.000000	
d(Rxx::R){Double Float}=2.424350E-19	
d(Rxx::Theta){Double Float}=0.000000	
d(Rxx::X){Double Float}=2.424350E-19	
d(Rxx::Y){Double Float}=0.000000	
d(Rxy::R){Double Float}=6.063093E-9	
d(Rxy::Theta){Double Float}=0.047168	
d(Rxy::X){Double Float}=6.816094E-9	
d(Rxy::Y){Double Float}=6.009452E-9	
iterate result{U16}=5	
iterator{I32}=100	
multi[0]:Control: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values,Adaptive Step Ramp))}=List of Values	
multi[0]:Control: Monitor Update Timeout{Double Float}=0.010000	
multi[0]:Control: Open T Window{Boolean}=False	
multi[0]:Control: Reverse Temperature Sense{Boolean}=False	
multi[0]:Iterator{I32}=0	
multi[0]:Ref: Temperature Window{LVObjVI Refnum (Void)}=	
multi[0]:iterate result{U16}=0	
multi[0]:iterator{I32}=4	
multi[0]:temperature:  rate window{Double Float}=120.000000	
multi[0]:temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[0]:temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':200.000000,'I':70.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':8.000000,'P':150.000000,'I':70.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':12.000000,'P':80.000000,'I':65.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':4,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':25.000000,'P':10.000000,'I':20.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':4,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':50.000000,'P':150.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':4,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':150.000000,'P':70.000000,'I':2.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':5,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':250.000000,'P':115.000000,'I':1.200000,'D':0.000000,'Manual Output':0.000000,'Heater Range':5,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':300.000000,'P':75.000000,'I':1.200000,'D':0.000000,'Manual Output':0.000000,'Heater Range':5,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':300.000000,'P':75.000000,'I':1.200000,'D':0.000000,'Manual Output':0.000000,'Heater Range':5,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':310.000000,'P':1.000000,'I':1.300000,'D':0.000000,'Manual Output':0.000000,'Heater Range':0,'Input Sensor':0,'Ramp Rate':8.000000}]	
multi[0]:temperature: T1{Double Float}=175.108000	
multi[0]:temperature: T2{Double Float}=171.697000	
multi[0]:temperature: T3{Double Float}=93.839500	
multi[0]:temperature: T4{Double Float}=73.561200	
multi[0]:temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
multi[0]:temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
multi[0]:temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
multi[0]:temperature: current temperature{Double Float}=72.727000	
multi[0]:temperature: current temperature 2{Double Float}=287.000000	
multi[0]:temperature: dT/dt{Double Float}=0.071310	
multi[0]:temperature: error{Double Float}=-0.134000	
multi[0]:temperature: gas{Double Float}=175.000000	
multi[0]:temperature: gas control{Boolean}=False	
multi[0]:temperature: gas control 2{Boolean}=False	
multi[0]:temperature: gass boost{I8}=0	
multi[0]:temperature: gass boost 2{I8}=0	
multi[0]:temperature: gast flow{I16}=0	
multi[0]:temperature: gast flow 2{I16}=10	
multi[0]:temperature: heater{Double Float}=4.200000	
multi[0]:temperature: heater output{Double Float}=100.000000	
multi[0]:temperature: heater output 2{Double Float}=0.000000	
multi[0]:temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
multi[0]:temperature: monitor timeout{Double Float}=0.010000	
multi[0]:temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':70.000000,'I':2.000000,'D':0.000000}	
multi[0]:temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
multi[0]:temperature: ramp rate{Double Float}=8.000000	
multi[0]:temperature: ramp rate 2{Double Float}=0.000000	
multi[0]:temperature: ramp target{Double Float}=60.000000	
multi[0]:temperature: ramp target 2{Double Float}=0.000000	
multi[0]:temperature: ramping{Boolean}=False	
multi[0]:temperature: setpoint{Double Float}=80.000000	
multi[0]:temperature: setpoint 2{Double Float}=287.000000	
multi[0]:temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
multi[0]:temperature: stability error{Extended Float}=0.040000	
multi[0]:temperature: stability script{String}=	
multi[0]:temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':1.000000,'temperature:stability rate':0.200000,'temperature:history window':420.000000}	
multi[0]:temperature: temp control mode{U16}=2	
multi[0]:temperature: temp control mode 2{U16}=3	
multi[0]:temperature: temp control mode 2.__text__{String}=Open Loop	
multi[0]:temperature: temp control mode.__text__{String}=Zone	
multi[0]:temperature: temp control sensor{U16}=0	
multi[0]:temperature: temp control sensor 2{U16}=0	
multi[0]:temperature: temp control sensor 2.__text__{String}=Sensor 1	
multi[0]:temperature: temp control sensor.__text__{String}=Sensor A	
multi[0]:temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
multi[0]:temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
multi[0]:temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
multi[0]:temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
multi[0]:temperature: temp loop{U16}=0	
multi[0]:temperature: temp loop 2{U16}=0	
multi[0]:temperature: temp loop 2.__text__{String}=Heater	
multi[0]:temperature: temp loop.__text__{String}=Loop 1	
multi[0]:temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
multi[0]:temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[0]:temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[0]:temperature:error for gas boost{Double Float}=0.000000	
multi[0]:temperature:error for gas boost 2{Double Float}=0.000000	
multi[0]:temperature:heater range{U16}=5	
multi[0]:temperature:heater range 2{U16}=0	
multi[0]:temperature:heater range 2.__text__{String}=Off	
multi[0]:temperature:heater range.__text__{String}=40W	
multi[0]:temperature:history window{Extended Float}=300.000000	
multi[0]:temperature:is stable?{Boolean}=True	
multi[0]:temperature:monitor{Boolean}=True	
multi[0]:temperature:ramping{Boolean}=False	
multi[0]:temperature:ramping on{Boolean}=False	
multi[0]:temperature:ramping on 2{Boolean}=False	
multi[0]:temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
multi[0]:temperature:stability code{U32}=16711680	
multi[0]:temperature:stability rate{Extended Float}=0.040000	
multi[0]:y{Double Float}=175.000000	
multi[1]:Control: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values,Adaptive Step Ramp))}=Multi-Segment Ramp	
multi[1]:Control: Gate delay{Double Float}=0.000000	
multi[1]:Control: Monitor Update Timeout{Double Float}=0.010000	
multi[1]:Control: Open T Window{Boolean}=False	
multi[1]:Control: Reverse Temperature Sense{Boolean}=False	
multi[1]:Control:Magnet Output{Double Float}=-0.000100	
multi[1]:Iterator{I32}=0	
multi[1]:Magnet: Final Switch Heater{Enum U8 ((False,True,Mixed))}=	
multi[1]:Magnet: Power Supply{Enum U16 ((IPS120,LS625,PS110,Hg iPS,SMS Series,Cryomagnetics 4G,DMG Little CryoFree,DMG Big CryoFree))}=Hg iPS	
multi[1]:Magnet: Rate{Double Float}=0.500000	
multi[1]:Magnet: Units{Enum U16 ((Field,Current))}=Field	
multi[1]:Magnet: VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[1]:Multi-segment_Stage{I32}=0	
multi[1]:Multi-segment_Stage_Changed{Boolean}=False	
multi[1]:Ref: Temperature Window{LVObjVI Refnum (Void)}=	
multi[1]:iterate result{U16}=4	
multi[1]:iterator{I32}=21	
multi[1]:measure point{Boolean}=False	
multi[1]:temperature:  rate window{Double Float}=120.000000	
multi[1]:temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[1]:temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':200.000000,'I':70.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':8.000000,'P':150.000000,'I':70.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':12.000000,'P':80.000000,'I':65.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':4,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':25.000000,'P':10.000000,'I':20.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':4,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':50.000000,'P':150.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':4,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':150.000000,'P':70.000000,'I':2.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':5,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':250.000000,'P':115.000000,'I':1.200000,'D':0.000000,'Manual Output':0.000000,'Heater Range':5,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':300.000000,'P':75.000000,'I':1.200000,'D':0.000000,'Manual Output':0.000000,'Heater Range':5,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':300.000000,'P':75.000000,'I':1.200000,'D':0.000000,'Manual Output':0.000000,'Heater Range':5,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':310.000000,'P':1.000000,'I':1.300000,'D':0.000000,'Manual Output':0.000000,'Heater Range':0,'Input Sensor':0,'Ramp Rate':8.000000}]	
multi[1]:temperature: T1{Double Float}=1.842400	
multi[1]:temperature: T2{Double Float}=1.465600	
multi[1]:temperature: T3{Double Float}=86.318100	
multi[1]:temperature: T4{Double Float}=66.769200	
multi[1]:temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
multi[1]:temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
multi[1]:temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
multi[1]:temperature: current temperature{Double Float}=1.657800	
multi[1]:temperature: current temperature 2{Double Float}=287.000000	
multi[1]:temperature: dT/dt{Double Float}=-0.001864	
multi[1]:temperature: error{Double Float}=-0.003000	
multi[1]:temperature: gas{Double Float}=40.000000	
multi[1]:temperature: gas control{Boolean}=False	
multi[1]:temperature: gas control 2{Boolean}=False	
multi[1]:temperature: gass boost{I8}=0	
multi[1]:temperature: gass boost 2{I8}=0	
multi[1]:temperature: gast flow{I16}=0	
multi[1]:temperature: gast flow 2{I16}=10	
multi[1]:temperature: heater{Double Float}=6.200000	
multi[1]:temperature: heater output{Double Float}=0.000000	
multi[1]:temperature: heater output 2{Double Float}=0.000000	
multi[1]:temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
multi[1]:temperature: monitor timeout{Double Float}=1.000000	
multi[1]:temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':200.000000,'I':70.000000,'D':0.000000}	
multi[1]:temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
multi[1]:temperature: ramp rate{Double Float}=8.000000	
multi[1]:temperature: ramp rate 2{Double Float}=0.000000	
multi[1]:temperature: ramp target{Double Float}=0.000000	
multi[1]:temperature: ramp target 2{Double Float}=0.000000	
multi[1]:temperature: ramping{Boolean}=False	
multi[1]:temperature: setpoint{Double Float}=1.600000	
multi[1]:temperature: setpoint 2{Double Float}=287.000000	
multi[1]:temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
multi[1]:temperature: stability error{Extended Float}=0.040000	
multi[1]:temperature: stability script{String}=	
multi[1]:temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.100000,'temperature:history window':420.000000}	
multi[1]:temperature: temp control mode{U16}=2	
multi[1]:temperature: temp control mode 2{U16}=3	
multi[1]:temperature: temp control mode 2.__text__{String}=Open Loop	
multi[1]:temperature: temp control mode.__text__{String}=Zone	
multi[1]:temperature: temp control sensor{U16}=0	
multi[1]:temperature: temp control sensor 2{U16}=0	
multi[1]:temperature: temp control sensor 2.__text__{String}=Sensor 1	
multi[1]:temperature: temp control sensor.__text__{String}=Sensor A	
multi[1]:temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
multi[1]:temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
multi[1]:temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
multi[1]:temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
multi[1]:temperature: temp loop{U16}=0	
multi[1]:temperature: temp loop 2{U16}=0	
multi[1]:temperature: temp loop 2.__text__{String}=Heater	
multi[1]:temperature: temp loop.__text__{String}=Loop 1	
multi[1]:temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
multi[1]:temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[1]:temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[1]:temperature:error for gas boost{Double Float}=0.000000	
multi[1]:temperature:error for gas boost 2{Double Float}=0.000000	
multi[1]:temperature:heater range{U16}=4	
multi[1]:temperature:heater range 2{U16}=0	
multi[1]:temperature:heater range 2.__text__{String}=Off	
multi[1]:temperature:heater range.__text__{String}=4W	
multi[1]:temperature:history window{Extended Float}=300.000000	
multi[1]:temperature:is stable?{Boolean}=False	
multi[1]:temperature:monitor{Boolean}=True	
multi[1]:temperature:ramping{Boolean}=False	
multi[1]:temperature:ramping on{Boolean}=False	
multi[1]:temperature:ramping on 2{Boolean}=False	
multi[1]:temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
multi[1]:temperature:stability code{U32}=16860	
multi[1]:temperature:stability rate{Extended Float}=0.040000	
multi[1]:y{Double Float}=0.000000	
parameter: Termination{String}=False	
parameter: delta time{Double Float}=1.000000	
parameter: progress{Double Float}=100.000000	
temperature:  rate window{Double Float}=120.000000	
temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':200.000000,'I':70.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':8.000000,'P':150.000000,'I':70.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':12.000000,'P':80.000000,'I':65.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':4,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':25.000000,'P':10.000000,'I':20.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':4,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':50.000000,'P':150.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':4,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':150.000000,'P':70.000000,'I':2.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':5,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':250.000000,'P':115.000000,'I':1.200000,'D':0.000000,'Manual Output':0.000000,'Heater Range':5,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':300.000000,'P':75.000000,'I':1.200000,'D':0.000000,'Manual Output':0.000000,'Heater Range':5,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':300.000000,'P':75.000000,'I':1.200000,'D':0.000000,'Manual Output':0.000000,'Heater Range':5,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':310.000000,'P':1.000000,'I':1.300000,'D':0.000000,'Manual Output':0.000000,'Heater Range':0,'Input Sensor':0,'Ramp Rate':8.000000}]	
temperature: T1{Double Float}=175.108000	
temperature: T2{Double Float}=171.697000	
temperature: T3{Double Float}=93.839500	
temperature: T4{Double Float}=73.561200	
temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
temperature: current temperature{Double Float}=72.727000	
temperature: current temperature 2{Double Float}=287.000000	
temperature: dT/dt{Double Float}=0.071310	
temperature: gas control{Boolean}=False	
temperature: gas control 2{Boolean}=False	
temperature: gass boost{I8}=0	
temperature: gass boost 2{I8}=0	
temperature: gast flow{I16}=0	
temperature: gast flow 2{I16}=10	
temperature: heater output{Double Float}=100.000000	
temperature: heater output 2{Double Float}=0.000000	
temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
temperature: monitor timeout{Double Float}=0.010000	
temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':70.000000,'I':2.000000,'D':0.000000}	
temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
temperature: ramp rate{Double Float}=8.000000	
temperature: ramp rate 2{Double Float}=0.000000	
temperature: ramp target{Double Float}=60.000000	
temperature: ramp target 2{Double Float}=0.000000	
temperature: ramping{Boolean}=False	
temperature: setpoint{Double Float}=80.000000	
temperature: setpoint 2{Double Float}=287.000000	
temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
temperature: stability error{Extended Float}=0.040000	
temperature: stability script{String}=	
temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':1.000000,'temperature:stability rate':0.200000,'temperature:history window':420.000000}	
temperature: temp control mode{U16}=2	
temperature: temp control mode 2{U16}=3	
temperature: temp control mode 2.__text__{String}=Open Loop	
temperature: temp control mode.__text__{String}=Zone	
temperature: temp control sensor{U16}=0	
temperature: temp control sensor 2{U16}=0	
temperature: temp control sensor 2.__text__{String}=Sensor 1	
temperature: temp control sensor.__text__{String}=Sensor A	
temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
temperature: temp loop{U16}=0	
temperature: temp loop 2{U16}=0	
temperature: temp loop 2.__text__{String}=Heater	
temperature: temp loop.__text__{String}=Loop 1	
temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
temperature:error for gas boost{Double Float}=0.000000	
temperature:error for gas boost 2{Double Float}=0.000000	
temperature:heater range{U16}=5	
temperature:heater range 2{U16}=0	
temperature:heater range 2.__text__{String}=Off	
temperature:heater range.__text__{String}=40W	
temperature:history window{Extended Float}=300.000000	
temperature:is stable?{Boolean}=True	
temperature:monitor{Boolean}=True	
temperature:ramping{Boolean}=False	
temperature:ramping on{Boolean}=False	
temperature:ramping on 2{Boolean}=False	
temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
temperature:stability code{U32}=16711680	
temperature:stability rate{Extended Float}=0.040000	
y{Double Float}=175.000000	
