TDI Format 1.5	Offset	Rxx::R	Rxx::Theta	Rxx::X	Rxx::Y	Rxy::R	Rxy::Theta	Rxy::X	Rxy::Y	temperature: T1	temperature: T2	temperature: T3	temperature: T4	temperature: dT/dt	iterator	multi[0]:iterator	multi[0]:y	multi[0]:temperature: setpoint	multi[0]:temperature: T1	multi[0]:temperature: T2	multi[0]:temperature: T3	multi[0]:temperature: T4	multi[0]:temperature: heater	multi[0]:temperature: gas	multi[0]:temperature: dT/dt	multi[0]:temperature: current temperature	multi[0]:temperature: error	multi[1]:iterator	multi[1]:y	multi[1]:Control:Magnet Output
2nd Parameter Class{String}=Multi-Parameter	0E+0	1.228333574E-3	1.56E-1	1.228333574E-3	3.371767975E-6	5.921657254E-7	-6.756E+0	5.879510861E-7	-7.112314765E-8	1.0044E+1	9.934E+0	8.59599E+1	6.39289E+1	2.17702277E-2	4.49E+2	8E+0	1E+1	1E+1	1.0023E+1	9.926E+0	8.59241E+1	6.39289E+1	2.3E+0	1E+1	9.855110198E-3	1.0025E+1	-2.5E-2	0E+0	0E+0	0E+0
2nd Parameter Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	0E+0	1.232209934E-3	1.524E-1	1.232209934E-3	3.270614936E-6	7.150252458E-6	-4.608E-1	7.150252458E-6	-5.900591129E-8	1.0021E+1	9.9247E+0	8.63539E+1	6.39289E+1	-9.073426016E-3	4.5E+2	8E+0	1E+1	1.8E+0	1.0044E+1	9.934E+0	8.59599E+1	6.39289E+1	2.3E+0	1E+1	2.17702277E-2	1.4649E+0	-2.5E-2	1E+0	5E-1	4.999E-1
Analysis Class{String}=Basic Plot	0E+0	1.236255999E-3	1.56E-1	1.236255999E-3	3.371767975E-6	1.369306342E-5	-2.172E-1	1.369306342E-5	-5.37375415E-8	9.9867E+0	9.9216E+0	8.62106E+1	6.39289E+1	-1.147866156E-2	4.51E+2	8E+0	1E+1	1.8E+0	1.0021E+1	9.9247E+0	8.63539E+1	6.39289E+1	2.3E+0	1E+1	-9.073426016E-3	1.4649E+0	-2.5E-2	2E+0	1E+0	9.999E-1
Analysis Class Path{Path}=C\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV\\\\plugins\\\\Plotting\\\\Plotting_Base_class\\\\Plotting_Base.lvclass	0E+0	1.242157512E-3	1.56E-1	1.242157512E-3	3.371767975E-6	2.028327317E-5	-1.008E-1	2.028327317E-5	-3.635182222E-8	1.0007E+1	9.9194E+0	8.58524E+1	6.39289E+1	-1.401203964E-2	4.52E+2	8E+0	1E+1	1.8E+0	9.9867E+0	9.9216E+0	8.62106E+1	6.39289E+1	2.3E+0	1E+1	-1.147866156E-2	1.4649E+0	-2.5E-2	3E+0	1.5E+0	1.4999E+0
Analysis.# pre-routines{I32}=5	0E+0	1.242157512E-3	1.548E-1	1.242157512E-3	3.338050296E-6	2.028378228E-5	-9E-2	2.028378228E-5	-3.319080035E-8	1.0019E+1	9.9254E+0	8.58524E+1	6.39289E+1	-4.132336937E-3	4.53E+2	8E+0	1E+1	1.8E+0	1.0007E+1	9.9194E+0	8.58524E+1	6.39289E+1	2.3E+0	1E+1	-1.401203964E-2	1.4649E+0	-2.5E-2	4E+0	1.5E+0	1.5E+0
Analysis:Pre[0]:T Control Measure{1D Array (I32)}=[1,2,3,4,7]	0E+0	1.239459192E-3	1.56E-1	1.239459192E-3	3.371767975E-6	1.76248628E-5	-1.824E-1	1.76248628E-5	-5.742538621E-8	1.001E+1	9.9205E+0	8.65688E+1	6.39289E+1	-4.728003871E-3	4.54E+2	8E+0	1E+1	1.8E+0	1.0019E+1	9.9254E+0	8.58524E+1	6.39289E+1	2.3E+0	1E+1	-4.132336937E-3	1.4649E+0	-2.5E-2	5E+0	1.3E+0	1.3002E+0
Autosave Tabs{Enum U32 ((XY Measurement Save,Parameter Plot Save 2))}=Parameter Plot Save 2	0E+0	1.237268576E-3	1.56E-1	1.237268576E-3	3.371767975E-6	1.498701509E-5	-1.596E-1	1.498701509E-5	-4.320077365E-8	9.9753E+0	9.9053E+0	8.6533E+1	6.39289E+1	-3.255028278E-2	4.55E+2	8E+0	1E+1	1.8E+0	1.001E+1	9.9205E+0	8.65688E+1	6.39289E+1	2.3E+0	1E+1	-4.728003871E-3	1.4649E+0	-2.5E-2	6E+0	1.1E+0	1.1001E+0
Control:Magnet Output{Double Float}=-0.007000	0E+0	1.235413127E-3	1.56E-1	1.235413127E-3	3.371767975E-6	1.238598785E-5	-2.28E-1	1.238598785E-5	-5.004966851E-8	9.9796E+0	9.9103E+0	8.64613E+1	6.39289E+1	-2.760135755E-2	4.56E+2	8E+0	1E+1	1.8E+0	9.9753E+0	9.9053E+0	8.6533E+1	6.39289E+1	2.3E+0	1E+1	-3.255028278E-2	1.4649E+0	-2.5E-2	7E+0	9E-1	9.001E-1
Control:Magnet Rate{Double Float}=0.500000	0E+0	1.233727385E-3	1.548E-1	1.233727385E-3	3.338050296E-6	9.76388317E-6	-3.672E-1	9.76388317E-6	-6.374742995E-8	9.9872E+0	9.9148E+0	8.64613E+1	6.35264E+1	-1.909100264E-2	4.57E+2	8E+0	1E+1	1.8E+0	9.9796E+0	9.9103E+0	8.64613E+1	6.39289E+1	2.3E+0	1E+1	-2.760135755E-2	1.4649E+0	-2.5E-2	8E+0	7E-1	7.001E-1
Display Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	0E+0	1.232209934E-3	1.56E-1	1.232209934E-3	3.371767975E-6	7.137083301E-6	-5.376E-1	7.137083301E-6	-6.796209749E-8	9.9932E+0	9.9194E+0	8.58883E+1	6.35264E+1	-1.24126086E-2	4.58E+2	8E+0	1E+1	1.8E+0	9.9872E+0	9.9148E+0	8.64613E+1	6.35264E+1	2.3E+0	1E+1	-1.909100264E-2	1.4649E+0	-2.5E-2	9E+0	5E-1	5E-1
Elapsed Time{Double Float}=12790.950867	0E+0	1.23103048E-3	1.56E-1	1.23103048E-3	3.304332616E-6	4.513422986E-6	-7.728E-1	4.513422986E-6	-6.216690487E-8	1.0002E+1	9.927E+0	8.55301E+1	6.35264E+1	4.766650964E-3	4.59E+2	8E+0	1E+1	1.8E+0	9.9932E+0	9.9194E+0	8.58883E+1	6.35264E+1	2.3E+0	1E+1	-1.24126086E-2	1.4649E+0	-2.5E-2	1E+1	3E-1	3.001E-1
File:Autodel{Boolean}=True	0E+0	1.229513028E-3	1.56E-1	1.229513028E-3	3.371767975E-6	1.879758525E-6	-2.1084E+0	1.878177434E-6	-7.059629653E-8	9.9941E+0	9.9264E+0	8.65688E+1	6.35264E+1	-1.238453668E-3	4.6E+2	8E+0	1E+1	1.8E+0	1.0002E+1	9.927E+0	8.55301E+1	6.35264E+1	2.3E+0	1E+1	4.766650964E-3	1.4649E+0	-2.5E-2	1.1E+1	1E-1	1.001E-1
File:Autosave{Boolean}=False	0E+0	1.229546687E-3	1.56E-1	1.229546687E-3	3.338050296E-6	1.885027885E-6	-2.1492E+0	1.882917878E-6	-7.164997048E-8	9.99E+0	9.9215E+0	8.6533E+1	6.35264E+1	-9.127479978E-3	4.61E+2	8E+0	1E+1	1.8E+0	9.9941E+0	9.9264E+0	8.65688E+1	6.35264E+1	2.3E+0	1E+1	-1.238453668E-3	1.4649E+0	-2.5E-2	1.2E+1	1E-1	1E-1
File:Export Config{Boolean}=True	0E+0	1.229513028E-3	1.56E-1	1.229513028E-3	3.371767975E-6	1.745416722E-6	-2.5212E+0	1.743835631E-6	-7.849892191E-8	1.0007E+1	9.9272E+0	8.64613E+1	6.35264E+1	-5.917989765E-4	4.62E+2	8E+0	1E+1	1.8E+0	9.99E+0	9.9215E+0	8.6533E+1	6.35264E+1	2.3E+0	1E+1	-9.127479978E-3	1.4649E+0	-2.5E-2	1.3E+1	9E-2	9E-2
File:Final Autosave{Boolean}=True	0E+0	1.229344737E-3	1.56E-1	1.229344737E-3	3.371767975E-6	1.614234272E-6	-2.8092E+0	1.611601006E-6	-8.060635468E-8	1.0005E+1	9.9286E+0	8.64255E+1	6.35264E+1	1.513763797E-3	4.63E+2	8E+0	1E+1	1.8E+0	1.0007E+1	9.9272E+0	8.64613E+1	6.35264E+1	2.3E+0	1E+1	-5.917989765E-4	1.4649E+0	-2.5E-2	1.4E+1	8E-2	8.01E-2
Filter:Enable{Enum U16 ((None,Analog,Digital,Analog&Digitial))}=None	0E+0	1.229344737E-3	1.56E-1	1.229344737E-3	3.338050296E-6	1.482525734E-6	-3.1896E+0	1.479892469E-6	-8.376723513E-8	9.9996E+0	9.9265E+0	8.63897E+1	6.35264E+1	-2.24834308E-3	4.64E+2	8E+0	1E+1	1.8E+0	1.0005E+1	9.9286E+0	8.64255E+1	6.35264E+1	2.3E+0	1E+1	1.513763797E-3	1.4649E+0	-2.5E-2	1.5E+1	7E-2	7.01E-2
Filter:Points{I32}=1	0E+0	1.229176446E-3	1.56E-1	1.229176446E-3	3.338050296E-6	1.356084294E-6	-3.6276E+0	1.353449897E-6	-8.692837014E-8	1.0009E+1	9.9335E+0	8.63539E+1	6.35264E+1	8.334265091E-3	4.65E+2	8E+0	1E+1	1.8E+0	9.9996E+0	9.9265E+0	8.63897E+1	6.35264E+1	2.3E+0	1E+1	-2.24834308E-3	1.4649E+0	-2.5E-2	1.6E+1	6E-2	6.01E-2
Filter:Type{U16}=1	0E+0	1.22900674E-3	1.56E-1	1.22900674E-3	3.338050296E-6	1.219629656E-6	-3.2784E+0	1.217522195E-6	-7.112320421E-8	1.0006E+1	9.9323E+0	8.63539E+1	6.35264E+1	7.981752977E-3	4.66E+2	8E+0	1E+1	1.8E+0	1.0009E+1	9.9335E+0	8.63539E+1	6.35264E+1	2.3E+0	1E+1	8.334265091E-3	1.4649E+0	-2.5E-2	1.7E+1	5E-2	5.01E-2
Filter:Type.__text__{String}=Repeat	0E+0	1.22900674E-3	1.56E-1	1.22900674E-3	3.371767975E-6	1.218576066E-6	-4.254E+0	1.215414451E-6	-9.219682477E-8	1.0005E+1	9.9323E+0	8.63539E+1	6.35264E+1	8.118379861E-3	4.67E+2	8E+0	1E+1	1.8E+0	1.0006E+1	9.9323E+0	8.63539E+1	6.35264E+1	2.3E+0	1E+1	7.981752977E-3	1.4649E+0	-2.5E-2	1.8E+1	5E-2	5E-2
Filter:Window{Double Float}=1.000000	0E+0	1.22900674E-3	1.56E-1	1.22900674E-3	3.371767975E-6	1.150087118E-6	-4.53E+0	1.146399415E-6	-9.166994537E-8	1.0003E+1	9.9298E+0	8.63539E+1	6.35264E+1	2.996569965E-3	4.68E+2	8E+0	1E+1	1.8E+0	1.0005E+1	9.9323E+0	8.63539E+1	6.35264E+1	2.3E+0	1E+1	8.118379861E-3	1.4649E+0	-2.5E-2	1.9E+1	4.5E-2	4.49E-2
Iterator{I32}=0	0E+0	1.228838449E-3	1.56E-1	1.228838449E-3	3.371767975E-6	1.078964621E-6	-4.302E+0	1.076330507E-6	-8.271367431E-8	1.001E+1	9.9314E+0	8.63539E+1	6.35264E+1	2.391766291E-3	4.69E+2	8E+0	1E+1	1.8E+0	1.0003E+1	9.9298E+0	8.63539E+1	6.35264E+1	2.3E+0	1E+1	2.996569965E-3	1.4649E+0	-2.5E-2	2E+1	4E-2	3.99E-2
Magnet: Control Mode{Boolean}=False	0E+0	1.228838449E-3	1.56E-1	1.228838449E-3	3.338050296E-6	1.018905234E-6	-4.6416E+0	1.014690877E-6	-8.429419939E-8	1.0004E+1	9.9337E+0	8.63181E+1	6.35264E+1	4.680385347E-3	4.7E+2	8E+0	1E+1	1.8E+0	1.001E+1	9.9314E+0	8.63539E+1	6.35264E+1	2.3E+0	1E+1	2.391766291E-3	1.4649E+0	-2.5E-2	2.1E+1	3.5E-2	3.5E-2
Magnet: Final Switch Heater{Enum U8 ((False,True,Mixed))}=	0E+0	1.228838449E-3	1.56E-1	1.228838449E-3	3.371767975E-6	9.630604855E-7	-4.9368E+0	9.593724994E-7	-8.429419939E-8	1.0002E+1	9.9322E+0	8.63181E+1	6.35264E+1	8.721182821E-4	4.71E+2	8E+0	1E+1	1.8E+0	1.0004E+1	9.9337E+0	8.63181E+1	6.35264E+1	2.3E+0	1E+1	4.680385347E-3	1.4649E+0	-2.5E-2	2.2E+1	3E-2	3E-2
Magnet: Power Supply{Enum U16 ((IPS120,LS625,PS110,Hg iPS,SMS Series,Cryomagnetics 4G,DMG Little CryoFree,DMG Big CryoFree))}=Hg iPS	0E+0	1.228670157E-3	1.56E-1	1.228670157E-3	3.338050296E-6	8.893035914E-7	-5.4792E+0	8.84562299E-7	-8.587469618E-8	1.0003E+1	9.9318E+0	8.63181E+1	6.35264E+1	2.139129065E-4	4.72E+2	8E+0	1E+1	1.8E+0	1.0002E+1	9.9322E+0	8.63181E+1	6.35264E+1	2.3E+0	1E+1	8.721182821E-4	1.4649E+0	-2.5E-2	2.3E+1	2.5E-2	2.51E-2
Magnet: Rate{Double Float}=0.500000	0E+0	1.228670157E-3	1.56E-1	1.228670157E-3	3.338050296E-6	8.308250121E-7	-6.1272E+0	8.255567837E-7	-9.008942029E-8	1.0005E+1	9.934E+0	8.63181E+1	6.35264E+1	3.633366432E-3	4.73E+2	8E+0	1E+1	1.8E+0	1.0003E+1	9.9318E+0	8.63181E+1	6.35264E+1	2.3E+0	1E+1	2.139129065E-4	1.4649E+0	-2.5E-2	2.4E+1	2E-2	1.99E-2
Magnet: Setpoint{Double Float}=0.000000	0E+0	1.228569182E-3	1.56E-1	1.228569182E-3	3.371767975E-6	7.549606569E-7	-5.9292E+0	7.502187988E-7	-7.955262415E-8	1.0003E+1	9.933E+0	8.63181E+1	6.35264E+1	1.76800834E-3	4.74E+2	8E+0	1E+1	1.8E+0	1.0005E+1	9.934E+0	8.63181E+1	6.35264E+1	2.3E+0	1E+1	3.633366432E-3	1.4649E+0	-2.5E-2	2.5E+1	1.5E-2	1.5E-2
Magnet: Units{Enum U16 ((Field,Current))}=Field	0E+0	1.228501866E-3	1.56E-1	1.228501866E-3	3.338050296E-6	6.949015525E-7	-7.1952E+0	6.901596944E-7	-8.850889521E-8	1.0009E+1	9.9368E+0	8.63539E+1	6.35264E+1	5.588065833E-3	4.75E+2	8E+0	1E+1	1.8E+0	1.0003E+1	9.933E+0	8.63181E+1	6.35264E+1	2.3E+0	1E+1	1.76800834E-3	1.4649E+0	-2.5E-2	2.6E+1	1E-2	1E-2
Magnet: VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	0E+0	1.228434549E-3	1.56E-1	1.228434549E-3	3.371767975E-6	6.269369942E-7	-7.2468E+0	6.221951362E-7	-8.060629811E-8	9.9893E+0	9.9348E+0	8.56375E+1	6.35264E+1	1.518374425E-3	4.76E+2	8E+0	1E+1	1.8E+0	1.0009E+1	9.9368E+0	8.63539E+1	6.35264E+1	2.3E+0	1E+1	5.588065833E-3	1.4649E+0	-2.5E-2	2.7E+1	5E-3	5E-3
Main Screen Path{Path}=C:\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV\\\\1Code.vi	0E+0	1.228333574E-3	1.56E-1	1.228333574E-3	3.304332616E-6	5.605557895E-7	-9.5988E+0	5.537064704E-7	-9.535787493E-8	1E+1	9.9313E+0	8.56017E+1	6.35264E+1	-3.978260793E-3	4.77E+2	8E+0	1E+1	1.8E+0	9.9893E+0	9.9348E+0	8.56375E+1	6.35264E+1	2.3E+0	1E+1	1.518374425E-3	1.4649E+0	-2.5E-2	2.8E+1	0E+0	-2E-4
Measurement Timestamp{Timestamp}=<23:23:44.673 17/05/2023>T	0E+0	1.228501866E-3	1.56E-1	1.228501866E-3	3.371767975E-6	4.989155943E-7	-9.654E+0	4.910135346E-7	-8.534790163E-8	1.0004E+1	9.9353E+0	8.56017E+1	6.35264E+1	7.457330939E-4	4.78E+2	8E+0	1E+1	1.8E+0	1E+1	9.9313E+0	8.56017E+1	6.35264E+1	2.3E+0	1E+1	-3.978260793E-3	1.4649E+0	-2.5E-2	2.9E+1	-5E-3	-5E-3
Measurement Title{String}=	0E+0	1.228501866E-3	1.56E-1	1.228501866E-3	3.338050296E-6	4.304274943E-7	-1.00596E+1	4.23051522E-7	-7.639146086E-8	1.0021E+1	9.9536E+0	8.54943E+1	6.35264E+1	2.577592432E-2	4.79E+2	8E+0	1E+1	1.8E+0	1.0004E+1	9.9353E+0	8.56017E+1	6.35264E+1	2.3E+0	1E+1	7.457330939E-4	1.4649E+0	-2.5E-2	3E+1	-1E-2	-1.01E-2
Measurment Select{U16}=4	0E+0	1.228670157E-3	1.56E-1	1.228670157E-3	3.371767975E-6	3.677339928E-7	-1.23552E+1	3.587774955E-7	-8.060635468E-8	9.9944E+0	9.9303E+0	8.54226E+1	6.35264E+1	-1.05599761E-2	4.8E+2	8E+0	1E+1	1.8E+0	1.0021E+1	9.9536E+0	8.54943E+1	6.35264E+1	2.3E+0	1E+1	2.577592432E-2	1.4649E+0	-2.5E-2	3.1E+1	-1.5E-2	-1.51E-2
Measurment Select.__text__{String}=6221-Lockin-DAQ	0E+0	1.228670157E-3	1.56E-1	1.228670157E-3	3.304332616E-6	2.960828627E-7	-1.6092E+1	2.84492534E-7	-8.429425595E-8	9.9959E+0	9.9313E+0	8.54585E+1	6.35264E+1	-9.841587394E-3	4.81E+2	8E+0	1E+1	1.8E+0	9.9944E+0	9.9303E+0	8.54226E+1	6.35264E+1	2.3E+0	1E+1	-1.05599761E-2	1.4649E+0	-2.5E-2	3.2E+1	-2E-2	-2.01E-2
Notes{String}=I+1A I-1E\\nrxx+1B Rxx-1C\\nRxy+1D Rxy-4A	0E+0	1.228670157E-3	1.56E-1	1.228670157E-3	3.371767975E-6	2.318088362E-7	-2.00808E+1	2.186382653E-7	-8.113303609E-8	1E+1	9.9333E+0	8.66046E+1	6.35264E+1	-3.634780413E-3	4.82E+2	8E+0	1E+1	1.8E+0	9.9959E+0	9.9313E+0	8.54585E+1	6.35264E+1	2.3E+0	1E+1	-9.841587394E-3	1.4649E+0	-2.5E-2	3.3E+1	-2.5E-2	-2.5E-2
Offset{Double Float}=0.000000	0E+0	1.228838449E-3	1.56E-1	1.228838449E-3	3.371767975E-6	1.691153347E-7	-2.7222E+1	1.501490338E-7	-7.955262415E-8	1.0008E+1	9.9362E+0	8.65688E+1	6.35264E+1	-4.184559803E-4	4.83E+2	8E+0	1E+1	1.8E+0	1E+1	9.9333E+0	8.66046E+1	6.35264E+1	2.3E+0	1E+1	-3.634780413E-3	1.4649E+0	-2.5E-2	3.4E+1	-3E-2	-3.01E-2
Option: 2182 Autozero{Boolean}=True	0E+0	1.228838449E-3	1.56E-1	1.228838449E-3	3.371767975E-6	1.190655248E-7	-3.9192E+1	9.167003022E-8	-7.691836855E-8	9.9998E+0	9.9336E+0	8.64971E+1	6.35264E+1	-5.406955257E-3	4.84E+2	8E+0	1E+1	1.8E+0	1.0008E+1	9.9362E+0	8.65688E+1	6.35264E+1	2.3E+0	1E+1	-4.184559803E-4	1.4649E+0	-2.5E-2	3.5E+1	-3.5E-2	-3.51E-2
Option: 2182 Front Autozero{Boolean}=True	0E+0	1.228939423E-3	1.56E-1	1.228939423E-3	3.371767975E-6	8.060635468E-8	-7.04724E+1	2.52882485E-8	-7.84989502E-8	1.0003E+1	9.9351E+0	8.64971E+1	6.35264E+1	-2.939595375E-3	4.85E+2	8E+0	1E+1	1.8E+0	9.9998E+0	9.9336E+0	8.64971E+1	6.35264E+1	2.3E+0	1E+1	-5.406955257E-3	1.4649E+0	-2.5E-2	3.6E+1	-4E-2	-4.04E-2
Option: 2182 Hold{Boolean}=False	0E+0	1.22900674E-3	1.56E-1	1.22900674E-3	3.371767975E-6	9.061629969E-8	-1.18698E+2	-4.530812156E-8	-8.21867949E-8	1.0003E+1	9.9362E+0	8.64613E+1	6.35264E+1	5.505141802E-3	4.86E+2	8E+0	1E+1	1.8E+0	1.0003E+1	9.9351E+0	8.64971E+1	6.35264E+1	2.3E+0	1E+1	-2.939595375E-3	1.4649E+0	-2.5E-2	3.7E+1	-4.5E-2	-4.52E-2
Option: 2182 Hold Count{I32}=10	0E+0	1.22900674E-3	1.56E-1	1.22900674E-3	3.371767975E-6	1.390850754E-7	-1.425288E+2	-1.1221663E-7	-8.692845499E-8	1.0001E+1	9.9346E+0	8.64613E+1	6.35264E+1	1.992781647E-3	4.87E+2	8E+0	1E+1	1.8E+0	1.0003E+1	9.9362E+0	8.64613E+1	6.35264E+1	2.3E+0	1E+1	5.505141802E-3	1.4649E+0	-2.5E-2	3.8E+1	-5E-2	-5E-2
Option: 2182 Hold Window{Double Float}=1.000000	0E+0	1.22900674E-3	1.56E-1	1.22900674E-3	3.371767975E-6	1.343436133E-7	-1.411632E+2	-1.074751396E-7	-8.745527782E-8	1.0004E+1	9.9353E+0	8.64613E+1	6.35264E+1	2.713253023E-3	4.88E+2	8E+0	1E+1	1.8E+0	1.0001E+1	9.9346E+0	8.64613E+1	6.35264E+1	2.3E+0	1E+1	1.992781647E-3	1.4649E+0	-2.5E-2	3.9E+1	-5E-2	-5E-2
Option: 2182 Line Sync{Boolean}=False	0E+0	1.229176446E-3	1.56E-1	1.229176446E-3	3.371767975E-6	2.412919866E-7	-1.630932E+2	-2.328624253E-7	-7.164999877E-8	1.0004E+1	9.9372E+0	8.64255E+1	6.35264E+1	4.208271857E-3	4.89E+2	8E+0	1E+1	1.8E+0	1.0004E+1	9.9353E+0	8.64613E+1	6.35264E+1	2.3E+0	1E+1	2.713253023E-3	1.4649E+0	-2.5E-2	4E+1	-6E-2	-6E-2
Option: 2182 Reference Reading{Double Float}=0.000000	0E+0	1.229344737E-3	1.56E-1	1.229344737E-3	3.371767975E-6	3.840661796E-7	-1.680936E+2	-3.787971027E-7	-8.166002864E-8	1.003E+1	9.9443E+0	8.64613E+1	6.35264E+1	1.374273188E-2	4.9E+2	8E+0	1E+1	1.8E+0	1.0004E+1	9.9372E+0	8.64255E+1	6.35264E+1	2.3E+0	1E+1	4.208271857E-3	1.4649E+0	-2.5E-2	4.1E+1	-7E-2	-7E-2
Option: 2182 Relative Mode{Boolean}=False	0E+0	1.229513028E-3	1.56E-1	1.229513028E-3	3.371767975E-6	5.036574524E-7	-1.70316E+2	-4.989158772E-7	-8.640151901E-8	1.0109E+1	9.9854E+0	8.64613E+1	6.35264E+1	7.44119063E-2	4.91E+2	8E+0	1E+1	1.8E+0	1.003E+1	9.9443E+0	8.64613E+1	6.35264E+1	2.3E+0	1E+1	1.374273188E-2	1.4649E+0	-2.5E-2	4.2E+1	-8E-2	-8E-2
Option: 2182 Trigger Delay{Cluster (Boolean,Double Float)}={'Auto':True,'Time(s)':0.000000}	0E+0	1.229580345E-3	1.56E-1	1.229580345E-3	3.371767975E-6	6.300980444E-7	-1.73088E+2	-6.279905833E-7	-7.691836855E-8	1.0373E+1	1.0103E+1	8.64613E+1	6.35264E+1	2.42753759E-1	4.92E+2	8E+0	1E+1	1.8E+0	1.0109E+1	9.9854E+0	8.64613E+1	6.35264E+1	2.3E+0	1E+1	7.44119063E-2	1.4649E+0	-2.5E-2	4.3E+1	-9E-2	-8.99E-2
Option: 2182 Trigger Source{Enum U16 ((Immediate,Timer,Manual,Bus,Trigger link))}=Bus	0E+0	1.22968132E-3	1.56E-1	1.22968132E-3	3.371767975E-6	7.581214242E-7	-1.730856E+2	-7.54960374E-7	-9.272370418E-8	1.023E+1	1.0117E+1	8.64613E+1	6.35264E+1	2.473613471E-1	4.93E+2	8E+0	1E+1	1.8E+0	1.0373E+1	1.0103E+1	8.64613E+1	6.35264E+1	2.3E+0	1E+1	2.42753759E-1	1.4649E+0	-2.5E-2	4.4E+1	-1E-1	-9.99E-2
Option: 2182 Trigger Timer{Double Float}=0.000000	0E+0	1.22968132E-3	1.56E-1	1.22968132E-3	3.338050296E-6	7.560145288E-7	-1.739664E+2	-7.539070678E-7	-8.113314923E-8	1.0141E+1	1.0092E+1	8.64255E+1	6.35264E+1	1.974149495E-1	4.94E+2	8E+0	1E+1	1.8E+0	1.023E+1	1.0117E+1	8.64613E+1	6.35264E+1	2.3E+0	1E+1	2.473613471E-1	1.4649E+0	-2.5E-2	4.5E+1	-1E-1	-1E-1
Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	0E+0	1.230862188E-3	1.56E-1	1.230862188E-3	3.371767975E-6	3.371770804E-6	-1.784952E+2	-3.372822979E-6	-9.061627141E-8	9.7305E+0	9.6296E+0	8.64255E+1	6.35264E+1	-5.584072471E-1	4.95E+2	8E+0	1E+1	1.8E+0	1.0141E+1	1.0092E+1	8.64255E+1	6.35264E+1	2.3E+0	1E+1	1.974149495E-1	1.4649E+0	-2.5E-2	4.6E+1	-3E-1	-2.999E-1
Option: 560 Enabled{Boolean}=False	0E+0	1.232176275E-3	1.56E-1	1.232176275E-3	3.371767975E-6	5.989103927E-6	-1.791612E+2	-5.991742849E-6	-8.903577462E-8	9.9615E+0	9.8513E+0	8.54585E+1	6.35264E+1	1.910625398E-1	4.96E+2	8E+0	1E+1	1.8E+0	9.7305E+0	9.6296E+0	8.64255E+1	6.35264E+1	2.3E+0	1E+1	-5.584072471E-1	1.4649E+0	-2.5E-2	4.7E+1	-5E-1	-4.999E-1
Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	0E+0	1.233559093E-3	1.56E-1	1.233559093E-3	3.371767975E-6	8.600104202E-6	-1.793148E+2	-8.602737467E-6	-1.037872666E-7	1.0028E+1	9.9146E+0	8.66762E+1	6.35264E+1	1.63613975E-1	4.97E+2	8E+0	1E+1	1.8E+0	9.9615E+0	9.8513E+0	8.54585E+1	6.35264E+1	2.3E+0	1E+1	1.910625398E-1	1.4649E+0	-2.5E-2	4.8E+1	-7E-1	-7E-1
Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	0E+0	1.235244836E-3	1.56E-1	1.235244836E-3	3.371767975E-6	1.121483234E-5	-1.79454E+2	-1.121746561E-5	-1.090556364E-7	1.0015E+1	9.9182E+0	8.64971E+1	6.35264E+1	2.745896578E-2	4.98E+2	8E+0	1E+1	1.8E+0	1.0028E+1	9.9146E+0	8.66762E+1	6.35264E+1	2.3E+0	1E+1	1.63613975E-1	1.4649E+0	-2.5E-2	4.9E+1	-9E-1	-9E-1
Option: 6221 Adjust Mode{Enum U16 ((Offset,Frequency,Amplitude))}=Offset	0E+0	1.23709887E-3	1.56E-1	1.23709887E-3	3.371767975E-6	1.38342585E-5	-1.795272E+2	-1.38368946E-5	-1.153776235E-7	1.0053E+1	9.9446E+0	8.63539E+1	6.35264E+1	3.600671515E-2	4.99E+2	8E+0	1E+1	1.8E+0	1.0015E+1	9.9182E+0	8.64971E+1	6.35264E+1	2.3E+0	1E+1	2.745896578E-2	1.4649E+0	-2.5E-2	5E+1	-1.1E+0	-1.0999E+0
Option: 6221 Amplitude{Double Float}=1.000000E-6	0E+0	1.239290901E-3	1.56E-1	1.239290901E-3	3.371767975E-6	1.644583295E-5	-1.795548E+2	-1.644840682E-5	-1.29075385E-7	1.0039E+1	9.9356E+0	8.63539E+1	6.35264E+1	1.21945776E-2	5E+2	8E+0	1E+1	1.8E+0	1.0053E+1	9.9446E+0	8.63539E+1	6.35264E+1	2.3E+0	1E+1	3.600671515E-2	1.4649E+0	-2.5E-2	5.1E+1	-1.3E+0	-1.2999E+0
Option: 6221 Compliance{Double Float}=10.000000	0E+0	1.241819515E-3	1.56E-1	1.241819515E-3	3.371767975E-6	1.908206845E-5	-1.796052E+2	-1.908469889E-5	-1.327631731E-7	9.9976E+0	9.9263E+0	8.63181E+1	6.35264E+1	1.415257342E-3	5.01E+2	8E+0	1E+1	1.8E+0	1.0039E+1	9.9356E+0	8.63539E+1	6.35264E+1	2.3E+0	1E+1	1.21945776E-2	1.4649E+0	-2.5E-2	5.2E+1	-1.5E+0	-1.4999E+0
Option: 6221 Duty Cycle{Double Float}=50.000000	0E+0	1.241819515E-3	1.56E-1	1.241819515E-3	3.371767975E-6	1.908102193E-5	-1.796172E+2	-1.908362408E-5	-1.290752718E-7	9.997E+0	9.9173E+0	8.59957E+1	6.35264E+1	-1.356343739E-2	5.02E+2	8E+0	1E+1	1.8E+0	9.9976E+0	9.9263E+0	8.63181E+1	6.35264E+1	2.3E+0	1E+1	1.415257342E-3	1.4649E+0	-2.5E-2	5.3E+1	-1.5E+0	-1.4999E+0
Option: 6221 External Trigger{Boolean}=False	0E+0	1.236087707E-3	1.56E-1	1.236087707E-3	3.371767975E-6	1.252928445E-5	-1.794684E+2	-1.253192338E-5	-1.169581486E-7	1.0012E+1	9.9261E+0	8.66404E+1	6.35264E+1	-5.270003807E-3	5.03E+2	8E+0	1E+1	1.8E+0	9.997E+0	9.9173E+0	8.59957E+1	6.35264E+1	2.3E+0	1E+1	-1.356343739E-2	1.4649E+0	-2.5E-2	5.4E+1	-1E+0	-1.0001E+0
Option: 6221 External Trigger Ignore Multiple{Boolean}=False	0E+0	1.232209934E-3	1.548E-1	1.232209934E-3	3.338050296E-6	5.98647349E-6	-1.790712E+2	-5.989106755E-6	-9.904574792E-8	1.0012E+1	9.9308E+0	8.64255E+1	6.35264E+1	-1.961709E-3	5.04E+2	8E+0	1E+1	1.8E+0	1.0012E+1	9.9261E+0	8.66404E+1	6.35264E+1	2.3E+0	1E+1	-5.270003807E-3	1.4649E+0	-2.5E-2	5.5E+1	-5E-1	-5.002E-1
Option: 6221 Frequency{Double Float}=119.770000	
Option: 6221 Function{U16}=1	
Option: 6221 Function.__text__{String}=Sine	
Option: 6221 Idle Level{Double Float}=0.000000	
Option: 6221 Input trigger Line{U8}=5	
Option: 6221 Offset{Double Float}=0.000000	
Option: 6221 Output Trigger Line{U8}=4	
Option: 6221 Pass Through{Boolean}=True	
Option: 6221 Phase Marker{Boolean}=True	
Option: 6221 Phase Marker Phase{Double Float}=0.000000	
Option: 6221 Range Level{Double Float}=2.000000E-12	
Option: 6221 Ranging{U16}=1	
Option: 6221 Ranging.__text__{String}=Best	
Option: 6221 Update Clock{Double Float}=0.000000	
Option: 6221 VISA{Visa Refnum (Void)}=GPIB0::13::INSTR	
Option: Confirm Config{Boolean}=False	
Option: Control Panel Ref{LVObjVI Refnum (Void)}=	
Option: DAQ Global Channel{Boolean}=False	
Option: DAQ Input Rate{Double Float}=10000.000000	
Option: DAQ Input Samples{I32}=200	
Option: DAQ Measurement Channels{1D Array (Cluster (UserDefinedRefnumTag Refnum (Void),\tkDAQmxPhysChanTagType Tag,\tkDAQmxScaleTagType Tag,Boolean,Double Float,String))}=[]	
Option: Differential{I32}=10106	
Option: Differential.__text__{String}=Differential	
Option: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values))}=Function Generator	
Option: Lockin Standoff Time{Double Float}=0.000000	
Option: Paranoid Save Data{Boolean}=True	
Option: Plot Autoback Path{Path}=C:\\\\TEMP\\\\XY Multiparam\\\\Backup.txt	
Option: SR830  Ref Phase{Double Float}=0.000000	
Option: SR830  Synch Filter{Boolean}=False	
Option: SR830  Time Constant{I16}=8	
Option: SR830  Time Constant.__text__{String}=100 ms	
Option: SR830 2x Line Filter{Boolean}=True	
Option: SR830 Adjust Gains{Boolean}=False	
Option: SR830 Auto Gain Lower.__text__{String}=2 nV/fA	
Option: SR830 Auto Gain Upper.__text__{String}=1 V/uA	
Option: SR830 Auto Offset 1{Boolean}=False	
Option: SR830 Auto Offset 2{Boolean}=False	
Option: SR830 Autophase{Boolean}=False	
Option: SR830 DC Coupling?{Boolean}=False	
Option: SR830 Display 1{U16}=0	
Option: SR830 Display 1.__text__{String}=X	
Option: SR830 Display 2{U16}=0	
Option: SR830 Display 2.__text__{String}=Y	
Option: SR830 Dynamic Reserve{I16}=1	
Option: SR830 Dynamic Reserve.__text__{String}=Normal	
Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Option: SR830 Filter Slope{I32}=1	
Option: SR830 Filter Slope.__text__{String}=12 dB/oct	
Option: SR830 Gain{I32}=-1	
Option: SR830 Gain.__text__{String}=Auto Gain	
Option: SR830 Ground Shield?{Boolean}=False	
Option: SR830 Harmonic{I32}=1	
Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A	
Option: SR830 Line Filter{Boolean}=True	
Option: SR830 No Reset{Boolean}=False	
Option: SR830 Offset 1{Double Float}=0.000000	
Option: SR830 Offset 2{Double Float}=0.000000	
Option: SR830 Output Channel 1{Boolean}=False	
Option: SR830 Output Channel 2{Boolean}=False	
Option: SR830 Ratio 1{U16}=0	
Option: SR830 Ratio 1.__text__{String}=None	
Option: SR830 Ratio 2{U16}=0	
Option: SR830 Ratio 2.__text__{String}=None	
Option: SR830 Ref Amplitude{Double Float}=0.100000	
Option: SR830 Ref Frequency{Double Float}=1013.000000	
Option: SR830 Ref Source{Boolean}=False	
Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta]	
Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Option: SR830 VISA{Visa Refnum (Void)}=	
Option: Sense Autorange{Boolean}=False	
Option: Sense Range Level{Double Float}=0.100000	
Option: Sense Rate{Double Float}=1.000000	
Option:560 Comport{Visa Refnum (Void)}=COM1	
Option:560 Filter High Pass{U16}=0	
Option:560 Filter High Pass.__text__{String}=0.03	
Option:560 Filter Lowpass{U16}=0	
Option:560 Filter Lowpass.__text__{String}=0.03	
Option:560 Filter Mode{U16}=0	
Option:560 Filter Mode.__text__{String}=6 dB high pass	
Option:560 Invert{Boolean}=False	
Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Option:570 Enabled{Boolean}=False	
Option:570 Filter High Pass{U16}=0	
Option:570 Filter High Pass.__text__{String}=0.03	
Option:570 Filter Lowpass{U16}=0	
Option:570 Filter Lowpass.__text__{String}=0.03	
Option:570 Filter Mode{U16}=0	
Option:570 Filter Mode.__text__{String}=6 dB high pass	
Option:570 Gain Mode{U16}=0	
Option:570 Gain Mode.__text__{String}=Low Noise	
Option:570 Input Offset{U16}=0	
Option:570 Input Offset On{Boolean}=False	
Option:570 Input Offset.__text__{String}=1pA	
Option:570 Sensitivity{U16}=0	
Option:570 Sensitivity.__text__{String}=1pA/V	
Option:Debug On{Boolean}=False	
Option:GPIB 2182{Visa Refnum (Void)}=	
Option:Parallel Config Voltage Measurers{Boolean}=True	
Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Option:SR830 Settle Time{Double Float}=5.000000	
Option:Sense Digits{I32}=8	
Output Names{1D Array (String)}=['Offset','Rxx::R','Rxx::Theta','Rxx::X','Rxx::Y','Rxy::R','Rxy::Theta','Rxy::X','Rxy::Y','temperature: T1','temperature: T2','temperature: T3','temperature: T4','temperature: dT/dt','iterator','multi[0]:iterator','multi[0]:y','multi[0]:temperature: setpoint','multi[0]:temperature: T1','multi[0]:temperature: T2','multi[0]:temperature: T3','multi[0]:temperature: T4','multi[0]:temperature: heater','multi[0]:temperature: gas','multi[0]:temperature: dT/dt','multi[0]:temperature: current temperature','multi[0]:temperature: error','multi[1]:iterator','multi[1]:y','multi[1]:Control:Magnet Output']	
Parameter Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Parameter Select{U16}=6	
Parameter Select.__text__{String}=Multi-Parameter	
Paths{U32}=0	
Plot: Column Renames{1D Array (Cluster (String,String))}=[]	
Plot: No dups{Boolean}=False	
Plot: StdDevs{Boolean}=False	
Plotting Class{String}=Parameter Plot	
Plotting Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	
Plotting Select{U16}=1	
Plotting Select.__text__{String}=Parameter Plot	
Project Code{String}=Topological_Insulators	
Ref: Temperature Window{LVObjVI Refnum (Void)}=	
Ref:Control Subpanel{LVObjUnknown Refnum (Void)}=	
Ref:Main Screen{LVObjVI Refnum (Void)}=	
Ref:Plotting Subpanel{LVObjUnknown Refnum (Void)}=	
Ref:Toolbar{LVObjUnknown Refnum (Void)}=	
Ref:XY Subpanel{LVObjUnknown Refnum (Void)}=	
Rxx::R{Double Float}=0.001232	
Rxx::Theta{Double Float}=0.154800	
Rxx::X{Double Float}=0.001232	
Rxx::Y{Double Float}=3.338050E-6	
Rxx:Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	
Rxx:Option: 560 Enabled{Boolean}=False	
Rxx:Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	
Rxx:Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	
Rxx:Option: Lockin Standoff Time{Double Float}=0.000000	
Rxx:Option: Lockin Type{Enum U16 ((SRS 830,EG&G 5302))}=SRS 830	
Rxx:Option: SR803 Full Scale Reading{Double Float}=0.000000	
Rxx:Option: SR830  Ref Phase{Double Float}=0.000000	
Rxx:Option: SR830  Synch Filter{Boolean}=False	
Rxx:Option: SR830  Time Constant{I16}=8	
Rxx:Option: SR830 2x Line Filter{Boolean}=False	
Rxx:Option: SR830 Adjust Gains{Boolean}=False	
Rxx:Option: SR830 Auto Gain Lower{I32}=0	
Rxx:Option: SR830 Auto Gain Upper{I32}=26	
Rxx:Option: SR830 Auto Offset 1{Boolean}=False	
Rxx:Option: SR830 Auto Offset 2{Boolean}=False	
Rxx:Option: SR830 Autophase{Boolean}=False	
Rxx:Option: SR830 DC Coupling?{Boolean}=False	
Rxx:Option: SR830 Display 1{U16}=0	
Rxx:Option: SR830 Display 2{U16}=0	
Rxx:Option: SR830 Dynamic Reserve{I16}=2	
Rxx:Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Rxx:Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Rxx:Option: SR830 Filter Slope{I32}=3	
Rxx:Option: SR830 Gain{I32}=18	
Rxx:Option: SR830 Ground Shield?{Boolean}=False	
Rxx:Option: SR830 Harmonic{I32}=1	
Rxx:Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A-B	
Rxx:Option: SR830 Line Filter{Boolean}=False	
Rxx:Option: SR830 No Reset{Boolean}=False	
Rxx:Option: SR830 Offset 1{Double Float}=0.000000	
Rxx:Option: SR830 Offset 2{Double Float}=0.000000	
Rxx:Option: SR830 Output Channel 1{Boolean}=False	
Rxx:Option: SR830 Output Channel 2{Boolean}=False	
Rxx:Option: SR830 Ratio 1{U16}=0	
Rxx:Option: SR830 Ratio 2{U16}=0	
Rxx:Option: SR830 Ref Amplitude{Double Float}=0.100000	
Rxx:Option: SR830 Ref Frequency{Double Float}=1013.000000	
Rxx:Option: SR830 Ref Source{Boolean}=False	
Rxx:Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta,X,Y]	
Rxx:Option: SR830 Time Constant value{Double Float}=0.000000	
Rxx:Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Rxx:Option: SR830 VISA{Visa Refnum (Void)}=GPIB0::5::INSTR	
Rxx:Option:560 Comport{Visa Refnum (Void)}=COM1	
Rxx:Option:560 Filter High Pass{U16}=0	
Rxx:Option:560 Filter Lowpass{U16}=0	
Rxx:Option:560 Filter Mode{U16}=0	
Rxx:Option:560 Invert{Boolean}=False	
Rxx:Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Rxx:Option:570 Enabled{Boolean}=False	
Rxx:Option:570 Filter High Pass{U16}=0	
Rxx:Option:570 Filter Lowpass{U16}=0	
Rxx:Option:570 Filter Mode{U16}=0	
Rxx:Option:570 Gain Mode{U16}=0	
Rxx:Option:570 Input Offset{U16}=0	
Rxx:Option:570 Input Offset On{Boolean}=False	
Rxx:Option:570 Sensitivity{U16}=0	
Rxx:Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Rxx:Option:SR830 Autogain Lower Threshold{Double Float}=0.100000	
Rxx:Option:SR830 Autogain Standoff{Double Float}=3.000000	
Rxx:Option:SR830 Autogain Upper Threshold{Double Float}=0.900000	
Rxx:Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Rxx:Option:SR830 Settle Time{Double Float}=0.000000	
Rxy::R{Double Float}=5.986473E-6	
Rxy::Theta{Double Float}=-179.071200	
Rxy::X{Double Float}=-5.989107E-6	
Rxy::Y{Double Float}=-9.904575E-8	
Rxy:Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	
Rxy:Option: 560 Enabled{Boolean}=False	
Rxy:Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	
Rxy:Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	
Rxy:Option: Lockin Standoff Time{Double Float}=0.000000	
Rxy:Option: Lockin Type{Enum U16 ((SRS 830,EG&G 5302))}=SRS 830	
Rxy:Option: SR803 Full Scale Reading{Double Float}=0.000000	
Rxy:Option: SR830  Ref Phase{Double Float}=0.000000	
Rxy:Option: SR830  Synch Filter{Boolean}=False	
Rxy:Option: SR830  Time Constant{I16}=8	
Rxy:Option: SR830 2x Line Filter{Boolean}=False	
Rxy:Option: SR830 Adjust Gains{Boolean}=False	
Rxy:Option: SR830 Auto Gain Lower{I32}=0	
Rxy:Option: SR830 Auto Gain Upper{I32}=26	
Rxy:Option: SR830 Auto Offset 1{Boolean}=False	
Rxy:Option: SR830 Auto Offset 2{Boolean}=False	
Rxy:Option: SR830 Autophase{Boolean}=False	
Rxy:Option: SR830 DC Coupling?{Boolean}=False	
Rxy:Option: SR830 Display 1{U16}=0	
Rxy:Option: SR830 Display 2{U16}=1	
Rxy:Option: SR830 Dynamic Reserve{I16}=2	
Rxy:Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Rxy:Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Rxy:Option: SR830 Filter Slope{I32}=3	
Rxy:Option: SR830 Gain{I32}=18	
Rxy:Option: SR830 Ground Shield?{Boolean}=False	
Rxy:Option: SR830 Harmonic{I32}=1	
Rxy:Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A-B	
Rxy:Option: SR830 Line Filter{Boolean}=False	
Rxy:Option: SR830 No Reset{Boolean}=False	
Rxy:Option: SR830 Offset 1{Double Float}=0.000000	
Rxy:Option: SR830 Offset 2{Double Float}=0.000000	
Rxy:Option: SR830 Output Channel 1{Boolean}=False	
Rxy:Option: SR830 Output Channel 2{Boolean}=False	
Rxy:Option: SR830 Ratio 1{U16}=0	
Rxy:Option: SR830 Ratio 2{U16}=0	
Rxy:Option: SR830 Ref Amplitude{Double Float}=0.100000	
Rxy:Option: SR830 Ref Frequency{Double Float}=1013.000000	
Rxy:Option: SR830 Ref Source{Boolean}=False	
Rxy:Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta,X,Y]	
Rxy:Option: SR830 Time Constant value{Double Float}=0.000000	
Rxy:Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Rxy:Option: SR830 VISA{Visa Refnum (Void)}=GPIB0::6::INSTR	
Rxy:Option:560 Comport{Visa Refnum (Void)}=COM1	
Rxy:Option:560 Filter High Pass{U16}=0	
Rxy:Option:560 Filter Lowpass{U16}=0	
Rxy:Option:560 Filter Mode{U16}=0	
Rxy:Option:560 Invert{Boolean}=False	
Rxy:Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Rxy:Option:570 Enabled{Boolean}=False	
Rxy:Option:570 Filter High Pass{U16}=0	
Rxy:Option:570 Filter Lowpass{U16}=0	
Rxy:Option:570 Filter Mode{U16}=0	
Rxy:Option:570 Gain Mode{U16}=0	
Rxy:Option:570 Input Offset{U16}=0	
Rxy:Option:570 Input Offset On{Boolean}=False	
Rxy:Option:570 Sensitivity{U16}=0	
Rxy:Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Rxy:Option:SR830 Autogain Lower Threshold{Double Float}=0.100000	
Rxy:Option:SR830 Autogain Standoff{Double Float}=3.000000	
Rxy:Option:SR830 Autogain Upper Threshold{Double Float}=0.900000	
Rxy:Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Rxy:Option:SR830 Settle Time{Double Float}=0.000000	
Sample ID{String}=MBE202221213_PA_D1 750C Cracker WAL	
Save:Filename{String}=${X-Y Class} ${2nd Parameter Class} ${iterator}{%04d} ${y}{%04.2g}.txt	
Save:Final Filename{String}=${X-Y Class} ${2nd Parameter Class} .txt	
Save:Final path{Path}=C:\\\\Data\\\\${Project Code}\\\\${User}\\\\${Sample ID}\\\\${Measurement Timestamp}{%Y%m%d}\\\\${X-Y Class}	
Save:Path{Path}=C:\\\\Data\\\\${Project Code}\\\\${User}\\\\${Sample ID}\\\\${Measurement Timestamp}{%Y%m%d}\\\\${X-Y Class}	
Startup path{Path}=C:\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV	
Sub Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Sweep Step{I32}=3	
T Control Measure.__text__{1D Array (String)}=['temperature: T1','temperature: T2','temperature: T3','temperature: T4','temperature: dT/dt']	
Timestamp{Timestamp}=<23:24:53.384 17/05/2023>T	
Toolbar{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Unaved Data{Boolean}=True	
Unsaved Data{Boolean}=False	
User{String}=Craig	
X-Y Class{String}=6221-Lockin-DAQ	
X-Y Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	
d(Offset){Double Float}=0.000000	
d(Rxx::R){Double Float}=0.000000	
d(Rxx::Theta){Double Float}=0.002683	
d(Rxx::X){Double Float}=0.000000	
d(Rxx::Y){Double Float}=7.539502E-8	
d(Rxy::R){Double Float}=1.651213E-8	
d(Rxy::Theta){Double Float}=0.085424	
d(Rxy::X){Double Float}=1.651518E-8	
d(Rxy::Y){Double Float}=8.854954E-9	
iterate result{U16}=5	
iterator{I32}=504	
multi[0]:Control: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values,Adaptive Step Ramp))}=List of Values	
multi[0]:Control: Monitor Update Timeout{Double Float}=0.010000	
multi[0]:Control: Open T Window{Boolean}=False	
multi[0]:Control: Reverse Temperature Sense{Boolean}=False	
multi[0]:Iterator{I32}=0	
multi[0]:Ref: Temperature Window{LVObjVI Refnum (Void)}=	
multi[0]:iterate result{U16}=0	
multi[0]:iterator{I32}=8	
multi[0]:temperature:  rate window{Double Float}=120.000000	
multi[0]:temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[0]:temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
multi[0]:temperature: T1{Double Float}=9.994800	
multi[0]:temperature: T2{Double Float}=9.924400	
multi[0]:temperature: T3{Double Float}=85.673400	
multi[0]:temperature: T4{Double Float}=63.526400	
multi[0]:temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
multi[0]:temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
multi[0]:temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
multi[0]:temperature: current temperature{Double Float}=1.464900	
multi[0]:temperature: current temperature 2{Double Float}=287.100000	
multi[0]:temperature: dT/dt{Double Float}=-0.014813	
multi[0]:temperature: error{Double Float}=-0.025000	
multi[0]:temperature: gas{Double Float}=10.000000	
multi[0]:temperature: gas control{Boolean}=False	
multi[0]:temperature: gas control 2{Boolean}=False	
multi[0]:temperature: gass boost{I8}=0	
multi[0]:temperature: gass boost 2{I8}=0	
multi[0]:temperature: gast flow{I16}=0	
multi[0]:temperature: gast flow 2{I16}=7	
multi[0]:temperature: heater{Double Float}=2.300000	
multi[0]:temperature: heater output{Double Float}=0.000000	
multi[0]:temperature: heater output 2{Double Float}=0.000000	
multi[0]:temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
multi[0]:temperature: monitor timeout{Double Float}=0.010000	
multi[0]:temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
multi[0]:temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
multi[0]:temperature: ramp rate{Double Float}=8.000000	
multi[0]:temperature: ramp rate 2{Double Float}=0.000000	
multi[0]:temperature: ramp target{Double Float}=20.000000	
multi[0]:temperature: ramp target 2{Double Float}=0.000000	
multi[0]:temperature: ramping{Boolean}=False	
multi[0]:temperature: setpoint{Double Float}=1.800000	
multi[0]:temperature: setpoint 2{Double Float}=287.100000	
multi[0]:temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
multi[0]:temperature: stability error{Extended Float}=0.040000	
multi[0]:temperature: stability script{String}=	
multi[0]:temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
multi[0]:temperature: temp control mode{U16}=2	
multi[0]:temperature: temp control mode 2{U16}=3	
multi[0]:temperature: temp control mode 2.__text__{String}=Open Loop	
multi[0]:temperature: temp control mode.__text__{String}=Zone	
multi[0]:temperature: temp control sensor{U16}=0	
multi[0]:temperature: temp control sensor 2{U16}=0	
multi[0]:temperature: temp control sensor 2.__text__{String}=Sensor 1	
multi[0]:temperature: temp control sensor.__text__{String}=Sensor A	
multi[0]:temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
multi[0]:temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
multi[0]:temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
multi[0]:temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
multi[0]:temperature: temp loop{U16}=0	
multi[0]:temperature: temp loop 2{U16}=0	
multi[0]:temperature: temp loop 2.__text__{String}=Heater	
multi[0]:temperature: temp loop.__text__{String}=Loop 1	
multi[0]:temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
multi[0]:temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[0]:temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[0]:temperature:error for gas boost{Double Float}=0.000000	
multi[0]:temperature:error for gas boost 2{Double Float}=0.000000	
multi[0]:temperature:heater range{U16}=2	
multi[0]:temperature:heater range 2{U16}=0	
multi[0]:temperature:heater range 2.__text__{String}=Off	
multi[0]:temperature:heater range.__text__{String}=40mW	
multi[0]:temperature:history window{Extended Float}=300.000000	
multi[0]:temperature:is stable?{Boolean}=True	
multi[0]:temperature:monitor{Boolean}=True	
multi[0]:temperature:ramping{Boolean}=False	
multi[0]:temperature:ramping on{Boolean}=False	
multi[0]:temperature:ramping on 2{Boolean}=False	
multi[0]:temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
multi[0]:temperature:stability code{U32}=6618880	
multi[0]:temperature:stability rate{Extended Float}=0.040000	
multi[0]:y{Double Float}=10.000000	
multi[1]:Control: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values,Adaptive Step Ramp))}=Multi-Segment Ramp	
multi[1]:Control: Gate delay{Double Float}=0.000000	
multi[1]:Control: Monitor Update Timeout{Double Float}=0.010000	
multi[1]:Control: Open T Window{Boolean}=False	
multi[1]:Control: Reverse Temperature Sense{Boolean}=False	
multi[1]:Control:Magnet Output{Double Float}=-0.000000	
multi[1]:Iterator{I32}=0	
multi[1]:Magnet: Final Switch Heater{Enum U8 ((False,True,Mixed))}=	
multi[1]:Magnet: Power Supply{Enum U16 ((IPS120,LS625,PS110,Hg iPS,SMS Series,Cryomagnetics 4G,DMG Little CryoFree,DMG Big CryoFree))}=Hg iPS	
multi[1]:Magnet: Rate{Double Float}=0.500000	
multi[1]:Magnet: Units{Enum U16 ((Field,Current))}=Field	
multi[1]:Magnet: VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[1]:Multi-segment_Stage{I32}=0	
multi[1]:Multi-segment_Stage_Changed{Boolean}=False	
multi[1]:Ref: Temperature Window{LVObjVI Refnum (Void)}=	
multi[1]:iterate result{U16}=4	
multi[1]:iterator{I32}=57	
multi[1]:measure point{Boolean}=False	
multi[1]:temperature:  rate window{Double Float}=120.000000	
multi[1]:temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[1]:temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
multi[1]:temperature: T1{Double Float}=1.842400	
multi[1]:temperature: T2{Double Float}=1.465600	
multi[1]:temperature: T3{Double Float}=86.318100	
multi[1]:temperature: T4{Double Float}=66.769200	
multi[1]:temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
multi[1]:temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
multi[1]:temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
multi[1]:temperature: current temperature{Double Float}=1.465600	
multi[1]:temperature: current temperature 2{Double Float}=287.100000	
multi[1]:temperature: dT/dt{Double Float}=-0.001864	
multi[1]:temperature: gas control{Boolean}=False	
multi[1]:temperature: gas control 2{Boolean}=False	
multi[1]:temperature: gass boost{I8}=0	
multi[1]:temperature: gass boost 2{I8}=0	
multi[1]:temperature: gast flow{I16}=0	
multi[1]:temperature: gast flow 2{I16}=7	
multi[1]:temperature: heater output{Double Float}=0.000000	
multi[1]:temperature: heater output 2{Double Float}=0.000000	
multi[1]:temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
multi[1]:temperature: monitor timeout{Double Float}=1.000000	
multi[1]:temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
multi[1]:temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
multi[1]:temperature: ramp rate{Double Float}=8.000000	
multi[1]:temperature: ramp rate 2{Double Float}=0.000000	
multi[1]:temperature: ramp target{Double Float}=20.000000	
multi[1]:temperature: ramp target 2{Double Float}=0.000000	
multi[1]:temperature: ramping{Boolean}=False	
multi[1]:temperature: setpoint{Double Float}=1.800000	
multi[1]:temperature: setpoint 2{Double Float}=287.100000	
multi[1]:temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
multi[1]:temperature: stability error{Extended Float}=0.040000	
multi[1]:temperature: stability script{String}=	
multi[1]:temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
multi[1]:temperature: temp control mode{U16}=2	
multi[1]:temperature: temp control mode 2{U16}=3	
multi[1]:temperature: temp control mode 2.__text__{String}=Open Loop	
multi[1]:temperature: temp control mode.__text__{String}=Zone	
multi[1]:temperature: temp control sensor{U16}=0	
multi[1]:temperature: temp control sensor 2{U16}=0	
multi[1]:temperature: temp control sensor 2.__text__{String}=Sensor 1	
multi[1]:temperature: temp control sensor.__text__{String}=Sensor A	
multi[1]:temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
multi[1]:temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
multi[1]:temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
multi[1]:temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
multi[1]:temperature: temp loop{U16}=0	
multi[1]:temperature: temp loop 2{U16}=0	
multi[1]:temperature: temp loop 2.__text__{String}=Heater	
multi[1]:temperature: temp loop.__text__{String}=Loop 1	
multi[1]:temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
multi[1]:temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[1]:temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[1]:temperature:error for gas boost{Double Float}=0.000000	
multi[1]:temperature:error for gas boost 2{Double Float}=0.000000	
multi[1]:temperature:heater range{U16}=2	
multi[1]:temperature:heater range 2{U16}=0	
multi[1]:temperature:heater range 2.__text__{String}=Off	
multi[1]:temperature:heater range.__text__{String}=40mW	
multi[1]:temperature:history window{Extended Float}=300.000000	
multi[1]:temperature:is stable?{Boolean}=True	
multi[1]:temperature:monitor{Boolean}=True	
multi[1]:temperature:ramping{Boolean}=False	
multi[1]:temperature:ramping on{Boolean}=False	
multi[1]:temperature:ramping on 2{Boolean}=False	
multi[1]:temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
multi[1]:temperature:stability code{U32}=6618880	
multi[1]:temperature:stability rate{Extended Float}=0.040000	
multi[1]:y{Double Float}=0.000000	
parameter: Termination{String}=False	
parameter: delta time{Double Float}=1.000000	
parameter: progress{Double Float}=100.000000	
temperature:  rate window{Double Float}=120.000000	
temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
temperature: T1{Double Float}=9.994800	
temperature: T2{Double Float}=9.924400	
temperature: T3{Double Float}=85.673400	
temperature: T4{Double Float}=63.526400	
temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
temperature: current temperature{Double Float}=1.464900	
temperature: current temperature 2{Double Float}=287.100000	
temperature: dT/dt{Double Float}=-0.014813	
temperature: gas control{Boolean}=False	
temperature: gas control 2{Boolean}=False	
temperature: gass boost{I8}=0	
temperature: gass boost 2{I8}=0	
temperature: gast flow{I16}=0	
temperature: gast flow 2{I16}=7	
temperature: heater output{Double Float}=0.000000	
temperature: heater output 2{Double Float}=0.000000	
temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
temperature: monitor timeout{Double Float}=0.010000	
temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
temperature: ramp rate{Double Float}=8.000000	
temperature: ramp rate 2{Double Float}=0.000000	
temperature: ramp target{Double Float}=20.000000	
temperature: ramp target 2{Double Float}=0.000000	
temperature: ramping{Boolean}=False	
temperature: setpoint{Double Float}=1.800000	
temperature: setpoint 2{Double Float}=287.100000	
temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
temperature: stability error{Extended Float}=0.040000	
temperature: stability script{String}=	
temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
temperature: temp control mode{U16}=2	
temperature: temp control mode 2{U16}=3	
temperature: temp control mode 2.__text__{String}=Open Loop	
temperature: temp control mode.__text__{String}=Zone	
temperature: temp control sensor{U16}=0	
temperature: temp control sensor 2{U16}=0	
temperature: temp control sensor 2.__text__{String}=Sensor 1	
temperature: temp control sensor.__text__{String}=Sensor A	
temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
temperature: temp loop{U16}=0	
temperature: temp loop 2{U16}=0	
temperature: temp loop 2.__text__{String}=Heater	
temperature: temp loop.__text__{String}=Loop 1	
temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
temperature:error for gas boost{Double Float}=0.000000	
temperature:error for gas boost 2{Double Float}=0.000000	
temperature:heater range{U16}=2	
temperature:heater range 2{U16}=0	
temperature:heater range 2.__text__{String}=Off	
temperature:heater range.__text__{String}=40mW	
temperature:history window{Extended Float}=300.000000	
temperature:is stable?{Boolean}=True	
temperature:monitor{Boolean}=True	
temperature:ramping{Boolean}=False	
temperature:ramping on{Boolean}=False	
temperature:ramping on 2{Boolean}=False	
temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
temperature:stability code{U32}=6618880	
temperature:stability rate{Extended Float}=0.040000	
y{Double Float}=10.000000	
