TDI Format 1.5	Offset	Rxx::R	Rxx::Theta	Rxx::X	Rxx::Y	Rxy::R	Rxy::Theta	Rxy::X	Rxy::Y	temperature: T1	temperature: T2	temperature: T3	temperature: T4	temperature: dT/dt	iterator	multi[0]:iterator	multi[0]:y	multi[0]:temperature: setpoint	multi[0]:temperature: T1	multi[0]:temperature: T2	multi[0]:temperature: T3	multi[0]:temperature: T4	multi[0]:temperature: heater	multi[0]:temperature: gas	multi[0]:temperature: dT/dt	multi[0]:temperature: current temperature	multi[0]:temperature: error	multi[1]:iterator	multi[1]:y	multi[1]:Control:Magnet Output
2nd Parameter Class{String}=Multi-Parameter	0E+0	1.226141543E-3	1.56E-1	1.226141543E-3	3.371767975E-6	5.969073006E-7	-7.434E+0	5.911121363E-7	-7.902577303E-8	4.0407E+0	4.0916E+0	8.59957E+1	6.43465E+1	3.427777812E-2	3.93E+2	7E+0	4E+0	4E+0	4.0508E+0	4.0932E+0	8.59957E+1	6.43465E+1	4.9E+0	4E+0	3.75302285E-2	4.0504E+0	-5.04E-2	0E+0	0E+0	0E+0
2nd Parameter Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	0E+0	1.232041642E-3	1.56E-1	1.232041642E-3	3.371767975E-6	7.183446878E-6	-4.14E-1	7.183446878E-6	-5.268386754E-8	3.9972E+0	4.0501E+0	8.59241E+1	6.43465E+1	-2.116951905E-2	3.94E+2	7E+0	4E+0	1.8E+0	4.0407E+0	4.0916E+0	8.59957E+1	6.43465E+1	4.9E+0	4E+0	3.427777812E-2	1.4649E+0	-5.04E-2	1E+0	5E-1	4.998E-1
Analysis Class{String}=Basic Plot	0E+0	1.236087707E-3	1.56E-1	1.236087707E-3	3.371767975E-6	1.376577097E-5	-1.428E-1	1.376577097E-5	-3.582499938E-8	4.2853E+0	4.1732E+0	8.56734E+1	6.43465E+1	1.270204484E-1	3.95E+2	7E+0	4E+0	1.8E+0	3.9972E+0	4.0501E+0	8.59241E+1	6.43465E+1	4.9E+0	4E+0	-2.116951905E-2	1.4649E+0	-5.04E-2	2E+0	1E+0	9.999E-1
Analysis Class Path{Path}=C\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV\\\\plugins\\\\Plotting\\\\Plotting_Base_class\\\\Plotting_Base.lvclass	0E+0	1.242292145E-3	1.56E-1	1.242292145E-3	3.371767975E-6	2.038388032E-5	-6.48E-2	2.038388032E-5	-2.476142567E-8	3.7792E+0	3.8305E+0	8.59241E+1	6.39289E+1	-8.254215717E-1	3.96E+2	7E+0	4E+0	1.8E+0	4.2853E+0	4.1732E+0	8.56734E+1	6.43465E+1	4.9E+0	4E+0	1.270204484E-1	1.4649E+0	-5.04E-2	3E+0	1.5E+0	1.4999E+0
Analysis.# pre-routines{I32}=5	0E+0	1.242157512E-3	1.56E-1	1.242157512E-3	3.371767975E-6	2.038600164E-5	-1.02E-1	2.038600164E-5	-3.793231901E-8	3.8478E+0	3.8943E+0	8.59241E+1	6.39289E+1	-6.544510126E-1	3.97E+2	7E+0	4E+0	1.8E+0	3.7792E+0	3.8305E+0	8.59241E+1	6.39289E+1	4.9E+0	4E+0	-8.254215717E-1	1.4649E+0	-5.04E-2	4E+0	1.5E+0	1.5E+0
Analysis:Pre[0]:T Control Measure{1D Array (I32)}=[1,2,3,4,7]	0E+0	1.239459192E-3	1.56E-1	1.239459192E-3	3.371767975E-6	1.773019342E-5	-1.584E-1	1.773019342E-5	-5.004966851E-8	4.0437E+0	4.0864E+0	8.59241E+1	6.39289E+1	4.711430073E-1	3.98E+2	7E+0	4E+0	1.8E+0	3.8478E+0	3.8943E+0	8.59241E+1	6.39289E+1	4.9E+0	4E+0	-6.544510126E-1	1.4649E+0	-5.04E-2	5E+0	1.3E+0	1.3002E+0
Autosave Tabs{Enum U32 ((XY Measurement Save,Parameter Plot Save 2))}=Parameter Plot Save 2	0E+0	1.237268576E-3	1.56E-1	1.237268576E-3	3.371767975E-6	1.50844544E-5	-1.548E-1	1.50844544E-5	-4.214709969E-8	4.0022E+0	4.0498E+0	8.58883E+1	6.39289E+1	4.931851849E-2	3.99E+2	7E+0	4E+0	1.8E+0	4.0437E+0	4.0864E+0	8.59241E+1	6.39289E+1	4.9E+0	4E+0	4.711430073E-1	1.4649E+0	-5.04E-2	6E+0	1.1E+0	1.1001E+0
Control:Magnet Output{Double Float}=-0.007000	0E+0	1.235244836E-3	1.56E-1	1.235244836E-3	3.371767975E-6	1.244973494E-5	-2.256E-1	1.244973494E-5	-5.004969679E-8	4.0047E+0	4.0651E+0	8.56734E+1	6.39289E+1	9.761753492E-3	4E+2	7E+0	4E+0	1.8E+0	4.0022E+0	4.0498E+0	8.58883E+1	6.39289E+1	4.9E+0	4E+0	4.931851849E-2	1.4649E+0	-5.04E-2	7E+0	9E-1	9.001E-1
Control:Magnet Rate{Double Float}=0.500000	0E+0	1.233559093E-3	1.56E-1	1.233559093E-3	3.371767975E-6	9.820256551E-6	-3.144E-1	9.820256551E-6	-5.479124374E-8	3.9755E+0	4.0391E+0	8.60315E+1	6.39289E+1	-5.93803376E-2	4.01E+2	7E+0	4E+0	1.8E+0	4.0047E+0	4.0651E+0	8.56734E+1	6.39289E+1	4.9E+0	4E+0	9.761753492E-3	1.4649E+0	-5.04E-2	8E+0	7E-1	7.001E-1
Display Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	0E+0	1.232041642E-3	1.56E-1	1.232041642E-3	3.371767975E-6	7.173437075E-6	-5.496E-1	7.173437075E-6	-7.006947369E-8	4.006E+0	4.0799E+0	8.59957E+1	6.39289E+1	1.482236478E-2	4.02E+2	7E+0	4E+0	1.8E+0	3.9755E+0	4.0391E+0	8.60315E+1	6.39289E+1	4.9E+0	4E+0	-5.93803376E-2	1.4649E+0	-5.04E-2	9E+0	5E-1	5.001E-1
Elapsed Time{Double Float}=12790.950867	0E+0	1.230693897E-3	1.56E-1	1.230693897E-3	3.338050296E-6	4.536599118E-6	-9.42E-1	4.536599118E-6	-7.586472288E-8	4.0136E+0	4.0663E+0	8.59241E+1	6.39289E+1	-7.562481798E-3	4.03E+2	7E+0	4E+0	1.8E+0	4.006E+0	4.0799E+0	8.59957E+1	6.39289E+1	4.9E+0	4E+0	1.482236478E-2	1.4649E+0	-5.04E-2	1E+1	3E-1	3.001E-1
File:Autodel{Boolean}=True	0E+0	1.22900674E-3	1.56E-1	1.22900674E-3	3.371767975E-6	1.882397447E-6	-2.5392E+0	1.880287441E-6	-8.482099394E-8	4.0285E+0	4.0852E+0	8.59599E+1	6.39289E+1	2.630825154E-2	4.04E+2	7E+0	4E+0	1.8E+0	4.0136E+0	4.0663E+0	8.59241E+1	6.39289E+1	4.9E+0	4E+0	-7.562481798E-3	1.4649E+0	-5.04E-2	1.1E+1	1E-1	1.001E-1
File:Autosave{Boolean}=False	0E+0	1.22900674E-3	1.56E-1	1.22900674E-3	3.371767975E-6	1.895560947E-6	-2.5488E+0	1.89293051E-6	-8.534784506E-8	3.9945E+0	4.0612E+0	8.59241E+1	6.39289E+1	-1.394273806E-2	4.05E+2	7E+0	4E+0	1.8E+0	4.0285E+0	4.0852E+0	8.59599E+1	6.39289E+1	4.9E+0	4E+0	2.630825154E-2	1.4649E+0	-5.04E-2	1.2E+1	1E-1	1E-1
File:Export Config{Boolean}=True	0E+0	1.228838449E-3	1.56E-1	1.228838449E-3	3.371767975E-6	1.758056963E-6	-2.7192E+0	1.755426525E-6	-8.482110707E-8	3.9751E+0	4.0321E+0	8.59241E+1	6.39289E+1	-5.133159459E-2	4.06E+2	7E+0	4E+0	1.8E+0	3.9945E+0	4.0612E+0	8.59241E+1	6.39289E+1	4.9E+0	4E+0	-1.394273806E-2	1.4649E+0	-5.04E-2	1.3E+1	9E-2	9.01E-2
File:Final Autosave{Boolean}=True	0E+0	1.228670157E-3	1.56E-1	1.228670157E-3	3.371767975E-6	1.612656009E-6	-2.5812E+0	1.610019915E-6	-7.37573184E-8	4.0494E+0	4.0913E+0	8.59241E+1	6.39289E+1	3.100604191E-2	4.07E+2	7E+0	4E+0	1.8E+0	3.9751E+0	4.0321E+0	8.59241E+1	6.39289E+1	4.9E+0	4E+0	-5.133159459E-2	1.4649E+0	-5.04E-2	1.4E+1	8E-2	8.01E-2
Filter:Enable{Enum U16 ((None,Analog,Digital,Analog&Digitial))}=None	0E+0	1.228535524E-3	1.56E-1	1.228535524E-3	3.371767975E-6	1.483051822E-6	-2.8056E+0	1.480418556E-6	-7.323043899E-8	4.0471E+0	4.0856E+0	8.59241E+1	6.39289E+1	1.726508699E-2	4.08E+2	7E+0	4E+0	1.8E+0	4.0494E+0	4.0913E+0	8.59241E+1	6.39289E+1	4.9E+0	4E+0	3.100604191E-2	1.4649E+0	-5.04E-2	1.5E+1	7E-2	7E-2
Filter:Points{I32}=1	0E+0	1.228333574E-3	1.56E-1	1.228333574E-3	3.371767975E-6	1.352924092E-6	-3.5508E+0	1.349762476E-6	-8.534781677E-8	4.0549E+0	4.0948E+0	8.56375E+1	6.39289E+1	3.760141879E-2	4.09E+2	7E+0	4E+0	1.8E+0	4.0471E+0	4.0856E+0	8.59241E+1	6.39289E+1	4.9E+0	4E+0	1.726508699E-2	1.4649E+0	-5.04E-2	1.6E+1	6E-2	6E-2
Filter:Type{U16}=1	0E+0	1.228029236E-3	1.56E-1	1.228029236E-3	3.371767975E-6	1.223844295E-6	-3.642E+0	1.221209898E-6	-7.902574475E-8	4.057E+0	4.1027E+0	8.56734E+1	6.39289E+1	4.890619963E-2	4.1E+2	7E+0	4E+0	1.8E+0	4.0549E+0	4.0948E+0	8.56375E+1	6.39289E+1	4.9E+0	4E+0	3.760141879E-2	1.4649E+0	-5.04E-2	1.7E+1	5E-2	5E-2
Filter:Type.__text__{String}=Repeat	0E+0	1.228163869E-3	1.56E-1	1.228163869E-3	3.371767975E-6	1.229639459E-6	-3.7992E+0	1.226478126E-6	-8.324052543E-8	3.939E+0	4.0496E+0	8.57092E+1	6.39289E+1	-2.960513532E-2	4.11E+2	7E+0	4E+0	1.8E+0	4.057E+0	4.1027E+0	8.56734E+1	6.39289E+1	4.9E+0	4E+0	4.890619963E-2	1.4649E+0	-5.04E-2	1.8E+1	5E-2	5E-2
Filter:Window{Double Float}=1.000000	0E+0	1.227995577E-3	1.56E-1	1.227995577E-3	3.371767975E-6	1.15061462E-6	-3.5688E+0	1.14797994E-6	-7.323052384E-8	4.0129E+0	4.0707E+0	8.56734E+1	6.39289E+1	4.427489825E-3	4.12E+2	7E+0	4E+0	1.8E+0	3.939E+0	4.0496E+0	8.57092E+1	6.39289E+1	4.9E+0	4E+0	-2.960513532E-2	1.4649E+0	-5.04E-2	1.9E+1	4.5E-2	4.49E-2
Iterator{I32}=0	0E+0	1.227827286E-3	1.56E-1	1.227827286E-3	3.338050296E-6	1.082125671E-6	-3.3672E+0	1.079491557E-6	-6.532795503E-8	4.0195E+0	4.0801E+0	8.57808E+1	6.39289E+1	1.300178934E-2	4.13E+2	7E+0	4E+0	1.8E+0	4.0129E+0	4.0707E+0	8.56734E+1	6.39289E+1	4.9E+0	4E+0	4.427489825E-3	1.4649E+0	-5.04E-2	2E+1	4E-2	3.99E-2
Magnet: Control Mode{Boolean}=False	0E+0	1.227658995E-3	1.56E-1	1.227658995E-3	3.304332616E-6	1.019959105E-6	-4.392E+0	1.017324708E-6	-7.955262415E-8	4.0348E+0	4.0916E+0	8.58166E+1	6.39289E+1	2.354307659E-2	4.14E+2	7E+0	4E+0	1.8E+0	4.0195E+0	4.0801E+0	8.57808E+1	6.39289E+1	4.9E+0	4E+0	1.300178934E-2	1.4649E+0	-5.04E-2	2.1E+1	3.5E-2	3.46E-2
Magnet: Final Switch Heater{Enum U8 ((False,True,Mixed))}=	0E+0	1.227490703E-3	1.56E-1	1.227490703E-3	3.338050296E-6	9.688559327E-7	-4.9884E+0	9.651679466E-7	-8.587475275E-8	3.9949E+0	4.0498E+0	8.58524E+1	6.39289E+1	-3.124343976E-2	4.15E+2	7E+0	4E+0	1.8E+0	4.0348E+0	4.0916E+0	8.58166E+1	6.39289E+1	4.9E+0	4E+0	2.354307659E-2	1.4649E+0	-5.04E-2	2.2E+1	3E-2	2.99E-2
Magnet: Power Supply{Enum U16 ((IPS120,LS625,PS110,Hg iPS,SMS Series,Cryomagnetics 4G,DMG Little CryoFree,DMG Big CryoFree))}=Hg iPS	0E+0	1.227320997E-3	1.56E-1	1.227320997E-3	3.371767975E-6	8.78766569E-7	-5.7156E+0	8.745524954E-7	-8.903577462E-8	3.9885E+0	4.0482E+0	8.6139E+1	6.39289E+1	-3.18254903E-2	4.16E+2	7E+0	4E+0	1.8E+0	3.9949E+0	4.0498E+0	8.58524E+1	6.39289E+1	4.9E+0	4E+0	-3.124343976E-2	1.4649E+0	-5.04E-2	2.3E+1	2.5E-2	2.49E-2
Magnet: Rate{Double Float}=0.500000	0E+0	1.227152706E-3	1.56E-1	1.227152706E-3	3.371767975E-6	8.187074646E-7	-5.5104E+0	8.150200441E-7	-8.007944699E-8	4.0489E+0	4.0996E+0	8.60673E+1	6.39289E+1	5.011832714E-2	4.17E+2	7E+0	4E+0	1.8E+0	3.9885E+0	4.0482E+0	8.6139E+1	6.39289E+1	4.9E+0	4E+0	-3.18254903E-2	1.4649E+0	-5.04E-2	2.4E+1	2E-2	1.99E-2
Magnet: Setpoint{Double Float}=0.000000	0E+0	1.226816123E-3	1.56E-1	1.226816123E-3	3.371767975E-6	7.438969813E-7	-6.2436E+0	7.391556889E-7	-8.271361774E-8	4.062E+0	4.1131E+0	8.60673E+1	6.39289E+1	7.760020345E-2	4.18E+2	7E+0	4E+0	1.8E+0	4.0489E+0	4.0996E+0	8.60673E+1	6.39289E+1	4.9E+0	4E+0	5.011832714E-2	1.4649E+0	-5.04E-2	2.5E+1	1.5E-2	1.49E-2
Magnet: Units{Enum U16 ((Field,Current))}=Field	0E+0	1.226478126E-3	1.56E-1	1.226478126E-3	3.371767975E-6	6.933210274E-7	-6.3984E+0	6.880522333E-7	-7.849886534E-8	4.0088E+0	4.0764E+0	8.60315E+1	6.39289E+1	1.423993707E-2	4.19E+2	7E+0	4E+0	1.8E+0	4.062E+0	4.1131E+0	8.60673E+1	6.39289E+1	4.9E+0	4E+0	7.760020345E-2	1.4649E+0	-5.04E-2	2.6E+1	1E-2	1E-2
Magnet: VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	0E+0	1.226309835E-3	1.56E-1	1.226309835E-3	3.338050296E-6	6.295711084E-7	-7.8624E+0	6.227220721E-7	-8.798210066E-8	3.9396E+0	4.0224E+0	8.59957E+1	6.39289E+1	-7.345190644E-2	4.2E+2	7E+0	4E+0	1.8E+0	4.0088E+0	4.0764E+0	8.60315E+1	6.39289E+1	4.9E+0	4E+0	1.423993707E-2	1.4649E+0	-5.04E-2	2.7E+1	5E-3	5E-3
Main Screen Path{Path}=C:\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV\\\\1Code.vi	0E+0	1.226141543E-3	1.56E-1	1.226141543E-3	3.371767975E-6	5.505457031E-7	-8.1816E+0	5.442238856E-7	-8.007944699E-8	4.0001E+0	4.0588E+0	8.59957E+1	6.39289E+1	-2.013279684E-2	4.21E+2	7E+0	4E+0	1.8E+0	3.9396E+0	4.0224E+0	8.59957E+1	6.39289E+1	4.9E+0	4E+0	-7.345190644E-2	1.4649E+0	-5.04E-2	2.8E+1	0E+0	-1E-4
Measurement Timestamp{Timestamp}=<22:56:18.405 17/05/2023>T	0E+0	1.226309835E-3	1.56E-1	1.226309835E-3	3.371767975E-6	5.026035805E-7	-9.2652E+0	4.95754827E-7	-8.218671005E-8	3.9862E+0	4.0589E+0	8.59957E+1	6.39289E+1	-2.395525761E-2	4.22E+2	7E+0	4E+0	1.8E+0	4.0001E+0	4.0588E+0	8.59957E+1	6.39289E+1	4.9E+0	4E+0	-2.013279684E-2	1.4649E+0	-5.04E-2	2.9E+1	-5E-3	-5.1E-3
Measurement Title{String}=	0E+0	1.226647832E-3	1.56E-1	1.226647832E-3	3.338050296E-6	4.251589831E-7	-8.8224E+0	4.204174078E-7	-6.690842353E-8	3.9966E+0	4.0574E+0	8.59599E+1	6.39289E+1	-3.354703262E-2	4.23E+2	7E+0	4E+0	1.8E+0	3.9862E+0	4.0589E+0	8.59957E+1	6.39289E+1	4.9E+0	4E+0	-2.395525761E-2	1.4649E+0	-5.04E-2	3E+1	-1E-2	-1.04E-2
Measurment Select{U16}=4	0E+0	1.226984415E-3	1.56E-1	1.226984415E-3	3.371767975E-6	3.535092671E-7	-1.19856E+1	3.445527698E-7	-7.481102064E-8	3.9997E+0	4.0662E+0	8.59599E+1	6.39289E+1	-1.097173337E-2	4.24E+2	7E+0	4E+0	1.8E+0	3.9966E+0	4.0574E+0	8.59599E+1	6.39289E+1	4.9E+0	4E+0	-3.354703262E-2	1.4649E+0	-5.04E-2	3.1E+1	-1.5E-2	-1.5E-2
Measurment Select.__text__{String}=6221-Lockin-DAQ	0E+0	1.227152706E-3	1.56E-1	1.227152706E-3	3.338050296E-6	3.092537164E-7	-1.51188E+1	2.987172597E-7	-8.21867949E-8	4.0163E+0	4.0727E+0	8.59599E+1	6.39289E+1	1.208891906E-2	4.25E+2	7E+0	4E+0	1.8E+0	3.9997E+0	4.0662E+0	8.59599E+1	6.39289E+1	4.9E+0	4E+0	-1.097173337E-2	1.4649E+0	-5.04E-2	3.2E+1	-2E-2	-2.01E-2
Notes{String}=I+1A I-1E\\nrxx+1B Rxx-1C\\nRxy+1D Rxy-4A	0E+0	1.227320997E-3	1.56E-1	1.227320997E-3	3.371767975E-6	2.365504114E-7	-2.12868E+1	2.191652012E-7	-8.745524954E-8	4.0105E+0	4.0694E+0	8.59599E+1	6.39289E+1	1.395956054E-2	4.26E+2	7E+0	4E+0	1.8E+0	4.0163E+0	4.0727E+0	8.59599E+1	6.39289E+1	4.9E+0	4E+0	1.208891906E-2	1.4649E+0	-5.04E-2	3.3E+1	-2.5E-2	-2.5E-2
Offset{Double Float}=0.000000	0E+0	1.227490703E-3	1.56E-1	1.227490703E-3	3.338050296E-6	1.733302568E-7	-3.06444E+1	1.480418556E-7	-9.008947686E-8	4.0073E+0	4.0644E+0	8.59599E+1	6.39289E+1	-3.584156802E-4	4.27E+2	7E+0	4E+0	1.8E+0	4.0105E+0	4.0694E+0	8.59599E+1	6.39289E+1	4.9E+0	4E+0	1.395956054E-2	1.4649E+0	-5.04E-2	3.4E+1	-3E-2	-3.01E-2
Option: 2182 Autozero{Boolean}=True	0E+0	1.227827286E-3	1.56E-1	1.227827286E-3	3.371767975E-6	1.101093103E-7	-4.0014E+1	8.324052543E-8	-7.270370101E-8	4.0158E+0	4.0707E+0	8.59599E+1	6.39289E+1	4.325348418E-3	4.28E+2	7E+0	4E+0	1.8E+0	4.0073E+0	4.0644E+0	8.59599E+1	6.39289E+1	4.9E+0	4E+0	-3.584156802E-4	1.4649E+0	-5.04E-2	3.5E+1	-3.5E-2	-3.5E-2
Option: 2182 Front Autozero{Boolean}=True	0E+0	1.227827286E-3	1.56E-1	1.227827286E-3	3.371767975E-6	8.850895178E-8	-7.27128E+1	2.52882881E-8	-8.798210066E-8	4.0014E+0	4.0675E+0	8.59241E+1	6.39289E+1	-4.025208764E-3	4.29E+2	7E+0	4E+0	1.8E+0	4.0158E+0	4.0707E+0	8.59599E+1	6.39289E+1	4.9E+0	4E+0	4.325348418E-3	1.4649E+0	-5.04E-2	3.6E+1	-4E-2	-3.99E-2
Option: 2182 Hold{Boolean}=False	0E+0	1.227995577E-3	1.56E-1	1.227995577E-3	3.338050296E-6	9.641157717E-8	-1.1304E+2	-3.898604954E-8	-9.061624313E-8	4.0048E+0	4.0651E+0	8.59599E+1	6.39289E+1	-5.902066827E-3	4.3E+2	7E+0	4E+0	1.8E+0	4.0014E+0	4.0675E+0	8.59241E+1	6.39289E+1	4.9E+0	4E+0	-4.025208764E-3	1.4649E+0	-5.04E-2	3.7E+1	-4.5E-2	-4.52E-2
Option: 2182 Hold Count{I32}=10	0E+0	1.228163869E-3	1.56E-1	1.228163869E-3	3.338050296E-6	1.401388908E-7	-1.43634E+2	-1.148507724E-7	-8.534792991E-8	4.0127E+0	4.071E+0	8.56734E+1	6.39289E+1	4.333510529E-3	4.31E+2	7E+0	4E+0	1.8E+0	4.0048E+0	4.0651E+0	8.59599E+1	6.39289E+1	4.9E+0	4E+0	-5.902066827E-3	1.4649E+0	-5.04E-2	3.8E+1	-5E-2	-5.01E-2
Option: 2182 Hold Window{Double Float}=1.000000	0E+0	1.228163869E-3	1.56E-1	1.228163869E-3	3.371767975E-6	1.343436699E-7	-1.462104E+2	-1.143239779E-7	-7.691839683E-8	4.0171E+0	4.0771E+0	8.56734E+1	6.39289E+1	1.359083969E-2	4.32E+2	7E+0	4E+0	1.8E+0	4.0127E+0	4.071E+0	8.56734E+1	6.39289E+1	4.9E+0	4E+0	4.333510529E-3	1.4649E+0	-5.04E-2	3.9E+1	-5E-2	-5E-2
Option: 2182 Line Sync{Boolean}=False	0E+0	1.228333574E-3	1.56E-1	1.228333574E-3	3.338050296E-6	2.486676761E-7	-1.591008E+2	-2.349698863E-7	-9.114303768E-8	3.9998E+0	4.0649E+0	8.5745E+1	6.39289E+1	-5.094471853E-3	4.33E+2	7E+0	4E+0	1.8E+0	4.0171E+0	4.0771E+0	8.56734E+1	6.39289E+1	4.9E+0	4E+0	1.359083969E-2	1.4649E+0	-5.04E-2	4E+1	-6E-2	-6E-2
Option: 2182 Reference Reading{Double Float}=0.000000	0E+0	1.228501866E-3	1.56E-1	1.228501866E-3	3.371767975E-6	3.787971027E-7	-1.665288E+2	-3.708947601E-7	-8.956256917E-8	4.0183E+0	4.0812E+0	8.57092E+1	6.39289E+1	1.731209084E-2	4.34E+2	7E+0	4E+0	1.8E+0	3.9998E+0	4.0649E+0	8.5745E+1	6.39289E+1	4.9E+0	4E+0	-5.094471853E-3	1.4649E+0	-5.04E-2	4.1E+1	-7E-2	-7E-2
Option: 2182 Relative Mode{Boolean}=False	0E+0	1.228670157E-3	1.56E-1	1.228670157E-3	3.371767975E-6	5.083990277E-7	-1.716648E+2	-5.062915666E-7	-7.533784347E-8	4.0074E+0	4.0707E+0	8.5745E+1	6.39289E+1	-2.027486917E-3	4.35E+2	7E+0	4E+0	1.8E+0	4.0183E+0	4.0812E+0	8.57092E+1	6.39289E+1	4.9E+0	4E+0	1.731209084E-2	1.4649E+0	-5.04E-2	4.2E+1	-8E-2	-7.99E-2
Option: 2182 Trigger Delay{Cluster (Boolean,Double Float)}={'Auto':True,'Time(s)':0.000000}	0E+0	1.228838449E-3	1.56E-1	1.228838449E-3	3.371767975E-6	6.448497061E-7	-1.72194E+2	-6.411614371E-7	-8.903571805E-8	3.9972E+0	4.0645E+0	8.5745E+1	6.39289E+1	-3.870947519E-3	4.36E+2	7E+0	4E+0	1.8E+0	4.0074E+0	4.0707E+0	8.5745E+1	6.39289E+1	4.9E+0	4E+0	-2.027486917E-3	1.4649E+0	-5.04E-2	4.3E+1	-9E-2	-8.99E-2
Option: 2182 Trigger Source{Enum U16 ((Immediate,Timer,Manual,Bus,Trigger link))}=Bus	0E+0	1.22900674E-3	1.56E-1	1.22900674E-3	3.371767975E-6	7.828826066E-7	-1.730652E+2	-7.802487753E-7	-9.588464119E-8	4.0192E+0	4.0764E+0	8.61032E+1	6.39289E+1	1.078316197E-2	4.37E+2	7E+0	4E+0	1.8E+0	3.9972E+0	4.0645E+0	8.5745E+1	6.39289E+1	4.9E+0	4E+0	-3.870947519E-3	1.4649E+0	-5.04E-2	4.4E+1	-1E-1	-9.99E-2
Option: 2182 Trigger Timer{Double Float}=0.000000	0E+0	1.22900674E-3	1.56E-1	1.22900674E-3	3.371767975E-6	7.765607891E-7	-1.739124E+2	-7.749802641E-7	-8.42941711E-8	4.0104E+0	4.0763E+0	8.6139E+1	6.39289E+1	1.01019796E-2	4.38E+2	7E+0	4E+0	1.8E+0	4.0192E+0	4.0764E+0	8.61032E+1	6.39289E+1	4.9E+0	4E+0	1.078316197E-2	1.4649E+0	-5.04E-2	4.5E+1	-1E-1	-9.99E-2
Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	0E+0	1.2303559E-3	1.56E-1	1.2303559E-3	3.371767975E-6	3.392839757E-6	-1.784796E+2	-3.393894761E-6	-9.114312253E-8	4.8594E+0	4.6874E+0	8.60673E+1	6.39289E+1	8.63695085E-1	4.39E+2	7E+0	4E+0	1.8E+0	4.0104E+0	4.0763E+0	8.6139E+1	6.39289E+1	4.9E+0	4E+0	1.01019796E-2	1.4649E+0	-5.04E-2	4.6E+1	-3E-1	-2.998E-1
Option: 560 Enabled{Boolean}=False	0E+0	1.232446956E-3	1.524E-1	1.232446956E-3	3.270614936E-6	6.031255976E-6	-1.790736E+2	-6.033886414E-6	-9.957257075E-8	3.2266E+0	3.39E+0	8.59599E+1	6.39289E+1	-1.529096603E+0	4.4E+2	7E+0	4E+0	1.8E+0	4.8594E+0	4.6874E+0	8.60673E+1	6.39289E+1	4.9E+0	4E+0	8.63695085E-1	1.4649E+0	-5.04E-2	4.7E+1	-5E-1	-4.999E-1
Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	0E+0	1.233559093E-3	1.56E-1	1.233559093E-3	3.371767975E-6	8.643305598E-6	-1.792956E+2	-8.645941692E-6	-1.074751113E-7	3.8771E+0	3.9225E+0	8.59599E+1	6.39289E+1	-4.478380084E-1	4.41E+2	7E+0	4E+0	1.8E+0	3.2266E+0	3.39E+0	8.59599E+1	6.39289E+1	4.9E+0	4E+0	-1.529096603E+0	1.4649E+0	-5.04E-2	4.8E+1	-7E-1	-6.999E-1
Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	0E+0	1.235076545E-3	1.548E-1	1.235076545E-3	3.338050296E-6	1.126698854E-5	-1.793832E+2	-1.126962181E-5	-1.227533412E-7	3.9922E+0	4.0382E+0	8.56375E+1	6.39289E+1	2.61760354E-1	4.42E+2	7E+0	4E+0	1.8E+0	3.8771E+0	3.9225E+0	8.59599E+1	6.39289E+1	4.9E+0	4E+0	-4.478380084E-1	1.4649E+0	-5.04E-2	4.9E+1	-9E-1	-8.998E-1
Option: 6221 Adjust Mode{Enum U16 ((Offset,Frequency,Amplitude))}=Offset	0E+0	1.236930579E-3	1.56E-1	1.236930579E-3	3.371767975E-6	1.389905494E-5	-1.794672E+2	-1.390169386E-5	-1.301290024E-7	4.0076E+0	4.061E+0	8.57092E+1	6.39289E+1	3.509793431E-2	4.43E+2	7E+0	4E+0	1.8E+0	3.9922E+0	4.0382E+0	8.56375E+1	6.39289E+1	4.9E+0	4E+0	2.61760354E-1	1.4649E+0	-5.04E-2	5E+1	-1.1E+0	-1.1E+0
Option: 6221 Amplitude{Double Float}=1.000000E-6	0E+0	1.239290901E-3	1.56E-1	1.239290901E-3	3.371767975E-6	1.653215654E-5	-1.795908E+2	-1.653481527E-5	-1.195924325E-7	4.0045E+0	4.0651E+0	8.60673E+1	6.39289E+1	-3.091142979E-3	4.44E+2	7E+0	4E+0	1.8E+0	4.0076E+0	4.061E+0	8.57092E+1	6.39289E+1	4.9E+0	4E+0	3.509793431E-2	1.4649E+0	-5.04E-2	5.1E+1	-1.3E+0	-1.2998E+0
Option: 6221 Compliance{Double Float}=10.000000	0E+0	1.241651223E-3	1.56E-1	1.241651223E-3	3.371767975E-6	1.919008608E-5	-1.79592E+2	-1.919271652E-5	-1.385585637E-7	4.037E+0	4.0731E+0	8.59599E+1	6.39289E+1	-1.069670636E-2	4.45E+2	7E+0	4E+0	1.8E+0	4.0045E+0	4.0651E+0	8.60673E+1	6.39289E+1	4.9E+0	4E+0	-3.091142979E-3	1.4649E+0	-5.04E-2	5.2E+1	-1.5E+0	-1.4999E+0
Option: 6221 Duty Cycle{Double Float}=50.000000	0E+0	1.241819515E-3	1.56E-1	1.241819515E-3	3.371767975E-6	1.918216649E-5	-1.796208E+2	-1.918479692E-5	-1.280218242E-7	3.9574E+0	4.0485E+0	8.59599E+1	6.39289E+1	-4.383438826E-2	4.46E+2	7E+0	4E+0	1.8E+0	4.037E+0	4.0731E+0	8.59599E+1	6.39289E+1	4.9E+0	4E+0	-1.069670636E-2	1.4649E+0	-5.04E-2	5.3E+1	-1.5E+0	-1.5E+0
Option: 6221 External Trigger{Boolean}=False	0E+0	1.236087707E-3	1.56E-1	1.236087707E-3	3.371767975E-6	1.258302457E-5	-1.79472E+2	-1.258565783E-5	-1.169580638E-7	3.9503E+0	4.0407E+0	8.59241E+1	6.39289E+1	-6.210357323E-2	4.47E+2	7E+0	4E+0	1.8E+0	3.9574E+0	4.0485E+0	8.59599E+1	6.39289E+1	4.9E+0	4E+0	-4.383438826E-2	1.4649E+0	-5.04E-2	5.4E+1	-1E+0	-1.0001E+0
Option: 6221 External Trigger Ignore Multiple{Boolean}=False	0E+0	1.232041642E-3	1.56E-1	1.232041642E-3	3.371767975E-6	6.01281746E-6	-1.792728E+2	-6.015450726E-6	-7.797209908E-8	4.064E+0	4.0997E+0	8.61032E+1	6.39289E+1	3.686305508E-2	4.48E+2	7E+0	4E+0	1.8E+0	3.9503E+0	4.0407E+0	8.59241E+1	6.39289E+1	4.9E+0	4E+0	-6.210357323E-2	1.4649E+0	-5.04E-2	5.5E+1	-5E-1	-5.001E-1
Option: 6221 Frequency{Double Float}=119.770000	
Option: 6221 Function{U16}=1	
Option: 6221 Function.__text__{String}=Sine	
Option: 6221 Idle Level{Double Float}=0.000000	
Option: 6221 Input trigger Line{U8}=5	
Option: 6221 Offset{Double Float}=0.000000	
Option: 6221 Output Trigger Line{U8}=4	
Option: 6221 Pass Through{Boolean}=True	
Option: 6221 Phase Marker{Boolean}=True	
Option: 6221 Phase Marker Phase{Double Float}=0.000000	
Option: 6221 Range Level{Double Float}=2.000000E-12	
Option: 6221 Ranging{U16}=1	
Option: 6221 Ranging.__text__{String}=Best	
Option: 6221 Update Clock{Double Float}=0.000000	
Option: 6221 VISA{Visa Refnum (Void)}=GPIB0::13::INSTR	
Option: Confirm Config{Boolean}=False	
Option: Control Panel Ref{LVObjVI Refnum (Void)}=	
Option: DAQ Global Channel{Boolean}=False	
Option: DAQ Input Rate{Double Float}=10000.000000	
Option: DAQ Input Samples{I32}=200	
Option: DAQ Measurement Channels{1D Array (Cluster (UserDefinedRefnumTag Refnum (Void),\tkDAQmxPhysChanTagType Tag,\tkDAQmxScaleTagType Tag,Boolean,Double Float,String))}=[]	
Option: Differential{I32}=10106	
Option: Differential.__text__{String}=Differential	
Option: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values))}=Function Generator	
Option: Lockin Standoff Time{Double Float}=0.000000	
Option: Paranoid Save Data{Boolean}=True	
Option: Plot Autoback Path{Path}=C:\\\\TEMP\\\\XY Multiparam\\\\Backup.txt	
Option: SR830  Ref Phase{Double Float}=0.000000	
Option: SR830  Synch Filter{Boolean}=False	
Option: SR830  Time Constant{I16}=8	
Option: SR830  Time Constant.__text__{String}=100 ms	
Option: SR830 2x Line Filter{Boolean}=True	
Option: SR830 Adjust Gains{Boolean}=False	
Option: SR830 Auto Gain Lower.__text__{String}=2 nV/fA	
Option: SR830 Auto Gain Upper.__text__{String}=1 V/uA	
Option: SR830 Auto Offset 1{Boolean}=False	
Option: SR830 Auto Offset 2{Boolean}=False	
Option: SR830 Autophase{Boolean}=False	
Option: SR830 DC Coupling?{Boolean}=False	
Option: SR830 Display 1{U16}=0	
Option: SR830 Display 1.__text__{String}=X	
Option: SR830 Display 2{U16}=0	
Option: SR830 Display 2.__text__{String}=Y	
Option: SR830 Dynamic Reserve{I16}=1	
Option: SR830 Dynamic Reserve.__text__{String}=Normal	
Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Option: SR830 Filter Slope{I32}=1	
Option: SR830 Filter Slope.__text__{String}=12 dB/oct	
Option: SR830 Gain{I32}=-1	
Option: SR830 Gain.__text__{String}=Auto Gain	
Option: SR830 Ground Shield?{Boolean}=False	
Option: SR830 Harmonic{I32}=1	
Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A	
Option: SR830 Line Filter{Boolean}=True	
Option: SR830 No Reset{Boolean}=False	
Option: SR830 Offset 1{Double Float}=0.000000	
Option: SR830 Offset 2{Double Float}=0.000000	
Option: SR830 Output Channel 1{Boolean}=False	
Option: SR830 Output Channel 2{Boolean}=False	
Option: SR830 Ratio 1{U16}=0	
Option: SR830 Ratio 1.__text__{String}=None	
Option: SR830 Ratio 2{U16}=0	
Option: SR830 Ratio 2.__text__{String}=None	
Option: SR830 Ref Amplitude{Double Float}=0.100000	
Option: SR830 Ref Frequency{Double Float}=1013.000000	
Option: SR830 Ref Source{Boolean}=False	
Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta]	
Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Option: SR830 VISA{Visa Refnum (Void)}=	
Option: Sense Autorange{Boolean}=False	
Option: Sense Range Level{Double Float}=0.100000	
Option: Sense Rate{Double Float}=1.000000	
Option:560 Comport{Visa Refnum (Void)}=COM1	
Option:560 Filter High Pass{U16}=0	
Option:560 Filter High Pass.__text__{String}=0.03	
Option:560 Filter Lowpass{U16}=0	
Option:560 Filter Lowpass.__text__{String}=0.03	
Option:560 Filter Mode{U16}=0	
Option:560 Filter Mode.__text__{String}=6 dB high pass	
Option:560 Invert{Boolean}=False	
Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Option:570 Enabled{Boolean}=False	
Option:570 Filter High Pass{U16}=0	
Option:570 Filter High Pass.__text__{String}=0.03	
Option:570 Filter Lowpass{U16}=0	
Option:570 Filter Lowpass.__text__{String}=0.03	
Option:570 Filter Mode{U16}=0	
Option:570 Filter Mode.__text__{String}=6 dB high pass	
Option:570 Gain Mode{U16}=0	
Option:570 Gain Mode.__text__{String}=Low Noise	
Option:570 Input Offset{U16}=0	
Option:570 Input Offset On{Boolean}=False	
Option:570 Input Offset.__text__{String}=1pA	
Option:570 Sensitivity{U16}=0	
Option:570 Sensitivity.__text__{String}=1pA/V	
Option:Debug On{Boolean}=False	
Option:GPIB 2182{Visa Refnum (Void)}=	
Option:Parallel Config Voltage Measurers{Boolean}=True	
Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Option:SR830 Settle Time{Double Float}=5.000000	
Option:Sense Digits{I32}=8	
Output Names{1D Array (String)}=['Offset','Rxx::R','Rxx::Theta','Rxx::X','Rxx::Y','Rxy::R','Rxy::Theta','Rxy::X','Rxy::Y','temperature: T1','temperature: T2','temperature: T3','temperature: T4','temperature: dT/dt','iterator','multi[0]:iterator','multi[0]:y','multi[0]:temperature: setpoint','multi[0]:temperature: T1','multi[0]:temperature: T2','multi[0]:temperature: T3','multi[0]:temperature: T4','multi[0]:temperature: heater','multi[0]:temperature: gas','multi[0]:temperature: dT/dt','multi[0]:temperature: current temperature','multi[0]:temperature: error','multi[1]:iterator','multi[1]:y','multi[1]:Control:Magnet Output']	
Parameter Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Parameter Select{U16}=6	
Parameter Select.__text__{String}=Multi-Parameter	
Paths{U32}=0	
Plot: Column Renames{1D Array (Cluster (String,String))}=[]	
Plot: No dups{Boolean}=False	
Plot: StdDevs{Boolean}=False	
Plotting Class{String}=Parameter Plot	
Plotting Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	
Plotting Select{U16}=1	
Plotting Select.__text__{String}=Parameter Plot	
Project Code{String}=Topological_Insulators	
Ref: Temperature Window{LVObjVI Refnum (Void)}=	
Ref:Control Subpanel{LVObjUnknown Refnum (Void)}=	
Ref:Main Screen{LVObjVI Refnum (Void)}=	
Ref:Plotting Subpanel{LVObjUnknown Refnum (Void)}=	
Ref:Toolbar{LVObjUnknown Refnum (Void)}=	
Ref:XY Subpanel{LVObjUnknown Refnum (Void)}=	
Rxx::R{Double Float}=0.001232	
Rxx::Theta{Double Float}=0.156000	
Rxx::X{Double Float}=0.001232	
Rxx::Y{Double Float}=3.371768E-6	
Rxx:Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	
Rxx:Option: 560 Enabled{Boolean}=False	
Rxx:Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	
Rxx:Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	
Rxx:Option: Lockin Standoff Time{Double Float}=0.000000	
Rxx:Option: Lockin Type{Enum U16 ((SRS 830,EG&G 5302))}=SRS 830	
Rxx:Option: SR803 Full Scale Reading{Double Float}=0.000000	
Rxx:Option: SR830  Ref Phase{Double Float}=0.000000	
Rxx:Option: SR830  Synch Filter{Boolean}=False	
Rxx:Option: SR830  Time Constant{I16}=8	
Rxx:Option: SR830 2x Line Filter{Boolean}=False	
Rxx:Option: SR830 Adjust Gains{Boolean}=False	
Rxx:Option: SR830 Auto Gain Lower{I32}=0	
Rxx:Option: SR830 Auto Gain Upper{I32}=26	
Rxx:Option: SR830 Auto Offset 1{Boolean}=False	
Rxx:Option: SR830 Auto Offset 2{Boolean}=False	
Rxx:Option: SR830 Autophase{Boolean}=False	
Rxx:Option: SR830 DC Coupling?{Boolean}=False	
Rxx:Option: SR830 Display 1{U16}=0	
Rxx:Option: SR830 Display 2{U16}=0	
Rxx:Option: SR830 Dynamic Reserve{I16}=2	
Rxx:Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Rxx:Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Rxx:Option: SR830 Filter Slope{I32}=3	
Rxx:Option: SR830 Gain{I32}=18	
Rxx:Option: SR830 Ground Shield?{Boolean}=False	
Rxx:Option: SR830 Harmonic{I32}=1	
Rxx:Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A-B	
Rxx:Option: SR830 Line Filter{Boolean}=False	
Rxx:Option: SR830 No Reset{Boolean}=False	
Rxx:Option: SR830 Offset 1{Double Float}=0.000000	
Rxx:Option: SR830 Offset 2{Double Float}=0.000000	
Rxx:Option: SR830 Output Channel 1{Boolean}=False	
Rxx:Option: SR830 Output Channel 2{Boolean}=False	
Rxx:Option: SR830 Ratio 1{U16}=0	
Rxx:Option: SR830 Ratio 2{U16}=0	
Rxx:Option: SR830 Ref Amplitude{Double Float}=0.100000	
Rxx:Option: SR830 Ref Frequency{Double Float}=1013.000000	
Rxx:Option: SR830 Ref Source{Boolean}=False	
Rxx:Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta,X,Y]	
Rxx:Option: SR830 Time Constant value{Double Float}=0.000000	
Rxx:Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Rxx:Option: SR830 VISA{Visa Refnum (Void)}=GPIB0::5::INSTR	
Rxx:Option:560 Comport{Visa Refnum (Void)}=COM1	
Rxx:Option:560 Filter High Pass{U16}=0	
Rxx:Option:560 Filter Lowpass{U16}=0	
Rxx:Option:560 Filter Mode{U16}=0	
Rxx:Option:560 Invert{Boolean}=False	
Rxx:Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Rxx:Option:570 Enabled{Boolean}=False	
Rxx:Option:570 Filter High Pass{U16}=0	
Rxx:Option:570 Filter Lowpass{U16}=0	
Rxx:Option:570 Filter Mode{U16}=0	
Rxx:Option:570 Gain Mode{U16}=0	
Rxx:Option:570 Input Offset{U16}=0	
Rxx:Option:570 Input Offset On{Boolean}=False	
Rxx:Option:570 Sensitivity{U16}=0	
Rxx:Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Rxx:Option:SR830 Autogain Lower Threshold{Double Float}=0.100000	
Rxx:Option:SR830 Autogain Standoff{Double Float}=3.000000	
Rxx:Option:SR830 Autogain Upper Threshold{Double Float}=0.900000	
Rxx:Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Rxx:Option:SR830 Settle Time{Double Float}=0.000000	
Rxy::R{Double Float}=6.012817E-6	
Rxy::Theta{Double Float}=-179.272800	
Rxy::X{Double Float}=-6.015451E-6	
Rxy::Y{Double Float}=-7.797210E-8	
Rxy:Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	
Rxy:Option: 560 Enabled{Boolean}=False	
Rxy:Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	
Rxy:Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	
Rxy:Option: Lockin Standoff Time{Double Float}=0.000000	
Rxy:Option: Lockin Type{Enum U16 ((SRS 830,EG&G 5302))}=SRS 830	
Rxy:Option: SR803 Full Scale Reading{Double Float}=0.000000	
Rxy:Option: SR830  Ref Phase{Double Float}=0.000000	
Rxy:Option: SR830  Synch Filter{Boolean}=False	
Rxy:Option: SR830  Time Constant{I16}=8	
Rxy:Option: SR830 2x Line Filter{Boolean}=False	
Rxy:Option: SR830 Adjust Gains{Boolean}=False	
Rxy:Option: SR830 Auto Gain Lower{I32}=0	
Rxy:Option: SR830 Auto Gain Upper{I32}=26	
Rxy:Option: SR830 Auto Offset 1{Boolean}=False	
Rxy:Option: SR830 Auto Offset 2{Boolean}=False	
Rxy:Option: SR830 Autophase{Boolean}=False	
Rxy:Option: SR830 DC Coupling?{Boolean}=False	
Rxy:Option: SR830 Display 1{U16}=0	
Rxy:Option: SR830 Display 2{U16}=1	
Rxy:Option: SR830 Dynamic Reserve{I16}=2	
Rxy:Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Rxy:Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Rxy:Option: SR830 Filter Slope{I32}=3	
Rxy:Option: SR830 Gain{I32}=18	
Rxy:Option: SR830 Ground Shield?{Boolean}=False	
Rxy:Option: SR830 Harmonic{I32}=1	
Rxy:Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A-B	
Rxy:Option: SR830 Line Filter{Boolean}=False	
Rxy:Option: SR830 No Reset{Boolean}=False	
Rxy:Option: SR830 Offset 1{Double Float}=0.000000	
Rxy:Option: SR830 Offset 2{Double Float}=0.000000	
Rxy:Option: SR830 Output Channel 1{Boolean}=False	
Rxy:Option: SR830 Output Channel 2{Boolean}=False	
Rxy:Option: SR830 Ratio 1{U16}=0	
Rxy:Option: SR830 Ratio 2{U16}=0	
Rxy:Option: SR830 Ref Amplitude{Double Float}=0.100000	
Rxy:Option: SR830 Ref Frequency{Double Float}=1013.000000	
Rxy:Option: SR830 Ref Source{Boolean}=False	
Rxy:Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta,X,Y]	
Rxy:Option: SR830 Time Constant value{Double Float}=0.000000	
Rxy:Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Rxy:Option: SR830 VISA{Visa Refnum (Void)}=GPIB0::6::INSTR	
Rxy:Option:560 Comport{Visa Refnum (Void)}=COM1	
Rxy:Option:560 Filter High Pass{U16}=0	
Rxy:Option:560 Filter Lowpass{U16}=0	
Rxy:Option:560 Filter Mode{U16}=0	
Rxy:Option:560 Invert{Boolean}=False	
Rxy:Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Rxy:Option:570 Enabled{Boolean}=False	
Rxy:Option:570 Filter High Pass{U16}=0	
Rxy:Option:570 Filter Lowpass{U16}=0	
Rxy:Option:570 Filter Mode{U16}=0	
Rxy:Option:570 Gain Mode{U16}=0	
Rxy:Option:570 Input Offset{U16}=0	
Rxy:Option:570 Input Offset On{Boolean}=False	
Rxy:Option:570 Sensitivity{U16}=0	
Rxy:Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Rxy:Option:SR830 Autogain Lower Threshold{Double Float}=0.100000	
Rxy:Option:SR830 Autogain Standoff{Double Float}=3.000000	
Rxy:Option:SR830 Autogain Upper Threshold{Double Float}=0.900000	
Rxy:Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Rxy:Option:SR830 Settle Time{Double Float}=0.000000	
Sample ID{String}=MBE202221213_PA_D1 750C Cracker WAL	
Save:Filename{String}=${X-Y Class} ${2nd Parameter Class} ${iterator}{%04d} ${y}{%04.2g}.txt	
Save:Final Filename{String}=${X-Y Class} ${2nd Parameter Class} .txt	
Save:Final path{Path}=C:\\\\Data\\\\${Project Code}\\\\${User}\\\\${Sample ID}\\\\${Measurement Timestamp}{%Y%m%d}\\\\${X-Y Class}	
Save:Path{Path}=C:\\\\Data\\\\${Project Code}\\\\${User}\\\\${Sample ID}\\\\${Measurement Timestamp}{%Y%m%d}\\\\${X-Y Class}	
Startup path{Path}=C:\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV	
Sub Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Sweep Step{I32}=3	
T Control Measure.__text__{1D Array (String)}=['temperature: T1','temperature: T2','temperature: T3','temperature: T4','temperature: dT/dt']	
Timestamp{Timestamp}=<22:57:27.929 17/05/2023>T	
Toolbar{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Unaved Data{Boolean}=True	
Unsaved Data{Boolean}=False	
User{String}=Craig	
X-Y Class{String}=6221-Lockin-DAQ	
X-Y Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	
d(Offset){Double Float}=0.000000	
d(Rxx::R){Double Float}=0.000000	
d(Rxx::Theta){Double Float}=0.000000	
d(Rxx::X){Double Float}=0.000000	
d(Rxx::Y){Double Float}=4.735058E-22	
d(Rxy::R){Double Float}=8.032886E-9	
d(Rxy::Theta){Double Float}=0.098900	
d(Rxy::X){Double Float}=8.035668E-9	
d(Rxy::Y){Double Float}=1.063519E-8	
iterate result{U16}=5	
iterator{I32}=448	
multi[0]:Control: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values,Adaptive Step Ramp))}=List of Values	
multi[0]:Control: Monitor Update Timeout{Double Float}=0.010000	
multi[0]:Control: Open T Window{Boolean}=False	
multi[0]:Control: Reverse Temperature Sense{Boolean}=False	
multi[0]:Iterator{I32}=0	
multi[0]:Ref: Temperature Window{LVObjVI Refnum (Void)}=	
multi[0]:iterate result{U16}=0	
multi[0]:iterator{I32}=7	
multi[0]:temperature:  rate window{Double Float}=120.000000	
multi[0]:temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[0]:temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
multi[0]:temperature: T1{Double Float}=3.974800	
multi[0]:temperature: T2{Double Float}=4.045200	
multi[0]:temperature: T3{Double Float}=85.959900	
multi[0]:temperature: T4{Double Float}=63.928900	
multi[0]:temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
multi[0]:temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
multi[0]:temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
multi[0]:temperature: current temperature{Double Float}=1.464900	
multi[0]:temperature: current temperature 2{Double Float}=287.100000	
multi[0]:temperature: dT/dt{Double Float}=-0.036044	
multi[0]:temperature: error{Double Float}=-0.050400	
multi[0]:temperature: gas{Double Float}=4.000000	
multi[0]:temperature: gas control{Boolean}=False	
multi[0]:temperature: gas control 2{Boolean}=False	
multi[0]:temperature: gass boost{I8}=0	
multi[0]:temperature: gass boost 2{I8}=0	
multi[0]:temperature: gast flow{I16}=0	
multi[0]:temperature: gast flow 2{I16}=7	
multi[0]:temperature: heater{Double Float}=4.900000	
multi[0]:temperature: heater output{Double Float}=0.000000	
multi[0]:temperature: heater output 2{Double Float}=0.000000	
multi[0]:temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
multi[0]:temperature: monitor timeout{Double Float}=0.010000	
multi[0]:temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
multi[0]:temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
multi[0]:temperature: ramp rate{Double Float}=8.000000	
multi[0]:temperature: ramp rate 2{Double Float}=0.000000	
multi[0]:temperature: ramp target{Double Float}=20.000000	
multi[0]:temperature: ramp target 2{Double Float}=0.000000	
multi[0]:temperature: ramping{Boolean}=False	
multi[0]:temperature: setpoint{Double Float}=1.800000	
multi[0]:temperature: setpoint 2{Double Float}=287.100000	
multi[0]:temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
multi[0]:temperature: stability error{Extended Float}=0.040000	
multi[0]:temperature: stability script{String}=	
multi[0]:temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
multi[0]:temperature: temp control mode{U16}=2	
multi[0]:temperature: temp control mode 2{U16}=3	
multi[0]:temperature: temp control mode 2.__text__{String}=Open Loop	
multi[0]:temperature: temp control mode.__text__{String}=Zone	
multi[0]:temperature: temp control sensor{U16}=0	
multi[0]:temperature: temp control sensor 2{U16}=0	
multi[0]:temperature: temp control sensor 2.__text__{String}=Sensor 1	
multi[0]:temperature: temp control sensor.__text__{String}=Sensor A	
multi[0]:temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
multi[0]:temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
multi[0]:temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
multi[0]:temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
multi[0]:temperature: temp loop{U16}=0	
multi[0]:temperature: temp loop 2{U16}=0	
multi[0]:temperature: temp loop 2.__text__{String}=Heater	
multi[0]:temperature: temp loop.__text__{String}=Loop 1	
multi[0]:temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
multi[0]:temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[0]:temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[0]:temperature:error for gas boost{Double Float}=0.000000	
multi[0]:temperature:error for gas boost 2{Double Float}=0.000000	
multi[0]:temperature:heater range{U16}=2	
multi[0]:temperature:heater range 2{U16}=0	
multi[0]:temperature:heater range 2.__text__{String}=Off	
multi[0]:temperature:heater range.__text__{String}=40mW	
multi[0]:temperature:history window{Extended Float}=300.000000	
multi[0]:temperature:is stable?{Boolean}=True	
multi[0]:temperature:monitor{Boolean}=True	
multi[0]:temperature:ramping{Boolean}=False	
multi[0]:temperature:ramping on{Boolean}=False	
multi[0]:temperature:ramping on 2{Boolean}=False	
multi[0]:temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
multi[0]:temperature:stability code{U32}=6618880	
multi[0]:temperature:stability rate{Extended Float}=0.040000	
multi[0]:y{Double Float}=4.000000	
multi[1]:Control: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values,Adaptive Step Ramp))}=Multi-Segment Ramp	
multi[1]:Control: Gate delay{Double Float}=0.000000	
multi[1]:Control: Monitor Update Timeout{Double Float}=0.010000	
multi[1]:Control: Open T Window{Boolean}=False	
multi[1]:Control: Reverse Temperature Sense{Boolean}=False	
multi[1]:Control:Magnet Output{Double Float}=-0.000000	
multi[1]:Iterator{I32}=0	
multi[1]:Magnet: Final Switch Heater{Enum U8 ((False,True,Mixed))}=	
multi[1]:Magnet: Power Supply{Enum U16 ((IPS120,LS625,PS110,Hg iPS,SMS Series,Cryomagnetics 4G,DMG Little CryoFree,DMG Big CryoFree))}=Hg iPS	
multi[1]:Magnet: Rate{Double Float}=0.500000	
multi[1]:Magnet: Units{Enum U16 ((Field,Current))}=Field	
multi[1]:Magnet: VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[1]:Multi-segment_Stage{I32}=0	
multi[1]:Multi-segment_Stage_Changed{Boolean}=False	
multi[1]:Ref: Temperature Window{LVObjVI Refnum (Void)}=	
multi[1]:iterate result{U16}=4	
multi[1]:iterator{I32}=57	
multi[1]:measure point{Boolean}=False	
multi[1]:temperature:  rate window{Double Float}=120.000000	
multi[1]:temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[1]:temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
multi[1]:temperature: T1{Double Float}=1.842400	
multi[1]:temperature: T2{Double Float}=1.465600	
multi[1]:temperature: T3{Double Float}=86.318100	
multi[1]:temperature: T4{Double Float}=66.769200	
multi[1]:temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
multi[1]:temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
multi[1]:temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
multi[1]:temperature: current temperature{Double Float}=1.465600	
multi[1]:temperature: current temperature 2{Double Float}=287.100000	
multi[1]:temperature: dT/dt{Double Float}=-0.001864	
multi[1]:temperature: gas control{Boolean}=False	
multi[1]:temperature: gas control 2{Boolean}=False	
multi[1]:temperature: gass boost{I8}=0	
multi[1]:temperature: gass boost 2{I8}=0	
multi[1]:temperature: gast flow{I16}=0	
multi[1]:temperature: gast flow 2{I16}=7	
multi[1]:temperature: heater output{Double Float}=0.000000	
multi[1]:temperature: heater output 2{Double Float}=0.000000	
multi[1]:temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
multi[1]:temperature: monitor timeout{Double Float}=1.000000	
multi[1]:temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
multi[1]:temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
multi[1]:temperature: ramp rate{Double Float}=8.000000	
multi[1]:temperature: ramp rate 2{Double Float}=0.000000	
multi[1]:temperature: ramp target{Double Float}=20.000000	
multi[1]:temperature: ramp target 2{Double Float}=0.000000	
multi[1]:temperature: ramping{Boolean}=False	
multi[1]:temperature: setpoint{Double Float}=1.800000	
multi[1]:temperature: setpoint 2{Double Float}=287.100000	
multi[1]:temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
multi[1]:temperature: stability error{Extended Float}=0.040000	
multi[1]:temperature: stability script{String}=	
multi[1]:temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
multi[1]:temperature: temp control mode{U16}=2	
multi[1]:temperature: temp control mode 2{U16}=3	
multi[1]:temperature: temp control mode 2.__text__{String}=Open Loop	
multi[1]:temperature: temp control mode.__text__{String}=Zone	
multi[1]:temperature: temp control sensor{U16}=0	
multi[1]:temperature: temp control sensor 2{U16}=0	
multi[1]:temperature: temp control sensor 2.__text__{String}=Sensor 1	
multi[1]:temperature: temp control sensor.__text__{String}=Sensor A	
multi[1]:temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
multi[1]:temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
multi[1]:temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
multi[1]:temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
multi[1]:temperature: temp loop{U16}=0	
multi[1]:temperature: temp loop 2{U16}=0	
multi[1]:temperature: temp loop 2.__text__{String}=Heater	
multi[1]:temperature: temp loop.__text__{String}=Loop 1	
multi[1]:temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
multi[1]:temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[1]:temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[1]:temperature:error for gas boost{Double Float}=0.000000	
multi[1]:temperature:error for gas boost 2{Double Float}=0.000000	
multi[1]:temperature:heater range{U16}=2	
multi[1]:temperature:heater range 2{U16}=0	
multi[1]:temperature:heater range 2.__text__{String}=Off	
multi[1]:temperature:heater range.__text__{String}=40mW	
multi[1]:temperature:history window{Extended Float}=300.000000	
multi[1]:temperature:is stable?{Boolean}=True	
multi[1]:temperature:monitor{Boolean}=True	
multi[1]:temperature:ramping{Boolean}=False	
multi[1]:temperature:ramping on{Boolean}=False	
multi[1]:temperature:ramping on 2{Boolean}=False	
multi[1]:temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
multi[1]:temperature:stability code{U32}=6618880	
multi[1]:temperature:stability rate{Extended Float}=0.040000	
multi[1]:y{Double Float}=0.000000	
parameter: Termination{String}=False	
parameter: delta time{Double Float}=1.000000	
parameter: progress{Double Float}=100.000000	
temperature:  rate window{Double Float}=120.000000	
temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
temperature: T1{Double Float}=3.974800	
temperature: T2{Double Float}=4.045200	
temperature: T3{Double Float}=85.959900	
temperature: T4{Double Float}=63.928900	
temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
temperature: current temperature{Double Float}=1.464900	
temperature: current temperature 2{Double Float}=287.100000	
temperature: dT/dt{Double Float}=-0.036044	
temperature: gas control{Boolean}=False	
temperature: gas control 2{Boolean}=False	
temperature: gass boost{I8}=0	
temperature: gass boost 2{I8}=0	
temperature: gast flow{I16}=0	
temperature: gast flow 2{I16}=7	
temperature: heater output{Double Float}=0.000000	
temperature: heater output 2{Double Float}=0.000000	
temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
temperature: monitor timeout{Double Float}=0.010000	
temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
temperature: ramp rate{Double Float}=8.000000	
temperature: ramp rate 2{Double Float}=0.000000	
temperature: ramp target{Double Float}=20.000000	
temperature: ramp target 2{Double Float}=0.000000	
temperature: ramping{Boolean}=False	
temperature: setpoint{Double Float}=1.800000	
temperature: setpoint 2{Double Float}=287.100000	
temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
temperature: stability error{Extended Float}=0.040000	
temperature: stability script{String}=	
temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
temperature: temp control mode{U16}=2	
temperature: temp control mode 2{U16}=3	
temperature: temp control mode 2.__text__{String}=Open Loop	
temperature: temp control mode.__text__{String}=Zone	
temperature: temp control sensor{U16}=0	
temperature: temp control sensor 2{U16}=0	
temperature: temp control sensor 2.__text__{String}=Sensor 1	
temperature: temp control sensor.__text__{String}=Sensor A	
temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
temperature: temp loop{U16}=0	
temperature: temp loop 2{U16}=0	
temperature: temp loop 2.__text__{String}=Heater	
temperature: temp loop.__text__{String}=Loop 1	
temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
temperature:error for gas boost{Double Float}=0.000000	
temperature:error for gas boost 2{Double Float}=0.000000	
temperature:heater range{U16}=2	
temperature:heater range 2{U16}=0	
temperature:heater range 2.__text__{String}=Off	
temperature:heater range.__text__{String}=40mW	
temperature:history window{Extended Float}=300.000000	
temperature:is stable?{Boolean}=True	
temperature:monitor{Boolean}=True	
temperature:ramping{Boolean}=False	
temperature:ramping on{Boolean}=False	
temperature:ramping on 2{Boolean}=False	
temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
temperature:stability code{U32}=6618880	
temperature:stability rate{Extended Float}=0.040000	
y{Double Float}=4.000000	
