TDI Format 1.5	Offset	Rxx::R	Rxx::Theta	Rxx::X	Rxx::Y	Rxy::R	Rxy::Theta	Rxy::X	Rxy::Y	temperature: T1	temperature: T2	temperature: T3	temperature: T4	temperature: dT/dt	iterator	multi[0]:iterator	multi[0]:y	multi[0]:temperature: setpoint	multi[0]:temperature: T1	multi[0]:temperature: T2	multi[0]:temperature: T3	multi[0]:temperature: T4	multi[0]:temperature: heater	multi[0]:temperature: gas	multi[0]:temperature: dT/dt	multi[0]:temperature: current temperature	multi[0]:temperature: error	multi[1]:iterator	multi[1]:y	multi[1]:Control:Magnet Output
2nd Parameter Class{String}=Multi-Parameter	0E+0	1.242662386E-3	1.56E-1	1.242662386E-3	3.371767975E-6	5.937462505E-7	-7.3248E+0	5.884780221E-7	-7.744519139E-8	2.0066E+1	2.069E+1	8.57092E+1	6.23121E+1	-9.45667699E-2	6.17E+2	1.1E+1	2E+1	2E+1	2.0069E+1	2.0692E+1	8.56375E+1	6.23121E+1	3.2E+0	2E+1	-9.823337197E-2	2.0069E+1	-6.9E-2	0E+0	0E+0	-0E+0
2nd Parameter Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	0E+0	1.244888075E-3	1.56E-1	1.244888075E-3	3.371767975E-6	7.099680181E-6	-5.508E-1	7.099680181E-6	-6.954265085E-8	2.001E+1	2.0658E+1	8.59599E+1	6.23121E+1	-1.470994018E-2	6.18E+2	1.1E+1	2E+1	1.8E+0	2.0066E+1	2.069E+1	8.57092E+1	6.23121E+1	3.2E+0	2E+1	-9.45667699E-2	1.4649E+0	-6.9E-2	1E+0	5E-1	4.998E-1
Analysis Class{String}=Basic Plot	0E+0	1.248900482E-3	1.56E-1	1.248900482E-3	3.371767975E-6	1.360508519E-5	-2.196E-1	1.360508519E-5	-5.426436434E-8	2.0032E+1	2.0696E+1	8.59241E+1	6.23121E+1	4.082338884E-2	6.19E+2	1.1E+1	2E+1	1.8E+0	2.001E+1	2.0658E+1	8.59599E+1	6.23121E+1	3.2E+0	2E+1	-1.470994018E-2	1.4649E+0	-6.9E-2	2E+0	1E+0	9.999E-1
Analysis Class Path{Path}=C\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV\\\\plugins\\\\Plotting\\\\Plotting_Base_class\\\\Plotting_Base.lvclass	0E+0	1.25463229E-3	1.56E-1	1.25463229E-3	3.371767975E-6	2.013834456E-5	-7.8E-2	2.013834456E-5	-2.844927037E-8	2.0073E+1	2.0753E+1	8.56734E+1	6.23121E+1	5.45464009E-2	6.2E+2	1.1E+1	2E+1	1.8E+0	2.0032E+1	2.0696E+1	8.59241E+1	6.23121E+1	3.2E+0	2E+1	4.082338884E-2	1.4649E+0	-6.9E-2	3E+0	1.5E+0	1.4999E+0
Analysis.# pre-routines{I32}=5	0E+0	1.25463229E-3	1.56E-1	1.25463229E-3	3.371767975E-6	2.013308369E-5	-1.032E-1	2.013308369E-5	-3.740552446E-8	2.0072E+1	2.0754E+1	8.56734E+1	6.23121E+1	5.209775642E-2	6.21E+2	1.1E+1	2E+1	1.8E+0	2.0073E+1	2.0753E+1	8.56734E+1	6.23121E+1	3.2E+0	2E+1	5.45464009E-2	1.4649E+0	-6.9E-2	4E+0	1.5E+0	1.5E+0
Analysis:Pre[0]:T Control Measure{1D Array (I32)}=[1,2,3,4,7]	0E+0	1.252103676E-3	1.56E-1	1.252103676E-3	3.371767975E-6	1.751630776E-5	-1.32E-1	1.751630776E-5	-4.162024857E-8	2.0094E+1	2.0781E+1	8.59599E+1	6.23121E+1	4.931819439E-2	6.22E+2	1.1E+1	2E+1	1.8E+0	2.0072E+1	2.0754E+1	8.56734E+1	6.23121E+1	3.2E+0	2E+1	5.209775642E-2	1.4649E+0	-6.9E-2	5E+0	1.3E+0	1.3002E+0
Autosave Tabs{Enum U32 ((XY Measurement Save,Parameter Plot Save 2))}=Parameter Plot Save 2	0E+0	1.250081351E-3	1.56E-1	1.250081351E-3	3.371767975E-6	1.490846967E-5	-1.656E-1	1.490846967E-5	-4.425441932E-8	2.0123E+1	2.0813E+1	8.59599E+1	6.23121E+1	5.907767639E-2	6.23E+2	1.1E+1	2E+1	1.8E+0	2.0094E+1	2.0781E+1	8.59599E+1	6.23121E+1	3.2E+0	2E+1	4.931819439E-2	1.4649E+0	-6.9E-2	6E+0	1.1E+0	1.1E+0
Control:Magnet Output{Double Float}=-0.007000	0E+0	1.248225902E-3	1.56E-1	1.248225902E-3	3.371767975E-6	1.228957525E-5	-2.7E-1	1.228957525E-5	-5.9005883E-8	2.05E+1	2.0876E+1	8.59241E+1	6.23121E+1	1.066538543E-1	6.24E+2	1.1E+1	2E+1	1.8E+0	2.0123E+1	2.0813E+1	8.59599E+1	6.23121E+1	3.2E+0	2E+1	5.907767639E-2	1.4649E+0	-6.9E-2	7E+0	9E-1	9.001E-1
Control:Magnet Rate{Double Float}=0.500000	0E+0	1.247282056E-3	1.572E-1	1.247282056E-3	3.371767975E-6	9.678009294E-6	-3.768E-1	9.678009294E-6	-6.480110391E-8	2.0786E+1	2.1351E+1	8.59241E+1	6.23121E+1	6.794359088E-1	6.25E+2	1.1E+1	2E+1	1.8E+0	2.05E+1	2.0876E+1	8.59241E+1	6.23121E+1	3.2E+0	2E+1	1.066538543E-1	1.4649E+0	-6.9E-2	8E+0	7E-1	7.002E-1
Display Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	0E+0	1.244854417E-3	1.56E-1	1.244854417E-3	3.371767975E-6	7.087031455E-6	-5.22E-1	7.087031455E-6	-6.585477786E-8	1.9136E+1	2.048E+1	8.57092E+1	6.23121E+1	-9.491357207E-1	6.26E+2	1.1E+1	2E+1	1.8E+0	2.0786E+1	2.1351E+1	8.59241E+1	6.23121E+1	3.2E+0	2E+1	6.794359088E-1	1.4649E+0	-6.9E-2	9E+0	5E-1	5.001E-1
Elapsed Time{Double Float}=12790.950867	0E+0	1.241819515E-3	1.56E-1	1.241819515E-3	3.371767975E-6	4.476014209E-6	-9.6E-1	4.476014209E-6	-7.639154571E-8	1.7941E+1	1.9247E+1	8.60673E+1	6.23121E+1	-2.221034765E+0	6.27E+2	1.1E+1	2E+1	1.8E+0	1.9136E+1	2.048E+1	8.57092E+1	6.23121E+1	3.2E+0	2E+1	-9.491357207E-1	1.4649E+0	-6.9E-2	1E+1	3E-1	3.001E-1
File:Autodel{Boolean}=True	0E+0	1.240302064E-3	1.56E-1	1.240302064E-3	3.371767975E-6	1.886085716E-6	-2.2176E+0	1.885030713E-6	-7.428425437E-8	1.7972E+1	1.8817E+1	8.60315E+1	6.23121E+1	-1.114821196E+0	6.28E+2	1.1E+1	2E+1	1.8E+0	1.7941E+1	1.9247E+1	8.60673E+1	6.23121E+1	3.2E+0	2E+1	-2.221034765E+0	1.4649E+0	-6.9E-2	1.1E+1	1E-1	1E-1
File:Autosave{Boolean}=False	0E+0	1.240302064E-3	1.56E-1	1.240302064E-3	3.371767975E-6	1.877654175E-6	-2.5008E+0	1.876073084E-6	-8.376737655E-8	1.8037E+1	1.8818E+1	8.60315E+1	6.23121E+1	-9.080225229E-1	6.29E+2	1.1E+1	2E+1	1.8E+0	1.7972E+1	1.8817E+1	8.60315E+1	6.23121E+1	3.2E+0	2E+1	-1.114821196E+0	1.4649E+0	-6.9E-2	1.2E+1	1E-1	1E-1
File:Export Config{Boolean}=True	0E+0	1.240302064E-3	1.56E-1	1.240302064E-3	3.371767975E-6	1.757533704E-6	-2.1636E+0	1.756481529E-6	-6.796212578E-8	1.8258E+1	1.8885E+1	8.60315E+1	6.23121E+1	-4.179689884E-1	6.3E+2	1.1E+1	2E+1	1.8E+0	1.8037E+1	1.8818E+1	8.60315E+1	6.23121E+1	3.2E+0	2E+1	-9.080225229E-1	1.4649E+0	-6.9E-2	1.3E+1	9E-2	9.01E-2
File:Final Autosave{Boolean}=True	0E+0	1.240471769E-3	1.56E-1	1.240471769E-3	3.371767975E-6	1.606860562E-6	-3.2592E+0	1.604224468E-6	-9.272361932E-8	1.8458E+1	1.8977E+1	8.59599E+1	6.23121E+1	-5.973557383E-2	6.31E+2	1.1E+1	2E+1	1.8E+0	1.8258E+1	1.8885E+1	8.60315E+1	6.23121E+1	3.2E+0	2E+1	-4.179689884E-1	1.4649E+0	-6.9E-2	1.4E+1	8E-2	8.01E-2
Filter:Enable{Enum U16 ((None,Analog,Digital,Analog&Digitial))}=None	0E+0	1.240471769E-3	1.56E-1	1.240471769E-3	3.371767975E-6	1.479892469E-6	-2.8116E+0	1.47778529E-6	-7.42841978E-8	1.864E+1	1.9085E+1	8.59599E+1	6.23121E+1	2.435620725E-1	6.32E+2	1.1E+1	2E+1	1.8E+0	1.8458E+1	1.8977E+1	8.59599E+1	6.23121E+1	3.2E+0	2E+1	-5.973557383E-2	1.4649E+0	-6.9E-2	1.5E+1	7E-2	7E-2
Filter:Points{I32}=1	0E+0	1.240640061E-3	1.56E-1	1.240640061E-3	3.371767975E-6	1.355030705E-6	-3.3048E+0	1.352395176E-6	-8.007950356E-8	1.8849E+1	1.9219E+1	8.59599E+1	6.23121E+1	4.854756296E-1	6.33E+2	1.1E+1	2E+1	1.8E+0	1.864E+1	1.9085E+1	8.59599E+1	6.23121E+1	3.2E+0	2E+1	2.435620725E-1	1.4649E+0	-6.9E-2	1.6E+1	6E-2	6E-2
Filter:Type{U16}=1	0E+0	1.240808352E-3	1.56E-1	1.240808352E-3	3.371767975E-6	1.227005345E-6	-3.7404E+0	1.224370948E-6	-8.113309266E-8	1.9062E+1	1.937E+1	8.59599E+1	6.23121E+1	6.681578159E-1	6.34E+2	1.1E+1	2E+1	1.8E+0	1.8849E+1	1.9219E+1	8.59599E+1	6.23121E+1	3.2E+0	2E+1	4.854756296E-1	1.4649E+0	-6.9E-2	1.7E+1	5E-2	5.01E-2
Filter:Type.__text__{String}=Repeat	0E+0	1.240808352E-3	1.56E-1	1.240808352E-3	3.371767975E-6	1.223844578E-6	-3.3984E+0	1.220682962E-6	-7.428422609E-8	1.9122E+1	1.9421E+1	8.59599E+1	6.23121E+1	7.16563046E-1	6.35E+2	1.1E+1	2E+1	1.8E+0	1.9062E+1	1.937E+1	8.59599E+1	6.23121E+1	3.2E+0	2E+1	6.681578159E-1	1.4649E+0	-6.9E-2	1.8E+1	5E-2	5E-2
Filter:Window{Double Float}=1.000000	0E+0	1.240976644E-3	1.548E-1	1.240976644E-3	3.338050296E-6	1.15430204E-6	-3.7428E+0	1.152721515E-6	-7.639148915E-8	1.929E+1	1.9575E+1	8.59241E+1	6.23121E+1	8.201611042E-1	6.36E+2	1.1E+1	2E+1	1.8E+0	1.9122E+1	1.9421E+1	8.59599E+1	6.23121E+1	3.2E+0	2E+1	7.16563046E-1	1.4649E+0	-6.9E-2	1.9E+1	4.5E-2	4.49E-2
Iterator{I32}=0	0E+0	1.241314641E-3	1.56E-1	1.241314641E-3	3.371767975E-6	1.085286438E-6	-4.5072E+0	1.081598735E-6	-8.692839842E-8	1.9433E+1	1.9719E+1	8.59241E+1	6.23121E+1	8.739891648E-1	6.37E+2	1.1E+1	2E+1	1.8E+0	1.929E+1	1.9575E+1	8.59241E+1	6.23121E+1	3.2E+0	2E+1	8.201611042E-1	1.4649E+0	-6.9E-2	2E+1	4E-2	3.99E-2
Magnet: Control Mode{Boolean}=False	0E+0	1.241482932E-3	1.56E-1	1.241482932E-3	3.371767975E-6	1.02259322E-6	-4.4328E+0	1.019431887E-6	-8.060635468E-8	1.9591E+1	1.9885E+1	8.59241E+1	6.23121E+1	9.30332005E-1	6.38E+2	1.1E+1	2E+1	1.8E+0	1.9433E+1	1.9719E+1	8.59241E+1	6.23121E+1	3.2E+0	2E+1	8.739891648E-1	1.4649E+0	-6.9E-2	2.1E+1	3.5E-2	3.49E-2
Magnet: Final Switch Heater{Enum U8 ((False,True,Mixed))}=	0E+0	1.241651223E-3	1.56E-1	1.241651223E-3	3.371767975E-6	9.456755582E-7	-4.8852E+0	9.414600704E-7	-8.218685147E-8	1.9711E+1	2.0038E+1	8.59599E+1	6.23121E+1	9.405722618E-1	6.39E+2	1.1E+1	2E+1	1.8E+0	1.9591E+1	1.9885E+1	8.59241E+1	6.23121E+1	3.2E+0	2E+1	9.30332005E-1	1.4649E+0	-6.9E-2	2.2E+1	3E-2	3E-2
Magnet: Power Supply{Enum U16 ((IPS120,LS625,PS110,Hg iPS,SMS Series,Cryomagnetics 4G,DMG Little CryoFree,DMG Big CryoFree))}=Hg iPS	0E+0	1.241819515E-3	1.56E-1	1.241819515E-3	3.371767975E-6	8.903571805E-7	-5.3724E+0	8.866694772E-7	-8.482099394E-8	1.9836E+1	2.0178E+1	8.58166E+1	6.23121E+1	9.402118921E-1	6.4E+2	1.1E+1	2E+1	1.8E+0	1.9711E+1	2.0038E+1	8.59599E+1	6.23121E+1	3.2E+0	2E+1	9.405722618E-1	1.4649E+0	-6.9E-2	2.3E+1	2.5E-2	2.5E-2
Magnet: Rate{Double Float}=0.500000	0E+0	1.242157512E-3	1.56E-1	1.242157512E-3	3.371767975E-6	8.366198935E-7	-5.8464E+0	8.324055371E-7	-8.69284267E-8	1.9931E+1	2.0308E+1	8.56375E+1	6.23121E+1	9.281747937E-1	6.41E+2	1.1E+1	2E+1	1.8E+0	1.9836E+1	2.0178E+1	8.58166E+1	6.23121E+1	3.2E+0	2E+1	9.402118921E-1	1.4649E+0	-6.9E-2	2.4E+1	2E-2	1.99E-2
Magnet: Setpoint{Double Float}=0.000000	0E+0	1.242325803E-3	1.56E-1	1.242325803E-3	3.371767975E-6	7.591752961E-7	-5.2644E+0	7.565408991E-7	-7.112317593E-8	2.0011E+1	2.0422E+1	8.5745E+1	6.23121E+1	8.919547796E-1	6.42E+2	1.1E+1	2E+1	1.8E+0	1.9931E+1	2.0308E+1	8.56375E+1	6.23121E+1	3.2E+0	2E+1	9.281747937E-1	1.4649E+0	-6.9E-2	2.5E+1	1.5E-2	1.48E-2
Magnet: Units{Enum U16 ((Field,Current))}=Field	0E+0	1.242494095E-3	1.56E-1	1.242494095E-3	3.371767975E-6	7.038572013E-7	-6.3348E+0	7.001697808E-7	-7.955259587E-8	2.0133E+1	2.0545E+1	8.56734E+1	6.23121E+1	8.439463973E-1	6.43E+2	1.1E+1	2E+1	1.8E+0	2.0011E+1	2.0422E+1	8.5745E+1	6.23121E+1	3.2E+0	2E+1	8.919547796E-1	1.4649E+0	-6.9E-2	2.6E+1	1E-2	9.9E-3
Magnet: VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	0E+0	1.242662386E-3	1.56E-1	1.242662386E-3	3.371767975E-6	6.300977615E-7	-7.3068E+0	6.243025972E-7	-8.113317751E-8	2.0257E+1	2.0663E+1	8.57092E+1	6.23121E+1	7.909411788E-1	6.44E+2	1.1E+1	2E+1	1.8E+0	2.0133E+1	2.0545E+1	8.56734E+1	6.23121E+1	3.2E+0	2E+1	8.439463973E-1	1.4649E+0	-6.9E-2	2.7E+1	5E-3	4.9E-3
Main Screen Path{Path}=C:\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV\\\\1Code.vi	0E+0	1.242832092E-3	1.56E-1	1.242832092E-3	3.371767975E-6	5.674048258E-7	-8.3688E+0	5.621360318E-7	-8.42941711E-8	2.033E+1	2.0772E+1	8.58166E+1	6.23121E+1	7.516415119E-1	6.45E+2	1.1E+1	2E+1	1.8E+0	2.0257E+1	2.0663E+1	8.57092E+1	6.23121E+1	3.2E+0	2E+1	7.909411788E-1	1.4649E+0	-6.9E-2	2.8E+1	0E+0	-2E-4
Measurement Timestamp{Timestamp}=<00:37:58.215 18/05/2023>T	0E+0	1.243000383E-3	1.524E-1	1.243000383E-3	3.270614936E-6	5.062915666E-7	-1.0464E+1	4.983889412E-7	-9.377732156E-8	2.038E+1	2.0858E+1	8.61032E+1	6.23121E+1	6.85695231E-1	6.46E+2	1.1E+1	2E+1	1.8E+0	2.033E+1	2.0772E+1	8.58166E+1	6.23121E+1	3.2E+0	2E+1	7.516415119E-1	1.4649E+0	-6.9E-2	2.9E+1	-5E-3	-4.9E-3
Measurement Title{String}=	0E+0	1.2430677E-3	1.56E-1	1.2430677E-3	3.371767975E-6	4.309541474E-7	-1.07016E+1	4.23578458E-7	-8.113303609E-8	2.0416E+1	2.0908E+1	8.60673E+1	6.23121E+1	6.469355226E-1	6.47E+2	1.1E+1	2E+1	1.8E+0	2.038E+1	2.0858E+1	8.61032E+1	6.23121E+1	3.2E+0	2E+1	6.85695231E-1	1.4649E+0	-6.9E-2	3E+1	-1E-2	-1.04E-2
Measurment Select{U16}=4	0E+0	1.243168675E-3	1.56E-1	1.243168675E-3	3.371767975E-6	3.640460067E-7	-1.28964E+1	3.550895094E-7	-8.324055371E-8	2.0446E+1	2.095E+1	8.61032E+1	6.23121E+1	6.132313013E-1	6.48E+2	1.1E+1	2E+1	1.8E+0	2.0416E+1	2.0908E+1	8.60673E+1	6.23121E+1	3.2E+0	2E+1	6.469355226E-1	1.4649E+0	-6.9E-2	3.1E+1	-1.5E-2	-1.51E-2
Measurment Select.__text__{String}=6221-Lockin-DAQ	0E+0	1.243235991E-3	1.56E-1	1.243235991E-3	3.371767975E-6	3.029316161E-7	-1.42416E+1	2.939756845E-7	-7.639160228E-8	2.0474E+1	2.0995E+1	8.60673E+1	6.23121E+1	5.794093013E-1	6.49E+2	1.1E+1	2E+1	1.8E+0	2.0446E+1	2.095E+1	8.61032E+1	6.23121E+1	3.2E+0	2E+1	6.132313013E-1	1.4649E+0	-6.9E-2	3.2E+1	-2E-2	-2.01E-2
Notes{String}=I+1A I-1E\\nrxx+1B Rxx-1C\\nRxy+1D Rxy-4A	0E+0	1.243336966E-3	1.56E-1	1.243336966E-3	3.371767975E-6	2.465604978E-7	-1.83756E+1	2.344429504E-7	-7.955259587E-8	2.0517E+1	2.1072E+1	8.59957E+1	6.23121E+1	5.247415304E-1	6.5E+2	1.1E+1	2E+1	1.8E+0	2.0474E+1	2.0995E+1	8.60673E+1	6.23121E+1	3.2E+0	2E+1	5.794093013E-1	1.4649E+0	-6.9E-2	3.3E+1	-2.5E-2	-2.5E-2
Offset{Double Float}=0.000000	0E+0	1.243437941E-3	1.56E-1	1.243437941E-3	3.371767975E-6	1.870277637E-7	-2.3688E+1	1.717497318E-7	-7.744527624E-8	2.0538E+1	2.1125E+1	8.59957E+1	6.23121E+1	4.64697361E-1	6.51E+2	1.1E+1	2E+1	1.8E+0	2.0517E+1	2.1072E+1	8.59957E+1	6.23121E+1	3.2E+0	2E+1	5.247415304E-1	1.4649E+0	-6.9E-2	3.4E+1	-3E-2	-3.01E-2
Option: 2182 Autozero{Boolean}=True	0E+0	1.243674963E-3	1.56E-1	1.243674963E-3	3.371767975E-6	1.253875686E-7	-3.70752E+1	9.957251418E-8	-7.691842512E-8	2.056E+1	2.117E+1	8.59599E+1	6.23121E+1	4.130463898E-1	6.52E+2	1.1E+1	2E+1	1.8E+0	2.0538E+1	2.1125E+1	8.59957E+1	6.23121E+1	3.2E+0	2E+1	4.64697361E-1	1.4649E+0	-6.9E-2	3.5E+1	-3.5E-2	-3.51E-2
Option: 2182 Front Autozero{Boolean}=True	0E+0	1.243674963E-3	1.56E-1	1.243674963E-3	3.371767975E-6	8.218676662E-8	-6.85356E+1	2.897613281E-8	-7.902577303E-8	2.0567E+1	2.121E+1	8.59957E+1	6.23121E+1	3.596879244E-1	6.53E+2	1.1E+1	2E+1	1.8E+0	2.056E+1	2.117E+1	8.59599E+1	6.23121E+1	3.2E+0	2E+1	4.130463898E-1	1.4649E+0	-6.9E-2	3.6E+1	-4E-2	-4E-2
Option: 2182 Hold{Boolean}=False	0E+0	1.243674963E-3	1.56E-1	1.243674963E-3	3.371767975E-6	8.903574633E-8	-1.020648E+2	-2.054671852E-8	-8.903571805E-8	2.0569E+1	2.124E+1	8.59599E+1	6.23121E+1	3.078793883E-1	6.54E+2	1.1E+1	2E+1	1.8E+0	2.0567E+1	2.121E+1	8.59957E+1	6.23121E+1	3.2E+0	2E+1	3.596879244E-1	1.4649E+0	-6.9E-2	3.7E+1	-4.5E-2	-4.5E-2
Option: 2182 Hold Count{I32}=10	0E+0	1.243843255E-3	1.548E-1	1.243843255E-3	3.338050296E-6	1.311826198E-7	-1.396704E+2	-1.016799187E-7	-8.692837014E-8	2.0561E+1	2.1261E+1	8.59599E+1	6.23121E+1	2.511324883E-1	6.55E+2	1.1E+1	2E+1	1.8E+0	2.0569E+1	2.124E+1	8.59599E+1	6.23121E+1	3.2E+0	2E+1	3.078793883E-1	1.4649E+0	-6.9E-2	3.8E+1	-5E-2	-5.02E-2
Option: 2182 Hold Window{Double Float}=1.000000	0E+0	1.243843255E-3	1.56E-1	1.243843255E-3	3.371767975E-6	1.280217393E-7	-1.390572E+2	-9.799204568E-8	-8.534778849E-8	2.0561E+1	2.1267E+1	8.59599E+1	6.23121E+1	2.353148162E-1	6.56E+2	1.1E+1	2E+1	1.8E+0	2.0561E+1	2.1261E+1	8.59599E+1	6.23121E+1	3.2E+0	2E+1	2.511324883E-1	1.4649E+0	-6.9E-2	3.9E+1	-5E-2	-5E-2
Option: 2182 Line Sync{Boolean}=False	0E+0	1.243843255E-3	1.56E-1	1.243843255E-3	3.371767975E-6	2.391848084E-7	-1.597932E+2	-2.270669781E-7	-8.482107879E-8	2.056E+1	2.1285E+1	8.59599E+1	6.23121E+1	1.832659096E-1	6.57E+2	1.1E+1	2E+1	1.8E+0	2.0561E+1	2.1267E+1	8.59599E+1	6.23121E+1	3.2E+0	2E+1	2.353148162E-1	1.4649E+0	-6.9E-2	4E+1	-6E-2	-5.99E-2
Option: 2182 Reference Reading{Double Float}=0.000000	0E+0	1.243876913E-3	1.56E-1	1.243876913E-3	3.371767975E-6	3.545622905E-7	-1.664088E+2	-3.47186884E-7	-8.482110707E-8	2.0559E+1	2.1301E+1	8.59599E+1	6.23121E+1	1.479796767E-1	6.58E+2	1.1E+1	2E+1	1.8E+0	2.056E+1	2.1285E+1	8.59599E+1	6.23121E+1	3.2E+0	2E+1	1.832659096E-1	1.4649E+0	-6.9E-2	4.1E+1	-7E-2	-7E-2
Option: 2182 Relative Mode{Boolean}=False	0E+0	1.244011546E-3	1.56E-1	1.244011546E-3	3.371767975E-6	4.904865987E-7	-1.70058E+2	-4.857450234E-7	-8.64015473E-8	2.0539E+1	2.1311E+1	8.59241E+1	6.23121E+1	1.128451377E-1	6.59E+2	1.1E+1	2E+1	1.8E+0	2.0559E+1	2.1301E+1	8.59599E+1	6.23121E+1	3.2E+0	2E+1	1.479796767E-1	1.4649E+0	-6.9E-2	4.2E+1	-8E-2	-7.99E-2
Option: 2182 Trigger Delay{Cluster (Boolean,Double Float)}={'Auto':True,'Time(s)':0.000000}	0E+0	1.244011546E-3	1.56E-1	1.244011546E-3	3.371767975E-6	6.211418299E-7	-1.714356E+2	-6.179804969E-7	-9.377729328E-8	2.0525E+1	2.1311E+1	8.59241E+1	6.23121E+1	7.48475343E-2	6.6E+2	1.1E+1	2E+1	1.8E+0	2.0539E+1	2.1311E+1	8.59241E+1	6.23121E+1	3.2E+0	2E+1	1.128451377E-1	1.4649E+0	-6.9E-2	4.3E+1	-9E-2	-8.99E-2
Option: 2182 Trigger Source{Enum U16 ((Immediate,Timer,Manual,Bus,Trigger link))}=Bus	0E+0	1.244011546E-3	1.56E-1	1.244011546E-3	3.371767975E-6	7.528531958E-7	-1.740528E+2	-7.523265427E-7	-7.955259587E-8	2.0516E+1	2.1314E+1	8.59241E+1	6.23121E+1	5.397170782E-2	6.61E+2	1.1E+1	2E+1	1.8E+0	2.0525E+1	2.1311E+1	8.59241E+1	6.23121E+1	3.2E+0	2E+1	7.48475343E-2	1.4649E+0	-6.9E-2	4.4E+1	-1E-1	-1E-1
Option: 2182 Trigger Timer{Double Float}=0.000000	0E+0	1.244011546E-3	1.56E-1	1.244011546E-3	3.371767975E-6	7.586483602E-7	-1.735152E+2	-7.565411819E-7	-8.692839842E-8	2.0499E+1	2.1312E+1	8.59241E+1	6.23121E+1	4.047015682E-2	6.62E+2	1.1E+1	2E+1	1.8E+0	2.0516E+1	2.1314E+1	8.59241E+1	6.23121E+1	3.2E+0	2E+1	5.397170782E-2	1.4649E+0	-6.9E-2	4.5E+1	-1E-1	-1E-1
Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	0E+0	1.244854417E-3	1.56E-1	1.244854417E-3	3.371767975E-6	3.348062928E-6	-1.784604E+2	-3.349117931E-6	-9.114312253E-8	2.043E+1	2.1281E+1	8.57092E+1	6.23121E+1	-4.087629542E-2	6.63E+2	1.1E+1	2E+1	1.8E+0	2.0499E+1	2.1312E+1	8.59241E+1	6.23121E+1	3.2E+0	2E+1	4.047015682E-2	1.4649E+0	-6.9E-2	4.6E+1	-3E-1	-2.998E-1
Option: 560 Enabled{Boolean}=False	0E+0	1.245764605E-3	1.56E-1	1.245764605E-3	3.371767975E-6	5.930626196E-6	-1.791144E+2	-5.933265119E-6	-9.32505553E-8	2.0323E+1	2.1221E+1	8.61032E+1	6.23121E+1	-9.563466161E-2	6.64E+2	1.1E+1	2E+1	1.8E+0	2.043E+1	2.1281E+1	8.57092E+1	6.23121E+1	3.2E+0	2E+1	-4.087629542E-2	1.4649E+0	-6.9E-2	4.7E+1	-5E-1	-4.999E-1
Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	0E+0	1.247046448E-3	1.56E-1	1.247046448E-3	3.371767975E-6	8.528454486E-6	-1.793256E+2	-8.53109058E-6	-1.016799187E-7	2.026E+1	2.1163E+1	8.59957E+1	6.23121E+1	-1.087218374E-1	6.65E+2	1.1E+1	2E+1	1.8E+0	2.0323E+1	2.1221E+1	8.61032E+1	6.23121E+1	3.2E+0	2E+1	-9.563466161E-2	1.4649E+0	-6.9E-2	4.8E+1	-7E-1	-6.999E-1
Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	0E+0	1.248563899E-3	1.56E-1	1.248563899E-3	3.371767975E-6	1.112948456E-5	-1.793916E+2	-1.113211782E-5	-1.190654682E-7	2.0202E+1	2.1109E+1	8.59599E+1	6.23121E+1	-9.888031334E-2	6.66E+2	1.1E+1	2E+1	1.8E+0	2.026E+1	2.1163E+1	8.59957E+1	6.23121E+1	3.2E+0	2E+1	-1.087218374E-1	1.4649E+0	-6.9E-2	4.9E+1	-9E-1	-8.999E-1
Option: 6221 Adjust Mode{Enum U16 ((Offset,Frequency,Amplitude))}=Offset	0E+0	1.250249642E-3	1.56E-1	1.250249642E-3	3.371767975E-6	1.371045259E-5	-1.79538E+2	-1.371308586E-5	-1.116897788E-7	2.0162E+1	2.1075E+1	8.59599E+1	6.23121E+1	-7.204460353E-2	6.67E+2	1.1E+1	2E+1	1.8E+0	2.0202E+1	2.1109E+1	8.59599E+1	6.23121E+1	3.2E+0	2E+1	-9.888031334E-2	1.4649E+0	-6.9E-2	5E+1	-1.1E+0	-1.0999E+0
Option: 6221 Amplitude{Double Float}=1.000000E-6	0E+0	1.252441673E-3	1.56E-1	1.252441673E-3	3.371767975E-6	1.632460656E-5	-1.795368E+2	-1.632726528E-5	-1.332900525E-7	2.0145E+1	2.1055E+1	8.56375E+1	6.23121E+1	-4.73276861E-2	6.68E+2	1.1E+1	2E+1	1.8E+0	2.0162E+1	2.1075E+1	8.59599E+1	6.23121E+1	3.2E+0	2E+1	-7.204460353E-2	1.4649E+0	-6.9E-2	5.1E+1	-1.3E+0	-1.2999E+0
Option: 6221 Compliance{Double Float}=10.000000	0E+0	1.254800581E-3	1.56E-1	1.254800581E-3	3.371767975E-6	1.892033899E-5	-1.796112E+2	-1.892350683E-5	-1.301288892E-7	2.0146E+1	2.103E+1	8.56734E+1	6.23121E+1	-4.104846343E-2	6.69E+2	1.1E+1	2E+1	1.8E+0	2.0145E+1	2.1055E+1	8.56375E+1	6.23121E+1	3.2E+0	2E+1	-4.73276861E-2	1.4649E+0	-6.9E-2	5.2E+1	-1.5E+0	-1.4998E+0
Option: 6221 Duty Cycle{Double Float}=50.000000	0E+0	1.254800581E-3	1.56E-1	1.254800581E-3	3.371767975E-6	1.893351946E-5	-1.796184E+2	-1.893617818E-5	-1.269679805E-7	2.0144E+1	2.1032E+1	8.56734E+1	6.23121E+1	-3.354865313E-2	6.7E+2	1.1E+1	2E+1	1.8E+0	2.0146E+1	2.103E+1	8.56734E+1	6.23121E+1	3.2E+0	2E+1	-4.104846343E-2	1.4649E+0	-6.9E-2	5.3E+1	-1.5E+0	-1.5E+0
Option: 6221 External Trigger{Boolean}=False	0E+0	1.249238479E-3	1.56E-1	1.249238479E-3	3.371767975E-6	1.241601726E-5	-1.795008E+2	-1.241865053E-5	-1.095824592E-7	2.0174E+1	2.1047E+1	8.59599E+1	6.23121E+1	3.186753765E-2	6.71E+2	1.1E+1	2E+1	1.8E+0	2.0144E+1	2.1032E+1	8.56734E+1	6.23121E+1	3.2E+0	2E+1	-3.354865313E-2	1.4649E+0	-6.9E-2	5.4E+1	-1E+0	-1.0001E+0
Option: 6221 External Trigger Ignore Multiple{Boolean}=False	0E+0	1.245528997E-3	1.56E-1	1.245528997E-3	3.371767975E-6	5.932210115E-6	-1.789956E+2	-5.934840553E-6	-1.058946145E-7	2.0169E+1	2.1056E+1	8.59241E+1	6.23121E+1	1.158616878E-2	6.72E+2	1.1E+1	2E+1	1.8E+0	2.0174E+1	2.1047E+1	8.59599E+1	6.23121E+1	3.2E+0	2E+1	3.186753765E-2	1.4649E+0	-6.9E-2	5.5E+1	-5E-1	-5.001E-1
Option: 6221 Frequency{Double Float}=119.770000	
Option: 6221 Function{U16}=1	
Option: 6221 Function.__text__{String}=Sine	
Option: 6221 Idle Level{Double Float}=0.000000	
Option: 6221 Input trigger Line{U8}=5	
Option: 6221 Offset{Double Float}=0.000000	
Option: 6221 Output Trigger Line{U8}=4	
Option: 6221 Pass Through{Boolean}=True	
Option: 6221 Phase Marker{Boolean}=True	
Option: 6221 Phase Marker Phase{Double Float}=0.000000	
Option: 6221 Range Level{Double Float}=2.000000E-12	
Option: 6221 Ranging{U16}=1	
Option: 6221 Ranging.__text__{String}=Best	
Option: 6221 Update Clock{Double Float}=0.000000	
Option: 6221 VISA{Visa Refnum (Void)}=GPIB0::13::INSTR	
Option: Confirm Config{Boolean}=False	
Option: Control Panel Ref{LVObjVI Refnum (Void)}=	
Option: DAQ Global Channel{Boolean}=False	
Option: DAQ Input Rate{Double Float}=10000.000000	
Option: DAQ Input Samples{I32}=200	
Option: DAQ Measurement Channels{1D Array (Cluster (UserDefinedRefnumTag Refnum (Void),\tkDAQmxPhysChanTagType Tag,\tkDAQmxScaleTagType Tag,Boolean,Double Float,String))}=[]	
Option: Differential{I32}=10106	
Option: Differential.__text__{String}=Differential	
Option: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values))}=Function Generator	
Option: Lockin Standoff Time{Double Float}=0.000000	
Option: Paranoid Save Data{Boolean}=True	
Option: Plot Autoback Path{Path}=C:\\\\TEMP\\\\XY Multiparam\\\\Backup.txt	
Option: SR830  Ref Phase{Double Float}=0.000000	
Option: SR830  Synch Filter{Boolean}=False	
Option: SR830  Time Constant{I16}=8	
Option: SR830  Time Constant.__text__{String}=100 ms	
Option: SR830 2x Line Filter{Boolean}=True	
Option: SR830 Adjust Gains{Boolean}=False	
Option: SR830 Auto Gain Lower.__text__{String}=2 nV/fA	
Option: SR830 Auto Gain Upper.__text__{String}=1 V/uA	
Option: SR830 Auto Offset 1{Boolean}=False	
Option: SR830 Auto Offset 2{Boolean}=False	
Option: SR830 Autophase{Boolean}=False	
Option: SR830 DC Coupling?{Boolean}=False	
Option: SR830 Display 1{U16}=0	
Option: SR830 Display 1.__text__{String}=X	
Option: SR830 Display 2{U16}=0	
Option: SR830 Display 2.__text__{String}=Y	
Option: SR830 Dynamic Reserve{I16}=1	
Option: SR830 Dynamic Reserve.__text__{String}=Normal	
Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Option: SR830 Filter Slope{I32}=1	
Option: SR830 Filter Slope.__text__{String}=12 dB/oct	
Option: SR830 Gain{I32}=-1	
Option: SR830 Gain.__text__{String}=Auto Gain	
Option: SR830 Ground Shield?{Boolean}=False	
Option: SR830 Harmonic{I32}=1	
Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A	
Option: SR830 Line Filter{Boolean}=True	
Option: SR830 No Reset{Boolean}=False	
Option: SR830 Offset 1{Double Float}=0.000000	
Option: SR830 Offset 2{Double Float}=0.000000	
Option: SR830 Output Channel 1{Boolean}=False	
Option: SR830 Output Channel 2{Boolean}=False	
Option: SR830 Ratio 1{U16}=0	
Option: SR830 Ratio 1.__text__{String}=None	
Option: SR830 Ratio 2{U16}=0	
Option: SR830 Ratio 2.__text__{String}=None	
Option: SR830 Ref Amplitude{Double Float}=0.100000	
Option: SR830 Ref Frequency{Double Float}=1013.000000	
Option: SR830 Ref Source{Boolean}=False	
Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta]	
Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Option: SR830 VISA{Visa Refnum (Void)}=	
Option: Sense Autorange{Boolean}=False	
Option: Sense Range Level{Double Float}=0.100000	
Option: Sense Rate{Double Float}=1.000000	
Option:560 Comport{Visa Refnum (Void)}=COM1	
Option:560 Filter High Pass{U16}=0	
Option:560 Filter High Pass.__text__{String}=0.03	
Option:560 Filter Lowpass{U16}=0	
Option:560 Filter Lowpass.__text__{String}=0.03	
Option:560 Filter Mode{U16}=0	
Option:560 Filter Mode.__text__{String}=6 dB high pass	
Option:560 Invert{Boolean}=False	
Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Option:570 Enabled{Boolean}=False	
Option:570 Filter High Pass{U16}=0	
Option:570 Filter High Pass.__text__{String}=0.03	
Option:570 Filter Lowpass{U16}=0	
Option:570 Filter Lowpass.__text__{String}=0.03	
Option:570 Filter Mode{U16}=0	
Option:570 Filter Mode.__text__{String}=6 dB high pass	
Option:570 Gain Mode{U16}=0	
Option:570 Gain Mode.__text__{String}=Low Noise	
Option:570 Input Offset{U16}=0	
Option:570 Input Offset On{Boolean}=False	
Option:570 Input Offset.__text__{String}=1pA	
Option:570 Sensitivity{U16}=0	
Option:570 Sensitivity.__text__{String}=1pA/V	
Option:Debug On{Boolean}=False	
Option:GPIB 2182{Visa Refnum (Void)}=	
Option:Parallel Config Voltage Measurers{Boolean}=True	
Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Option:SR830 Settle Time{Double Float}=5.000000	
Option:Sense Digits{I32}=8	
Output Names{1D Array (String)}=['Offset','Rxx::R','Rxx::Theta','Rxx::X','Rxx::Y','Rxy::R','Rxy::Theta','Rxy::X','Rxy::Y','temperature: T1','temperature: T2','temperature: T3','temperature: T4','temperature: dT/dt','iterator','multi[0]:iterator','multi[0]:y','multi[0]:temperature: setpoint','multi[0]:temperature: T1','multi[0]:temperature: T2','multi[0]:temperature: T3','multi[0]:temperature: T4','multi[0]:temperature: heater','multi[0]:temperature: gas','multi[0]:temperature: dT/dt','multi[0]:temperature: current temperature','multi[0]:temperature: error','multi[1]:iterator','multi[1]:y','multi[1]:Control:Magnet Output']	
Parameter Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Parameter Select{U16}=6	
Parameter Select.__text__{String}=Multi-Parameter	
Paths{U32}=0	
Plot: Column Renames{1D Array (Cluster (String,String))}=[]	
Plot: No dups{Boolean}=False	
Plot: StdDevs{Boolean}=False	
Plotting Class{String}=Parameter Plot	
Plotting Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	
Plotting Select{U16}=1	
Plotting Select.__text__{String}=Parameter Plot	
Project Code{String}=Topological_Insulators	
Ref: Temperature Window{LVObjVI Refnum (Void)}=	
Ref:Control Subpanel{LVObjUnknown Refnum (Void)}=	
Ref:Main Screen{LVObjVI Refnum (Void)}=	
Ref:Plotting Subpanel{LVObjUnknown Refnum (Void)}=	
Ref:Toolbar{LVObjUnknown Refnum (Void)}=	
Ref:XY Subpanel{LVObjUnknown Refnum (Void)}=	
Rxx::R{Double Float}=0.001246	
Rxx::Theta{Double Float}=0.156000	
Rxx::X{Double Float}=0.001246	
Rxx::Y{Double Float}=3.371768E-6	
Rxx:Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	
Rxx:Option: 560 Enabled{Boolean}=False	
Rxx:Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	
Rxx:Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	
Rxx:Option: Lockin Standoff Time{Double Float}=0.000000	
Rxx:Option: Lockin Type{Enum U16 ((SRS 830,EG&G 5302))}=SRS 830	
Rxx:Option: SR803 Full Scale Reading{Double Float}=0.000000	
Rxx:Option: SR830  Ref Phase{Double Float}=0.000000	
Rxx:Option: SR830  Synch Filter{Boolean}=False	
Rxx:Option: SR830  Time Constant{I16}=8	
Rxx:Option: SR830 2x Line Filter{Boolean}=False	
Rxx:Option: SR830 Adjust Gains{Boolean}=False	
Rxx:Option: SR830 Auto Gain Lower{I32}=0	
Rxx:Option: SR830 Auto Gain Upper{I32}=26	
Rxx:Option: SR830 Auto Offset 1{Boolean}=False	
Rxx:Option: SR830 Auto Offset 2{Boolean}=False	
Rxx:Option: SR830 Autophase{Boolean}=False	
Rxx:Option: SR830 DC Coupling?{Boolean}=False	
Rxx:Option: SR830 Display 1{U16}=0	
Rxx:Option: SR830 Display 2{U16}=0	
Rxx:Option: SR830 Dynamic Reserve{I16}=2	
Rxx:Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Rxx:Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Rxx:Option: SR830 Filter Slope{I32}=3	
Rxx:Option: SR830 Gain{I32}=18	
Rxx:Option: SR830 Ground Shield?{Boolean}=False	
Rxx:Option: SR830 Harmonic{I32}=1	
Rxx:Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A-B	
Rxx:Option: SR830 Line Filter{Boolean}=False	
Rxx:Option: SR830 No Reset{Boolean}=False	
Rxx:Option: SR830 Offset 1{Double Float}=0.000000	
Rxx:Option: SR830 Offset 2{Double Float}=0.000000	
Rxx:Option: SR830 Output Channel 1{Boolean}=False	
Rxx:Option: SR830 Output Channel 2{Boolean}=False	
Rxx:Option: SR830 Ratio 1{U16}=0	
Rxx:Option: SR830 Ratio 2{U16}=0	
Rxx:Option: SR830 Ref Amplitude{Double Float}=0.100000	
Rxx:Option: SR830 Ref Frequency{Double Float}=1013.000000	
Rxx:Option: SR830 Ref Source{Boolean}=False	
Rxx:Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta,X,Y]	
Rxx:Option: SR830 Time Constant value{Double Float}=0.000000	
Rxx:Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Rxx:Option: SR830 VISA{Visa Refnum (Void)}=GPIB0::5::INSTR	
Rxx:Option:560 Comport{Visa Refnum (Void)}=COM1	
Rxx:Option:560 Filter High Pass{U16}=0	
Rxx:Option:560 Filter Lowpass{U16}=0	
Rxx:Option:560 Filter Mode{U16}=0	
Rxx:Option:560 Invert{Boolean}=False	
Rxx:Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Rxx:Option:570 Enabled{Boolean}=False	
Rxx:Option:570 Filter High Pass{U16}=0	
Rxx:Option:570 Filter Lowpass{U16}=0	
Rxx:Option:570 Filter Mode{U16}=0	
Rxx:Option:570 Gain Mode{U16}=0	
Rxx:Option:570 Input Offset{U16}=0	
Rxx:Option:570 Input Offset On{Boolean}=False	
Rxx:Option:570 Sensitivity{U16}=0	
Rxx:Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Rxx:Option:SR830 Autogain Lower Threshold{Double Float}=0.100000	
Rxx:Option:SR830 Autogain Standoff{Double Float}=3.000000	
Rxx:Option:SR830 Autogain Upper Threshold{Double Float}=0.900000	
Rxx:Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Rxx:Option:SR830 Settle Time{Double Float}=0.000000	
Rxy::R{Double Float}=5.932210E-6	
Rxy::Theta{Double Float}=-178.995600	
Rxy::X{Double Float}=-5.934841E-6	
Rxy::Y{Double Float}=-1.058946E-7	
Rxy:Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	
Rxy:Option: 560 Enabled{Boolean}=False	
Rxy:Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	
Rxy:Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	
Rxy:Option: Lockin Standoff Time{Double Float}=0.000000	
Rxy:Option: Lockin Type{Enum U16 ((SRS 830,EG&G 5302))}=SRS 830	
Rxy:Option: SR803 Full Scale Reading{Double Float}=0.000000	
Rxy:Option: SR830  Ref Phase{Double Float}=0.000000	
Rxy:Option: SR830  Synch Filter{Boolean}=False	
Rxy:Option: SR830  Time Constant{I16}=8	
Rxy:Option: SR830 2x Line Filter{Boolean}=False	
Rxy:Option: SR830 Adjust Gains{Boolean}=False	
Rxy:Option: SR830 Auto Gain Lower{I32}=0	
Rxy:Option: SR830 Auto Gain Upper{I32}=26	
Rxy:Option: SR830 Auto Offset 1{Boolean}=False	
Rxy:Option: SR830 Auto Offset 2{Boolean}=False	
Rxy:Option: SR830 Autophase{Boolean}=False	
Rxy:Option: SR830 DC Coupling?{Boolean}=False	
Rxy:Option: SR830 Display 1{U16}=0	
Rxy:Option: SR830 Display 2{U16}=1	
Rxy:Option: SR830 Dynamic Reserve{I16}=2	
Rxy:Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Rxy:Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Rxy:Option: SR830 Filter Slope{I32}=3	
Rxy:Option: SR830 Gain{I32}=18	
Rxy:Option: SR830 Ground Shield?{Boolean}=False	
Rxy:Option: SR830 Harmonic{I32}=1	
Rxy:Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A-B	
Rxy:Option: SR830 Line Filter{Boolean}=False	
Rxy:Option: SR830 No Reset{Boolean}=False	
Rxy:Option: SR830 Offset 1{Double Float}=0.000000	
Rxy:Option: SR830 Offset 2{Double Float}=0.000000	
Rxy:Option: SR830 Output Channel 1{Boolean}=False	
Rxy:Option: SR830 Output Channel 2{Boolean}=False	
Rxy:Option: SR830 Ratio 1{U16}=0	
Rxy:Option: SR830 Ratio 2{U16}=0	
Rxy:Option: SR830 Ref Amplitude{Double Float}=0.100000	
Rxy:Option: SR830 Ref Frequency{Double Float}=1013.000000	
Rxy:Option: SR830 Ref Source{Boolean}=False	
Rxy:Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta,X,Y]	
Rxy:Option: SR830 Time Constant value{Double Float}=0.000000	
Rxy:Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Rxy:Option: SR830 VISA{Visa Refnum (Void)}=GPIB0::6::INSTR	
Rxy:Option:560 Comport{Visa Refnum (Void)}=COM1	
Rxy:Option:560 Filter High Pass{U16}=0	
Rxy:Option:560 Filter Lowpass{U16}=0	
Rxy:Option:560 Filter Mode{U16}=0	
Rxy:Option:560 Invert{Boolean}=False	
Rxy:Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Rxy:Option:570 Enabled{Boolean}=False	
Rxy:Option:570 Filter High Pass{U16}=0	
Rxy:Option:570 Filter Lowpass{U16}=0	
Rxy:Option:570 Filter Mode{U16}=0	
Rxy:Option:570 Gain Mode{U16}=0	
Rxy:Option:570 Input Offset{U16}=0	
Rxy:Option:570 Input Offset On{Boolean}=False	
Rxy:Option:570 Sensitivity{U16}=0	
Rxy:Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Rxy:Option:SR830 Autogain Lower Threshold{Double Float}=0.100000	
Rxy:Option:SR830 Autogain Standoff{Double Float}=3.000000	
Rxy:Option:SR830 Autogain Upper Threshold{Double Float}=0.900000	
Rxy:Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Rxy:Option:SR830 Settle Time{Double Float}=0.000000	
Sample ID{String}=MBE202221213_PA_D1 750C Cracker WAL	
Save:Filename{String}=${X-Y Class} ${2nd Parameter Class} ${iterator}{%04d} ${y}{%04.2g}.txt	
Save:Final Filename{String}=${X-Y Class} ${2nd Parameter Class} .txt	
Save:Final path{Path}=C:\\\\Data\\\\${Project Code}\\\\${User}\\\\${Sample ID}\\\\${Measurement Timestamp}{%Y%m%d}\\\\${X-Y Class}	
Save:Path{Path}=C:\\\\Data\\\\${Project Code}\\\\${User}\\\\${Sample ID}\\\\${Measurement Timestamp}{%Y%m%d}\\\\${X-Y Class}	
Startup path{Path}=C:\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV	
Sub Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Sweep Step{I32}=3	
T Control Measure.__text__{1D Array (String)}=['temperature: T1','temperature: T2','temperature: T3','temperature: T4','temperature: dT/dt']	
Timestamp{Timestamp}=<00:39:06.503 18/05/2023>T	
Toolbar{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Unaved Data{Boolean}=True	
Unsaved Data{Boolean}=False	
User{String}=Craig	
X-Y Class{String}=6221-Lockin-DAQ	
X-Y Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	
d(Offset){Double Float}=0.000000	
d(Rxx::R){Double Float}=0.000000	
d(Rxx::Theta){Double Float}=0.000000	
d(Rxx::X){Double Float}=0.000000	
d(Rxx::Y){Double Float}=4.735058E-22	
d(Rxy::R){Double Float}=8.932758E-9	
d(Rxy::Theta){Double Float}=0.036150	
d(Rxy::X){Double Float}=8.932758E-9	
d(Rxy::Y){Double Float}=4.328446E-9	
iterate result{U16}=5	
iterator{I32}=672	
multi[0]:Control: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values,Adaptive Step Ramp))}=List of Values	
multi[0]:Control: Monitor Update Timeout{Double Float}=0.010000	
multi[0]:Control: Open T Window{Boolean}=False	
multi[0]:Control: Reverse Temperature Sense{Boolean}=False	
multi[0]:Iterator{I32}=0	
multi[0]:Ref: Temperature Window{LVObjVI Refnum (Void)}=	
multi[0]:iterate result{U16}=0	
multi[0]:iterator{I32}=11	
multi[0]:temperature:  rate window{Double Float}=120.000000	
multi[0]:temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[0]:temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
multi[0]:temperature: T1{Double Float}=20.146000	
multi[0]:temperature: T2{Double Float}=21.048000	
multi[0]:temperature: T3{Double Float}=86.067300	
multi[0]:temperature: T4{Double Float}=62.312100	
multi[0]:temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
multi[0]:temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
multi[0]:temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
multi[0]:temperature: current temperature{Double Float}=1.464900	
multi[0]:temperature: current temperature 2{Double Float}=287.100000	
multi[0]:temperature: dT/dt{Double Float}=-0.008575	
multi[0]:temperature: error{Double Float}=-0.069000	
multi[0]:temperature: gas{Double Float}=20.000000	
multi[0]:temperature: gas control{Boolean}=False	
multi[0]:temperature: gas control 2{Boolean}=False	
multi[0]:temperature: gass boost{I8}=0	
multi[0]:temperature: gass boost 2{I8}=0	
multi[0]:temperature: gast flow{I16}=0	
multi[0]:temperature: gast flow 2{I16}=7	
multi[0]:temperature: heater{Double Float}=3.200000	
multi[0]:temperature: heater output{Double Float}=0.000000	
multi[0]:temperature: heater output 2{Double Float}=0.000000	
multi[0]:temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
multi[0]:temperature: monitor timeout{Double Float}=0.010000	
multi[0]:temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
multi[0]:temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
multi[0]:temperature: ramp rate{Double Float}=8.000000	
multi[0]:temperature: ramp rate 2{Double Float}=0.000000	
multi[0]:temperature: ramp target{Double Float}=20.000000	
multi[0]:temperature: ramp target 2{Double Float}=0.000000	
multi[0]:temperature: ramping{Boolean}=False	
multi[0]:temperature: setpoint{Double Float}=1.800000	
multi[0]:temperature: setpoint 2{Double Float}=287.100000	
multi[0]:temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
multi[0]:temperature: stability error{Extended Float}=0.040000	
multi[0]:temperature: stability script{String}=	
multi[0]:temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
multi[0]:temperature: temp control mode{U16}=2	
multi[0]:temperature: temp control mode 2{U16}=3	
multi[0]:temperature: temp control mode 2.__text__{String}=Open Loop	
multi[0]:temperature: temp control mode.__text__{String}=Zone	
multi[0]:temperature: temp control sensor{U16}=0	
multi[0]:temperature: temp control sensor 2{U16}=0	
multi[0]:temperature: temp control sensor 2.__text__{String}=Sensor 1	
multi[0]:temperature: temp control sensor.__text__{String}=Sensor A	
multi[0]:temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
multi[0]:temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
multi[0]:temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
multi[0]:temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
multi[0]:temperature: temp loop{U16}=0	
multi[0]:temperature: temp loop 2{U16}=0	
multi[0]:temperature: temp loop 2.__text__{String}=Heater	
multi[0]:temperature: temp loop.__text__{String}=Loop 1	
multi[0]:temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
multi[0]:temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[0]:temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[0]:temperature:error for gas boost{Double Float}=0.000000	
multi[0]:temperature:error for gas boost 2{Double Float}=0.000000	
multi[0]:temperature:heater range{U16}=2	
multi[0]:temperature:heater range 2{U16}=0	
multi[0]:temperature:heater range 2.__text__{String}=Off	
multi[0]:temperature:heater range.__text__{String}=40mW	
multi[0]:temperature:history window{Extended Float}=300.000000	
multi[0]:temperature:is stable?{Boolean}=True	
multi[0]:temperature:monitor{Boolean}=True	
multi[0]:temperature:ramping{Boolean}=False	
multi[0]:temperature:ramping on{Boolean}=False	
multi[0]:temperature:ramping on 2{Boolean}=False	
multi[0]:temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
multi[0]:temperature:stability code{U32}=6618880	
multi[0]:temperature:stability rate{Extended Float}=0.040000	
multi[0]:y{Double Float}=20.000000	
multi[1]:Control: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values,Adaptive Step Ramp))}=Multi-Segment Ramp	
multi[1]:Control: Gate delay{Double Float}=0.000000	
multi[1]:Control: Monitor Update Timeout{Double Float}=0.010000	
multi[1]:Control: Open T Window{Boolean}=False	
multi[1]:Control: Reverse Temperature Sense{Boolean}=False	
multi[1]:Control:Magnet Output{Double Float}=-0.000000	
multi[1]:Iterator{I32}=0	
multi[1]:Magnet: Final Switch Heater{Enum U8 ((False,True,Mixed))}=	
multi[1]:Magnet: Power Supply{Enum U16 ((IPS120,LS625,PS110,Hg iPS,SMS Series,Cryomagnetics 4G,DMG Little CryoFree,DMG Big CryoFree))}=Hg iPS	
multi[1]:Magnet: Rate{Double Float}=0.500000	
multi[1]:Magnet: Units{Enum U16 ((Field,Current))}=Field	
multi[1]:Magnet: VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[1]:Multi-segment_Stage{I32}=0	
multi[1]:Multi-segment_Stage_Changed{Boolean}=False	
multi[1]:Ref: Temperature Window{LVObjVI Refnum (Void)}=	
multi[1]:iterate result{U16}=4	
multi[1]:iterator{I32}=57	
multi[1]:measure point{Boolean}=False	
multi[1]:temperature:  rate window{Double Float}=120.000000	
multi[1]:temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[1]:temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
multi[1]:temperature: T1{Double Float}=1.842400	
multi[1]:temperature: T2{Double Float}=1.465600	
multi[1]:temperature: T3{Double Float}=86.318100	
multi[1]:temperature: T4{Double Float}=66.769200	
multi[1]:temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
multi[1]:temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
multi[1]:temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
multi[1]:temperature: current temperature{Double Float}=1.465600	
multi[1]:temperature: current temperature 2{Double Float}=287.100000	
multi[1]:temperature: dT/dt{Double Float}=-0.001864	
multi[1]:temperature: gas control{Boolean}=False	
multi[1]:temperature: gas control 2{Boolean}=False	
multi[1]:temperature: gass boost{I8}=0	
multi[1]:temperature: gass boost 2{I8}=0	
multi[1]:temperature: gast flow{I16}=0	
multi[1]:temperature: gast flow 2{I16}=7	
multi[1]:temperature: heater output{Double Float}=0.000000	
multi[1]:temperature: heater output 2{Double Float}=0.000000	
multi[1]:temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
multi[1]:temperature: monitor timeout{Double Float}=1.000000	
multi[1]:temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
multi[1]:temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
multi[1]:temperature: ramp rate{Double Float}=8.000000	
multi[1]:temperature: ramp rate 2{Double Float}=0.000000	
multi[1]:temperature: ramp target{Double Float}=20.000000	
multi[1]:temperature: ramp target 2{Double Float}=0.000000	
multi[1]:temperature: ramping{Boolean}=False	
multi[1]:temperature: setpoint{Double Float}=1.800000	
multi[1]:temperature: setpoint 2{Double Float}=287.100000	
multi[1]:temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
multi[1]:temperature: stability error{Extended Float}=0.040000	
multi[1]:temperature: stability script{String}=	
multi[1]:temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
multi[1]:temperature: temp control mode{U16}=2	
multi[1]:temperature: temp control mode 2{U16}=3	
multi[1]:temperature: temp control mode 2.__text__{String}=Open Loop	
multi[1]:temperature: temp control mode.__text__{String}=Zone	
multi[1]:temperature: temp control sensor{U16}=0	
multi[1]:temperature: temp control sensor 2{U16}=0	
multi[1]:temperature: temp control sensor 2.__text__{String}=Sensor 1	
multi[1]:temperature: temp control sensor.__text__{String}=Sensor A	
multi[1]:temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
multi[1]:temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
multi[1]:temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
multi[1]:temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
multi[1]:temperature: temp loop{U16}=0	
multi[1]:temperature: temp loop 2{U16}=0	
multi[1]:temperature: temp loop 2.__text__{String}=Heater	
multi[1]:temperature: temp loop.__text__{String}=Loop 1	
multi[1]:temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
multi[1]:temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[1]:temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[1]:temperature:error for gas boost{Double Float}=0.000000	
multi[1]:temperature:error for gas boost 2{Double Float}=0.000000	
multi[1]:temperature:heater range{U16}=2	
multi[1]:temperature:heater range 2{U16}=0	
multi[1]:temperature:heater range 2.__text__{String}=Off	
multi[1]:temperature:heater range.__text__{String}=40mW	
multi[1]:temperature:history window{Extended Float}=300.000000	
multi[1]:temperature:is stable?{Boolean}=True	
multi[1]:temperature:monitor{Boolean}=True	
multi[1]:temperature:ramping{Boolean}=False	
multi[1]:temperature:ramping on{Boolean}=False	
multi[1]:temperature:ramping on 2{Boolean}=False	
multi[1]:temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
multi[1]:temperature:stability code{U32}=6618880	
multi[1]:temperature:stability rate{Extended Float}=0.040000	
multi[1]:y{Double Float}=0.000000	
parameter: Termination{String}=False	
parameter: delta time{Double Float}=1.000000	
parameter: progress{Double Float}=100.000000	
temperature:  rate window{Double Float}=120.000000	
temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
temperature: T1{Double Float}=20.146000	
temperature: T2{Double Float}=21.048000	
temperature: T3{Double Float}=86.067300	
temperature: T4{Double Float}=62.312100	
temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
temperature: current temperature{Double Float}=1.464900	
temperature: current temperature 2{Double Float}=287.100000	
temperature: dT/dt{Double Float}=-0.008575	
temperature: gas control{Boolean}=False	
temperature: gas control 2{Boolean}=False	
temperature: gass boost{I8}=0	
temperature: gass boost 2{I8}=0	
temperature: gast flow{I16}=0	
temperature: gast flow 2{I16}=7	
temperature: heater output{Double Float}=0.000000	
temperature: heater output 2{Double Float}=0.000000	
temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
temperature: monitor timeout{Double Float}=0.010000	
temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
temperature: ramp rate{Double Float}=8.000000	
temperature: ramp rate 2{Double Float}=0.000000	
temperature: ramp target{Double Float}=20.000000	
temperature: ramp target 2{Double Float}=0.000000	
temperature: ramping{Boolean}=False	
temperature: setpoint{Double Float}=1.800000	
temperature: setpoint 2{Double Float}=287.100000	
temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
temperature: stability error{Extended Float}=0.040000	
temperature: stability script{String}=	
temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
temperature: temp control mode{U16}=2	
temperature: temp control mode 2{U16}=3	
temperature: temp control mode 2.__text__{String}=Open Loop	
temperature: temp control mode.__text__{String}=Zone	
temperature: temp control sensor{U16}=0	
temperature: temp control sensor 2{U16}=0	
temperature: temp control sensor 2.__text__{String}=Sensor 1	
temperature: temp control sensor.__text__{String}=Sensor A	
temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
temperature: temp loop{U16}=0	
temperature: temp loop 2{U16}=0	
temperature: temp loop 2.__text__{String}=Heater	
temperature: temp loop.__text__{String}=Loop 1	
temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
temperature:error for gas boost{Double Float}=0.000000	
temperature:error for gas boost 2{Double Float}=0.000000	
temperature:heater range{U16}=2	
temperature:heater range 2{U16}=0	
temperature:heater range 2.__text__{String}=Off	
temperature:heater range.__text__{String}=40mW	
temperature:history window{Extended Float}=300.000000	
temperature:is stable?{Boolean}=True	
temperature:monitor{Boolean}=True	
temperature:ramping{Boolean}=False	
temperature:ramping on{Boolean}=False	
temperature:ramping on 2{Boolean}=False	
temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
temperature:stability code{U32}=6618880	
temperature:stability rate{Extended Float}=0.040000	
y{Double Float}=20.000000	
