TDI Format 1.5	Offset	Rxx::R	Rxx::Theta	Rxx::X	Rxx::Y	Rxy::R	Rxy::Theta	Rxy::X	Rxy::Y	temperature: T1	temperature: T2	temperature: T3	temperature: T4	temperature: dT/dt	iterator	multi[0]:iterator	multi[0]:y	multi[0]:temperature: setpoint	multi[0]:temperature: T1	multi[0]:temperature: T2	multi[0]:temperature: T3	multi[0]:temperature: T4	multi[0]:temperature: heater	multi[0]:temperature: gas	multi[0]:temperature: dT/dt	multi[0]:temperature: current temperature	multi[0]:temperature: error	multi[1]:iterator	multi[1]:y	multi[1]:Control:Magnet Output
2nd Parameter Class{String}=Multi-Parameter	0E+0	1.226309835E-3	1.56E-1	1.226309835E-3	3.338050296E-6	5.789948716E-7	-7.7988E+0	5.731994244E-7	-7.955262415E-8	6.0525E+0	6.0564E+0	8.6139E+1	6.58035E+1	5.567317456E-2	1.69E+2	3E+0	6E+0	6E+0	6.0583E+0	6.0509E+0	8.6139E+1	6.58035E+1	1.04E+1	6E+0	4.640540481E-2	6.0589E+0	-5.89E-2	0E+0	0E+0	-0E+0
2nd Parameter Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	0E+0	1.231367062E-3	1.56E-1	1.231367062E-3	3.338050296E-6	7.168690974E-6	-4.896E-1	7.168690974E-6	-6.322057883E-8	6.0048E+0	6.0273E+0	8.61032E+1	6.58035E+1	1.479635108E-2	1.7E+2	3E+0	6E+0	1.8E+0	6.0525E+0	6.0564E+0	8.6139E+1	6.58035E+1	1.04E+1	6E+0	5.567317456E-2	1.4649E+0	-5.89E-2	1E+0	5E-1	4.999E-1
Analysis Class{String}=Basic Plot	0E+0	1.235413127E-3	1.56E-1	1.235413127E-3	3.371767975E-6	1.373837199E-5	-1.68E-1	1.373837199E-5	-4.214709969E-8	5.9884E+0	6.0028E+0	8.62464E+1	6.58035E+1	-2.724291012E-2	1.71E+2	3E+0	6E+0	1.8E+0	6.0048E+0	6.0273E+0	8.61032E+1	6.58035E+1	1.04E+1	6E+0	1.479635108E-2	1.4649E+0	-5.89E-2	2E+0	1E+0	9.999E-1
Analysis Class Path{Path}=C\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV\\\\plugins\\\\Plotting\\\\Plotting_Base_class\\\\Plotting_Base.lvclass	0E+0	1.241314641E-3	1.56E-1	1.241314641E-3	3.371767975E-6	2.034544199E-5	-7.56E-2	2.034544199E-5	-2.792245885E-8	6.0388E+0	6.0379E+0	8.61032E+1	6.58035E+1	3.662927821E-2	1.72E+2	3E+0	6E+0	1.8E+0	5.9884E+0	6.0028E+0	8.62464E+1	6.58035E+1	1.04E+1	6E+0	-2.724291012E-2	1.4649E+0	-5.89E-2	3E+0	1.5E+0	1.4999E+0
Analysis.# pre-routines{I32}=5	0E+0	1.241314641E-3	1.56E-1	1.241314641E-3	3.371767975E-6	2.035542634E-5	-9E-2	2.035542634E-5	-3.371765147E-8	6.0139E+0	6.0189E+0	8.61032E+1	6.58035E+1	8.888636716E-3	1.73E+2	3E+0	6E+0	1.8E+0	6.0388E+0	6.0379E+0	8.61032E+1	6.58035E+1	1.04E+1	6E+0	3.662927821E-2	1.4649E+0	-5.89E-2	4E+0	1.5E+0	1.5E+0
Analysis:Pre[0]:T Control Measure{1D Array (I32)}=[1,2,3,4,7]	0E+0	1.238718145E-3	1.56E-1	1.238718145E-3	3.371767975E-6	1.768595682E-5	-1.2E-1	1.768595682E-5	-3.845919842E-8	5.9891E+0	6.0084E+0	8.60673E+1	6.58035E+1	-1.68211963E-2	1.74E+2	3E+0	6E+0	1.8E+0	6.0139E+0	6.0189E+0	8.61032E+1	6.58035E+1	1.04E+1	6E+0	8.888636716E-3	1.4649E+0	-5.89E-2	5E+0	1.3E+0	1.3001E+0
Autosave Tabs{Enum U32 ((XY Measurement Save,Parameter Plot Save 2))}=Parameter Plot Save 2	0E+0	1.236593996E-3	1.56E-1	1.236593996E-3	3.371767975E-6	1.506867178E-5	-1.344E-1	1.506867178E-5	-3.687870162E-8	6.0167E+0	6.0365E+0	8.57808E+1	6.58035E+1	2.599442005E-2	1.75E+2	3E+0	6E+0	1.8E+0	5.9891E+0	6.0084E+0	8.60673E+1	6.58035E+1	1.04E+1	6E+0	-1.68211963E-2	1.4649E+0	-5.89E-2	6E+0	1.1E+0	1.1001E+0
Control:Magnet Output{Double Float}=-0.007000	0E+0	1.234570256E-3	1.548E-1	1.234570256E-3	3.338050296E-6	1.241865618E-5	-2.04E-1	1.241865618E-5	-4.530812156E-8	5.9771E+0	6.0015E+0	8.58883E+1	6.58035E+1	-2.738590166E-2	1.76E+2	3E+0	6E+0	1.8E+0	6.0167E+0	6.0365E+0	8.57808E+1	6.58035E+1	1.04E+1	6E+0	2.599442005E-2	1.4649E+0	-5.89E-2	7E+0	9E-1	9.001E-1
Control:Magnet Rate{Double Float}=0.500000	0E+0	1.232884514E-3	1.536E-1	1.232884514E-3	3.304332616E-6	9.78285343E-6	-3.084E-1	9.78285343E-6	-5.37375415E-8	6.0173E+0	6.0383E+0	8.61748E+1	6.58035E+1	4.630676284E-2	1.77E+2	3E+0	6E+0	1.8E+0	5.9771E+0	6.0015E+0	8.58883E+1	6.58035E+1	1.04E+1	6E+0	-2.738590166E-2	1.4649E+0	-5.89E-2	8E+0	7E-1	7.001E-1
Display Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	0E+0	1.231367062E-3	1.56E-1	1.231367062E-3	3.338050296E-6	7.162372268E-6	-5.484E-1	7.162372268E-6	-7.059638138E-8	6.0295E+0	6.034E+0	8.61032E+1	6.58035E+1	1.903869584E-2	1.78E+2	3E+0	6E+0	1.8E+0	6.0173E+0	6.0383E+0	8.61748E+1	6.58035E+1	1.04E+1	6E+0	4.630676284E-2	1.4649E+0	-5.89E-2	9E+0	5E-1	5.001E-1
Elapsed Time{Double Float}=12790.950867	0E+0	1.230019317E-3	1.56E-1	1.230019317E-3	3.371767975E-6	4.521322783E-6	-8.652E-1	4.521322783E-6	-6.954259428E-8	6.0096E+0	6.0227E+0	8.61032E+1	6.58035E+1	1.333932579E-2	1.79E+2	3E+0	6E+0	1.8E+0	6.0295E+0	6.034E+0	8.61032E+1	6.58035E+1	1.04E+1	6E+0	1.903869584E-2	1.4649E+0	-5.89E-2	1E+1	3E-1	3E-1
File:Autodel{Boolean}=True	0E+0	1.228333574E-3	1.56E-1	1.228333574E-3	3.371767975E-6	1.887666807E-6	-2.2884E+0	1.885553972E-6	-7.639154571E-8	6.0134E+0	6.0226E+0	8.60673E+1	6.58035E+1	3.918239847E-3	1.8E+2	3E+0	6E+0	1.8E+0	6.0096E+0	6.0227E+0	8.61032E+1	6.58035E+1	1.04E+1	6E+0	1.333932579E-2	1.4649E+0	-5.89E-2	1.1E+1	1E-1	1.001E-1
File:Autosave{Boolean}=False	0E+0	1.228333574E-3	1.56E-1	1.228333574E-3	3.371767975E-6	1.876073084E-6	-2.2164E+0	1.873965906E-6	-7.323043899E-8	6.0159E+0	6.0283E+0	8.60673E+1	6.58035E+1	6.321476772E-3	1.81E+2	3E+0	6E+0	1.8E+0	6.0134E+0	6.0226E+0	8.60673E+1	6.58035E+1	1.04E+1	6E+0	3.918239847E-3	1.4649E+0	-5.89E-2	1.2E+1	1E-1	1E-1
File:Export Config{Boolean}=True	0E+0	1.228163869E-3	1.56E-1	1.228163869E-3	3.371767975E-6	1.744364547E-6	-2.4936E+0	1.74225454E-6	-7.691836855E-8	6.0066E+0	6.0134E+0	8.60673E+1	6.58035E+1	-1.274617109E-2	1.82E+2	3E+0	6E+0	1.8E+0	6.0159E+0	6.0283E+0	8.60673E+1	6.58035E+1	1.04E+1	6E+0	6.321476772E-3	1.4649E+0	-5.89E-2	1.3E+1	9E-2	9E-2
File:Final Autosave{Boolean}=True	0E+0	1.22813021E-3	1.56E-1	1.22813021E-3	3.371767975E-6	1.611074919E-6	-2.7504E+0	1.608438825E-6	-7.84989502E-8	5.9555E+0	5.9756E+0	8.60673E+1	6.58035E+1	-5.822097883E-2	1.83E+2	3E+0	6E+0	1.8E+0	6.0066E+0	6.0134E+0	8.60673E+1	6.58035E+1	1.04E+1	6E+0	-1.274617109E-2	1.4649E+0	-5.89E-2	1.4E+1	8E-2	8.01E-2
Filter:Enable{Enum U16 ((None,Analog,Digital,Analog&Digitial))}=None	0E+0	1.227995577E-3	1.56E-1	1.227995577E-3	3.371767975E-6	1.486740091E-6	-2.9796E+0	1.484103997E-6	-7.849892191E-8	6.014E+0	6.0329E+0	8.57808E+1	6.58035E+1	3.294657171E-2	1.84E+2	3E+0	6E+0	1.8E+0	5.9555E+0	5.9756E+0	8.60673E+1	6.58035E+1	1.04E+1	6E+0	-5.822097883E-2	1.4649E+0	-5.89E-2	1.5E+1	7E-2	7.01E-2
Filter:Points{I32}=1	0E+0	1.227827286E-3	1.56E-1	1.227827286E-3	3.371767975E-6	1.360825586E-6	-3.2148E+0	1.358191472E-6	-7.744527624E-8	6.0216E+0	6.02E+0	8.57808E+1	6.58035E+1	1.192218903E-2	1.85E+2	3E+0	6E+0	1.8E+0	6.014E+0	6.0329E+0	8.57808E+1	6.58035E+1	1.04E+1	6E+0	3.294657171E-2	1.4649E+0	-5.89E-2	1.6E+1	6E-2	6E-2
Filter:Type{U16}=1	0E+0	1.227490703E-3	1.56E-1	1.227490703E-3	3.371767975E-6	1.231219984E-6	-3.114E+0	1.22858587E-6	-6.84889769E-8	6.0077E+0	6.0178E+0	8.58524E+1	6.58035E+1	1.151939947E-2	1.86E+2	3E+0	6E+0	1.8E+0	6.0216E+0	6.02E+0	8.57808E+1	6.58035E+1	1.04E+1	6E+0	1.192218903E-2	1.4649E+0	-5.89E-2	1.7E+1	5E-2	5E-2
Filter:Type.__text__{String}=Repeat	0E+0	1.227490703E-3	1.56E-1	1.227490703E-3	3.371767975E-6	1.219629938E-6	-4.008E+0	1.217522195E-6	-8.640157558E-8	6.0289E+0	6.0305E+0	8.58166E+1	6.58035E+1	2.966136113E-2	1.87E+2	3E+0	6E+0	1.8E+0	6.0077E+0	6.0178E+0	8.58524E+1	6.58035E+1	1.04E+1	6E+0	1.151939947E-2	1.4649E+0	-5.89E-2	1.8E+1	5E-2	5E-2
Filter:Window{Double Float}=1.000000	0E+0	1.227490703E-3	1.56E-1	1.227490703E-3	3.338050296E-6	1.170107008E-6	-4.0608E+0	1.166945958E-6	-8.42941711E-8	6.0356E+0	6.0269E+0	8.58883E+1	6.58035E+1	2.725278772E-2	1.88E+2	3E+0	6E+0	1.8E+0	6.0289E+0	6.0305E+0	8.58166E+1	6.58035E+1	1.04E+1	6E+0	2.966136113E-2	1.4649E+0	-5.89E-2	1.9E+1	4.5E-2	4.5E-2
Iterator{I32}=0	0E+0	1.227320997E-3	1.56E-1	1.227320997E-3	3.371767975E-6	1.090027731E-6	-3.7404E+0	1.087393899E-6	-7.21768216E-8	6.0017E+0	6.0251E+0	8.58166E+1	6.58035E+1	2.012250759E-2	1.89E+2	3E+0	6E+0	1.8E+0	6.0356E+0	6.0269E+0	8.58883E+1	6.58035E+1	1.04E+1	6E+0	2.725278772E-2	1.4649E+0	-5.89E-2	2E+1	4E-2	4E-2
Magnet: Control Mode{Boolean}=False	0E+0	1.227220023E-3	1.56E-1	1.227220023E-3	3.371767975E-6	1.028388384E-6	-4.8528E+0	1.025227051E-6	-8.850895178E-8	5.985E+0	6.0074E+0	8.59241E+1	6.58035E+1	-1.786468737E-2	1.9E+2	3E+0	6E+0	1.8E+0	6.0017E+0	6.0251E+0	8.58166E+1	6.58035E+1	1.04E+1	6E+0	2.012250759E-2	1.4649E+0	-5.89E-2	2.1E+1	3.5E-2	3.5E-2
Magnet: Final Switch Heater{Enum U8 ((False,True,Mixed))}=	0E+0	1.227152706E-3	1.56E-1	1.227152706E-3	3.371767975E-6	9.5779254E-7	-5.4168E+0	9.530506819E-7	-9.114306596E-8	5.9765E+0	5.9973E+0	8.62106E+1	6.58035E+1	-3.282603994E-2	1.91E+2	3E+0	6E+0	1.8E+0	5.985E+0	6.0074E+0	8.59241E+1	6.58035E+1	1.04E+1	6E+0	-1.786468737E-2	1.4649E+0	-5.89E-2	2.2E+1	3E-2	2.99E-2
Magnet: Power Supply{Enum U16 ((IPS120,LS625,PS110,Hg iPS,SMS Series,Cryomagnetics 4G,DMG Little CryoFree,DMG Big CryoFree))}=Hg iPS	0E+0	1.226984415E-3	1.56E-1	1.226984415E-3	3.236897256E-6	8.882497194E-7	-5.1696E+0	8.84562299E-7	-8.16599155E-8	5.9909E+0	6.0049E+0	8.61748E+1	6.52378E+1	-2.505719103E-2	1.92E+2	3E+0	6E+0	1.8E+0	5.9765E+0	5.9973E+0	8.62106E+1	6.58035E+1	1.04E+1	6E+0	-3.282603994E-2	1.4649E+0	-5.89E-2	2.3E+1	2.5E-2	2.49E-2
Magnet: Rate{Double Float}=0.500000	0E+0	1.226816123E-3	1.56E-1	1.226816123E-3	3.371767975E-6	8.239759758E-7	-5.2752E+0	8.202879896E-7	-7.744527624E-8	5.9925E+0	6.0136E+0	8.6139E+1	6.52378E+1	-1.110744383E-2	1.93E+2	3E+0	6E+0	1.8E+0	5.9909E+0	6.0049E+0	8.61748E+1	6.52378E+1	1.04E+1	6E+0	-2.505719103E-2	1.4649E+0	-5.89E-2	2.4E+1	2E-2	1.99E-2
Magnet: Setpoint{Double Float}=0.000000	0E+0	1.226647832E-3	1.56E-1	1.226647832E-3	3.338050296E-6	7.502193645E-7	-5.3544E+0	7.475849675E-7	-7.217684989E-8	6.0288E+0	6.0319E+0	8.61032E+1	6.52378E+1	1.92695614E-2	1.94E+2	3E+0	6E+0	1.8E+0	5.9925E+0	6.0136E+0	8.6139E+1	6.52378E+1	1.04E+1	6E+0	-1.110744383E-2	1.4649E+0	-5.89E-2	2.5E+1	1.5E-2	1.49E-2
Magnet: Units{Enum U16 ((Field,Current))}=Field	0E+0	1.226478126E-3	1.56E-1	1.226478126E-3	3.371767975E-6	6.838373112E-7	-7.0812E+0	6.780418641E-7	-8.587469618E-8	5.9889E+0	6.0052E+0	8.60673E+1	6.52378E+1	-1.407759264E-2	1.95E+2	3E+0	6E+0	1.8E+0	6.0288E+0	6.0319E+0	8.61032E+1	6.52378E+1	1.04E+1	6E+0	1.92695614E-2	1.4649E+0	-5.89E-2	2.6E+1	1E-2	9.9E-3
Magnet: VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	0E+0	1.226309835E-3	1.56E-1	1.226309835E-3	3.304332616E-6	6.316785695E-7	-6.93E+0	6.279905833E-7	-7.797212736E-8	6.0134E+0	6.0145E+0	8.60673E+1	6.52378E+1	6.466121878E-3	1.96E+2	3E+0	6E+0	1.8E+0	5.9889E+0	6.0052E+0	8.60673E+1	6.52378E+1	1.04E+1	6E+0	-1.407759264E-2	1.4649E+0	-5.89E-2	2.7E+1	5E-3	5E-3
Main Screen Path{Path}=C:\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV\\\\1Code.vi	0E+0	1.226309835E-3	1.56E-1	1.226309835E-3	3.371767975E-6	5.616093786E-7	-8.8512E+0	5.542336892E-7	-8.798204409E-8	5.9849E+0	5.9938E+0	8.60673E+1	6.52378E+1	-2.462041192E-2	1.97E+2	3E+0	6E+0	1.8E+0	6.0134E+0	6.0145E+0	8.60673E+1	6.52378E+1	1.04E+1	6E+0	6.466121878E-3	1.4649E+0	-5.89E-2	2.8E+1	0E+0	-2E-4
Measurement Timestamp{Timestamp}=<21:18:43.751 17/05/2023>T	0E+0	1.226343493E-3	1.56E-1	1.226343493E-3	3.371767975E-6	5.020769273E-7	-8.2404E+0	4.968081333E-7	-7.375734668E-8	5.9846E+0	5.9973E+0	8.60673E+1	6.52378E+1	-2.302198298E-2	1.98E+2	3E+0	6E+0	1.8E+0	5.9849E+0	5.9938E+0	8.60673E+1	6.52378E+1	1.04E+1	6E+0	-2.462041192E-2	1.4649E+0	-5.89E-2	2.9E+1	-5E-3	-5E-3
Measurement Title{String}=	0E+0	1.226478126E-3	1.56E-1	1.226478126E-3	3.371767975E-6	4.351687866E-7	-1.20192E+1	4.24105394E-7	-9.166997365E-8	6.011E+0	6.0126E+0	8.60673E+1	6.52378E+1	-7.203645073E-4	1.99E+2	3E+0	6E+0	1.8E+0	5.9846E+0	5.9973E+0	8.60673E+1	6.52378E+1	1.04E+1	6E+0	-2.302198298E-2	1.4649E+0	-5.89E-2	3E+1	-1E-2	-1.04E-2
Measurment Select{U16}=4	0E+0	1.226647832E-3	1.56E-1	1.226647832E-3	3.371767975E-6	3.450797058E-7	-1.39356E+1	3.345424005E-7	-8.482102222E-8	5.9841E+0	6.0053E+0	8.60673E+1	6.52378E+1	-8.415067568E-3	2E+2	3E+0	6E+0	1.8E+0	6.011E+0	6.0126E+0	8.60673E+1	6.52378E+1	1.04E+1	6E+0	-7.203645073E-4	1.4649E+0	-5.89E-2	3.1E+1	-1.5E-2	-1.51E-2
Measurment Select.__text__{String}=6221-Lockin-DAQ	0E+0	1.226984415E-3	1.56E-1	1.226984415E-3	3.338050296E-6	2.960828627E-7	-1.47456E+1	2.85546406E-7	-7.691836855E-8	6.024E+0	6.0351E+0	8.60673E+1	6.52378E+1	3.73946093E-2	2.01E+2	3E+0	6E+0	1.8E+0	5.9841E+0	6.0053E+0	8.60673E+1	6.52378E+1	1.04E+1	6E+0	-8.415067568E-3	1.4649E+0	-5.89E-2	3.2E+1	-2E-2	-2.01E-2
Notes{String}=I+1A I-1E\\nrxx+1B Rxx-1C\\nRxy+1D Rxy-4A	0E+0	1.226984415E-3	1.56E-1	1.226984415E-3	3.371767975E-6	2.354965395E-7	-2.19636E+1	2.17058023E-7	-8.850889521E-8	6.0186E+0	6.0297E+0	8.60673E+1	6.52378E+1	3.395888582E-2	2.02E+2	3E+0	6E+0	1.8E+0	6.024E+0	6.0351E+0	8.60673E+1	6.52378E+1	1.04E+1	6E+0	3.73946093E-2	1.4649E+0	-5.89E-2	3.3E+1	-2.5E-2	-2.51E-2
Offset{Double Float}=0.000000	0E+0	1.227152706E-3	1.56E-1	1.227152706E-3	3.371767975E-6	1.770179601E-7	-3.01212E+1	1.522559292E-7	-9.114312253E-8	6.0227E+0	6.0285E+0	8.60673E+1	6.52378E+1	2.511429042E-2	2.03E+2	3E+0	6E+0	1.8E+0	6.0186E+0	6.0297E+0	8.60673E+1	6.52378E+1	1.04E+1	6E+0	3.395888582E-2	1.4649E+0	-5.89E-2	3.4E+1	-3E-2	-3.01E-2
Option: 2182 Autozero{Boolean}=True	0E+0	1.227320997E-3	1.56E-1	1.227320997E-3	3.304332616E-6	1.248606609E-7	-4.48716E+1	8.798210066E-8	-9.061632798E-8	5.9983E+0	6.0106E+0	8.60673E+1	6.52378E+1	-5.742044654E-3	2.04E+2	3E+0	6E+0	1.8E+0	6.0227E+0	6.0285E+0	8.60673E+1	6.52378E+1	1.04E+1	6E+0	2.511429042E-2	1.4649E+0	-5.89E-2	3.5E+1	-3.5E-2	-3.51E-2
Option: 2182 Front Autozero{Boolean}=True	0E+0	1.227320997E-3	1.56E-1	1.227320997E-3	3.371767975E-6	9.008939201E-8	-8.4978E+1	7.375751639E-9	-9.272356276E-8	5.9841E+0	6.0032E+0	8.58166E+1	6.52378E+1	-2.557683922E-2	2.05E+2	3E+0	6E+0	1.8E+0	5.9983E+0	6.0106E+0	8.60673E+1	6.52378E+1	1.04E+1	6E+0	-5.742044654E-3	1.4649E+0	-5.89E-2	3.6E+1	-4E-2	-4.01E-2
Option: 2182 Hold{Boolean}=False	0E+0	1.227490703E-3	1.56E-1	1.227490703E-3	3.338050296E-6	8.376734826E-8	-1.1544E+2	-3.845925499E-8	-7.84989502E-8	6.0172E+0	6.0217E+0	8.58166E+1	6.52378E+1	-2.174597234E-3	2.06E+2	3E+0	6E+0	1.8E+0	5.9841E+0	6.0032E+0	8.58166E+1	6.52378E+1	1.04E+1	6E+0	-2.557683922E-2	1.4649E+0	-5.89E-2	3.7E+1	-4.5E-2	-4.5E-2
Option: 2182 Hold Count{I32}=10	0E+0	1.227490703E-3	1.56E-1	1.227490703E-3	3.371767975E-6	1.38031458E-7	-1.450764E+2	-1.159045029E-7	-8.060629811E-8	5.9921E+0	6.0023E+0	8.58166E+1	6.52378E+1	-3.251436725E-2	2.07E+2	3E+0	6E+0	1.8E+0	6.0172E+0	6.0217E+0	8.58166E+1	6.52378E+1	1.04E+1	6E+0	-2.174597234E-3	1.4649E+0	-5.89E-2	3.8E+1	-5E-2	-5.01E-2
Option: 2182 Hold Window{Double Float}=1.000000	0E+0	1.22755802E-3	1.56E-1	1.22755802E-3	3.371767975E-6	1.359241384E-7	-1.452852E+2	-1.137971267E-7	-8.007950356E-8	6.0047E+0	6.013E+0	8.58166E+1	6.52378E+1	-1.281724498E-2	2.08E+2	3E+0	6E+0	1.8E+0	5.9921E+0	6.0023E+0	8.58166E+1	6.52378E+1	1.04E+1	6E+0	-3.251436725E-2	1.4649E+0	-5.89E-2	3.9E+1	-5E-2	-5E-2
Option: 2182 Line Sync{Boolean}=False	0E+0	1.227827286E-3	1.56E-1	1.227827286E-3	3.371767975E-6	2.428727946E-7	-1.608636E+2	-2.312819002E-7	-8.166002864E-8	6.0038E+0	6.0085E+0	8.58166E+1	6.52378E+1	-1.278099697E-2	2.09E+2	3E+0	6E+0	1.8E+0	6.0047E+0	6.013E+0	8.58166E+1	6.52378E+1	1.04E+1	6E+0	-1.281724498E-2	1.4649E+0	-5.89E-2	4E+1	-6E-2	-6E-2
Option: 2182 Reference Reading{Double Float}=0.000000	0E+0	1.227995577E-3	1.56E-1	1.227995577E-3	3.338050296E-6	3.766899245E-7	-1.682976E+2	-3.719486321E-7	-7.797209908E-8	6.0394E+0	6.0122E+0	8.58883E+1	6.52378E+1	2.868316951E-4	2.1E+2	3E+0	6E+0	1.8E+0	6.0038E+0	6.0085E+0	8.58166E+1	6.52378E+1	1.04E+1	6E+0	-1.278099697E-2	1.4649E+0	-5.89E-2	4.1E+1	-7E-2	-7E-2
Option: 2182 Relative Mode{Boolean}=False	0E+0	1.228163869E-3	1.56E-1	1.228163869E-3	3.371767975E-6	5.120870138E-7	-1.705764E+2	-5.068182197E-7	-8.534787334E-8	6.0046E+0	6.0172E+0	8.59241E+1	6.52378E+1	1.244536228E-2	2.11E+2	3E+0	6E+0	1.8E+0	6.0394E+0	6.0122E+0	8.58883E+1	6.52378E+1	1.04E+1	6E+0	2.868316951E-4	1.4649E+0	-5.89E-2	4.2E+1	-8E-2	-8E-2
Option: 2182 Trigger Delay{Cluster (Boolean,Double Float)}={'Auto':True,'Time(s)':0.000000}	0E+0	1.22819781E-3	1.56E-1	1.22819781E-3	3.338050296E-6	6.527517658E-7	-1.725132E+2	-6.495909984E-7	-8.745524954E-8	6.0314E+0	6.0361E+0	8.62106E+1	6.52378E+1	4.013767838E-2	2.12E+2	3E+0	6E+0	1.8E+0	6.0046E+0	6.0172E+0	8.59241E+1	6.52378E+1	1.04E+1	6E+0	1.244536228E-2	1.4649E+0	-5.89E-2	4.3E+1	-9E-2	-9.04E-2
Option: 2182 Trigger Source{Enum U16 ((Immediate,Timer,Manual,Bus,Trigger link))}=Bus	0E+0	1.228333574E-3	1.56E-1	1.228333574E-3	3.371767975E-6	7.712922779E-7	-1.72602E+2	-7.665512684E-7	-1.011530958E-7	6.1082E+0	6.0603E+0	8.6139E+1	6.52378E+1	7.486955076E-2	2.13E+2	3E+0	6E+0	1.8E+0	6.0314E+0	6.0361E+0	8.62106E+1	6.52378E+1	1.04E+1	6E+0	4.013767838E-2	1.4649E+0	-5.89E-2	4.4E+1	-1E-1	-1E-1
Option: 2182 Trigger Timer{Double Float}=0.000000	0E+0	1.228333574E-3	1.56E-1	1.228333574E-3	3.371767975E-6	7.697117529E-7	-1.740684E+2	-7.686581637E-7	-8.060629811E-8	6.077E+0	6.1038E+0	8.6139E+1	6.52378E+1	1.403061152E-1	2.14E+2	3E+0	6E+0	1.8E+0	6.1082E+0	6.0603E+0	8.6139E+1	6.52378E+1	1.04E+1	6E+0	7.486955076E-2	1.4649E+0	-5.89E-2	4.5E+1	-1E-1	-1E-1
Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	0E+0	1.229849611E-3	1.56E-1	1.229849611E-3	3.371767975E-6	3.38862823E-6	-1.7859E+2	-3.391258667E-6	-8.534790163E-8	6.507E+0	6.4697E+0	8.60673E+1	6.52378E+1	5.887630582E-1	2.15E+2	3E+0	6E+0	1.8E+0	6.077E+0	6.1038E+0	8.6139E+1	6.52378E+1	1.04E+1	6E+0	1.403061152E-1	1.4649E+0	-5.89E-2	4.6E+1	-3E-1	-2.998E-1
Option: 560 Enabled{Boolean}=False	0E+0	1.231367062E-3	1.56E-1	1.231367062E-3	3.371767975E-6	6.022298348E-6	-1.790856E+2	-6.024934442E-6	-9.799201739E-8	5.6689E+0	5.6522E+0	8.60673E+1	6.52378E+1	-8.034272194E-1	2.16E+2	3E+0	6E+0	1.8E+0	6.507E+0	6.4697E+0	8.60673E+1	6.52378E+1	1.04E+1	6E+0	5.887630582E-1	1.4649E+0	-5.89E-2	4.7E+1	-5E-1	-4.998E-1
Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	0E+0	1.232716222E-3	1.56E-1	1.232716222E-3	3.371767975E-6	8.651737139E-6	-1.793652E+2	-8.654370405E-6	-9.69384E-8	6.0223E+0	5.9517E+0	8.60315E+1	6.52378E+1	3.270328939E-1	2.17E+2	3E+0	6E+0	1.8E+0	5.6689E+0	5.6522E+0	8.60673E+1	6.52378E+1	1.04E+1	6E+0	-8.034272194E-1	1.4649E+0	-5.89E-2	4.8E+1	-7E-1	-6.999E-1
Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	0E+0	1.234401965E-3	1.56E-1	1.234401965E-3	3.371767975E-6	1.125592373E-5	-1.794168E+2	-1.125855983E-5	-1.159045029E-7	6.0782E+0	5.9965E+0	8.58166E+1	6.52378E+1	2.134562135E-1	2.18E+2	3E+0	6E+0	1.8E+0	6.0223E+0	5.9517E+0	8.60315E+1	6.52378E+1	1.04E+1	6E+0	3.270328939E-1	1.4649E+0	-5.89E-2	4.9E+1	-9E-1	-9E-1
Option: 6221 Adjust Mode{Enum U16 ((Offset,Frequency,Amplitude))}=Offset	0E+0	1.236255999E-3	1.56E-1	1.236255999E-3	3.371767975E-6	1.387166728E-5	-1.79538E+2	-1.387429772E-5	-1.127434811E-7	6.1094E+0	6.0505E+0	8.6139E+1	6.52378E+1	1.173854023E-1	2.19E+2	3E+0	6E+0	1.8E+0	6.0782E+0	5.9965E+0	8.58166E+1	6.52378E+1	1.04E+1	6E+0	2.134562135E-1	1.4649E+0	-5.89E-2	5E+1	-1.1E+0	-1.0999E+0
Option: 6221 Amplitude{Double Float}=1.000000E-6	0E+0	1.23844803E-3	1.56E-1	1.23844803E-3	3.371767975E-6	1.650375914E-5	-1.795824E+2	-1.650636129E-5	-1.216996956E-7	6.0623E+0	6.0117E+0	8.60673E+1	6.52378E+1	3.266033158E-2	2.2E+2	3E+0	6E+0	1.8E+0	6.1094E+0	6.0505E+0	8.6139E+1	6.52378E+1	1.04E+1	6E+0	1.173854023E-1	1.4649E+0	-5.89E-2	5.1E+1	-1.3E+0	-1.2999E+0
Option: 6221 Compliance{Double Float}=10.000000	0E+0	1.240976644E-3	1.56E-1	1.240976644E-3	3.371767975E-6	1.914474639E-5	-1.796604E+2	-1.914740512E-5	-1.153776518E-7	6.0839E+0	6.0369E+0	8.60315E+1	6.52378E+1	8.891658485E-2	2.21E+2	3E+0	6E+0	1.8E+0	6.0623E+0	6.0117E+0	8.60673E+1	6.52378E+1	1.04E+1	6E+0	3.266033158E-2	1.4649E+0	-5.89E-2	5.2E+1	-1.5E+0	-1.4999E+0
Option: 6221 Duty Cycle{Double Float}=50.000000	0E+0	1.240976644E-3	1.56E-1	1.240976644E-3	3.371767975E-6	1.914579291E-5	-1.795992E+2	-1.914845163E-5	-1.353973721E-7	6.0144E+0	6.0034E+0	8.60315E+1	6.52378E+1	1.431031153E-2	2.22E+2	3E+0	6E+0	1.8E+0	6.0839E+0	6.0369E+0	8.60315E+1	6.52378E+1	1.04E+1	6E+0	8.891658485E-2	1.4649E+0	-5.89E-2	5.3E+1	-1.5E+0	-1.5E+0
Option: 6221 External Trigger{Boolean}=False	0E+0	1.235244836E-3	1.56E-1	1.235244836E-3	3.371767975E-6	1.255193733E-5	-1.794972E+2	-1.255457342E-5	-1.116898071E-7	5.9998E+0	5.9843E+0	8.57808E+1	6.52378E+1	-2.054025047E-2	2.23E+2	3E+0	6E+0	1.8E+0	6.0144E+0	6.0034E+0	8.60315E+1	6.52378E+1	1.04E+1	6E+0	1.431031153E-2	1.4649E+0	-5.89E-2	5.4E+1	-1E+0	-1.0001E+0
Option: 6221 External Trigger Ignore Multiple{Boolean}=False	0E+0	1.231198771E-3	1.56E-1	1.231198771E-3	3.304332616E-6	6.001226566E-6	-1.790676E+2	-6.003859831E-6	-9.904571963E-8	6.0114E+0	6.0143E+0	8.61032E+1	6.52378E+1	4.030097649E-2	2.24E+2	3E+0	6E+0	1.8E+0	5.9998E+0	5.9843E+0	8.57808E+1	6.52378E+1	1.04E+1	6E+0	-2.054025047E-2	1.4649E+0	-5.89E-2	5.5E+1	-5E-1	-5.001E-1
Option: 6221 Frequency{Double Float}=119.770000	
Option: 6221 Function{U16}=1	
Option: 6221 Function.__text__{String}=Sine	
Option: 6221 Idle Level{Double Float}=0.000000	
Option: 6221 Input trigger Line{U8}=5	
Option: 6221 Offset{Double Float}=0.000000	
Option: 6221 Output Trigger Line{U8}=4	
Option: 6221 Pass Through{Boolean}=True	
Option: 6221 Phase Marker{Boolean}=True	
Option: 6221 Phase Marker Phase{Double Float}=0.000000	
Option: 6221 Range Level{Double Float}=2.000000E-12	
Option: 6221 Ranging{U16}=1	
Option: 6221 Ranging.__text__{String}=Best	
Option: 6221 Update Clock{Double Float}=0.000000	
Option: 6221 VISA{Visa Refnum (Void)}=GPIB0::13::INSTR	
Option: Confirm Config{Boolean}=False	
Option: Control Panel Ref{LVObjVI Refnum (Void)}=	
Option: DAQ Global Channel{Boolean}=False	
Option: DAQ Input Rate{Double Float}=10000.000000	
Option: DAQ Input Samples{I32}=200	
Option: DAQ Measurement Channels{1D Array (Cluster (UserDefinedRefnumTag Refnum (Void),\tkDAQmxPhysChanTagType Tag,\tkDAQmxScaleTagType Tag,Boolean,Double Float,String))}=[]	
Option: Differential{I32}=10106	
Option: Differential.__text__{String}=Differential	
Option: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values))}=Function Generator	
Option: Lockin Standoff Time{Double Float}=0.000000	
Option: Paranoid Save Data{Boolean}=True	
Option: Plot Autoback Path{Path}=C:\\\\TEMP\\\\XY Multiparam\\\\Backup.txt	
Option: SR830  Ref Phase{Double Float}=0.000000	
Option: SR830  Synch Filter{Boolean}=False	
Option: SR830  Time Constant{I16}=8	
Option: SR830  Time Constant.__text__{String}=100 ms	
Option: SR830 2x Line Filter{Boolean}=True	
Option: SR830 Adjust Gains{Boolean}=False	
Option: SR830 Auto Gain Lower.__text__{String}=2 nV/fA	
Option: SR830 Auto Gain Upper.__text__{String}=1 V/uA	
Option: SR830 Auto Offset 1{Boolean}=False	
Option: SR830 Auto Offset 2{Boolean}=False	
Option: SR830 Autophase{Boolean}=False	
Option: SR830 DC Coupling?{Boolean}=False	
Option: SR830 Display 1{U16}=0	
Option: SR830 Display 1.__text__{String}=X	
Option: SR830 Display 2{U16}=0	
Option: SR830 Display 2.__text__{String}=Y	
Option: SR830 Dynamic Reserve{I16}=1	
Option: SR830 Dynamic Reserve.__text__{String}=Normal	
Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Option: SR830 Filter Slope{I32}=1	
Option: SR830 Filter Slope.__text__{String}=12 dB/oct	
Option: SR830 Gain{I32}=-1	
Option: SR830 Gain.__text__{String}=Auto Gain	
Option: SR830 Ground Shield?{Boolean}=False	
Option: SR830 Harmonic{I32}=1	
Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A	
Option: SR830 Line Filter{Boolean}=True	
Option: SR830 No Reset{Boolean}=False	
Option: SR830 Offset 1{Double Float}=0.000000	
Option: SR830 Offset 2{Double Float}=0.000000	
Option: SR830 Output Channel 1{Boolean}=False	
Option: SR830 Output Channel 2{Boolean}=False	
Option: SR830 Ratio 1{U16}=0	
Option: SR830 Ratio 1.__text__{String}=None	
Option: SR830 Ratio 2{U16}=0	
Option: SR830 Ratio 2.__text__{String}=None	
Option: SR830 Ref Amplitude{Double Float}=0.100000	
Option: SR830 Ref Frequency{Double Float}=1013.000000	
Option: SR830 Ref Source{Boolean}=False	
Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta]	
Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Option: SR830 VISA{Visa Refnum (Void)}=	
Option: Sense Autorange{Boolean}=False	
Option: Sense Range Level{Double Float}=0.100000	
Option: Sense Rate{Double Float}=1.000000	
Option:560 Comport{Visa Refnum (Void)}=COM1	
Option:560 Filter High Pass{U16}=0	
Option:560 Filter High Pass.__text__{String}=0.03	
Option:560 Filter Lowpass{U16}=0	
Option:560 Filter Lowpass.__text__{String}=0.03	
Option:560 Filter Mode{U16}=0	
Option:560 Filter Mode.__text__{String}=6 dB high pass	
Option:560 Invert{Boolean}=False	
Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Option:570 Enabled{Boolean}=False	
Option:570 Filter High Pass{U16}=0	
Option:570 Filter High Pass.__text__{String}=0.03	
Option:570 Filter Lowpass{U16}=0	
Option:570 Filter Lowpass.__text__{String}=0.03	
Option:570 Filter Mode{U16}=0	
Option:570 Filter Mode.__text__{String}=6 dB high pass	
Option:570 Gain Mode{U16}=0	
Option:570 Gain Mode.__text__{String}=Low Noise	
Option:570 Input Offset{U16}=0	
Option:570 Input Offset On{Boolean}=False	
Option:570 Input Offset.__text__{String}=1pA	
Option:570 Sensitivity{U16}=0	
Option:570 Sensitivity.__text__{String}=1pA/V	
Option:Debug On{Boolean}=False	
Option:GPIB 2182{Visa Refnum (Void)}=	
Option:Parallel Config Voltage Measurers{Boolean}=True	
Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Option:SR830 Settle Time{Double Float}=5.000000	
Option:Sense Digits{I32}=8	
Output Names{1D Array (String)}=['Offset','Rxx::R','Rxx::Theta','Rxx::X','Rxx::Y','Rxy::R','Rxy::Theta','Rxy::X','Rxy::Y','temperature: T1','temperature: T2','temperature: T3','temperature: T4','temperature: dT/dt','iterator','multi[0]:iterator','multi[0]:y','multi[0]:temperature: setpoint','multi[0]:temperature: T1','multi[0]:temperature: T2','multi[0]:temperature: T3','multi[0]:temperature: T4','multi[0]:temperature: heater','multi[0]:temperature: gas','multi[0]:temperature: dT/dt','multi[0]:temperature: current temperature','multi[0]:temperature: error','multi[1]:iterator','multi[1]:y','multi[1]:Control:Magnet Output']	
Parameter Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Parameter Select{U16}=6	
Parameter Select.__text__{String}=Multi-Parameter	
Paths{U32}=0	
Plot: Column Renames{1D Array (Cluster (String,String))}=[]	
Plot: No dups{Boolean}=False	
Plot: StdDevs{Boolean}=False	
Plotting Class{String}=Parameter Plot	
Plotting Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	
Plotting Select{U16}=1	
Plotting Select.__text__{String}=Parameter Plot	
Project Code{String}=Topological_Insulators	
Ref: Temperature Window{LVObjVI Refnum (Void)}=	
Ref:Control Subpanel{LVObjUnknown Refnum (Void)}=	
Ref:Main Screen{LVObjVI Refnum (Void)}=	
Ref:Plotting Subpanel{LVObjUnknown Refnum (Void)}=	
Ref:Toolbar{LVObjUnknown Refnum (Void)}=	
Ref:XY Subpanel{LVObjUnknown Refnum (Void)}=	
Rxx::R{Double Float}=0.001231	
Rxx::Theta{Double Float}=0.156000	
Rxx::X{Double Float}=0.001231	
Rxx::Y{Double Float}=3.304333E-6	
Rxx:Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	
Rxx:Option: 560 Enabled{Boolean}=False	
Rxx:Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	
Rxx:Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	
Rxx:Option: Lockin Standoff Time{Double Float}=0.000000	
Rxx:Option: Lockin Type{Enum U16 ((SRS 830,EG&G 5302))}=SRS 830	
Rxx:Option: SR803 Full Scale Reading{Double Float}=0.000000	
Rxx:Option: SR830  Ref Phase{Double Float}=0.000000	
Rxx:Option: SR830  Synch Filter{Boolean}=False	
Rxx:Option: SR830  Time Constant{I16}=8	
Rxx:Option: SR830 2x Line Filter{Boolean}=False	
Rxx:Option: SR830 Adjust Gains{Boolean}=False	
Rxx:Option: SR830 Auto Gain Lower{I32}=0	
Rxx:Option: SR830 Auto Gain Upper{I32}=26	
Rxx:Option: SR830 Auto Offset 1{Boolean}=False	
Rxx:Option: SR830 Auto Offset 2{Boolean}=False	
Rxx:Option: SR830 Autophase{Boolean}=False	
Rxx:Option: SR830 DC Coupling?{Boolean}=False	
Rxx:Option: SR830 Display 1{U16}=0	
Rxx:Option: SR830 Display 2{U16}=0	
Rxx:Option: SR830 Dynamic Reserve{I16}=2	
Rxx:Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Rxx:Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Rxx:Option: SR830 Filter Slope{I32}=3	
Rxx:Option: SR830 Gain{I32}=18	
Rxx:Option: SR830 Ground Shield?{Boolean}=False	
Rxx:Option: SR830 Harmonic{I32}=1	
Rxx:Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A-B	
Rxx:Option: SR830 Line Filter{Boolean}=False	
Rxx:Option: SR830 No Reset{Boolean}=False	
Rxx:Option: SR830 Offset 1{Double Float}=0.000000	
Rxx:Option: SR830 Offset 2{Double Float}=0.000000	
Rxx:Option: SR830 Output Channel 1{Boolean}=False	
Rxx:Option: SR830 Output Channel 2{Boolean}=False	
Rxx:Option: SR830 Ratio 1{U16}=0	
Rxx:Option: SR830 Ratio 2{U16}=0	
Rxx:Option: SR830 Ref Amplitude{Double Float}=0.100000	
Rxx:Option: SR830 Ref Frequency{Double Float}=1013.000000	
Rxx:Option: SR830 Ref Source{Boolean}=False	
Rxx:Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta,X,Y]	
Rxx:Option: SR830 Time Constant value{Double Float}=0.000000	
Rxx:Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Rxx:Option: SR830 VISA{Visa Refnum (Void)}=GPIB0::5::INSTR	
Rxx:Option:560 Comport{Visa Refnum (Void)}=COM1	
Rxx:Option:560 Filter High Pass{U16}=0	
Rxx:Option:560 Filter Lowpass{U16}=0	
Rxx:Option:560 Filter Mode{U16}=0	
Rxx:Option:560 Invert{Boolean}=False	
Rxx:Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Rxx:Option:570 Enabled{Boolean}=False	
Rxx:Option:570 Filter High Pass{U16}=0	
Rxx:Option:570 Filter Lowpass{U16}=0	
Rxx:Option:570 Filter Mode{U16}=0	
Rxx:Option:570 Gain Mode{U16}=0	
Rxx:Option:570 Input Offset{U16}=0	
Rxx:Option:570 Input Offset On{Boolean}=False	
Rxx:Option:570 Sensitivity{U16}=0	
Rxx:Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Rxx:Option:SR830 Autogain Lower Threshold{Double Float}=0.100000	
Rxx:Option:SR830 Autogain Standoff{Double Float}=3.000000	
Rxx:Option:SR830 Autogain Upper Threshold{Double Float}=0.900000	
Rxx:Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Rxx:Option:SR830 Settle Time{Double Float}=0.000000	
Rxy::R{Double Float}=6.001227E-6	
Rxy::Theta{Double Float}=-179.067600	
Rxy::X{Double Float}=-6.003860E-6	
Rxy::Y{Double Float}=-9.904572E-8	
Rxy:Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	
Rxy:Option: 560 Enabled{Boolean}=False	
Rxy:Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	
Rxy:Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	
Rxy:Option: Lockin Standoff Time{Double Float}=0.000000	
Rxy:Option: Lockin Type{Enum U16 ((SRS 830,EG&G 5302))}=SRS 830	
Rxy:Option: SR803 Full Scale Reading{Double Float}=0.000000	
Rxy:Option: SR830  Ref Phase{Double Float}=0.000000	
Rxy:Option: SR830  Synch Filter{Boolean}=False	
Rxy:Option: SR830  Time Constant{I16}=8	
Rxy:Option: SR830 2x Line Filter{Boolean}=False	
Rxy:Option: SR830 Adjust Gains{Boolean}=False	
Rxy:Option: SR830 Auto Gain Lower{I32}=0	
Rxy:Option: SR830 Auto Gain Upper{I32}=26	
Rxy:Option: SR830 Auto Offset 1{Boolean}=False	
Rxy:Option: SR830 Auto Offset 2{Boolean}=False	
Rxy:Option: SR830 Autophase{Boolean}=False	
Rxy:Option: SR830 DC Coupling?{Boolean}=False	
Rxy:Option: SR830 Display 1{U16}=0	
Rxy:Option: SR830 Display 2{U16}=1	
Rxy:Option: SR830 Dynamic Reserve{I16}=2	
Rxy:Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Rxy:Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Rxy:Option: SR830 Filter Slope{I32}=3	
Rxy:Option: SR830 Gain{I32}=18	
Rxy:Option: SR830 Ground Shield?{Boolean}=False	
Rxy:Option: SR830 Harmonic{I32}=1	
Rxy:Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A-B	
Rxy:Option: SR830 Line Filter{Boolean}=False	
Rxy:Option: SR830 No Reset{Boolean}=False	
Rxy:Option: SR830 Offset 1{Double Float}=0.000000	
Rxy:Option: SR830 Offset 2{Double Float}=0.000000	
Rxy:Option: SR830 Output Channel 1{Boolean}=False	
Rxy:Option: SR830 Output Channel 2{Boolean}=False	
Rxy:Option: SR830 Ratio 1{U16}=0	
Rxy:Option: SR830 Ratio 2{U16}=0	
Rxy:Option: SR830 Ref Amplitude{Double Float}=0.100000	
Rxy:Option: SR830 Ref Frequency{Double Float}=1013.000000	
Rxy:Option: SR830 Ref Source{Boolean}=False	
Rxy:Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta,X,Y]	
Rxy:Option: SR830 Time Constant value{Double Float}=0.000000	
Rxy:Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Rxy:Option: SR830 VISA{Visa Refnum (Void)}=GPIB0::6::INSTR	
Rxy:Option:560 Comport{Visa Refnum (Void)}=COM1	
Rxy:Option:560 Filter High Pass{U16}=0	
Rxy:Option:560 Filter Lowpass{U16}=0	
Rxy:Option:560 Filter Mode{U16}=0	
Rxy:Option:560 Invert{Boolean}=False	
Rxy:Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Rxy:Option:570 Enabled{Boolean}=False	
Rxy:Option:570 Filter High Pass{U16}=0	
Rxy:Option:570 Filter Lowpass{U16}=0	
Rxy:Option:570 Filter Mode{U16}=0	
Rxy:Option:570 Gain Mode{U16}=0	
Rxy:Option:570 Input Offset{U16}=0	
Rxy:Option:570 Input Offset On{Boolean}=False	
Rxy:Option:570 Sensitivity{U16}=0	
Rxy:Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Rxy:Option:SR830 Autogain Lower Threshold{Double Float}=0.100000	
Rxy:Option:SR830 Autogain Standoff{Double Float}=3.000000	
Rxy:Option:SR830 Autogain Upper Threshold{Double Float}=0.900000	
Rxy:Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Rxy:Option:SR830 Settle Time{Double Float}=0.000000	
Sample ID{String}=MBE202221213_PA_D1 750C Cracker WAL	
Save:Filename{String}=${X-Y Class} ${2nd Parameter Class} ${iterator}{%04d} ${y}{%04.2g}.txt	
Save:Final Filename{String}=${X-Y Class} ${2nd Parameter Class} .txt	
Save:Final path{Path}=C:\\\\Data\\\\${Project Code}\\\\${User}\\\\${Sample ID}\\\\${Measurement Timestamp}{%Y%m%d}\\\\${X-Y Class}	
Save:Path{Path}=C:\\\\Data\\\\${Project Code}\\\\${User}\\\\${Sample ID}\\\\${Measurement Timestamp}{%Y%m%d}\\\\${X-Y Class}	
Startup path{Path}=C:\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV	
Sub Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Sweep Step{I32}=3	
T Control Measure.__text__{1D Array (String)}=['temperature: T1','temperature: T2','temperature: T3','temperature: T4','temperature: dT/dt']	
Timestamp{Timestamp}=<21:19:52.447 17/05/2023>T	
Toolbar{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Unaved Data{Boolean}=True	
Unsaved Data{Boolean}=False	
User{String}=Craig	
X-Y Class{String}=6221-Lockin-DAQ	
X-Y Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	
d(Offset){Double Float}=0.000000	
d(Rxx::R){Double Float}=0.000000	
d(Rxx::Theta){Double Float}=0.000000	
d(Rxx::X){Double Float}=0.000000	
d(Rxx::Y){Double Float}=9.233967E-8	
d(Rxy::R){Double Float}=6.816094E-9	
d(Rxy::Theta){Double Float}=0.075966	
d(Rxy::X){Double Float}=6.819919E-9	
d(Rxy::Y){Double Float}=8.246294E-9	
iterate result{U16}=5	
iterator{I32}=224	
multi[0]:Control: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values,Adaptive Step Ramp))}=List of Values	
multi[0]:Control: Monitor Update Timeout{Double Float}=0.010000	
multi[0]:Control: Open T Window{Boolean}=False	
multi[0]:Control: Reverse Temperature Sense{Boolean}=False	
multi[0]:Iterator{I32}=0	
multi[0]:Ref: Temperature Window{LVObjVI Refnum (Void)}=	
multi[0]:iterate result{U16}=0	
multi[0]:iterator{I32}=3	
multi[0]:temperature:  rate window{Double Float}=120.000000	
multi[0]:temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[0]:temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
multi[0]:temperature: T1{Double Float}=6.012000	
multi[0]:temperature: T2{Double Float}=5.968400	
multi[0]:temperature: T3{Double Float}=86.103200	
multi[0]:temperature: T4{Double Float}=65.237800	
multi[0]:temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
multi[0]:temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
multi[0]:temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
multi[0]:temperature: current temperature{Double Float}=1.464900	
multi[0]:temperature: current temperature 2{Double Float}=287.100000	
multi[0]:temperature: dT/dt{Double Float}=-0.032603	
multi[0]:temperature: error{Double Float}=-0.058900	
multi[0]:temperature: gas{Double Float}=6.000000	
multi[0]:temperature: gas control{Boolean}=False	
multi[0]:temperature: gas control 2{Boolean}=False	
multi[0]:temperature: gass boost{I8}=0	
multi[0]:temperature: gass boost 2{I8}=0	
multi[0]:temperature: gast flow{I16}=0	
multi[0]:temperature: gast flow 2{I16}=7	
multi[0]:temperature: heater{Double Float}=10.400000	
multi[0]:temperature: heater output{Double Float}=0.000000	
multi[0]:temperature: heater output 2{Double Float}=0.000000	
multi[0]:temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
multi[0]:temperature: monitor timeout{Double Float}=0.010000	
multi[0]:temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
multi[0]:temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
multi[0]:temperature: ramp rate{Double Float}=8.000000	
multi[0]:temperature: ramp rate 2{Double Float}=0.000000	
multi[0]:temperature: ramp target{Double Float}=20.000000	
multi[0]:temperature: ramp target 2{Double Float}=0.000000	
multi[0]:temperature: ramping{Boolean}=False	
multi[0]:temperature: setpoint{Double Float}=1.800000	
multi[0]:temperature: setpoint 2{Double Float}=287.100000	
multi[0]:temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
multi[0]:temperature: stability error{Extended Float}=0.040000	
multi[0]:temperature: stability script{String}=	
multi[0]:temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
multi[0]:temperature: temp control mode{U16}=2	
multi[0]:temperature: temp control mode 2{U16}=3	
multi[0]:temperature: temp control mode 2.__text__{String}=Open Loop	
multi[0]:temperature: temp control mode.__text__{String}=Zone	
multi[0]:temperature: temp control sensor{U16}=0	
multi[0]:temperature: temp control sensor 2{U16}=0	
multi[0]:temperature: temp control sensor 2.__text__{String}=Sensor 1	
multi[0]:temperature: temp control sensor.__text__{String}=Sensor A	
multi[0]:temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
multi[0]:temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
multi[0]:temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
multi[0]:temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
multi[0]:temperature: temp loop{U16}=0	
multi[0]:temperature: temp loop 2{U16}=0	
multi[0]:temperature: temp loop 2.__text__{String}=Heater	
multi[0]:temperature: temp loop.__text__{String}=Loop 1	
multi[0]:temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
multi[0]:temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[0]:temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[0]:temperature:error for gas boost{Double Float}=0.000000	
multi[0]:temperature:error for gas boost 2{Double Float}=0.000000	
multi[0]:temperature:heater range{U16}=2	
multi[0]:temperature:heater range 2{U16}=0	
multi[0]:temperature:heater range 2.__text__{String}=Off	
multi[0]:temperature:heater range.__text__{String}=40mW	
multi[0]:temperature:history window{Extended Float}=300.000000	
multi[0]:temperature:is stable?{Boolean}=False	
multi[0]:temperature:monitor{Boolean}=True	
multi[0]:temperature:ramping{Boolean}=False	
multi[0]:temperature:ramping on{Boolean}=False	
multi[0]:temperature:ramping on 2{Boolean}=False	
multi[0]:temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
multi[0]:temperature:stability code{U32}=6618880	
multi[0]:temperature:stability rate{Extended Float}=0.040000	
multi[0]:y{Double Float}=6.000000	
multi[1]:Control: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values,Adaptive Step Ramp))}=Multi-Segment Ramp	
multi[1]:Control: Gate delay{Double Float}=0.000000	
multi[1]:Control: Monitor Update Timeout{Double Float}=0.010000	
multi[1]:Control: Open T Window{Boolean}=False	
multi[1]:Control: Reverse Temperature Sense{Boolean}=False	
multi[1]:Control:Magnet Output{Double Float}=-0.000100	
multi[1]:Iterator{I32}=0	
multi[1]:Magnet: Final Switch Heater{Enum U8 ((False,True,Mixed))}=	
multi[1]:Magnet: Power Supply{Enum U16 ((IPS120,LS625,PS110,Hg iPS,SMS Series,Cryomagnetics 4G,DMG Little CryoFree,DMG Big CryoFree))}=Hg iPS	
multi[1]:Magnet: Rate{Double Float}=0.500000	
multi[1]:Magnet: Units{Enum U16 ((Field,Current))}=Field	
multi[1]:Magnet: VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[1]:Multi-segment_Stage{I32}=0	
multi[1]:Multi-segment_Stage_Changed{Boolean}=False	
multi[1]:Ref: Temperature Window{LVObjVI Refnum (Void)}=	
multi[1]:iterate result{U16}=4	
multi[1]:iterator{I32}=57	
multi[1]:measure point{Boolean}=False	
multi[1]:temperature:  rate window{Double Float}=120.000000	
multi[1]:temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[1]:temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
multi[1]:temperature: T1{Double Float}=1.842400	
multi[1]:temperature: T2{Double Float}=1.465600	
multi[1]:temperature: T3{Double Float}=86.318100	
multi[1]:temperature: T4{Double Float}=66.769200	
multi[1]:temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
multi[1]:temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
multi[1]:temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
multi[1]:temperature: current temperature{Double Float}=1.465600	
multi[1]:temperature: current temperature 2{Double Float}=287.100000	
multi[1]:temperature: dT/dt{Double Float}=-0.001864	
multi[1]:temperature: gas control{Boolean}=False	
multi[1]:temperature: gas control 2{Boolean}=False	
multi[1]:temperature: gass boost{I8}=0	
multi[1]:temperature: gass boost 2{I8}=0	
multi[1]:temperature: gast flow{I16}=0	
multi[1]:temperature: gast flow 2{I16}=7	
multi[1]:temperature: heater output{Double Float}=0.000000	
multi[1]:temperature: heater output 2{Double Float}=0.000000	
multi[1]:temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
multi[1]:temperature: monitor timeout{Double Float}=1.000000	
multi[1]:temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
multi[1]:temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
multi[1]:temperature: ramp rate{Double Float}=8.000000	
multi[1]:temperature: ramp rate 2{Double Float}=0.000000	
multi[1]:temperature: ramp target{Double Float}=20.000000	
multi[1]:temperature: ramp target 2{Double Float}=0.000000	
multi[1]:temperature: ramping{Boolean}=False	
multi[1]:temperature: setpoint{Double Float}=1.800000	
multi[1]:temperature: setpoint 2{Double Float}=287.100000	
multi[1]:temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
multi[1]:temperature: stability error{Extended Float}=0.040000	
multi[1]:temperature: stability script{String}=	
multi[1]:temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
multi[1]:temperature: temp control mode{U16}=2	
multi[1]:temperature: temp control mode 2{U16}=3	
multi[1]:temperature: temp control mode 2.__text__{String}=Open Loop	
multi[1]:temperature: temp control mode.__text__{String}=Zone	
multi[1]:temperature: temp control sensor{U16}=0	
multi[1]:temperature: temp control sensor 2{U16}=0	
multi[1]:temperature: temp control sensor 2.__text__{String}=Sensor 1	
multi[1]:temperature: temp control sensor.__text__{String}=Sensor A	
multi[1]:temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
multi[1]:temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
multi[1]:temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
multi[1]:temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
multi[1]:temperature: temp loop{U16}=0	
multi[1]:temperature: temp loop 2{U16}=0	
multi[1]:temperature: temp loop 2.__text__{String}=Heater	
multi[1]:temperature: temp loop.__text__{String}=Loop 1	
multi[1]:temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
multi[1]:temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[1]:temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[1]:temperature:error for gas boost{Double Float}=0.000000	
multi[1]:temperature:error for gas boost 2{Double Float}=0.000000	
multi[1]:temperature:heater range{U16}=2	
multi[1]:temperature:heater range 2{U16}=0	
multi[1]:temperature:heater range 2.__text__{String}=Off	
multi[1]:temperature:heater range.__text__{String}=40mW	
multi[1]:temperature:history window{Extended Float}=300.000000	
multi[1]:temperature:is stable?{Boolean}=True	
multi[1]:temperature:monitor{Boolean}=True	
multi[1]:temperature:ramping{Boolean}=False	
multi[1]:temperature:ramping on{Boolean}=False	
multi[1]:temperature:ramping on 2{Boolean}=False	
multi[1]:temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
multi[1]:temperature:stability code{U32}=6618880	
multi[1]:temperature:stability rate{Extended Float}=0.040000	
multi[1]:y{Double Float}=0.000000	
parameter: Termination{String}=False	
parameter: delta time{Double Float}=1.000000	
parameter: progress{Double Float}=100.000000	
temperature:  rate window{Double Float}=120.000000	
temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
temperature: T1{Double Float}=6.012000	
temperature: T2{Double Float}=5.968400	
temperature: T3{Double Float}=86.103200	
temperature: T4{Double Float}=65.237800	
temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
temperature: current temperature{Double Float}=1.464900	
temperature: current temperature 2{Double Float}=287.100000	
temperature: dT/dt{Double Float}=-0.032603	
temperature: gas control{Boolean}=False	
temperature: gas control 2{Boolean}=False	
temperature: gass boost{I8}=0	
temperature: gass boost 2{I8}=0	
temperature: gast flow{I16}=0	
temperature: gast flow 2{I16}=7	
temperature: heater output{Double Float}=0.000000	
temperature: heater output 2{Double Float}=0.000000	
temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
temperature: monitor timeout{Double Float}=0.010000	
temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
temperature: ramp rate{Double Float}=8.000000	
temperature: ramp rate 2{Double Float}=0.000000	
temperature: ramp target{Double Float}=20.000000	
temperature: ramp target 2{Double Float}=0.000000	
temperature: ramping{Boolean}=False	
temperature: setpoint{Double Float}=1.800000	
temperature: setpoint 2{Double Float}=287.100000	
temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
temperature: stability error{Extended Float}=0.040000	
temperature: stability script{String}=	
temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
temperature: temp control mode{U16}=2	
temperature: temp control mode 2{U16}=3	
temperature: temp control mode 2.__text__{String}=Open Loop	
temperature: temp control mode.__text__{String}=Zone	
temperature: temp control sensor{U16}=0	
temperature: temp control sensor 2{U16}=0	
temperature: temp control sensor 2.__text__{String}=Sensor 1	
temperature: temp control sensor.__text__{String}=Sensor A	
temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
temperature: temp loop{U16}=0	
temperature: temp loop 2{U16}=0	
temperature: temp loop 2.__text__{String}=Heater	
temperature: temp loop.__text__{String}=Loop 1	
temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
temperature:error for gas boost{Double Float}=0.000000	
temperature:error for gas boost 2{Double Float}=0.000000	
temperature:heater range{U16}=2	
temperature:heater range 2{U16}=0	
temperature:heater range 2.__text__{String}=Off	
temperature:heater range.__text__{String}=40mW	
temperature:history window{Extended Float}=300.000000	
temperature:is stable?{Boolean}=False	
temperature:monitor{Boolean}=True	
temperature:ramping{Boolean}=False	
temperature:ramping on{Boolean}=False	
temperature:ramping on 2{Boolean}=False	
temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
temperature:stability code{U32}=6618880	
temperature:stability rate{Extended Float}=0.040000	
y{Double Float}=6.000000	
