TDI Format 1.5	Offset	Rxx::R	Rxx::Theta	Rxx::X	Rxx::Y	Rxy::R	Rxy::Theta	Rxy::X	Rxy::Y	temperature: T1	temperature: T2	temperature: T3	temperature: T4	temperature: dT/dt	iterator	multi[0]:iterator	multi[0]:y	multi[0]:temperature: setpoint	multi[0]:temperature: T1	multi[0]:temperature: T2	multi[0]:temperature: T3	multi[0]:temperature: T4	multi[0]:temperature: heater	multi[0]:temperature: gas	multi[0]:temperature: dT/dt	multi[0]:temperature: current temperature	multi[0]:temperature: error	multi[1]:iterator	multi[1]:y	multi[1]:Control:Magnet Output
2nd Parameter Class{String}=Multi-Parameter	0E+0	1.226141543E-3	1.56E-1	1.226141543E-3	3.371767975E-6	5.895316112E-7	-6.9204E+0	5.84790036E-7	-7.217676503E-8	5.0799E+0	5.0653E+0	8.57808E+1	6.47381E+1	7.846349478E-2	2.81E+2	5E+0	5E+0	5E+0	5.0559E+0	5.0402E+0	8.58524E+1	6.47381E+1	8.6E+0	5E+0	4.921570048E-2	5.058E+0	-5.8E-2	0E+0	0E+0	-0E+0
2nd Parameter Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	0E+0	1.23170506E-3	1.56E-1	1.23170506E-3	3.371767975E-6	7.172382071E-6	-5.328E-1	7.172382071E-6	-6.848892033E-8	4.9665E+0	4.9962E+0	8.60315E+1	6.47381E+1	-2.540126257E-2	2.82E+2	5E+0	5E+0	1.8E+0	5.0799E+0	5.0653E+0	8.57808E+1	6.47381E+1	8.6E+0	5E+0	7.846349478E-2	1.4649E+0	-5.8E-2	1E+0	5E-1	4.999E-1
Analysis Class{String}=Basic Plot	0E+0	1.235751125E-3	1.548E-1	1.235751125E-3	3.338050296E-6	1.37494368E-5	-2.148E-1	1.37494368E-5	-5.268383926E-8	4.9683E+0	4.9803E+0	8.59957E+1	6.47381E+1	-4.513835162E-2	2.83E+2	5E+0	5E+0	1.8E+0	4.9665E+0	4.9962E+0	8.60315E+1	6.47381E+1	8.6E+0	5E+0	-2.540126257E-2	1.4649E+0	-5.8E-2	2E+0	1E+0	1E+0
Analysis Class Path{Path}=C\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV\\\\plugins\\\\Plotting\\\\Plotting_Base_class\\\\Plotting_Base.lvclass	0E+0	1.241651223E-3	1.56E-1	1.241651223E-3	3.371767975E-6	2.037069985E-5	-6E-2	2.037069985E-5	-2.265406078E-8	4.9879E+0	4.9864E+0	8.59241E+1	6.47381E+1	-3.708254918E-2	2.84E+2	5E+0	5E+0	1.8E+0	4.9683E+0	4.9803E+0	8.59957E+1	6.47381E+1	8.6E+0	5E+0	-4.513835162E-2	1.4649E+0	-5.8E-2	3E+0	1.5E+0	1.4999E+0
Analysis.# pre-routines{I32}=5	0E+0	1.241651223E-3	1.56E-1	1.241651223E-3	3.371767975E-6	2.036914421E-5	-7.44E-2	2.036914421E-5	-2.739557944E-8	5.0087E+0	5.0081E+0	8.61032E+1	6.47381E+1	-3.972586244E-3	2.85E+2	5E+0	5E+0	1.8E+0	4.9879E+0	4.9864E+0	8.59241E+1	6.47381E+1	8.6E+0	5E+0	-3.708254918E-2	1.4649E+0	-5.8E-2	4E+0	1.5E+0	1.5E+0
Analysis:Pre[0]:T Control Measure{1D Array (I32)}=[1,2,3,4,7]	0E+0	1.239088951E-3	1.548E-1	1.239088951E-3	3.338050296E-6	1.770651949E-5	-1.164E-1	1.770651949E-5	-3.74055188E-8	4.9888E+0	4.9922E+0	8.60315E+1	6.47381E+1	-1.493528113E-2	2.86E+2	5E+0	5E+0	1.8E+0	5.0087E+0	5.0081E+0	8.61032E+1	6.47381E+1	8.6E+0	5E+0	-3.972586244E-3	1.4649E+0	-5.8E-2	5E+0	1.3E+0	1.3002E+0
Autosave Tabs{Enum U32 ((XY Measurement Save,Parameter Plot Save 2))}=Parameter Plot Save 2	0E+0	1.236762287E-3	1.56E-1	1.236762287E-3	3.371767975E-6	1.507548829E-5	-1.476E-1	1.507548829E-5	-4.003972349E-8	5.0388E+0	5.0388E+0	8.60315E+1	6.47381E+1	4.820050299E-2	2.87E+2	5E+0	5E+0	1.8E+0	4.9888E+0	4.9922E+0	8.60315E+1	6.47381E+1	8.6E+0	5E+0	-1.493528113E-2	1.4649E+0	-5.8E-2	6E+0	1.1E+0	1.1001E+0
Control:Magnet Output{Double Float}=-0.007000	0E+0	1.234908253E-3	1.56E-1	1.234908253E-3	3.371767975E-6	1.244183231E-5	-2.28E-1	1.244183231E-5	-5.110337075E-8	4.959E+0	4.9723E+0	8.60315E+1	6.47381E+1	-5.873987451E-2	2.88E+2	5E+0	5E+0	1.8E+0	5.0388E+0	5.0388E+0	8.60315E+1	6.47381E+1	8.6E+0	5E+0	4.820050299E-2	1.4649E+0	-5.8E-2	7E+0	9E-1	9.001E-1
Control:Magnet Rate{Double Float}=0.500000	0E+0	1.233052805E-3	1.548E-1	1.233052805E-3	3.338050296E-6	9.791808231E-6	-4.08E-1	9.791808231E-6	-7.112317593E-8	4.9749E+0	4.9893E+0	8.57092E+1	6.47381E+1	-2.947452478E-2	2.89E+2	5E+0	5E+0	1.8E+0	4.959E+0	4.9723E+0	8.60315E+1	6.47381E+1	8.6E+0	5E+0	-5.873987451E-2	1.4649E+0	-5.8E-2	8E+0	7E-1	7E-1
Display Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	0E+0	1.23170506E-3	1.56E-1	1.23170506E-3	3.371767975E-6	7.170274893E-6	-4.548E-1	7.170274893E-6	-5.795223733E-8	4.9906E+0	4.9987E+0	8.57808E+1	6.47381E+1	-1.163872797E-2	2.9E+2	5E+0	5E+0	1.8E+0	4.9749E+0	4.9893E+0	8.57092E+1	6.47381E+1	8.6E+0	5E+0	-2.947452478E-2	1.4649E+0	-5.8E-2	9E+0	5E-1	5.001E-1
Elapsed Time{Double Float}=12790.950867	0E+0	1.2303559E-3	1.56E-1	1.2303559E-3	3.371767975E-6	4.528699321E-6	-7.632E-1	4.528699321E-6	-6.164005375E-8	4.9927E+0	5.0169E+0	8.6139E+1	6.47381E+1	2.272778424E-3	2.91E+2	5E+0	5E+0	1.8E+0	4.9906E+0	4.9987E+0	8.57808E+1	6.47381E+1	8.6E+0	5E+0	-1.163872797E-2	1.4649E+0	-5.8E-2	1E+1	3E-1	3E-1
File:Autodel{Boolean}=True	0E+0	1.228670157E-3	1.56E-1	1.228670157E-3	3.371767975E-6	1.888190066E-6	-2.4312E+0	1.885553972E-6	-8.165994378E-8	5.0083E+0	5.0133E+0	8.60673E+1	6.47381E+1	-1.856606919E-3	2.92E+2	5E+0	5E+0	1.8E+0	4.9927E+0	5.0169E+0	8.6139E+1	6.47381E+1	8.6E+0	5E+0	2.272778424E-3	1.4649E+0	-5.8E-2	1.1E+1	1E-1	1E-1
File:Autosave{Boolean}=False	0E+0	1.228670157E-3	1.56E-1	1.228670157E-3	3.338050296E-6	1.885025056E-6	-2.31E+0	1.882917878E-6	-7.744527624E-8	5.0172E+0	5.024E+0	8.60315E+1	6.47381E+1	9.289126843E-3	2.93E+2	5E+0	5E+0	1.8E+0	5.0083E+0	5.0133E+0	8.60673E+1	6.47381E+1	8.6E+0	5E+0	-1.856606919E-3	1.4649E+0	-5.8E-2	1.2E+1	1E-1	1E-1
File:Export Config{Boolean}=True	0E+0	1.228501866E-3	1.56E-1	1.228501866E-3	3.371767975E-6	1.7475239E-6	-2.5644E+0	1.745942809E-6	-7.955262415E-8	4.969E+0	4.9925E+0	8.60315E+1	6.47381E+1	-4.502697289E-2	2.94E+2	5E+0	5E+0	1.8E+0	5.0172E+0	5.024E+0	8.60315E+1	6.47381E+1	8.6E+0	5E+0	9.289126843E-3	1.4649E+0	-5.8E-2	1.3E+1	9E-2	9.01E-2
File:Final Autosave{Boolean}=True	0E+0	1.228265692E-3	1.56E-1	1.228265692E-3	3.371767975E-6	1.626880169E-6	-2.7216E+0	1.624244075E-6	-7.849886534E-8	4.9989E+0	5.0006E+0	8.60315E+1	6.47381E+1	-2.258572355E-2	2.95E+2	5E+0	5E+0	1.8E+0	4.969E+0	4.9925E+0	8.60315E+1	6.47381E+1	8.6E+0	5E+0	-4.502697289E-2	1.4649E+0	-5.8E-2	1.4E+1	8E-2	8.01E-2
Filter:Enable{Enum U16 ((None,Analog,Digital,Analog&Digitial))}=None	0E+0	1.228163869E-3	1.56E-1	1.228163869E-3	3.338050296E-6	1.490954447E-6	-3.6408E+0	1.487792266E-6	-9.588472605E-8	5.0271E+0	5.0409E+0	8.59957E+1	6.47381E+1	4.923027009E-2	2.96E+2	5E+0	5E+0	1.8E+0	4.9989E+0	5.0006E+0	8.60315E+1	6.47381E+1	8.6E+0	5E+0	-2.258572355E-2	1.4649E+0	-5.8E-2	1.5E+1	7E-2	7E-2
Filter:Points{I32}=1	0E+0	1.227995577E-3	1.56E-1	1.227995577E-3	3.371767975E-6	1.354503486E-6	-2.8704E+0	1.352923244E-6	-6.848894861E-8	5.0073E+0	5.0199E+0	8.59957E+1	6.47381E+1	1.350119524E-2	2.97E+2	5E+0	5E+0	1.8E+0	5.0271E+0	5.0409E+0	8.59957E+1	6.47381E+1	8.6E+0	5E+0	4.923027009E-2	1.4649E+0	-5.8E-2	1.6E+1	6E-2	6E-2
Filter:Type{U16}=1	0E+0	1.227827286E-3	1.56E-1	1.227827286E-3	3.371767975E-6	1.234381317E-6	-3.852E+0	1.23174692E-6	-8.482107879E-8	4.9861E+0	5.0023E+0	8.59599E+1	6.47381E+1	-1.608838886E-2	2.98E+2	5E+0	5E+0	1.8E+0	5.0073E+0	5.0199E+0	8.59957E+1	6.47381E+1	8.6E+0	5E+0	1.350119524E-2	1.4649E+0	-5.8E-2	1.7E+1	5E-2	5.01E-2
Filter:Type.__text__{String}=Repeat	0E+0	1.227827286E-3	1.56E-1	1.227827286E-3	3.371767975E-6	1.220683528E-6	-3.2964E+0	1.218048848E-6	-7.164997048E-8	4.9901E+0	4.999E+0	8.59957E+1	6.47381E+1	-1.860215701E-2	2.99E+2	5E+0	5E+0	1.8E+0	4.9861E+0	5.0023E+0	8.59599E+1	6.47381E+1	8.6E+0	5E+0	-1.608838886E-2	1.4649E+0	-5.8E-2	1.8E+1	5E-2	5E-2
Filter:Window{Double Float}=1.000000	0E+0	1.227625336E-3	1.56E-1	1.227625336E-3	3.371767975E-6	1.165365433E-6	-4.1208E+0	1.162731318E-6	-8.534781677E-8	5.0289E+0	5.0297E+0	8.59957E+1	6.47381E+1	2.941622958E-2	3E+2	5E+0	5E+0	1.8E+0	4.9901E+0	4.999E+0	8.59957E+1	6.47381E+1	8.6E+0	5E+0	-1.860215701E-2	1.4649E+0	-5.8E-2	1.9E+1	4.5E-2	4.49E-2
Iterator{I32}=0	0E+0	1.227490703E-3	1.56E-1	1.227490703E-3	3.304332616E-6	1.089501077E-6	-3.8388E+0	1.087920835E-6	-7.42841978E-8	5.0253E+0	5.0302E+0	8.59957E+1	6.47381E+1	2.696163207E-2	3.01E+2	5E+0	5E+0	1.8E+0	5.0289E+0	5.0297E+0	8.59957E+1	6.47381E+1	8.6E+0	5E+0	2.941622958E-2	1.4649E+0	-5.8E-2	2E+1	4E-2	3.99E-2
Magnet: Control Mode{Boolean}=False	0E+0	1.227320997E-3	1.56E-1	1.227320997E-3	3.338050296E-6	1.029968909E-6	-4.6632E+0	1.027334512E-6	-8.534784506E-8	4.9983E+0	5.0104E+0	8.57808E+1	6.47381E+1	-1.580429077E-2	3.02E+2	5E+0	5E+0	1.8E+0	5.0253E+0	5.0302E+0	8.59957E+1	6.47381E+1	8.6E+0	5E+0	2.696163207E-2	1.4649E+0	-5.8E-2	2.1E+1	3.5E-2	3.49E-2
Magnet: Final Switch Heater{Enum U8 ((False,True,Mixed))}=	0E+0	1.227152706E-3	1.56E-1	1.227152706E-3	3.371767975E-6	9.556847961E-7	-5.2032E+0	9.504168506E-7	-8.850900835E-8	5.0055E+0	5.016E+0	8.57092E+1	6.47381E+1	-1.458076062E-3	3.03E+2	5E+0	5E+0	1.8E+0	4.9983E+0	5.0104E+0	8.57808E+1	6.47381E+1	8.6E+0	5E+0	-1.580429077E-2	1.4649E+0	-5.8E-2	2.2E+1	3E-2	2.99E-2
Magnet: Power Supply{Enum U16 ((IPS120,LS625,PS110,Hg iPS,SMS Series,Cryomagnetics 4G,DMG Little CryoFree,DMG Big CryoFree))}=Hg iPS	0E+0	1.226984415E-3	1.56E-1	1.226984415E-3	3.371767975E-6	8.8087403E-7	-5.2152E+0	8.766593908E-7	-8.165994378E-8	5.0027E+0	5.0131E+0	8.57092E+1	6.47381E+1	-1.34241418E-3	3.04E+2	5E+0	5E+0	1.8E+0	5.0055E+0	5.016E+0	8.57092E+1	6.47381E+1	8.6E+0	5E+0	-1.458076062E-3	1.4649E+0	-5.8E-2	2.3E+1	2.5E-2	2.5E-2
Magnet: Rate{Double Float}=0.500000	0E+0	1.226816123E-3	1.56E-1	1.226816123E-3	3.371767975E-6	8.271373088E-7	-5.292E+0	8.229223867E-7	-7.797209908E-8	4.9882E+0	5.003E+0	8.5745E+1	6.47381E+1	-1.492595766E-2	3.05E+2	5E+0	5E+0	1.8E+0	5.0027E+0	5.0131E+0	8.57092E+1	6.47381E+1	8.6E+0	5E+0	-1.34241418E-3	1.4649E+0	-5.8E-2	2.4E+1	2E-2	2E-2
Magnet: Setpoint{Double Float}=0.000000	0E+0	1.226647832E-3	1.56E-1	1.226647832E-3	3.371767975E-6	7.502187988E-7	-5.1912E+0	7.470580315E-7	-6.901579973E-8	5.0371E+0	5.0323E+0	8.5745E+1	6.47381E+1	2.406666242E-2	3.06E+2	5E+0	5E+0	1.8E+0	4.9882E+0	5.003E+0	8.5745E+1	6.47381E+1	8.6E+0	5E+0	-1.492595766E-2	1.4649E+0	-5.8E-2	2.5E+1	1.5E-2	1.49E-2
Magnet: Units{Enum U16 ((Field,Current))}=Field	0E+0	1.226478126E-3	1.56E-1	1.226478126E-3	3.338050296E-6	6.843642472E-7	-7.182E+0	6.796221063E-7	-8.745524954E-8	5.005E+0	5.0184E+0	8.58166E+1	6.47381E+1	1.772602787E-3	3.07E+2	5E+0	5E+0	1.8E+0	5.0371E+0	5.0323E+0	8.5745E+1	6.47381E+1	8.6E+0	5E+0	2.406666242E-2	1.4649E+0	-5.8E-2	2.6E+1	1E-2	9.9E-3
Magnet: VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	0E+0	1.226309835E-3	1.56E-1	1.226309835E-3	3.371767975E-6	6.232487253E-7	-7.5876E+0	6.174538438E-7	-8.429422767E-8	4.9958E+0	5.0109E+0	8.5745E+1	6.47381E+1	-5.925481208E-3	3.08E+2	5E+0	5E+0	1.8E+0	5.005E+0	5.0184E+0	8.58166E+1	6.47381E+1	8.6E+0	5E+0	1.772602787E-3	1.4649E+0	-5.8E-2	2.7E+1	5E-3	5E-3
Main Screen Path{Path}=C:\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV\\\\1Code.vi	0E+0	1.226141543E-3	1.56E-1	1.226141543E-3	3.338050296E-6	5.568678034E-7	-8.1108E+0	5.51599575E-7	-8.007944699E-8	5.0121E+0	5.0235E+0	8.61032E+1	6.47381E+1	1.436686702E-2	3.09E+2	5E+0	5E+0	1.8E+0	4.9958E+0	5.0109E+0	8.5745E+1	6.47381E+1	8.6E+0	5E+0	-5.925481208E-3	1.4649E+0	-5.8E-2	2.8E+1	0E+0	-1E-4
Measurement Timestamp{Timestamp}=<22:11:13.344 17/05/2023>T	0E+0	1.226309835E-3	1.56E-1	1.226309835E-3	3.304332616E-6	4.794229231E-7	-9.0684E+0	4.746819136E-7	-7.744530452E-8	5.0345E+0	5.0396E+0	8.60673E+1	6.47381E+1	3.781943023E-2	3.1E+2	5E+0	5E+0	1.8E+0	5.0121E+0	5.0235E+0	8.61032E+1	6.47381E+1	8.6E+0	5E+0	1.436686702E-2	1.4649E+0	-5.8E-2	2.9E+1	-5E-3	-5.2E-3
Measurement Title{String}=	0E+0	1.226478126E-3	1.56E-1	1.226478126E-3	3.338050296E-6	4.367493117E-7	-1.06812E+1	4.288466863E-7	-8.271373088E-8	5.2977E+0	5.1615E+0	8.60673E+1	6.47381E+1	2.209218293E-1	3.11E+2	5E+0	5E+0	1.8E+0	5.0345E+0	5.0396E+0	8.60673E+1	6.47381E+1	8.6E+0	5E+0	3.781943023E-2	1.4649E+0	-5.8E-2	3E+1	-1E-2	-1.03E-2
Measurment Select{U16}=4	0E+0	1.226647832E-3	1.56E-1	1.226647832E-3	3.338050296E-6	3.545631391E-7	-1.25256E+1	3.461332949E-7	-7.849892191E-8	5.5632E+0	5.363E+0	8.60673E+1	6.47381E+1	5.168938637E-1	3.12E+2	5E+0	5E+0	1.8E+0	5.2977E+0	5.1615E+0	8.60673E+1	6.47381E+1	8.6E+0	5E+0	2.209218293E-1	1.4649E+0	-5.8E-2	3.1E+1	-1.5E-2	-1.53E-2
Measurment Select.__text__{String}=6221-Lockin-DAQ	0E+0	1.226917098E-3	1.56E-1	1.226917098E-3	3.371767975E-6	2.808051136E-7	-1.51452E+1	2.718488991E-7	-7.533787176E-8	5.5378E+0	5.4384E+0	8.60315E+1	6.47381E+1	5.954332352E-1	3.13E+2	5E+0	5E+0	1.8E+0	5.5632E+0	5.363E+0	8.60673E+1	6.47381E+1	8.6E+0	5E+0	5.168938637E-1	1.4649E+0	-5.8E-2	3.2E+1	-2E-2	-2.01E-2
Notes{String}=I+1A I-1E\\nrxx+1B Rxx-1C\\nRxy+1D Rxy-4A	0E+0	1.226984415E-3	1.56E-1	1.226984415E-3	3.371767975E-6	2.339162972E-7	-2.13036E+1	2.175843933E-7	-8.692845499E-8	5.45E+0	5.4354E+0	8.59957E+1	6.47381E+1	5.351260304E-1	3.14E+2	5E+0	5E+0	1.8E+0	5.5378E+0	5.4384E+0	8.60315E+1	6.47381E+1	8.6E+0	5E+0	5.954332352E-1	1.4649E+0	-5.8E-2	3.3E+1	-2.5E-2	-2.51E-2
Offset{Double Float}=0.000000	0E+0	1.22738888E-3	1.56E-1	1.22738888E-3	3.371767975E-6	1.717494489E-7	-2.92848E+1	1.496219281E-7	-8.587461133E-8	4.1322E+0	4.3884E+0	8.59599E+1	6.47381E+1	-1.143293977E+0	3.15E+2	5E+0	5E+0	1.8E+0	5.45E+0	5.4354E+0	8.59957E+1	6.47381E+1	8.6E+0	5E+0	5.351260304E-1	1.4649E+0	-5.8E-2	3.4E+1	-3E-2	-3.01E-2
Option: 2182 Autozero{Boolean}=True	0E+0	1.227490703E-3	1.56E-1	1.227490703E-3	3.371767975E-6	1.043141177E-7	-4.0242E+1	7.955265244E-8	-6.901577145E-8	4.393E+0	4.3807E+0	8.59957E+1	6.47381E+1	-1.203702211E+0	3.16E+2	5E+0	5E+0	1.8E+0	4.1322E+0	4.3884E+0	8.59599E+1	6.47381E+1	8.6E+0	5E+0	-1.143293977E+0	1.4649E+0	-5.8E-2	3.5E+1	-3.5E-2	-3.51E-2
Option: 2182 Front Autozero{Boolean}=True	0E+0	1.227658995E-3	1.56E-1	1.227658995E-3	3.371767975E-6	8.745524954E-8	-7.97388E+1	1.527833177E-8	-8.798210066E-8	4.5791E+0	4.5945E+0	8.59599E+1	6.47381E+1	-8.765817881E-1	3.17E+2	5E+0	5E+0	1.8E+0	4.393E+0	4.3807E+0	8.59957E+1	6.47381E+1	8.6E+0	5E+0	-1.203702211E+0	1.4649E+0	-5.8E-2	3.6E+1	-4E-2	-4.01E-2
Option: 2182 Hold{Boolean}=False	0E+0	1.227827286E-3	1.56E-1	1.227827286E-3	3.371767975E-6	1.027335926E-7	-1.120812E+2	-4.162027686E-8	-9.746525112E-8	4.8238E+0	4.8148E+0	8.59599E+1	6.47381E+1	-4.704612494E-1	3.18E+2	5E+0	5E+0	1.8E+0	4.5791E+0	4.5945E+0	8.59599E+1	6.47381E+1	8.6E+0	5E+0	-8.765817881E-1	1.4649E+0	-5.8E-2	3.7E+1	-4.5E-2	-4.49E-2
Option: 2182 Hold Count{I32}=10	0E+0	1.227827286E-3	1.56E-1	1.227827286E-3	3.371767975E-6	1.306558818E-7	-1.368744E+2	-9.746525112E-8	-9.166991708E-8	4.8119E+0	4.8369E+0	8.59599E+1	6.47381E+1	-2.193853259E-1	3.19E+2	5E+0	5E+0	1.8E+0	4.8238E+0	4.8148E+0	8.59599E+1	6.47381E+1	8.6E+0	5E+0	-4.704612494E-1	1.4649E+0	-5.8E-2	3.8E+1	-5E-2	-5E-2
Option: 2182 Hold Window{Double Float}=1.000000	0E+0	1.227827286E-3	1.56E-1	1.227827286E-3	3.371767975E-6	1.322364068E-7	-1.441608E+2	-1.090556364E-7	-7.902577303E-8	4.9997E+0	4.8787E+0	8.59599E+1	6.47381E+1	-6.586601585E-2	3.2E+2	5E+0	5E+0	1.8E+0	4.8119E+0	4.8369E+0	8.59599E+1	6.47381E+1	8.6E+0	5E+0	-2.193853259E-1	1.4649E+0	-5.8E-2	3.9E+1	-5E-2	-5E-2
Option: 2182 Line Sync{Boolean}=False	0E+0	1.227995577E-3	1.56E-1	1.227995577E-3	3.371767975E-6	2.586774796E-7	-1.613364E+2	-2.460335619E-7	-8.429419939E-8	4.9239E+0	4.907E+0	8.59241E+1	6.47381E+1	3.005087674E-1	3.21E+2	5E+0	5E+0	1.8E+0	4.9997E+0	4.8787E+0	8.59599E+1	6.47381E+1	8.6E+0	5E+0	-6.586601585E-2	1.4649E+0	-5.8E-2	4E+1	-6E-2	-5.99E-2
Option: 2182 Reference Reading{Double Float}=0.000000	0E+0	1.228163869E-3	1.56E-1	1.228163869E-3	3.338050296E-6	3.730022212E-7	-1.689576E+2	-3.68260646E-7	-7.32306087E-8	4.9579E+0	4.959E+0	8.59241E+1	6.47381E+1	5.009405017E-1	3.22E+2	5E+0	5E+0	1.8E+0	4.9239E+0	4.907E+0	8.59241E+1	6.47381E+1	8.6E+0	5E+0	3.005087674E-1	1.4649E+0	-5.8E-2	4.1E+1	-7E-2	-7E-2
Option: 2182 Relative Mode{Boolean}=False	0E+0	1.228333574E-3	1.56E-1	1.228333574E-3	3.371767975E-6	5.152480639E-7	-1.715976E+2	-5.120870138E-7	-7.691836855E-8	4.9054E+0	4.9283E+0	8.59599E+1	6.47381E+1	2.855933905E-1	3.23E+2	5E+0	5E+0	1.8E+0	4.9579E+0	4.959E+0	8.59241E+1	6.47381E+1	8.6E+0	5E+0	5.009405017E-1	1.4649E+0	-5.8E-2	4.2E+1	-8E-2	-7.99E-2
Option: 2182 Trigger Delay{Cluster (Boolean,Double Float)}={'Auto':True,'Time(s)':0.000000}	0E+0	1.228367233E-3	1.56E-1	1.228367233E-3	3.304332616E-6	6.453760763E-7	-1.72584E+2	-6.42215309E-7	-8.482105051E-8	4.9336E+0	4.9501E+0	8.56734E+1	6.47381E+1	1.651268899E-1	3.24E+2	5E+0	5E+0	1.8E+0	4.9054E+0	4.9283E+0	8.59599E+1	6.47381E+1	8.6E+0	5E+0	2.855933905E-1	1.4649E+0	-5.8E-2	4.3E+1	-9E-2	-9E-2
Option: 2182 Trigger Source{Enum U16 ((Immediate,Timer,Manual,Bus,Trigger link))}=Bus	0E+0	1.228670157E-3	1.56E-1	1.228670157E-3	3.371767975E-6	7.839364785E-7	-1.739244E+2	-7.818290175E-7	-8.482110707E-8	5.024E+0	5.023E+0	8.56734E+1	6.47381E+1	1.72862187E-1	3.25E+2	5E+0	5E+0	1.8E+0	4.9336E+0	4.9501E+0	8.56734E+1	6.47381E+1	8.6E+0	5E+0	1.651268899E-1	1.4649E+0	-5.8E-2	4.4E+1	-1E-1	-9.99E-2
Option: 2182 Trigger Timer{Double Float}=0.000000	0E+0	1.228602841E-3	1.56E-1	1.228602841E-3	3.371767975E-6	7.807757112E-7	-1.741104E+2	-7.78668533E-7	-8.166002864E-8	4.9726E+0	4.9842E+0	8.57092E+1	6.47381E+1	9.176970273E-2	3.26E+2	5E+0	5E+0	1.8E+0	5.024E+0	5.023E+0	8.56734E+1	6.47381E+1	8.6E+0	5E+0	1.72862187E-1	1.4649E+0	-5.8E-2	4.5E+1	-1E-1	-9.99E-2
Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	0E+0	1.230187608E-3	1.56E-1	1.230187608E-3	3.371767975E-6	3.412862193E-6	-1.784244E+2	-3.414440455E-6	-9.588472605E-8	4.9438E+0	4.9609E+0	8.57808E+1	6.47381E+1	-6.789071113E-2	3.27E+2	5E+0	5E+0	1.8E+0	4.9726E+0	4.9842E+0	8.57092E+1	6.47381E+1	8.6E+0	5E+0	9.176970273E-2	1.4649E+0	-5.8E-2	4.6E+1	-3E-1	-2.999E-1
Option: 560 Enabled{Boolean}=False	0E+0	1.231536768E-3	1.56E-1	1.231536768E-3	3.371767975E-6	6.029148798E-6	-1.790448E+2	-6.031782064E-6	-1.016799187E-7	5.0145E+0	5.0156E+0	8.60315E+1	6.47381E+1	5.931053311E-4	3.28E+2	5E+0	5E+0	1.8E+0	4.9438E+0	4.9609E+0	8.57808E+1	6.47381E+1	8.6E+0	5E+0	-6.789071113E-2	1.4649E+0	-5.8E-2	4.7E+1	-5E-1	-5E-1
Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	0E+0	1.232884514E-3	1.56E-1	1.232884514E-3	3.371767975E-6	8.632243619E-6	-1.792512E+2	-8.634876885E-6	-1.143239779E-7	4.9587E+0	4.9729E+0	8.59599E+1	6.47381E+1	-6.086500362E-2	3.29E+2	5E+0	5E+0	1.8E+0	5.0145E+0	5.0156E+0	8.60315E+1	6.47381E+1	8.6E+0	5E+0	5.931053311E-4	1.4649E+0	-5.8E-2	4.8E+1	-7E-1	-6.999E-1
Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	0E+0	1.234570256E-3	1.56E-1	1.234570256E-3	3.371767975E-6	1.127489117E-5	-1.79448E+2	-1.127752443E-5	-1.090555798E-7	5.0006E+0	5.0159E+0	8.59241E+1	6.47381E+1	-7.173772901E-3	3.3E+2	5E+0	5E+0	1.8E+0	4.9587E+0	4.9729E+0	8.59599E+1	6.47381E+1	8.6E+0	5E+0	-6.086500362E-2	1.4649E+0	-5.8E-2	4.9E+1	-9E-1	-8.998E-1
Option: 6221 Adjust Mode{Enum U16 ((Offset,Frequency,Amplitude))}=Offset	0E+0	1.236593996E-3	1.548E-1	1.236593996E-3	3.338050296E-6	1.389431732E-5	-1.794924E+2	-1.389695342E-5	-1.243338663E-7	4.9922E+0	4.9961E+0	8.59241E+1	6.47381E+1	-3.439005092E-2	3.31E+2	5E+0	5E+0	1.8E+0	5.0006E+0	5.0159E+0	8.59241E+1	6.47381E+1	8.6E+0	5E+0	-7.173772901E-3	1.4649E+0	-5.8E-2	5E+1	-1.1E+0	-1.0999E+0
Option: 6221 Amplitude{Double Float}=1.000000E-6	0E+0	1.238718145E-3	1.56E-1	1.238718145E-3	3.371767975E-6	1.653009179E-5	-1.795572E+2	-1.653269395E-5	-1.29075385E-7	4.9894E+0	4.9988E+0	8.56375E+1	6.47381E+1	-1.685187034E-2	3.32E+2	5E+0	5E+0	1.8E+0	4.9922E+0	4.9961E+0	8.59241E+1	6.47381E+1	8.6E+0	5E+0	-3.439005092E-2	1.4649E+0	-5.8E-2	5.1E+1	-1.3E+0	-1.2999E+0
Option: 6221 Compliance{Double Float}=10.000000	0E+0	1.241314641E-3	1.56E-1	1.241314641E-3	3.371767975E-6	1.916844861E-5	-1.79634E+2	-1.917110734E-5	-1.238070152E-7	5.0028E+0	4.9961E+0	8.56734E+1	6.47381E+1	-3.220059723E-2	3.33E+2	5E+0	5E+0	1.8E+0	4.9894E+0	4.9988E+0	8.56375E+1	6.47381E+1	8.6E+0	5E+0	-1.685187034E-2	1.4649E+0	-5.8E-2	5.2E+1	-1.5E+0	-1.5E+0
Option: 6221 Duty Cycle{Double Float}=50.000000	0E+0	1.241314641E-3	1.56E-1	1.241314641E-3	3.371767975E-6	1.916106642E-5	-1.796196E+2	-1.916375343E-5	-1.28548449E-7	4.9947E+0	5.0081E+0	8.56734E+1	6.47381E+1	-1.003127545E-2	3.34E+2	5E+0	5E+0	1.8E+0	5.0028E+0	4.9961E+0	8.56734E+1	6.47381E+1	8.6E+0	5E+0	-3.220059723E-2	1.4649E+0	-5.8E-2	5.3E+1	-1.5E+0	-1.5E+0
Option: 6221 External Trigger{Boolean}=False	0E+0	1.235413127E-3	1.56E-1	1.235413127E-3	3.371767975E-6	1.256458605E-5	-1.794732E+2	-1.256721649E-5	-1.164313258E-7	5.0344E+0	5.0339E+0	8.59241E+1	6.47381E+1	1.94342006E-2	3.35E+2	5E+0	5E+0	1.8E+0	4.9947E+0	5.0081E+0	8.56734E+1	6.47381E+1	8.6E+0	5E+0	-1.003127545E-2	1.4649E+0	-5.8E-2	5.4E+1	-1E+0	-1.0001E+0
Option: 6221 External Trigger Ignore Multiple{Boolean}=False	0E+0	1.231536768E-3	1.56E-1	1.231536768E-3	3.371767975E-6	5.999642646E-6	-1.791132E+2	-6.002278741E-6	-9.483105209E-8	4.9894E+0	5.0046E+0	8.56375E+1	6.43465E+1	-1.521952171E-2	3.36E+2	5E+0	5E+0	1.8E+0	5.0344E+0	5.0339E+0	8.59241E+1	6.47381E+1	8.6E+0	5E+0	1.94342006E-2	1.4649E+0	-5.8E-2	5.5E+1	-5E-1	-5.001E-1
Option: 6221 Frequency{Double Float}=119.770000	
Option: 6221 Function{U16}=1	
Option: 6221 Function.__text__{String}=Sine	
Option: 6221 Idle Level{Double Float}=0.000000	
Option: 6221 Input trigger Line{U8}=5	
Option: 6221 Offset{Double Float}=0.000000	
Option: 6221 Output Trigger Line{U8}=4	
Option: 6221 Pass Through{Boolean}=True	
Option: 6221 Phase Marker{Boolean}=True	
Option: 6221 Phase Marker Phase{Double Float}=0.000000	
Option: 6221 Range Level{Double Float}=2.000000E-12	
Option: 6221 Ranging{U16}=1	
Option: 6221 Ranging.__text__{String}=Best	
Option: 6221 Update Clock{Double Float}=0.000000	
Option: 6221 VISA{Visa Refnum (Void)}=GPIB0::13::INSTR	
Option: Confirm Config{Boolean}=False	
Option: Control Panel Ref{LVObjVI Refnum (Void)}=	
Option: DAQ Global Channel{Boolean}=False	
Option: DAQ Input Rate{Double Float}=10000.000000	
Option: DAQ Input Samples{I32}=200	
Option: DAQ Measurement Channels{1D Array (Cluster (UserDefinedRefnumTag Refnum (Void),\tkDAQmxPhysChanTagType Tag,\tkDAQmxScaleTagType Tag,Boolean,Double Float,String))}=[]	
Option: Differential{I32}=10106	
Option: Differential.__text__{String}=Differential	
Option: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values))}=Function Generator	
Option: Lockin Standoff Time{Double Float}=0.000000	
Option: Paranoid Save Data{Boolean}=True	
Option: Plot Autoback Path{Path}=C:\\\\TEMP\\\\XY Multiparam\\\\Backup.txt	
Option: SR830  Ref Phase{Double Float}=0.000000	
Option: SR830  Synch Filter{Boolean}=False	
Option: SR830  Time Constant{I16}=8	
Option: SR830  Time Constant.__text__{String}=100 ms	
Option: SR830 2x Line Filter{Boolean}=True	
Option: SR830 Adjust Gains{Boolean}=False	
Option: SR830 Auto Gain Lower.__text__{String}=2 nV/fA	
Option: SR830 Auto Gain Upper.__text__{String}=1 V/uA	
Option: SR830 Auto Offset 1{Boolean}=False	
Option: SR830 Auto Offset 2{Boolean}=False	
Option: SR830 Autophase{Boolean}=False	
Option: SR830 DC Coupling?{Boolean}=False	
Option: SR830 Display 1{U16}=0	
Option: SR830 Display 1.__text__{String}=X	
Option: SR830 Display 2{U16}=0	
Option: SR830 Display 2.__text__{String}=Y	
Option: SR830 Dynamic Reserve{I16}=1	
Option: SR830 Dynamic Reserve.__text__{String}=Normal	
Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Option: SR830 Filter Slope{I32}=1	
Option: SR830 Filter Slope.__text__{String}=12 dB/oct	
Option: SR830 Gain{I32}=-1	
Option: SR830 Gain.__text__{String}=Auto Gain	
Option: SR830 Ground Shield?{Boolean}=False	
Option: SR830 Harmonic{I32}=1	
Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A	
Option: SR830 Line Filter{Boolean}=True	
Option: SR830 No Reset{Boolean}=False	
Option: SR830 Offset 1{Double Float}=0.000000	
Option: SR830 Offset 2{Double Float}=0.000000	
Option: SR830 Output Channel 1{Boolean}=False	
Option: SR830 Output Channel 2{Boolean}=False	
Option: SR830 Ratio 1{U16}=0	
Option: SR830 Ratio 1.__text__{String}=None	
Option: SR830 Ratio 2{U16}=0	
Option: SR830 Ratio 2.__text__{String}=None	
Option: SR830 Ref Amplitude{Double Float}=0.100000	
Option: SR830 Ref Frequency{Double Float}=1013.000000	
Option: SR830 Ref Source{Boolean}=False	
Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta]	
Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Option: SR830 VISA{Visa Refnum (Void)}=	
Option: Sense Autorange{Boolean}=False	
Option: Sense Range Level{Double Float}=0.100000	
Option: Sense Rate{Double Float}=1.000000	
Option:560 Comport{Visa Refnum (Void)}=COM1	
Option:560 Filter High Pass{U16}=0	
Option:560 Filter High Pass.__text__{String}=0.03	
Option:560 Filter Lowpass{U16}=0	
Option:560 Filter Lowpass.__text__{String}=0.03	
Option:560 Filter Mode{U16}=0	
Option:560 Filter Mode.__text__{String}=6 dB high pass	
Option:560 Invert{Boolean}=False	
Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Option:570 Enabled{Boolean}=False	
Option:570 Filter High Pass{U16}=0	
Option:570 Filter High Pass.__text__{String}=0.03	
Option:570 Filter Lowpass{U16}=0	
Option:570 Filter Lowpass.__text__{String}=0.03	
Option:570 Filter Mode{U16}=0	
Option:570 Filter Mode.__text__{String}=6 dB high pass	
Option:570 Gain Mode{U16}=0	
Option:570 Gain Mode.__text__{String}=Low Noise	
Option:570 Input Offset{U16}=0	
Option:570 Input Offset On{Boolean}=False	
Option:570 Input Offset.__text__{String}=1pA	
Option:570 Sensitivity{U16}=0	
Option:570 Sensitivity.__text__{String}=1pA/V	
Option:Debug On{Boolean}=False	
Option:GPIB 2182{Visa Refnum (Void)}=	
Option:Parallel Config Voltage Measurers{Boolean}=True	
Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Option:SR830 Settle Time{Double Float}=5.000000	
Option:Sense Digits{I32}=8	
Output Names{1D Array (String)}=['Offset','Rxx::R','Rxx::Theta','Rxx::X','Rxx::Y','Rxy::R','Rxy::Theta','Rxy::X','Rxy::Y','temperature: T1','temperature: T2','temperature: T3','temperature: T4','temperature: dT/dt','iterator','multi[0]:iterator','multi[0]:y','multi[0]:temperature: setpoint','multi[0]:temperature: T1','multi[0]:temperature: T2','multi[0]:temperature: T3','multi[0]:temperature: T4','multi[0]:temperature: heater','multi[0]:temperature: gas','multi[0]:temperature: dT/dt','multi[0]:temperature: current temperature','multi[0]:temperature: error','multi[1]:iterator','multi[1]:y','multi[1]:Control:Magnet Output']	
Parameter Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Parameter Select{U16}=6	
Parameter Select.__text__{String}=Multi-Parameter	
Paths{U32}=0	
Plot: Column Renames{1D Array (Cluster (String,String))}=[]	
Plot: No dups{Boolean}=False	
Plot: StdDevs{Boolean}=False	
Plotting Class{String}=Parameter Plot	
Plotting Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	
Plotting Select{U16}=1	
Plotting Select.__text__{String}=Parameter Plot	
Project Code{String}=Topological_Insulators	
Ref: Temperature Window{LVObjVI Refnum (Void)}=	
Ref:Control Subpanel{LVObjUnknown Refnum (Void)}=	
Ref:Main Screen{LVObjVI Refnum (Void)}=	
Ref:Plotting Subpanel{LVObjUnknown Refnum (Void)}=	
Ref:Toolbar{LVObjUnknown Refnum (Void)}=	
Ref:XY Subpanel{LVObjUnknown Refnum (Void)}=	
Rxx::R{Double Float}=0.001232	
Rxx::Theta{Double Float}=0.156000	
Rxx::X{Double Float}=0.001232	
Rxx::Y{Double Float}=3.371768E-6	
Rxx:Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	
Rxx:Option: 560 Enabled{Boolean}=False	
Rxx:Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	
Rxx:Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	
Rxx:Option: Lockin Standoff Time{Double Float}=0.000000	
Rxx:Option: Lockin Type{Enum U16 ((SRS 830,EG&G 5302))}=SRS 830	
Rxx:Option: SR803 Full Scale Reading{Double Float}=0.000000	
Rxx:Option: SR830  Ref Phase{Double Float}=0.000000	
Rxx:Option: SR830  Synch Filter{Boolean}=False	
Rxx:Option: SR830  Time Constant{I16}=8	
Rxx:Option: SR830 2x Line Filter{Boolean}=False	
Rxx:Option: SR830 Adjust Gains{Boolean}=False	
Rxx:Option: SR830 Auto Gain Lower{I32}=0	
Rxx:Option: SR830 Auto Gain Upper{I32}=26	
Rxx:Option: SR830 Auto Offset 1{Boolean}=False	
Rxx:Option: SR830 Auto Offset 2{Boolean}=False	
Rxx:Option: SR830 Autophase{Boolean}=False	
Rxx:Option: SR830 DC Coupling?{Boolean}=False	
Rxx:Option: SR830 Display 1{U16}=0	
Rxx:Option: SR830 Display 2{U16}=0	
Rxx:Option: SR830 Dynamic Reserve{I16}=2	
Rxx:Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Rxx:Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Rxx:Option: SR830 Filter Slope{I32}=3	
Rxx:Option: SR830 Gain{I32}=18	
Rxx:Option: SR830 Ground Shield?{Boolean}=False	
Rxx:Option: SR830 Harmonic{I32}=1	
Rxx:Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A-B	
Rxx:Option: SR830 Line Filter{Boolean}=False	
Rxx:Option: SR830 No Reset{Boolean}=False	
Rxx:Option: SR830 Offset 1{Double Float}=0.000000	
Rxx:Option: SR830 Offset 2{Double Float}=0.000000	
Rxx:Option: SR830 Output Channel 1{Boolean}=False	
Rxx:Option: SR830 Output Channel 2{Boolean}=False	
Rxx:Option: SR830 Ratio 1{U16}=0	
Rxx:Option: SR830 Ratio 2{U16}=0	
Rxx:Option: SR830 Ref Amplitude{Double Float}=0.100000	
Rxx:Option: SR830 Ref Frequency{Double Float}=1013.000000	
Rxx:Option: SR830 Ref Source{Boolean}=False	
Rxx:Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta,X,Y]	
Rxx:Option: SR830 Time Constant value{Double Float}=0.000000	
Rxx:Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Rxx:Option: SR830 VISA{Visa Refnum (Void)}=GPIB0::5::INSTR	
Rxx:Option:560 Comport{Visa Refnum (Void)}=COM1	
Rxx:Option:560 Filter High Pass{U16}=0	
Rxx:Option:560 Filter Lowpass{U16}=0	
Rxx:Option:560 Filter Mode{U16}=0	
Rxx:Option:560 Invert{Boolean}=False	
Rxx:Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Rxx:Option:570 Enabled{Boolean}=False	
Rxx:Option:570 Filter High Pass{U16}=0	
Rxx:Option:570 Filter Lowpass{U16}=0	
Rxx:Option:570 Filter Mode{U16}=0	
Rxx:Option:570 Gain Mode{U16}=0	
Rxx:Option:570 Input Offset{U16}=0	
Rxx:Option:570 Input Offset On{Boolean}=False	
Rxx:Option:570 Sensitivity{U16}=0	
Rxx:Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Rxx:Option:SR830 Autogain Lower Threshold{Double Float}=0.100000	
Rxx:Option:SR830 Autogain Standoff{Double Float}=3.000000	
Rxx:Option:SR830 Autogain Upper Threshold{Double Float}=0.900000	
Rxx:Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Rxx:Option:SR830 Settle Time{Double Float}=0.000000	
Rxy::R{Double Float}=5.999643E-6	
Rxy::Theta{Double Float}=-179.113200	
Rxy::X{Double Float}=-6.002279E-6	
Rxy::Y{Double Float}=-9.483105E-8	
Rxy:Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	
Rxy:Option: 560 Enabled{Boolean}=False	
Rxy:Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	
Rxy:Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	
Rxy:Option: Lockin Standoff Time{Double Float}=0.000000	
Rxy:Option: Lockin Type{Enum U16 ((SRS 830,EG&G 5302))}=SRS 830	
Rxy:Option: SR803 Full Scale Reading{Double Float}=0.000000	
Rxy:Option: SR830  Ref Phase{Double Float}=0.000000	
Rxy:Option: SR830  Synch Filter{Boolean}=False	
Rxy:Option: SR830  Time Constant{I16}=8	
Rxy:Option: SR830 2x Line Filter{Boolean}=False	
Rxy:Option: SR830 Adjust Gains{Boolean}=False	
Rxy:Option: SR830 Auto Gain Lower{I32}=0	
Rxy:Option: SR830 Auto Gain Upper{I32}=26	
Rxy:Option: SR830 Auto Offset 1{Boolean}=False	
Rxy:Option: SR830 Auto Offset 2{Boolean}=False	
Rxy:Option: SR830 Autophase{Boolean}=False	
Rxy:Option: SR830 DC Coupling?{Boolean}=False	
Rxy:Option: SR830 Display 1{U16}=0	
Rxy:Option: SR830 Display 2{U16}=1	
Rxy:Option: SR830 Dynamic Reserve{I16}=2	
Rxy:Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Rxy:Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Rxy:Option: SR830 Filter Slope{I32}=3	
Rxy:Option: SR830 Gain{I32}=18	
Rxy:Option: SR830 Ground Shield?{Boolean}=False	
Rxy:Option: SR830 Harmonic{I32}=1	
Rxy:Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A-B	
Rxy:Option: SR830 Line Filter{Boolean}=False	
Rxy:Option: SR830 No Reset{Boolean}=False	
Rxy:Option: SR830 Offset 1{Double Float}=0.000000	
Rxy:Option: SR830 Offset 2{Double Float}=0.000000	
Rxy:Option: SR830 Output Channel 1{Boolean}=False	
Rxy:Option: SR830 Output Channel 2{Boolean}=False	
Rxy:Option: SR830 Ratio 1{U16}=0	
Rxy:Option: SR830 Ratio 2{U16}=0	
Rxy:Option: SR830 Ref Amplitude{Double Float}=0.100000	
Rxy:Option: SR830 Ref Frequency{Double Float}=1013.000000	
Rxy:Option: SR830 Ref Source{Boolean}=False	
Rxy:Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta,X,Y]	
Rxy:Option: SR830 Time Constant value{Double Float}=0.000000	
Rxy:Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Rxy:Option: SR830 VISA{Visa Refnum (Void)}=GPIB0::6::INSTR	
Rxy:Option:560 Comport{Visa Refnum (Void)}=COM1	
Rxy:Option:560 Filter High Pass{U16}=0	
Rxy:Option:560 Filter Lowpass{U16}=0	
Rxy:Option:560 Filter Mode{U16}=0	
Rxy:Option:560 Invert{Boolean}=False	
Rxy:Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Rxy:Option:570 Enabled{Boolean}=False	
Rxy:Option:570 Filter High Pass{U16}=0	
Rxy:Option:570 Filter Lowpass{U16}=0	
Rxy:Option:570 Filter Mode{U16}=0	
Rxy:Option:570 Gain Mode{U16}=0	
Rxy:Option:570 Input Offset{U16}=0	
Rxy:Option:570 Input Offset On{Boolean}=False	
Rxy:Option:570 Sensitivity{U16}=0	
Rxy:Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Rxy:Option:SR830 Autogain Lower Threshold{Double Float}=0.100000	
Rxy:Option:SR830 Autogain Standoff{Double Float}=3.000000	
Rxy:Option:SR830 Autogain Upper Threshold{Double Float}=0.900000	
Rxy:Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Rxy:Option:SR830 Settle Time{Double Float}=0.000000	
Sample ID{String}=MBE202221213_PA_D1 750C Cracker WAL	
Save:Filename{String}=${X-Y Class} ${2nd Parameter Class} ${iterator}{%04d} ${y}{%04.2g}.txt	
Save:Final Filename{String}=${X-Y Class} ${2nd Parameter Class} .txt	
Save:Final path{Path}=C:\\\\Data\\\\${Project Code}\\\\${User}\\\\${Sample ID}\\\\${Measurement Timestamp}{%Y%m%d}\\\\${X-Y Class}	
Save:Path{Path}=C:\\\\Data\\\\${Project Code}\\\\${User}\\\\${Sample ID}\\\\${Measurement Timestamp}{%Y%m%d}\\\\${X-Y Class}	
Startup path{Path}=C:\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV	
Sub Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Sweep Step{I32}=3	
T Control Measure.__text__{1D Array (String)}=['temperature: T1','temperature: T2','temperature: T3','temperature: T4','temperature: dT/dt']	
Timestamp{Timestamp}=<22:12:22.069 17/05/2023>T	
Toolbar{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Unaved Data{Boolean}=True	
Unsaved Data{Boolean}=False	
User{String}=Craig	
X-Y Class{String}=6221-Lockin-DAQ	
X-Y Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	
d(Offset){Double Float}=0.000000	
d(Rxx::R){Double Float}=0.000000	
d(Rxx::Theta){Double Float}=0.000000	
d(Rxx::X){Double Float}=0.000000	
d(Rxx::Y){Double Float}=4.735058E-22	
d(Rxy::R){Double Float}=1.095904E-8	
d(Rxy::Theta){Double Float}=0.090737	
d(Rxy::X){Double Float}=1.095292E-8	
d(Rxy::Y){Double Float}=9.313270E-9	
iterate result{U16}=5	
iterator{I32}=336	
multi[0]:Control: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values,Adaptive Step Ramp))}=List of Values	
multi[0]:Control: Monitor Update Timeout{Double Float}=0.010000	
multi[0]:Control: Open T Window{Boolean}=False	
multi[0]:Control: Reverse Temperature Sense{Boolean}=False	
multi[0]:Iterator{I32}=0	
multi[0]:Ref: Temperature Window{LVObjVI Refnum (Void)}=	
multi[0]:iterate result{U16}=0	
multi[0]:iterator{I32}=5	
multi[0]:temperature:  rate window{Double Float}=120.000000	
multi[0]:temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[0]:temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
multi[0]:temperature: T1{Double Float}=5.002300	
multi[0]:temperature: T2{Double Float}=5.003000	
multi[0]:temperature: T3{Double Float}=85.995700	
multi[0]:temperature: T4{Double Float}=64.346500	
multi[0]:temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
multi[0]:temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
multi[0]:temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
multi[0]:temperature: current temperature{Double Float}=1.464900	
multi[0]:temperature: current temperature 2{Double Float}=287.100000	
multi[0]:temperature: dT/dt{Double Float}=-0.023586	
multi[0]:temperature: error{Double Float}=-0.058000	
multi[0]:temperature: gas{Double Float}=5.000000	
multi[0]:temperature: gas control{Boolean}=False	
multi[0]:temperature: gas control 2{Boolean}=False	
multi[0]:temperature: gass boost{I8}=0	
multi[0]:temperature: gass boost 2{I8}=0	
multi[0]:temperature: gast flow{I16}=0	
multi[0]:temperature: gast flow 2{I16}=7	
multi[0]:temperature: heater{Double Float}=8.600000	
multi[0]:temperature: heater output{Double Float}=0.000000	
multi[0]:temperature: heater output 2{Double Float}=0.000000	
multi[0]:temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
multi[0]:temperature: monitor timeout{Double Float}=0.010000	
multi[0]:temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
multi[0]:temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
multi[0]:temperature: ramp rate{Double Float}=8.000000	
multi[0]:temperature: ramp rate 2{Double Float}=0.000000	
multi[0]:temperature: ramp target{Double Float}=20.000000	
multi[0]:temperature: ramp target 2{Double Float}=0.000000	
multi[0]:temperature: ramping{Boolean}=False	
multi[0]:temperature: setpoint{Double Float}=1.800000	
multi[0]:temperature: setpoint 2{Double Float}=287.100000	
multi[0]:temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
multi[0]:temperature: stability error{Extended Float}=0.040000	
multi[0]:temperature: stability script{String}=	
multi[0]:temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
multi[0]:temperature: temp control mode{U16}=2	
multi[0]:temperature: temp control mode 2{U16}=3	
multi[0]:temperature: temp control mode 2.__text__{String}=Open Loop	
multi[0]:temperature: temp control mode.__text__{String}=Zone	
multi[0]:temperature: temp control sensor{U16}=0	
multi[0]:temperature: temp control sensor 2{U16}=0	
multi[0]:temperature: temp control sensor 2.__text__{String}=Sensor 1	
multi[0]:temperature: temp control sensor.__text__{String}=Sensor A	
multi[0]:temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
multi[0]:temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
multi[0]:temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
multi[0]:temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
multi[0]:temperature: temp loop{U16}=0	
multi[0]:temperature: temp loop 2{U16}=0	
multi[0]:temperature: temp loop 2.__text__{String}=Heater	
multi[0]:temperature: temp loop.__text__{String}=Loop 1	
multi[0]:temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
multi[0]:temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[0]:temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[0]:temperature:error for gas boost{Double Float}=0.000000	
multi[0]:temperature:error for gas boost 2{Double Float}=0.000000	
multi[0]:temperature:heater range{U16}=2	
multi[0]:temperature:heater range 2{U16}=0	
multi[0]:temperature:heater range 2.__text__{String}=Off	
multi[0]:temperature:heater range.__text__{String}=40mW	
multi[0]:temperature:history window{Extended Float}=300.000000	
multi[0]:temperature:is stable?{Boolean}=True	
multi[0]:temperature:monitor{Boolean}=True	
multi[0]:temperature:ramping{Boolean}=False	
multi[0]:temperature:ramping on{Boolean}=False	
multi[0]:temperature:ramping on 2{Boolean}=False	
multi[0]:temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
multi[0]:temperature:stability code{U32}=6618880	
multi[0]:temperature:stability rate{Extended Float}=0.040000	
multi[0]:y{Double Float}=5.000000	
multi[1]:Control: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values,Adaptive Step Ramp))}=Multi-Segment Ramp	
multi[1]:Control: Gate delay{Double Float}=0.000000	
multi[1]:Control: Monitor Update Timeout{Double Float}=0.010000	
multi[1]:Control: Open T Window{Boolean}=False	
multi[1]:Control: Reverse Temperature Sense{Boolean}=False	
multi[1]:Control:Magnet Output{Double Float}=-0.000100	
multi[1]:Iterator{I32}=0	
multi[1]:Magnet: Final Switch Heater{Enum U8 ((False,True,Mixed))}=	
multi[1]:Magnet: Power Supply{Enum U16 ((IPS120,LS625,PS110,Hg iPS,SMS Series,Cryomagnetics 4G,DMG Little CryoFree,DMG Big CryoFree))}=Hg iPS	
multi[1]:Magnet: Rate{Double Float}=0.500000	
multi[1]:Magnet: Units{Enum U16 ((Field,Current))}=Field	
multi[1]:Magnet: VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[1]:Multi-segment_Stage{I32}=0	
multi[1]:Multi-segment_Stage_Changed{Boolean}=False	
multi[1]:Ref: Temperature Window{LVObjVI Refnum (Void)}=	
multi[1]:iterate result{U16}=4	
multi[1]:iterator{I32}=57	
multi[1]:measure point{Boolean}=False	
multi[1]:temperature:  rate window{Double Float}=120.000000	
multi[1]:temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[1]:temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
multi[1]:temperature: T1{Double Float}=1.842400	
multi[1]:temperature: T2{Double Float}=1.465600	
multi[1]:temperature: T3{Double Float}=86.318100	
multi[1]:temperature: T4{Double Float}=66.769200	
multi[1]:temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
multi[1]:temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
multi[1]:temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
multi[1]:temperature: current temperature{Double Float}=1.465600	
multi[1]:temperature: current temperature 2{Double Float}=287.100000	
multi[1]:temperature: dT/dt{Double Float}=-0.001864	
multi[1]:temperature: gas control{Boolean}=False	
multi[1]:temperature: gas control 2{Boolean}=False	
multi[1]:temperature: gass boost{I8}=0	
multi[1]:temperature: gass boost 2{I8}=0	
multi[1]:temperature: gast flow{I16}=0	
multi[1]:temperature: gast flow 2{I16}=7	
multi[1]:temperature: heater output{Double Float}=0.000000	
multi[1]:temperature: heater output 2{Double Float}=0.000000	
multi[1]:temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
multi[1]:temperature: monitor timeout{Double Float}=1.000000	
multi[1]:temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
multi[1]:temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
multi[1]:temperature: ramp rate{Double Float}=8.000000	
multi[1]:temperature: ramp rate 2{Double Float}=0.000000	
multi[1]:temperature: ramp target{Double Float}=20.000000	
multi[1]:temperature: ramp target 2{Double Float}=0.000000	
multi[1]:temperature: ramping{Boolean}=False	
multi[1]:temperature: setpoint{Double Float}=1.800000	
multi[1]:temperature: setpoint 2{Double Float}=287.100000	
multi[1]:temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
multi[1]:temperature: stability error{Extended Float}=0.040000	
multi[1]:temperature: stability script{String}=	
multi[1]:temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
multi[1]:temperature: temp control mode{U16}=2	
multi[1]:temperature: temp control mode 2{U16}=3	
multi[1]:temperature: temp control mode 2.__text__{String}=Open Loop	
multi[1]:temperature: temp control mode.__text__{String}=Zone	
multi[1]:temperature: temp control sensor{U16}=0	
multi[1]:temperature: temp control sensor 2{U16}=0	
multi[1]:temperature: temp control sensor 2.__text__{String}=Sensor 1	
multi[1]:temperature: temp control sensor.__text__{String}=Sensor A	
multi[1]:temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
multi[1]:temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
multi[1]:temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
multi[1]:temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
multi[1]:temperature: temp loop{U16}=0	
multi[1]:temperature: temp loop 2{U16}=0	
multi[1]:temperature: temp loop 2.__text__{String}=Heater	
multi[1]:temperature: temp loop.__text__{String}=Loop 1	
multi[1]:temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
multi[1]:temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[1]:temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[1]:temperature:error for gas boost{Double Float}=0.000000	
multi[1]:temperature:error for gas boost 2{Double Float}=0.000000	
multi[1]:temperature:heater range{U16}=2	
multi[1]:temperature:heater range 2{U16}=0	
multi[1]:temperature:heater range 2.__text__{String}=Off	
multi[1]:temperature:heater range.__text__{String}=40mW	
multi[1]:temperature:history window{Extended Float}=300.000000	
multi[1]:temperature:is stable?{Boolean}=True	
multi[1]:temperature:monitor{Boolean}=True	
multi[1]:temperature:ramping{Boolean}=False	
multi[1]:temperature:ramping on{Boolean}=False	
multi[1]:temperature:ramping on 2{Boolean}=False	
multi[1]:temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
multi[1]:temperature:stability code{U32}=6618880	
multi[1]:temperature:stability rate{Extended Float}=0.040000	
multi[1]:y{Double Float}=0.000000	
parameter: Termination{String}=False	
parameter: delta time{Double Float}=1.000000	
parameter: progress{Double Float}=100.000000	
temperature:  rate window{Double Float}=120.000000	
temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
temperature: T1{Double Float}=5.002300	
temperature: T2{Double Float}=5.003000	
temperature: T3{Double Float}=85.995700	
temperature: T4{Double Float}=64.346500	
temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
temperature: current temperature{Double Float}=1.464900	
temperature: current temperature 2{Double Float}=287.100000	
temperature: dT/dt{Double Float}=-0.023586	
temperature: gas control{Boolean}=False	
temperature: gas control 2{Boolean}=False	
temperature: gass boost{I8}=0	
temperature: gass boost 2{I8}=0	
temperature: gast flow{I16}=0	
temperature: gast flow 2{I16}=7	
temperature: heater output{Double Float}=0.000000	
temperature: heater output 2{Double Float}=0.000000	
temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
temperature: monitor timeout{Double Float}=0.010000	
temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
temperature: ramp rate{Double Float}=8.000000	
temperature: ramp rate 2{Double Float}=0.000000	
temperature: ramp target{Double Float}=20.000000	
temperature: ramp target 2{Double Float}=0.000000	
temperature: ramping{Boolean}=False	
temperature: setpoint{Double Float}=1.800000	
temperature: setpoint 2{Double Float}=287.100000	
temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
temperature: stability error{Extended Float}=0.040000	
temperature: stability script{String}=	
temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
temperature: temp control mode{U16}=2	
temperature: temp control mode 2{U16}=3	
temperature: temp control mode 2.__text__{String}=Open Loop	
temperature: temp control mode.__text__{String}=Zone	
temperature: temp control sensor{U16}=0	
temperature: temp control sensor 2{U16}=0	
temperature: temp control sensor 2.__text__{String}=Sensor 1	
temperature: temp control sensor.__text__{String}=Sensor A	
temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
temperature: temp loop{U16}=0	
temperature: temp loop 2{U16}=0	
temperature: temp loop 2.__text__{String}=Heater	
temperature: temp loop.__text__{String}=Loop 1	
temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
temperature:error for gas boost{Double Float}=0.000000	
temperature:error for gas boost 2{Double Float}=0.000000	
temperature:heater range{U16}=2	
temperature:heater range 2{U16}=0	
temperature:heater range 2.__text__{String}=Off	
temperature:heater range.__text__{String}=40mW	
temperature:history window{Extended Float}=300.000000	
temperature:is stable?{Boolean}=True	
temperature:monitor{Boolean}=True	
temperature:ramping{Boolean}=False	
temperature:ramping on{Boolean}=False	
temperature:ramping on 2{Boolean}=False	
temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
temperature:stability code{U32}=6618880	
temperature:stability rate{Extended Float}=0.040000	
y{Double Float}=5.000000	
