TDI Format 1.5	Offset	Rxx::R	Rxx::Theta	Rxx::X	Rxx::Y	Rxy::R	Rxy::Theta	Rxy::X	Rxy::Y	temperature: T1	temperature: T2	temperature: T3	temperature: T4	temperature: dT/dt	iterator	multi[0]:iterator	multi[0]:y	multi[0]:temperature: setpoint	multi[0]:temperature: T1	multi[0]:temperature: T2	multi[0]:temperature: T3	multi[0]:temperature: T4	multi[0]:temperature: heater	multi[0]:temperature: gas	multi[0]:temperature: dT/dt	multi[0]:temperature: current temperature	multi[0]:temperature: error	multi[1]:iterator	multi[1]:y	multi[1]:Control:Magnet Output
2nd Parameter Class{String}=Multi-Parameter	0E+0	1.227490703E-3	1.56E-1	1.227490703E-3	3.371767975E-6	5.768874106E-7	-8.5308E+0	5.7003894E-7	-8.745527782E-8	1.841E+0	1.4648E+0	8.60315E+1	6.67692E+1	-1.962839626E-3	1E+0	0E+0	1.8E+0	1.8E+0	1.8411E+0	1.4649E+0	8.61032E+1	6.67692E+1	0E+0	1.8E+0	-1.969125587E-3	1.8411E+0	-4.11E-2	0E+0	0E+0	0E+0
2nd Parameter Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	0E+0	1.235244836E-3	1.56E-1	1.235244836E-3	3.371767975E-6	7.201359307E-6	-4.524E-1	7.201359307E-6	-5.847906016E-8	1.8404E+0	1.4719E+0	8.65688E+1	6.67692E+1	1.852636808E-3	2E+0	0E+0	1.8E+0	1.8E+0	1.841E+0	1.4648E+0	8.60315E+1	6.67692E+1	0E+0	1.8E+0	-1.962839626E-3	1.4649E+0	-4.11E-2	1E+0	5E-1	4.999E-1
Analysis Class{String}=Basic Plot	0E+0	1.235244836E-3	1.56E-1	1.235244836E-3	3.371767975E-6	7.201359307E-6	-4.524E-1	7.201359307E-6	-5.847906016E-8	1.8404E+0	1.4719E+0	8.65688E+1	6.67692E+1	1.852636808E-3	2E+0	0E+0	1.8E+0	1.8E+0	1.841E+0	1.4648E+0	8.60315E+1	6.67692E+1	0E+0	1.8E+0	-1.962839626E-3	1.4649E+0	-4.11E-2	1E+0	5E-1	4.999E-1
Analysis Class Path{Path}=C\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV\\\\plugins\\\\Plotting\\\\Plotting_Base_class\\\\Plotting_Base.lvclass	0E+0	1.239459192E-3	1.56E-1	1.239459192E-3	3.371767975E-6	1.382688196E-5	-1.908E-1	1.382688196E-5	-4.794234888E-8	1.8432E+0	1.4899E+0	8.64255E+1	6.67692E+1	1.899891719E-2	3E+0	0E+0	1.8E+0	1.8E+0	1.8404E+0	1.4719E+0	8.65688E+1	6.67692E+1	0E+0	1.8E+0	1.852636808E-3	1.4649E+0	-4.11E-2	2E+0	1E+0	1E+0
Analysis.# pre-routines{I32}=5	0E+0	1.245360706E-3	1.56E-1	1.245360706E-3	3.371767975E-6	2.046499961E-5	-1.02E-1	2.046499961E-5	-3.793237558E-8	1.8471E+0	1.509E+0	8.62822E+1	6.67692E+1	1.991373114E-2	4E+0	0E+0	1.8E+0	1.8E+0	1.8432E+0	1.4899E+0	8.64255E+1	6.67692E+1	0E+0	1.8E+0	1.899891719E-2	1.4649E+0	-4.11E-2	3E+0	1.5E+0	1.4999E+0
Analysis:Pre[0]:T Control Measure{1D Array (I32)}=[1,2,3,4,7]	0E+0	1.245360706E-3	1.56E-1	1.245360706E-3	3.371767975E-6	2.047396572E-5	-9E-2	2.047396572E-5	-3.319082863E-8	1.8468E+0	1.5088E+0	8.62822E+1	6.67692E+1	1.778150536E-2	5E+0	0E+0	1.8E+0	1.8E+0	1.8471E+0	1.509E+0	8.62822E+1	6.67692E+1	0E+0	1.8E+0	1.991373114E-2	1.4649E+0	-4.11E-2	4E+0	1.5E+0	1.5E+0
Autosave Tabs{Enum U32 ((XY Measurement Save,Parameter Plot Save 2))}=Parameter Plot Save 2	0E+0	1.242662386E-3	1.56E-1	1.242662386E-3	3.371767975E-6	1.779394617E-5	-9.36E-2	1.779394617E-5	-3.055665788E-8	1.8433E+0	1.5012E+0	8.66404E+1	6.67692E+1	-7.419028785E-3	6E+0	0E+0	1.8E+0	1.8E+0	1.8468E+0	1.5088E+0	8.62822E+1	6.67692E+1	0E+0	1.8E+0	1.778150536E-2	1.4649E+0	-4.11E-2	5E+0	1.3E+0	1.3E+0
Control:Magnet Output{Double Float}=-0.007000	0E+0	1.240471769E-3	1.56E-1	1.240471769E-3	3.371767975E-6	1.515131842E-5	-2.244E-1	1.515131842E-5	-6.111328748E-8	1.8403E+0	1.4939E+0	8.6533E+1	6.67692E+1	-1.400906965E-2	7E+0	0E+0	1.8E+0	1.8E+0	1.8433E+0	1.5012E+0	8.66404E+1	6.67692E+1	0E+0	1.8E+0	-7.419028785E-3	1.4649E+0	-4.11E-2	6E+0	1.1E+0	1.1002E+0
Control:Magnet Rate{Double Float}=0.500000	0E+0	1.23844803E-3	1.56E-1	1.23844803E-3	3.371767975E-6	1.249609569E-5	-2.292E-1	1.249609569E-5	-5.110337075E-8	1.8369E+0	1.4854E+0	8.64971E+1	6.67692E+1	-1.606257074E-2	8E+0	0E+0	1.8E+0	1.8E+0	1.8403E+0	1.4939E+0	8.6533E+1	6.67692E+1	0E+0	1.8E+0	-1.400906965E-2	1.4649E+0	-4.11E-2	7E+0	9E-1	9.001E-1
Display Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	0E+0	1.236762287E-3	1.56E-1	1.236762287E-3	3.371767975E-6	9.86134794E-6	-3.672E-1	9.86134794E-6	-6.374740166E-8	1.8322E+0	1.4748E+0	8.64613E+1	6.8541E+1	-1.917988062E-2	9E+0	0E+0	1.8E+0	1.8E+0	1.8369E+0	1.4854E+0	8.64971E+1	6.67692E+1	0E+0	1.8E+0	-1.606257074E-2	1.4649E+0	-4.11E-2	8E+0	7E-1	7.001E-1
Elapsed Time{Double Float}=12790.950867	0E+0	1.235244836E-3	1.56E-1	1.235244836E-3	3.371767975E-6	7.194508857E-6	-3.744E-1	7.194508857E-6	-4.846914343E-8	1.8312E+0	1.4701E+0	8.60315E+1	6.8541E+1	-1.322498266E-2	1E+1	0E+0	1.8E+0	1.8E+0	1.8322E+0	1.4748E+0	8.64613E+1	6.8541E+1	0E+0	1.8E+0	-1.917988062E-2	1.4649E+0	-4.11E-2	9E+0	5E-1	5E-1
File:Autodel{Boolean}=True	0E+0	1.233897091E-3	1.56E-1	1.233897091E-3	3.371767975E-6	4.547137838E-6	-8.028E-1	4.547137838E-6	-6.532792674E-8	1.8219E+0	1.4543E+0	8.59957E+1	6.8541E+1	-2.600904182E-2	1.1E+1	0E+0	1.8E+0	1.8E+0	1.8312E+0	1.4701E+0	8.60315E+1	6.8541E+1	0E+0	1.8E+0	-1.322498266E-2	1.4649E+0	-4.11E-2	1E+1	3E-1	3.001E-1
File:Autosave{Boolean}=False	0E+0	1.232041642E-3	1.56E-1	1.232041642E-3	3.371767975E-6	1.891346591E-6	-2.4708E+0	1.888716154E-6	-8.271361774E-8	1.8337E+0	1.4728E+0	8.66762E+1	6.8541E+1	1.644850709E-2	1.2E+1	0E+0	1.8E+0	1.8E+0	1.8219E+0	1.4543E+0	8.59957E+1	6.8541E+1	0E+0	1.8E+0	-2.600904182E-2	1.4649E+0	-4.11E-2	1.1E+1	1E-1	1.001E-1
File:Export Config{Boolean}=True	0E+0	1.232041642E-3	1.56E-1	1.232041642E-3	3.371767975E-6	1.889242241E-6	-2.274E+0	1.887135063E-6	-7.639160228E-8	1.834E+0	1.4733E+0	8.6712E+1	6.8541E+1	1.806778833E-2	1.3E+1	0E+0	1.8E+0	1.8E+0	1.8337E+0	1.4728E+0	8.66762E+1	6.8541E+1	0E+0	1.8E+0	1.644850709E-2	1.4649E+0	-4.11E-2	1.2E+1	1E-1	1E-1
File:Final Autosave{Boolean}=True	0E+0	1.232041642E-3	1.56E-1	1.232041642E-3	3.304332616E-6	1.748576075E-6	-2.4708E+0	1.746468897E-6	-7.639154571E-8	1.8345E+0	1.4747E+0	8.66762E+1	6.8541E+1	2.122165263E-2	1.4E+1	0E+0	1.8E+0	1.8E+0	1.834E+0	1.4733E+0	8.6712E+1	6.8541E+1	0E+0	1.8E+0	1.806778833E-2	1.4649E+0	-4.11E-2	1.3E+1	9E-2	9E-2
Filter:Enable{Enum U16 ((None,Analog,Digital,Analog&Digitial))}=None	0E+0	1.231873351E-3	1.56E-1	1.231873351E-3	3.371767975E-6	1.620558635E-6	-2.7504E+0	1.618448628E-6	-7.902574475E-8	1.8346E+0	1.4753E+0	8.66404E+1	6.8541E+1	2.088604309E-2	1.5E+1	0E+0	1.8E+0	1.8E+0	1.8345E+0	1.4747E+0	8.66762E+1	6.8541E+1	0E+0	1.8E+0	2.122165263E-2	1.4649E+0	-4.11E-2	1.4E+1	8E-2	8.01E-2
Filter:Points{I32}=1	0E+0	1.23170506E-3	1.56E-1	1.23170506E-3	3.338050296E-6	1.487792266E-6	-3.1584E+0	1.485687916E-6	-8.376734826E-8	1.8343E+0	1.4754E+0	8.66404E+1	6.8541E+1	1.459380426E-2	1.6E+1	0E+0	1.8E+0	1.8E+0	1.8346E+0	1.4753E+0	8.66404E+1	6.8541E+1	0E+0	1.8E+0	2.088604309E-2	1.4649E+0	-4.11E-2	1.5E+1	7E-2	7E-2
Filter:Type{U16}=1	0E+0	1.231367062E-3	1.56E-1	1.231367062E-3	3.371767975E-6	1.352921264E-6	-3.474E+0	1.350813803E-6	-8.376734826E-8	1.8342E+0	1.4758E+0	8.66404E+1	6.8541E+1	6.922741421E-3	1.7E+1	0E+0	1.8E+0	1.8E+0	1.8343E+0	1.4754E+0	8.66404E+1	6.8541E+1	0E+0	1.8E+0	1.459380426E-2	1.4649E+0	-4.11E-2	1.6E+1	6E-2	6E-2
Filter:Type.__text__{String}=Repeat	0E+0	1.231165113E-3	1.56E-1	1.231165113E-3	3.371767975E-6	1.225425103E-6	-3.504E+0	1.223317359E-6	-7.639151743E-8	1.8342E+0	1.4762E+0	8.66046E+1	6.8541E+1	3.676542081E-3	1.8E+1	0E+0	1.8E+0	1.8E+0	1.8342E+0	1.4758E+0	8.66404E+1	6.8541E+1	0E+0	1.8E+0	6.922741421E-3	1.4649E+0	-4.11E-2	1.7E+1	5E-2	5.01E-2
Filter:Window{Double Float}=1.000000	0E+0	1.231198771E-3	1.56E-1	1.231198771E-3	3.338050296E-6	1.217522195E-6	-3.4788E+0	1.215941952E-6	-7.586477945E-8	1.8341E+0	1.4763E+0	8.66046E+1	6.8541E+1	3.235878889E-3	1.9E+1	0E+0	1.8E+0	1.8E+0	1.8342E+0	1.4762E+0	8.66046E+1	6.8541E+1	0E+0	1.8E+0	3.676542081E-3	1.4649E+0	-4.11E-2	1.8E+1	5E-2	5E-2
Iterator{I32}=0	0E+0	1.23103048E-3	1.56E-1	1.23103048E-3	3.371767975E-6	1.14481889E-6	-4.0584E+0	1.142184775E-6	-8.218682319E-8	1.8337E+0	1.4762E+0	8.65688E+1	6.8541E+1	1.755622216E-3	2E+1	0E+0	1.8E+0	1.8E+0	1.8341E+0	1.4763E+0	8.66046E+1	6.8541E+1	0E+0	1.8E+0	3.235878889E-3	1.4649E+0	-4.11E-2	1.9E+1	4.5E-2	4.49E-2
Magnet: Control Mode{Boolean}=False	0E+0	1.230693897E-3	1.56E-1	1.230693897E-3	3.371767975E-6	1.095822895E-6	-4.2852E+0	1.093189064E-6	-8.324049714E-8	1.8331E+0	1.4756E+0	8.65688E+1	6.8541E+1	1.182226697E-4	2.1E+1	0E+0	1.8E+0	1.8E+0	1.8337E+0	1.4762E+0	8.65688E+1	6.8541E+1	0E+0	1.8E+0	1.755622216E-3	1.4649E+0	-4.11E-2	2E+1	4E-2	4E-2
Magnet: Final Switch Heater{Enum U8 ((False,True,Mixed))}=	0E+0	1.230524191E-3	1.56E-1	1.230524191E-3	3.338050296E-6	1.019432169E-6	-4.344E+0	1.016797772E-6	-7.902571646E-8	1.8325E+0	1.4752E+0	8.65688E+1	6.8541E+1	-8.053010679E-4	2.2E+1	0E+0	1.8E+0	1.8E+0	1.8331E+0	1.4756E+0	8.65688E+1	6.8541E+1	0E+0	1.8E+0	1.182226697E-4	1.4649E+0	-4.11E-2	2.1E+1	3.5E-2	3.49E-2
Magnet: Power Supply{Enum U16 ((IPS120,LS625,PS110,Hg iPS,SMS Series,Cryomagnetics 4G,DMG Little CryoFree,DMG Big CryoFree))}=Hg iPS	0E+0	1.2303559E-3	1.56E-1	1.2303559E-3	3.371767975E-6	9.472558004E-7	-4.9872E+0	9.435678143E-7	-8.376734826E-8	1.8319E+0	1.4748E+0	8.6533E+1	6.8541E+1	-1.55692664E-3	2.3E+1	0E+0	1.8E+0	1.8E+0	1.8325E+0	1.4752E+0	8.65688E+1	6.8541E+1	0E+0	1.8E+0	-8.053010679E-4	1.4649E+0	-4.11E-2	2.2E+1	3E-2	2.99E-2
Magnet: Rate{Double Float}=0.500000	0E+0	1.230187608E-3	1.56E-1	1.230187608E-3	3.371767975E-6	8.792937878E-7	-4.8504E+0	8.761324548E-7	-7.586466631E-8	1.8313E+0	1.4743E+0	8.6533E+1	6.8541E+1	-2.347911242E-3	2.4E+1	0E+0	1.8E+0	1.8E+0	1.8319E+0	1.4748E+0	8.6533E+1	6.8541E+1	0E+0	1.8E+0	-1.55692664E-3	1.4649E+0	-4.11E-2	2.3E+1	2.5E-2	2.49E-2
Magnet: Setpoint{Double Float}=0.000000	0E+0	1.229849611E-3	1.56E-1	1.229849611E-3	3.371767975E-6	8.366201764E-7	-5.7156E+0	8.318786012E-7	-8.534790163E-8	1.8308E+0	1.474E+0	8.60673E+1	6.8541E+1	-2.555502113E-3	2.5E+1	0E+0	1.8E+0	1.8E+0	1.8313E+0	1.4743E+0	8.6533E+1	6.8541E+1	0E+0	1.8E+0	-2.347911242E-3	1.4649E+0	-4.11E-2	2.4E+1	2E-2	1.99E-2
Magnet: Units{Enum U16 ((Field,Current))}=Field	0E+0	1.229344737E-3	1.56E-1	1.229344737E-3	3.371767975E-6	7.3546742E-7	-6.2076E+0	7.323066527E-7	-8.113317751E-8	1.8305E+0	1.4739E+0	8.59599E+1	6.8541E+1	-2.196621383E-3	2.6E+1	0E+0	1.8E+0	1.8E+0	1.8308E+0	1.474E+0	8.60673E+1	6.8541E+1	0E+0	1.8E+0	-2.555502113E-3	1.4649E+0	-4.11E-2	2.5E+1	1.5E-2	1.49E-2
Magnet: VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	0E+0	1.228838449E-3	1.56E-1	1.228838449E-3	3.371767975E-6	6.785685172E-7	-6.8928E+0	6.73300006E-7	-8.324052543E-8	1.83E+0	1.4737E+0	8.60673E+1	6.8541E+1	-1.82667037E-3	2.7E+1	0E+0	1.8E+0	1.8E+0	1.8305E+0	1.4739E+0	8.59599E+1	6.8541E+1	0E+0	1.8E+0	-2.196621383E-3	1.4649E+0	-4.11E-2	2.6E+1	1E-2	1E-2
Main Screen Path{Path}=C:\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV\\\\1Code.vi	0E+0	1.228163869E-3	1.56E-1	1.228163869E-3	3.371767975E-6	6.253564692E-7	-7.7412E+0	6.195613048E-7	-8.587469618E-8	1.8295E+0	1.4734E+0	8.58166E+1	6.8541E+1	-1.698280801E-3	2.8E+1	0E+0	1.8E+0	1.8E+0	1.83E+0	1.4737E+0	8.60673E+1	6.8541E+1	0E+0	1.8E+0	-1.82667037E-3	1.4649E+0	-4.11E-2	2.7E+1	5E-3	4.9E-3
Measurement Timestamp{Timestamp}=<19:21:00.901 17/05/2023>T	0E+0	1.227354939E-3	1.56E-1	1.227354939E-3	3.270614936E-6	5.626629677E-7	-7.2E+0	5.579219582E-7	-7.164997048E-8	1.8291E+0	1.4733E+0	8.59241E+1	6.8541E+1	-1.3448135E-3	2.9E+1	0E+0	1.8E+0	1.8E+0	1.8295E+0	1.4734E+0	8.58166E+1	6.8541E+1	0E+0	1.8E+0	-1.698280801E-3	1.4649E+0	-4.11E-2	2.8E+1	0E+0	-1E-4
Measurement Title{String}=	0E+0	1.228333574E-3	1.56E-1	1.228333574E-3	3.338050296E-6	4.767893746E-7	-8.2404E+0	4.709933618E-7	-7.006944541E-8	1.8285E+0	1.4728E+0	8.59241E+1	6.8541E+1	-1.711372635E-3	3E+1	0E+0	1.8E+0	1.8E+0	1.8291E+0	1.4733E+0	8.59241E+1	6.8541E+1	0E+0	1.8E+0	-1.3448135E-3	1.4649E+0	-4.11E-2	2.9E+1	-5E-3	-5.2E-3
Measurment Select{U16}=4	0E+0	1.22900674E-3	1.56E-1	1.22900674E-3	3.371767975E-6	4.183099468E-7	-1.19316E+1	4.088270792E-7	-8.798212894E-8	1.8279E+0	1.4724E+0	8.6712E+1	6.8541E+1	-1.98463141E-3	3.1E+1	0E+0	1.8E+0	1.8E+0	1.8285E+0	1.4728E+0	8.59241E+1	6.8541E+1	0E+0	1.8E+0	-1.711372635E-3	1.4649E+0	-4.11E-2	3E+1	-1E-2	-1E-2
Measurment Select.__text__{String}=6221-Lockin-DAQ	0E+0	1.229513028E-3	1.56E-1	1.229513028E-3	3.371767975E-6	3.529823312E-7	-1.08756E+1	3.461332949E-7	-6.796209749E-8	1.8275E+0	1.4723E+0	8.6712E+1	6.8541E+1	-1.746846479E-3	3.2E+1	0E+0	1.8E+0	1.8E+0	1.8279E+0	1.4724E+0	8.6712E+1	6.8541E+1	0E+0	1.8E+0	-1.98463141E-3	1.4649E+0	-4.11E-2	3.1E+1	-1.5E-2	-1.51E-2
Notes{String}=I+1A I-1E\\nrxx+1B Rxx-1C\\nRxy+1D Rxy-4A	0E+0	1.229849611E-3	1.56E-1	1.229849611E-3	3.270614936E-6	2.83965598E-7	-1.41864E+1	2.744827304E-7	-7.059629653E-8	1.8267E+0	1.4715E+0	8.6712E+1	6.8541E+1	-2.486439655E-3	3.3E+1	0E+0	1.8E+0	1.8E+0	1.8275E+0	1.4723E+0	8.6712E+1	6.8541E+1	0E+0	1.8E+0	-1.746846479E-3	1.4649E+0	-4.11E-2	3.2E+1	-2E-2	-2E-2
Offset{Double Float}=0.000000	0E+0	1.230187608E-3	1.56E-1	1.230187608E-3	3.371767975E-6	2.165305214E-7	-1.84164E+1	2.054671287E-7	-6.954259428E-8	1.8265E+0	1.4718E+0	8.66762E+1	6.8541E+1	-1.583170029E-3	3.4E+1	0E+0	1.8E+0	1.8E+0	1.8267E+0	1.4715E+0	8.6712E+1	6.8541E+1	0E+0	1.8E+0	-2.486439655E-3	1.4649E+0	-4.11E-2	3.3E+1	-2.5E-2	-2.51E-2
Option: 2182 Autozero{Boolean}=True	0E+0	1.230456875E-3	1.56E-1	1.230456875E-3	3.371767975E-6	1.643734767E-7	-2.52588E+1	1.480413182E-7	-7.112320421E-8	1.8262E+0	1.4718E+0	8.66046E+1	6.8541E+1	-1.069137943E-3	3.5E+1	0E+0	1.8E+0	1.8E+0	1.8265E+0	1.4718E+0	8.66762E+1	6.8541E+1	0E+0	1.8E+0	-1.583170029E-3	1.4649E+0	-4.11E-2	3.4E+1	-3E-2	-3.01E-2
Option: 2182 Front Autozero{Boolean}=True	0E+0	1.230693897E-3	1.56E-1	1.230693897E-3	3.371767975E-6	1.058945862E-7	-4.58388E+1	7.270364444E-8	-7.849900677E-8	1.8261E+0	1.472E+0	8.66404E+1	6.8541E+1	-4.576801148E-4	3.6E+1	0E+0	1.8E+0	1.8E+0	1.8262E+0	1.4718E+0	8.66046E+1	6.8541E+1	0E+0	1.8E+0	-1.069137943E-3	1.4649E+0	-4.11E-2	3.5E+1	-3.5E-2	-3.54E-2
Option: 2182 Hold{Boolean}=False	0E+0	1.230862188E-3	1.56E-1	1.230862188E-3	3.304332616E-6	8.007941871E-8	-8.02776E+1	1.159045878E-8	-8.113312095E-8	1.8261E+0	1.4724E+0	8.66404E+1	6.8541E+1	4.128914734E-4	3.7E+1	0E+0	1.8E+0	1.8E+0	1.8261E+0	1.472E+0	8.66404E+1	6.8541E+1	0E+0	1.8E+0	-4.576801148E-4	1.4649E+0	-4.11E-2	3.6E+1	-4E-2	-4.04E-2
Option: 2182 Hold Count{I32}=10	0E+0	1.23103048E-3	1.56E-1	1.23103048E-3	3.304332616E-6	9.114315082E-8	-1.25508E+2	-5.426433605E-8	-7.533787176E-8	1.8259E+0	1.4725E+0	8.66046E+1	6.8541E+1	7.553011528E-4	3.8E+1	0E+0	1.8E+0	1.8E+0	1.8261E+0	1.4724E+0	8.66404E+1	6.8541E+1	0E+0	1.8E+0	4.128914734E-4	1.4649E+0	-4.11E-2	3.7E+1	-4.5E-2	-4.51E-2
Option: 2182 Hold Window{Double Float}=1.000000	0E+0	1.231198771E-3	1.56E-1	1.231198771E-3	3.371767975E-6	1.438266507E-7	-1.497432E+2	-1.274948599E-7	-7.428411295E-8	1.8254E+0	1.4719E+0	8.66046E+1	6.8541E+1	-5.060244803E-5	3.9E+1	0E+0	1.8E+0	1.8E+0	1.8259E+0	1.4725E+0	8.66046E+1	6.8541E+1	0E+0	1.8E+0	7.553011528E-4	1.4649E+0	-4.11E-2	3.8E+1	-5E-2	-5.02E-2
Option: 2182 Line Sync{Boolean}=False	0E+0	1.231198771E-3	1.56E-1	1.231198771E-3	3.338050296E-6	1.385584223E-7	-1.447068E+2	-1.153776235E-7	-8.218685147E-8	1.8251E+0	1.4718E+0	8.66046E+1	6.8541E+1	-1.292290108E-4	4E+1	0E+0	1.8E+0	1.8E+0	1.8254E+0	1.4719E+0	8.66046E+1	6.8541E+1	0E+0	1.8E+0	-5.060244803E-5	1.4649E+0	-4.11E-2	3.9E+1	-5E-2	-5E-2
Option: 2182 Reference Reading{Double Float}=0.000000	0E+0	1.231367062E-3	1.56E-1	1.231367062E-3	3.371767975E-6	2.565700186E-7	-1.621944E+2	-2.46560215E-7	-8.060635468E-8	1.8249E+0	1.472E+0	8.66046E+1	6.8541E+1	1.51853892E-4	4.1E+1	0E+0	1.8E+0	1.8E+0	1.8251E+0	1.4718E+0	8.66046E+1	6.8541E+1	0E+0	1.8E+0	-1.292290108E-4	1.4649E+0	-4.11E-2	4E+1	-6E-2	-5.99E-2
Option: 2182 Relative Mode{Boolean}=False	0E+0	1.23170506E-3	1.56E-1	1.23170506E-3	3.371767975E-6	3.898613439E-7	-1.682676E+2	-3.85646139E-7	-8.113309266E-8	1.8246E+0	1.4721E+0	8.65688E+1	6.8541E+1	9.594681615E-5	4.2E+1	0E+0	1.8E+0	1.8E+0	1.8249E+0	1.472E+0	8.66046E+1	6.8541E+1	0E+0	1.8E+0	1.51853892E-4	1.4649E+0	-4.11E-2	4.1E+1	-7E-2	-7E-2
Option: 2182 Trigger Delay{Cluster (Boolean,Double Float)}={'Auto':True,'Time(s)':0.000000}	0E+0	1.231873351E-3	1.56E-1	1.231873351E-3	3.338050296E-6	5.242037127E-7	-1.703892E+2	-5.194624203E-7	-8.903577462E-8	1.8244E+0	1.4717E+0	8.65688E+1	6.8541E+1	-6.285551353E-4	4.3E+1	0E+0	1.8E+0	1.8E+0	1.8246E+0	1.4721E+0	8.65688E+1	6.8541E+1	0E+0	1.8E+0	9.594681615E-5	1.4649E+0	-4.11E-2	4.2E+1	-8E-2	-7.99E-2
Option: 2182 Trigger Source{Enum U16 ((Immediate,Timer,Manual,Bus,Trigger link))}=Bus	0E+0	1.232007984E-3	1.56E-1	1.232007984E-3	3.371767975E-6	6.469571671E-7	-1.734852E+2	-6.453763592E-7	-7.481102064E-8	1.824E+0	1.4715E+0	8.66046E+1	6.8541E+1	-9.598302422E-4	4.4E+1	0E+0	1.8E+0	1.8E+0	1.8244E+0	1.4717E+0	8.65688E+1	6.8541E+1	0E+0	1.8E+0	-6.285551353E-4	1.4649E+0	-4.11E-2	4.3E+1	-9E-2	-8.99E-2
Option: 2182 Trigger Timer{Double Float}=0.000000	0E+0	1.232041642E-3	1.56E-1	1.232041642E-3	3.371767975E-6	7.918391039E-7	-1.734912E+2	-7.886783366E-7	-9.114309425E-8	1.8235E+0	1.4713E+0	8.66404E+1	6.8541E+1	-1.052975887E-3	4.5E+1	0E+0	1.8E+0	1.8E+0	1.824E+0	1.4715E+0	8.66046E+1	6.8541E+1	0E+0	1.8E+0	-9.598302422E-4	1.4649E+0	-4.11E-2	4.4E+1	-1E-1	-1E-1
Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	0E+0	1.232041642E-3	1.56E-1	1.232041642E-3	3.371767975E-6	7.807757112E-7	-1.743E+2	-7.797218393E-7	-7.955268072E-8	1.8233E+0	1.4714E+0	8.66046E+1	6.8541E+1	-7.514430326E-4	4.6E+1	0E+0	1.8E+0	1.8E+0	1.8235E+0	1.4713E+0	8.66404E+1	6.8541E+1	0E+0	1.8E+0	-1.052975887E-3	1.4649E+0	-4.11E-2	4.5E+1	-1E-1	-1E-1
Option: 560 Enabled{Boolean}=False	0E+0	1.233897091E-3	1.56E-1	1.233897091E-3	3.371767975E-6	3.410749358E-6	-1.7826E+2	-3.411278274E-6	-1.053677917E-7	1.8222E+0	1.4733E+0	8.59957E+1	6.8541E+1	2.362616127E-3	4.7E+1	0E+0	1.8E+0	1.8E+0	1.8233E+0	1.4714E+0	8.66046E+1	6.8541E+1	0E+0	1.8E+0	-7.514430326E-4	1.4649E+0	-4.11E-2	4.6E+1	-3E-1	-2.999E-1
Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	0E+0	1.235244836E-3	1.56E-1	1.235244836E-3	3.371767975E-6	6.0607593E-6	-1.790412E+2	-6.063395394E-6	-1.022067415E-7	1.8218E+0	1.4773E+0	8.67837E+1	6.8541E+1	6.144011393E-3	4.8E+1	0E+0	1.8E+0	1.8E+0	1.8222E+0	1.4733E+0	8.59957E+1	6.8541E+1	0E+0	1.8E+0	2.362616127E-3	1.4649E+0	-4.11E-2	4.7E+1	-5E-1	-4.999E-1
Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	0E+0	1.236593996E-3	1.56E-1	1.236593996E-3	3.371767975E-6	8.681237634E-6	-1.793124E+2	-8.6838709E-6	-1.048409405E-7	1.8207E+0	1.4817E+0	8.68195E+1	6.8541E+1	8.362475783E-3	4.9E+1	0E+0	1.8E+0	1.8E+0	1.8218E+0	1.4773E+0	8.67837E+1	6.8541E+1	0E+0	1.8E+0	6.144011393E-3	1.4649E+0	-4.11E-2	4.8E+1	-7E-1	-6.999E-1
Option: 6221 Adjust Mode{Enum U16 ((Offset,Frequency,Amplitude))}=Offset	0E+0	1.238279738E-3	1.56E-1	1.238279738E-3	3.371767975E-6	1.132809954E-5	-1.79424E+2	-1.133073563E-5	-1.159044747E-7	1.8206E+0	1.4879E+0	8.66762E+1	6.8541E+1	1.093959808E-2	5E+1	0E+0	1.8E+0	1.8E+0	1.8207E+0	1.4817E+0	8.68195E+1	6.8541E+1	0E+0	1.8E+0	8.362475783E-3	1.4649E+0	-4.11E-2	4.9E+1	-9E-1	-8.999E-1
Option: 6221 Amplitude{Double Float}=1.000000E-6	0E+0	1.240133772E-3	1.56E-1	1.240133772E-3	3.371767975E-6	1.396965531E-5	-1.794912E+2	-1.397228857E-5	-1.253874837E-7	1.8228E+0	1.4951E+0	8.6712E+1	6.8541E+1	1.358795632E-2	5.1E+1	0E+0	1.8E+0	1.8E+0	1.8206E+0	1.4879E+0	8.66762E+1	6.8541E+1	0E+0	1.8E+0	1.093959808E-2	1.4649E+0	-4.11E-2	5E+1	-1.1E+0	-1.1E+0
Option: 6221 Compliance{Double Float}=10.000000	0E+0	1.242494095E-3	1.56E-1	1.242494095E-3	3.371767975E-6	1.661123937E-5	-1.795968E+2	-1.661381324E-5	-1.185386454E-7	1.8228E+0	1.5001E+0	8.62106E+1	6.8541E+1	1.092994213E-2	5.2E+1	0E+0	1.8E+0	1.8E+0	1.8228E+0	1.4951E+0	8.6712E+1	6.8541E+1	0E+0	1.8E+0	1.358795632E-2	1.4649E+0	-4.11E-2	5.1E+1	-1.3E+0	-1.3E+0
Option: 6221 Duty Cycle{Double Float}=50.000000	0E+0	1.245022709E-3	1.548E-1	1.245022709E-3	3.338050296E-6	1.927120537E-5	-1.795968E+2	-1.927386409E-5	-1.380314298E-7	1.8127E+0	1.4916E+0	8.60673E+1	6.8541E+1	-1.029574685E-2	5.3E+1	0E+0	1.8E+0	1.8E+0	1.8228E+0	1.5001E+0	8.62106E+1	6.8541E+1	0E+0	1.8E+0	1.092994213E-2	1.4649E+0	-4.11E-2	5.2E+1	-1.5E+0	-1.4999E+0
Option: 6221 External Trigger{Boolean}=False	0E+0	1.245022709E-3	1.56E-1	1.245022709E-3	3.371767975E-6	1.928594148E-5	-1.796088E+2	-1.92886002E-5	-1.332901939E-7	1.8135E+0	1.4945E+0	8.60315E+1	6.8541E+1	-6.514012814E-3	5.4E+1	0E+0	1.8E+0	1.8E+0	1.8127E+0	1.4916E+0	8.60673E+1	6.8541E+1	0E+0	1.8E+0	-1.029574685E-2	1.4649E+0	-4.11E-2	5.3E+1	-1.5E+0	-1.5E+0
Option: 6221 External Trigger Ignore Multiple{Boolean}=False	0E+0	1.23912261E-3	1.56E-1	1.23912261E-3	3.371767975E-6	1.263728794E-5	-1.794852E+2	-1.263992121E-5	-1.14850829E-7	1.8127E+0	1.4974E+0	8.67837E+1	6.8541E+1	-1.565170824E-4	5.5E+1	0E+0	1.8E+0	1.8E+0	1.8135E+0	1.4945E+0	8.60315E+1	6.8541E+1	0E+0	1.8E+0	-6.514012814E-3	1.4649E+0	-4.11E-2	5.4E+1	-1E+0	-1.0001E+0
Option: 6221 Frequency{Double Float}=119.770000	0E+0	1.235244836E-3	1.512E-1	1.235244836E-3	3.236897256E-6	6.050223409E-6	-1.789248E+2	-6.051807328E-6	-1.14850829E-7	1.8009E+0	1.4945E+0	8.6712E+1	6.8541E+1	-1.184720546E-2	5.6E+1	0E+0	1.8E+0	1.8E+0	1.8127E+0	1.4974E+0	8.67837E+1	6.8541E+1	0E+0	1.8E+0	-1.565170824E-4	1.4649E+0	-4.11E-2	5.5E+1	-5E-1	-5.001E-1
Option: 6221 Function{U16}=1	
Option: 6221 Function.__text__{String}=Sine	
Option: 6221 Idle Level{Double Float}=0.000000	
Option: 6221 Input trigger Line{U8}=5	
Option: 6221 Offset{Double Float}=0.000000	
Option: 6221 Output Trigger Line{U8}=4	
Option: 6221 Pass Through{Boolean}=True	
Option: 6221 Phase Marker{Boolean}=True	
Option: 6221 Phase Marker Phase{Double Float}=0.000000	
Option: 6221 Range Level{Double Float}=2.000000E-12	
Option: 6221 Ranging{U16}=1	
Option: 6221 Ranging.__text__{String}=Best	
Option: 6221 Update Clock{Double Float}=0.000000	
Option: 6221 VISA{Visa Refnum (Void)}=GPIB0::13::INSTR	
Option: Confirm Config{Boolean}=False	
Option: Control Panel Ref{LVObjVI Refnum (Void)}=	
Option: DAQ Global Channel{Boolean}=False	
Option: DAQ Input Rate{Double Float}=10000.000000	
Option: DAQ Input Samples{I32}=200	
Option: DAQ Measurement Channels{1D Array (Cluster (UserDefinedRefnumTag Refnum (Void),\tkDAQmxPhysChanTagType Tag,\tkDAQmxScaleTagType Tag,Boolean,Double Float,String))}=[]	
Option: Differential{I32}=10106	
Option: Differential.__text__{String}=Differential	
Option: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values))}=Function Generator	
Option: Lockin Standoff Time{Double Float}=0.000000	
Option: Paranoid Save Data{Boolean}=True	
Option: Plot Autoback Path{Path}=C:\\\\TEMP\\\\XY Multiparam\\\\Backup.txt	
Option: SR830  Ref Phase{Double Float}=0.000000	
Option: SR830  Synch Filter{Boolean}=False	
Option: SR830  Time Constant{I16}=8	
Option: SR830  Time Constant.__text__{String}=100 ms	
Option: SR830 2x Line Filter{Boolean}=True	
Option: SR830 Adjust Gains{Boolean}=False	
Option: SR830 Auto Gain Lower.__text__{String}=2 nV/fA	
Option: SR830 Auto Gain Upper.__text__{String}=1 V/uA	
Option: SR830 Auto Offset 1{Boolean}=False	
Option: SR830 Auto Offset 2{Boolean}=False	
Option: SR830 Autophase{Boolean}=False	
Option: SR830 DC Coupling?{Boolean}=False	
Option: SR830 Display 1{U16}=0	
Option: SR830 Display 1.__text__{String}=X	
Option: SR830 Display 2{U16}=0	
Option: SR830 Display 2.__text__{String}=Y	
Option: SR830 Dynamic Reserve{I16}=1	
Option: SR830 Dynamic Reserve.__text__{String}=Normal	
Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Option: SR830 Filter Slope{I32}=1	
Option: SR830 Filter Slope.__text__{String}=12 dB/oct	
Option: SR830 Gain{I32}=-1	
Option: SR830 Gain.__text__{String}=Auto Gain	
Option: SR830 Ground Shield?{Boolean}=False	
Option: SR830 Harmonic{I32}=1	
Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A	
Option: SR830 Line Filter{Boolean}=True	
Option: SR830 No Reset{Boolean}=False	
Option: SR830 Offset 1{Double Float}=0.000000	
Option: SR830 Offset 2{Double Float}=0.000000	
Option: SR830 Output Channel 1{Boolean}=False	
Option: SR830 Output Channel 2{Boolean}=False	
Option: SR830 Ratio 1{U16}=0	
Option: SR830 Ratio 1.__text__{String}=None	
Option: SR830 Ratio 2{U16}=0	
Option: SR830 Ratio 2.__text__{String}=None	
Option: SR830 Ref Amplitude{Double Float}=0.100000	
Option: SR830 Ref Frequency{Double Float}=1013.000000	
Option: SR830 Ref Source{Boolean}=False	
Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta]	
Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Option: SR830 VISA{Visa Refnum (Void)}=	
Option: Sense Autorange{Boolean}=False	
Option: Sense Range Level{Double Float}=0.100000	
Option: Sense Rate{Double Float}=1.000000	
Option:560 Comport{Visa Refnum (Void)}=COM1	
Option:560 Filter High Pass{U16}=0	
Option:560 Filter High Pass.__text__{String}=0.03	
Option:560 Filter Lowpass{U16}=0	
Option:560 Filter Lowpass.__text__{String}=0.03	
Option:560 Filter Mode{U16}=0	
Option:560 Filter Mode.__text__{String}=6 dB high pass	
Option:560 Invert{Boolean}=False	
Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Option:570 Enabled{Boolean}=False	
Option:570 Filter High Pass{U16}=0	
Option:570 Filter High Pass.__text__{String}=0.03	
Option:570 Filter Lowpass{U16}=0	
Option:570 Filter Lowpass.__text__{String}=0.03	
Option:570 Filter Mode{U16}=0	
Option:570 Filter Mode.__text__{String}=6 dB high pass	
Option:570 Gain Mode{U16}=0	
Option:570 Gain Mode.__text__{String}=Low Noise	
Option:570 Input Offset{U16}=0	
Option:570 Input Offset On{Boolean}=False	
Option:570 Input Offset.__text__{String}=1pA	
Option:570 Sensitivity{U16}=0	
Option:570 Sensitivity.__text__{String}=1pA/V	
Option:Debug On{Boolean}=False	
Option:GPIB 2182{Visa Refnum (Void)}=	
Option:Parallel Config Voltage Measurers{Boolean}=True	
Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Option:SR830 Settle Time{Double Float}=5.000000	
Option:Sense Digits{I32}=8	
Output Names{1D Array (String)}=['Offset','Rxx::R','Rxx::Theta','Rxx::X','Rxx::Y','Rxy::R','Rxy::Theta','Rxy::X','Rxy::Y','temperature: T1','temperature: T2','temperature: T3','temperature: T4','temperature: dT/dt','iterator','multi[0]:iterator','multi[0]:y','multi[0]:temperature: setpoint','multi[0]:temperature: T1','multi[0]:temperature: T2','multi[0]:temperature: T3','multi[0]:temperature: T4','multi[0]:temperature: heater','multi[0]:temperature: gas','multi[0]:temperature: dT/dt','multi[0]:temperature: current temperature','multi[0]:temperature: error','multi[1]:iterator','multi[1]:y','multi[1]:Control:Magnet Output']	
Parameter Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Parameter Select{U16}=6	
Parameter Select.__text__{String}=Multi-Parameter	
Paths{U32}=0	
Plot: Column Renames{1D Array (Cluster (String,String))}=[]	
Plot: No dups{Boolean}=False	
Plot: StdDevs{Boolean}=False	
Plotting Class{String}=Parameter Plot	
Plotting Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	
Plotting Select{U16}=1	
Plotting Select.__text__{String}=Parameter Plot	
Project Code{String}=Topological_Insulators	
Ref: Temperature Window{LVObjVI Refnum (Void)}=	
Ref:Control Subpanel{LVObjUnknown Refnum (Void)}=	
Ref:Main Screen{LVObjVI Refnum (Void)}=	
Ref:Plotting Subpanel{LVObjUnknown Refnum (Void)}=	
Ref:Toolbar{LVObjUnknown Refnum (Void)}=	
Ref:XY Subpanel{LVObjUnknown Refnum (Void)}=	
Rxx::R{Double Float}=0.001235	
Rxx::Theta{Double Float}=0.151200	
Rxx::X{Double Float}=0.001235	
Rxx::Y{Double Float}=3.236897E-6	
Rxx:Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	
Rxx:Option: 560 Enabled{Boolean}=False	
Rxx:Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	
Rxx:Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	
Rxx:Option: Lockin Standoff Time{Double Float}=0.000000	
Rxx:Option: Lockin Type{Enum U16 ((SRS 830,EG&G 5302))}=SRS 830	
Rxx:Option: SR803 Full Scale Reading{Double Float}=0.000000	
Rxx:Option: SR830  Ref Phase{Double Float}=0.000000	
Rxx:Option: SR830  Synch Filter{Boolean}=False	
Rxx:Option: SR830  Time Constant{I16}=8	
Rxx:Option: SR830 2x Line Filter{Boolean}=False	
Rxx:Option: SR830 Adjust Gains{Boolean}=False	
Rxx:Option: SR830 Auto Gain Lower{I32}=0	
Rxx:Option: SR830 Auto Gain Upper{I32}=26	
Rxx:Option: SR830 Auto Offset 1{Boolean}=False	
Rxx:Option: SR830 Auto Offset 2{Boolean}=False	
Rxx:Option: SR830 Autophase{Boolean}=False	
Rxx:Option: SR830 DC Coupling?{Boolean}=False	
Rxx:Option: SR830 Display 1{U16}=0	
Rxx:Option: SR830 Display 2{U16}=0	
Rxx:Option: SR830 Dynamic Reserve{I16}=2	
Rxx:Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Rxx:Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Rxx:Option: SR830 Filter Slope{I32}=3	
Rxx:Option: SR830 Gain{I32}=18	
Rxx:Option: SR830 Ground Shield?{Boolean}=False	
Rxx:Option: SR830 Harmonic{I32}=1	
Rxx:Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A-B	
Rxx:Option: SR830 Line Filter{Boolean}=False	
Rxx:Option: SR830 No Reset{Boolean}=False	
Rxx:Option: SR830 Offset 1{Double Float}=0.000000	
Rxx:Option: SR830 Offset 2{Double Float}=0.000000	
Rxx:Option: SR830 Output Channel 1{Boolean}=False	
Rxx:Option: SR830 Output Channel 2{Boolean}=False	
Rxx:Option: SR830 Ratio 1{U16}=0	
Rxx:Option: SR830 Ratio 2{U16}=0	
Rxx:Option: SR830 Ref Amplitude{Double Float}=0.100000	
Rxx:Option: SR830 Ref Frequency{Double Float}=1013.000000	
Rxx:Option: SR830 Ref Source{Boolean}=False	
Rxx:Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta,X,Y]	
Rxx:Option: SR830 Time Constant value{Double Float}=0.000000	
Rxx:Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Rxx:Option: SR830 VISA{Visa Refnum (Void)}=GPIB0::5::INSTR	
Rxx:Option:560 Comport{Visa Refnum (Void)}=COM1	
Rxx:Option:560 Filter High Pass{U16}=0	
Rxx:Option:560 Filter Lowpass{U16}=0	
Rxx:Option:560 Filter Mode{U16}=0	
Rxx:Option:560 Invert{Boolean}=False	
Rxx:Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Rxx:Option:570 Enabled{Boolean}=False	
Rxx:Option:570 Filter High Pass{U16}=0	
Rxx:Option:570 Filter Lowpass{U16}=0	
Rxx:Option:570 Filter Mode{U16}=0	
Rxx:Option:570 Gain Mode{U16}=0	
Rxx:Option:570 Input Offset{U16}=0	
Rxx:Option:570 Input Offset On{Boolean}=False	
Rxx:Option:570 Sensitivity{U16}=0	
Rxx:Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Rxx:Option:SR830 Autogain Lower Threshold{Double Float}=0.100000	
Rxx:Option:SR830 Autogain Standoff{Double Float}=3.000000	
Rxx:Option:SR830 Autogain Upper Threshold{Double Float}=0.900000	
Rxx:Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Rxx:Option:SR830 Settle Time{Double Float}=0.000000	
Rxy::R{Double Float}=6.050223E-6	
Rxy::Theta{Double Float}=-178.924800	
Rxy::X{Double Float}=-6.051807E-6	
Rxy::Y{Double Float}=-1.148508E-7	
Rxy:Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	
Rxy:Option: 560 Enabled{Boolean}=False	
Rxy:Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	
Rxy:Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	
Rxy:Option: Lockin Standoff Time{Double Float}=0.000000	
Rxy:Option: Lockin Type{Enum U16 ((SRS 830,EG&G 5302))}=SRS 830	
Rxy:Option: SR803 Full Scale Reading{Double Float}=0.000000	
Rxy:Option: SR830  Ref Phase{Double Float}=0.000000	
Rxy:Option: SR830  Synch Filter{Boolean}=False	
Rxy:Option: SR830  Time Constant{I16}=8	
Rxy:Option: SR830 2x Line Filter{Boolean}=False	
Rxy:Option: SR830 Adjust Gains{Boolean}=False	
Rxy:Option: SR830 Auto Gain Lower{I32}=0	
Rxy:Option: SR830 Auto Gain Upper{I32}=26	
Rxy:Option: SR830 Auto Offset 1{Boolean}=False	
Rxy:Option: SR830 Auto Offset 2{Boolean}=False	
Rxy:Option: SR830 Autophase{Boolean}=False	
Rxy:Option: SR830 DC Coupling?{Boolean}=False	
Rxy:Option: SR830 Display 1{U16}=0	
Rxy:Option: SR830 Display 2{U16}=1	
Rxy:Option: SR830 Dynamic Reserve{I16}=2	
Rxy:Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Rxy:Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Rxy:Option: SR830 Filter Slope{I32}=3	
Rxy:Option: SR830 Gain{I32}=18	
Rxy:Option: SR830 Ground Shield?{Boolean}=False	
Rxy:Option: SR830 Harmonic{I32}=1	
Rxy:Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A-B	
Rxy:Option: SR830 Line Filter{Boolean}=False	
Rxy:Option: SR830 No Reset{Boolean}=False	
Rxy:Option: SR830 Offset 1{Double Float}=0.000000	
Rxy:Option: SR830 Offset 2{Double Float}=0.000000	
Rxy:Option: SR830 Output Channel 1{Boolean}=False	
Rxy:Option: SR830 Output Channel 2{Boolean}=False	
Rxy:Option: SR830 Ratio 1{U16}=0	
Rxy:Option: SR830 Ratio 2{U16}=0	
Rxy:Option: SR830 Ref Amplitude{Double Float}=0.100000	
Rxy:Option: SR830 Ref Frequency{Double Float}=1013.000000	
Rxy:Option: SR830 Ref Source{Boolean}=False	
Rxy:Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta,X,Y]	
Rxy:Option: SR830 Time Constant value{Double Float}=0.000000	
Rxy:Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Rxy:Option: SR830 VISA{Visa Refnum (Void)}=GPIB0::6::INSTR	
Rxy:Option:560 Comport{Visa Refnum (Void)}=COM1	
Rxy:Option:560 Filter High Pass{U16}=0	
Rxy:Option:560 Filter Lowpass{U16}=0	
Rxy:Option:560 Filter Mode{U16}=0	
Rxy:Option:560 Invert{Boolean}=False	
Rxy:Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Rxy:Option:570 Enabled{Boolean}=False	
Rxy:Option:570 Filter High Pass{U16}=0	
Rxy:Option:570 Filter Lowpass{U16}=0	
Rxy:Option:570 Filter Mode{U16}=0	
Rxy:Option:570 Gain Mode{U16}=0	
Rxy:Option:570 Input Offset{U16}=0	
Rxy:Option:570 Input Offset On{Boolean}=False	
Rxy:Option:570 Sensitivity{U16}=0	
Rxy:Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Rxy:Option:SR830 Autogain Lower Threshold{Double Float}=0.100000	
Rxy:Option:SR830 Autogain Standoff{Double Float}=3.000000	
Rxy:Option:SR830 Autogain Upper Threshold{Double Float}=0.900000	
Rxy:Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Rxy:Option:SR830 Settle Time{Double Float}=0.000000	
Sample ID{String}=MBE202221213_PA_D1 750C Cracker WAL	
Save:Filename{String}=${X-Y Class} ${2nd Parameter Class} ${iterator}{%04d} ${y}{%04.2g}.txt	
Save:Final Filename{String}=${X-Y Class} ${2nd Parameter Class} .txt	
Save:Final path{Path}=C:\\\\Data\\\\${Project Code}\\\\${User}\\\\${Sample ID}\\\\${Measurement Timestamp}{%Y%m%d}\\\\${X-Y Class}	
Save:Path{Path}=C:\\\\Data\\\\${Project Code}\\\\${User}\\\\${Sample ID}\\\\${Measurement Timestamp}{%Y%m%d}\\\\${X-Y Class}	
Startup path{Path}=C:\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV	
Sub Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Sweep Step{I32}=3	
T Control Measure.__text__{1D Array (String)}=['temperature: T1','temperature: T2','temperature: T3','temperature: T4','temperature: dT/dt']	
Timestamp{Timestamp}=<19:22:09.342 17/05/2023>T	
Toolbar{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Unaved Data{Boolean}=True	
Unsaved Data{Boolean}=False	
User{String}=Craig	
X-Y Class{String}=6221-Lockin-DAQ	
X-Y Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	
d(Offset){Double Float}=0.000000	
d(Rxx::R){Double Float}=0.000000	
d(Rxx::Theta){Double Float}=0.002683	
d(Rxx::X){Double Float}=0.000000	
d(Rxx::Y){Double Float}=7.539502E-8	
d(Rxy::R){Double Float}=6.820466E-9	
d(Rxy::Theta){Double Float}=0.087299	
d(Rxy::X){Double Float}=6.612205E-9	
d(Rxy::Y){Double Float}=9.048714E-9	
iterate result{U16}=5	
iterator{I32}=56	
multi[0]:Control: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values,Adaptive Step Ramp))}=List of Values	
multi[0]:Control: Monitor Update Timeout{Double Float}=0.010000	
multi[0]:Control: Open T Window{Boolean}=False	
multi[0]:Control: Reverse Temperature Sense{Boolean}=False	
multi[0]:Iterator{I32}=0	
multi[0]:Ref: Temperature Window{LVObjVI Refnum (Void)}=	
multi[0]:iterate result{U16}=0	
multi[0]:iterator{I32}=0	
multi[0]:temperature:  rate window{Double Float}=120.000000	
multi[0]:temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[0]:temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
multi[0]:temperature: T1{Double Float}=1.795100	
multi[0]:temperature: T2{Double Float}=1.485200	
multi[0]:temperature: T3{Double Float}=85.709200	
multi[0]:temperature: T4{Double Float}=68.541000	
multi[0]:temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
multi[0]:temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
multi[0]:temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
multi[0]:temperature: current temperature{Double Float}=1.464900	
multi[0]:temperature: current temperature 2{Double Float}=287.100000	
multi[0]:temperature: dT/dt{Double Float}=-0.009348	
multi[0]:temperature: error{Double Float}=-0.041100	
multi[0]:temperature: gas{Double Float}=1.800000	
multi[0]:temperature: gas control{Boolean}=False	
multi[0]:temperature: gas control 2{Boolean}=False	
multi[0]:temperature: gass boost{I8}=0	
multi[0]:temperature: gass boost 2{I8}=0	
multi[0]:temperature: gast flow{I16}=0	
multi[0]:temperature: gast flow 2{I16}=7	
multi[0]:temperature: heater{Double Float}=0.000000	
multi[0]:temperature: heater output{Double Float}=0.000000	
multi[0]:temperature: heater output 2{Double Float}=0.000000	
multi[0]:temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
multi[0]:temperature: monitor timeout{Double Float}=0.010000	
multi[0]:temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
multi[0]:temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
multi[0]:temperature: ramp rate{Double Float}=8.000000	
multi[0]:temperature: ramp rate 2{Double Float}=0.000000	
multi[0]:temperature: ramp target{Double Float}=20.000000	
multi[0]:temperature: ramp target 2{Double Float}=0.000000	
multi[0]:temperature: ramping{Boolean}=False	
multi[0]:temperature: setpoint{Double Float}=1.800000	
multi[0]:temperature: setpoint 2{Double Float}=287.100000	
multi[0]:temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
multi[0]:temperature: stability error{Extended Float}=0.040000	
multi[0]:temperature: stability script{String}=	
multi[0]:temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
multi[0]:temperature: temp control mode{U16}=2	
multi[0]:temperature: temp control mode 2{U16}=3	
multi[0]:temperature: temp control mode 2.__text__{String}=Open Loop	
multi[0]:temperature: temp control mode.__text__{String}=Zone	
multi[0]:temperature: temp control sensor{U16}=0	
multi[0]:temperature: temp control sensor 2{U16}=0	
multi[0]:temperature: temp control sensor 2.__text__{String}=Sensor 1	
multi[0]:temperature: temp control sensor.__text__{String}=Sensor A	
multi[0]:temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
multi[0]:temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
multi[0]:temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
multi[0]:temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
multi[0]:temperature: temp loop{U16}=0	
multi[0]:temperature: temp loop 2{U16}=0	
multi[0]:temperature: temp loop 2.__text__{String}=Heater	
multi[0]:temperature: temp loop.__text__{String}=Loop 1	
multi[0]:temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
multi[0]:temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[0]:temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[0]:temperature:error for gas boost{Double Float}=0.000000	
multi[0]:temperature:error for gas boost 2{Double Float}=0.000000	
multi[0]:temperature:heater range{U16}=2	
multi[0]:temperature:heater range 2{U16}=0	
multi[0]:temperature:heater range 2.__text__{String}=Off	
multi[0]:temperature:heater range.__text__{String}=40mW	
multi[0]:temperature:history window{Extended Float}=300.000000	
multi[0]:temperature:is stable?{Boolean}=True	
multi[0]:temperature:monitor{Boolean}=True	
multi[0]:temperature:ramping{Boolean}=False	
multi[0]:temperature:ramping on{Boolean}=False	
multi[0]:temperature:ramping on 2{Boolean}=False	
multi[0]:temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
multi[0]:temperature:stability code{U32}=6618880	
multi[0]:temperature:stability rate{Extended Float}=0.040000	
multi[0]:y{Double Float}=1.800000	
multi[1]:Control: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values,Adaptive Step Ramp))}=Multi-Segment Ramp	
multi[1]:Control: Gate delay{Double Float}=0.000000	
multi[1]:Control: Monitor Update Timeout{Double Float}=0.010000	
multi[1]:Control: Open T Window{Boolean}=False	
multi[1]:Control: Reverse Temperature Sense{Boolean}=False	
multi[1]:Control:Magnet Output{Double Float}=-0.000100	
multi[1]:Iterator{I32}=0	
multi[1]:Magnet: Final Switch Heater{Enum U8 ((False,True,Mixed))}=	
multi[1]:Magnet: Power Supply{Enum U16 ((IPS120,LS625,PS110,Hg iPS,SMS Series,Cryomagnetics 4G,DMG Little CryoFree,DMG Big CryoFree))}=Hg iPS	
multi[1]:Magnet: Rate{Double Float}=0.500000	
multi[1]:Magnet: Units{Enum U16 ((Field,Current))}=Field	
multi[1]:Magnet: VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[1]:Multi-segment_Stage{I32}=0	
multi[1]:Multi-segment_Stage_Changed{Boolean}=False	
multi[1]:Ref: Temperature Window{LVObjVI Refnum (Void)}=	
multi[1]:iterate result{U16}=4	
multi[1]:iterator{I32}=57	
multi[1]:measure point{Boolean}=False	
multi[1]:temperature:  rate window{Double Float}=120.000000	
multi[1]:temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[1]:temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
multi[1]:temperature: T1{Double Float}=1.842400	
multi[1]:temperature: T2{Double Float}=1.465600	
multi[1]:temperature: T3{Double Float}=86.318100	
multi[1]:temperature: T4{Double Float}=66.769200	
multi[1]:temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
multi[1]:temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
multi[1]:temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
multi[1]:temperature: current temperature{Double Float}=1.465600	
multi[1]:temperature: current temperature 2{Double Float}=287.100000	
multi[1]:temperature: dT/dt{Double Float}=-0.001864	
multi[1]:temperature: gas control{Boolean}=False	
multi[1]:temperature: gas control 2{Boolean}=False	
multi[1]:temperature: gass boost{I8}=0	
multi[1]:temperature: gass boost 2{I8}=0	
multi[1]:temperature: gast flow{I16}=0	
multi[1]:temperature: gast flow 2{I16}=7	
multi[1]:temperature: heater output{Double Float}=0.000000	
multi[1]:temperature: heater output 2{Double Float}=0.000000	
multi[1]:temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
multi[1]:temperature: monitor timeout{Double Float}=1.000000	
multi[1]:temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
multi[1]:temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
multi[1]:temperature: ramp rate{Double Float}=8.000000	
multi[1]:temperature: ramp rate 2{Double Float}=0.000000	
multi[1]:temperature: ramp target{Double Float}=20.000000	
multi[1]:temperature: ramp target 2{Double Float}=0.000000	
multi[1]:temperature: ramping{Boolean}=False	
multi[1]:temperature: setpoint{Double Float}=1.800000	
multi[1]:temperature: setpoint 2{Double Float}=287.100000	
multi[1]:temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
multi[1]:temperature: stability error{Extended Float}=0.040000	
multi[1]:temperature: stability script{String}=	
multi[1]:temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
multi[1]:temperature: temp control mode{U16}=2	
multi[1]:temperature: temp control mode 2{U16}=3	
multi[1]:temperature: temp control mode 2.__text__{String}=Open Loop	
multi[1]:temperature: temp control mode.__text__{String}=Zone	
multi[1]:temperature: temp control sensor{U16}=0	
multi[1]:temperature: temp control sensor 2{U16}=0	
multi[1]:temperature: temp control sensor 2.__text__{String}=Sensor 1	
multi[1]:temperature: temp control sensor.__text__{String}=Sensor A	
multi[1]:temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
multi[1]:temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
multi[1]:temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
multi[1]:temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
multi[1]:temperature: temp loop{U16}=0	
multi[1]:temperature: temp loop 2{U16}=0	
multi[1]:temperature: temp loop 2.__text__{String}=Heater	
multi[1]:temperature: temp loop.__text__{String}=Loop 1	
multi[1]:temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
multi[1]:temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[1]:temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[1]:temperature:error for gas boost{Double Float}=0.000000	
multi[1]:temperature:error for gas boost 2{Double Float}=0.000000	
multi[1]:temperature:heater range{U16}=2	
multi[1]:temperature:heater range 2{U16}=0	
multi[1]:temperature:heater range 2.__text__{String}=Off	
multi[1]:temperature:heater range.__text__{String}=40mW	
multi[1]:temperature:history window{Extended Float}=300.000000	
multi[1]:temperature:is stable?{Boolean}=True	
multi[1]:temperature:monitor{Boolean}=True	
multi[1]:temperature:ramping{Boolean}=False	
multi[1]:temperature:ramping on{Boolean}=False	
multi[1]:temperature:ramping on 2{Boolean}=False	
multi[1]:temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
multi[1]:temperature:stability code{U32}=6618880	
multi[1]:temperature:stability rate{Extended Float}=0.040000	
multi[1]:y{Double Float}=0.000000	
parameter: Termination{String}=False	
parameter: delta time{Double Float}=1.000000	
parameter: progress{Double Float}=100.000000	
temperature:  rate window{Double Float}=120.000000	
temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
temperature: T1{Double Float}=1.795100	
temperature: T2{Double Float}=1.485200	
temperature: T3{Double Float}=85.709200	
temperature: T4{Double Float}=68.541000	
temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
temperature: current temperature{Double Float}=1.464900	
temperature: current temperature 2{Double Float}=287.100000	
temperature: dT/dt{Double Float}=-0.009348	
temperature: gas control{Boolean}=False	
temperature: gas control 2{Boolean}=False	
temperature: gass boost{I8}=0	
temperature: gass boost 2{I8}=0	
temperature: gast flow{I16}=0	
temperature: gast flow 2{I16}=7	
temperature: heater output{Double Float}=0.000000	
temperature: heater output 2{Double Float}=0.000000	
temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
temperature: monitor timeout{Double Float}=0.010000	
temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
temperature: ramp rate{Double Float}=8.000000	
temperature: ramp rate 2{Double Float}=0.000000	
temperature: ramp target{Double Float}=20.000000	
temperature: ramp target 2{Double Float}=0.000000	
temperature: ramping{Boolean}=False	
temperature: setpoint{Double Float}=1.800000	
temperature: setpoint 2{Double Float}=287.100000	
temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
temperature: stability error{Extended Float}=0.040000	
temperature: stability script{String}=	
temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
temperature: temp control mode{U16}=2	
temperature: temp control mode 2{U16}=3	
temperature: temp control mode 2.__text__{String}=Open Loop	
temperature: temp control mode.__text__{String}=Zone	
temperature: temp control sensor{U16}=0	
temperature: temp control sensor 2{U16}=0	
temperature: temp control sensor 2.__text__{String}=Sensor 1	
temperature: temp control sensor.__text__{String}=Sensor A	
temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
temperature: temp loop{U16}=0	
temperature: temp loop 2{U16}=0	
temperature: temp loop 2.__text__{String}=Heater	
temperature: temp loop.__text__{String}=Loop 1	
temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
temperature:error for gas boost{Double Float}=0.000000	
temperature:error for gas boost 2{Double Float}=0.000000	
temperature:heater range{U16}=2	
temperature:heater range 2{U16}=0	
temperature:heater range 2.__text__{String}=Off	
temperature:heater range.__text__{String}=40mW	
temperature:history window{Extended Float}=300.000000	
temperature:is stable?{Boolean}=True	
temperature:monitor{Boolean}=True	
temperature:ramping{Boolean}=False	
temperature:ramping on{Boolean}=False	
temperature:ramping on 2{Boolean}=False	
temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
temperature:stability code{U32}=6618880	
temperature:stability rate{Extended Float}=0.040000	
y{Double Float}=1.800000	
