TDI Format 1.5	Offset	Rxx::R	Rxx::Theta	Rxx::X	Rxx::Y	Rxy::R	Rxy::Theta	Rxy::X	Rxy::Y	temperature: T1	temperature: T2	temperature: T3	temperature: T4	temperature: dT/dt	iterator	multi[0]:iterator	multi[0]:y	multi[0]:temperature: setpoint	multi[0]:temperature: T1	multi[0]:temperature: T2	multi[0]:temperature: T3	multi[0]:temperature: T4	multi[0]:temperature: heater	multi[0]:temperature: gas	multi[0]:temperature: dT/dt	multi[0]:temperature: current temperature	multi[0]:temperature: error	multi[1]:iterator	multi[1]:y	multi[1]:Control:Magnet Output
2nd Parameter Class{String}=Multi-Parameter	0E+0	1.235751125E-3	1.56E-1	1.235751125E-3	3.371767975E-6	5.826828578E-7	-7.5528E+0	5.784676528E-7	-7.797209908E-8	1.6233E+1	1.6048E+1	8.57092E+1	6.2996E+1	-6.184649467E-2	5.61E+2	1E+1	1.6E+1	1.6E+1	1.6234E+1	1.6049E+1	8.5745E+1	6.2996E+1	4.4E+0	1.6E+1	-6.473425776E-2	1.6234E+1	-2.34E-1	0E+0	0E+0	-0E+0
2nd Parameter Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	0E+0	1.238380713E-3	1.56E-1	1.238380713E-3	3.371767975E-6	7.106524974E-6	-5.82E-1	7.106524974E-6	-7.323052384E-8	1.6182E+1	1.6012E+1	8.61032E+1	6.2996E+1	-3.996637464E-2	5.62E+2	1E+1	1.6E+1	1.8E+0	1.6233E+1	1.6048E+1	8.57092E+1	6.2996E+1	4.4E+0	1.6E+1	-6.184649467E-2	1.4649E+0	-2.34E-1	1E+0	5E-1	4.999E-1
Analysis Class{String}=Basic Plot	0E+0	1.242325803E-3	1.56E-1	1.242325803E-3	3.371767975E-6	1.364722876E-5	-2.388E-1	1.364722876E-5	-5.795220904E-8	1.6152E+1	1.5985E+1	8.59957E+1	6.2996E+1	-2.993991598E-2	5.63E+2	1E+1	1.6E+1	1.8E+0	1.6182E+1	1.6012E+1	8.61032E+1	6.2996E+1	4.4E+0	1.6E+1	-3.996637464E-2	1.4649E+0	-2.34E-1	2E+0	1E+0	9.999E-1
Analysis Class Path{Path}=C\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV\\\\plugins\\\\Plotting\\\\Plotting_Base_class\\\\Plotting_Base.lvclass	0E+0	1.248057611E-3	1.56E-1	1.248057611E-3	3.371767975E-6	2.018371253E-5	-1.176E-1	2.018371253E-5	-4.267392253E-8	1.6163E+1	1.5988E+1	8.57092E+1	6.2996E+1	-6.003120216E-4	5.64E+2	1E+1	1.6E+1	1.8E+0	1.6152E+1	1.5985E+1	8.59957E+1	6.2996E+1	4.4E+0	1.6E+1	-2.993991598E-2	1.4649E+0	-2.34E-1	3E+0	1.5E+0	1.4999E+0
Analysis.# pre-routines{I32}=5	0E+0	1.248057611E-3	1.56E-1	1.248057611E-3	3.371767975E-6	2.018263773E-5	-1.356E-1	2.018263773E-5	-4.899599455E-8	1.6155E+1	1.5987E+1	8.57092E+1	6.2996E+1	-2.989652101E-3	5.65E+2	1E+1	1.6E+1	1.8E+0	1.6163E+1	1.5988E+1	8.57092E+1	6.2996E+1	4.4E+0	1.6E+1	-6.003120216E-4	1.4649E+0	-2.34E-1	4E+0	1.5E+0	1.4999E+0
Analysis:Pre[0]:T Control Measure{1D Array (I32)}=[1,2,3,4,7]	0E+0	1.245528997E-3	1.56E-1	1.245528997E-3	3.371767975E-6	1.755106913E-5	-1.596E-1	1.755106913E-5	-5.057649135E-8	1.6145E+1	1.5983E+1	8.58166E+1	6.2996E+1	-6.172624882E-3	5.66E+2	1E+1	1.6E+1	1.8E+0	1.6155E+1	1.5987E+1	8.57092E+1	6.2996E+1	4.4E+0	1.6E+1	-2.989652101E-3	1.4649E+0	-2.34E-1	5E+0	1.3E+0	1.3001E+0
Autosave Tabs{Enum U32 ((XY Measurement Save,Parameter Plot Save 2))}=Parameter Plot Save 2	0E+0	1.243336966E-3	1.56E-1	1.243336966E-3	3.371767975E-6	1.494009148E-5	-1.764E-1	1.494009148E-5	-4.688864664E-8	1.6194E+1	1.6003E+1	8.60673E+1	6.2996E+1	2.134473063E-2	5.67E+2	1E+1	1.6E+1	1.8E+0	1.6145E+1	1.5983E+1	8.58166E+1	6.2996E+1	4.4E+0	1.6E+1	-6.172624882E-3	1.4649E+0	-2.34E-1	6E+0	1.1E+0	1.1001E+0
Control:Magnet Output{Double Float}=-0.007000	0E+0	1.241348299E-3	1.56E-1	1.241348299E-3	3.371767975E-6	1.232434511E-5	-2.316E-1	1.232434511E-5	-5.163019359E-8	1.6162E+1	1.6015E+1	8.59957E+1	6.2996E+1	2.741054446E-2	5.68E+2	1E+1	1.6E+1	1.8E+0	1.6194E+1	1.6003E+1	8.60673E+1	6.2996E+1	4.4E+0	1.6E+1	2.134473063E-2	1.4649E+0	-2.34E-1	7E+0	9E-1	9.001E-1
Control:Magnet Rate{Double Float}=0.500000	0E+0	1.23979719E-3	1.56E-1	1.23979719E-3	3.371767975E-6	9.717522421E-6	-3.24E-1	9.717522421E-6	-5.584486113E-8	1.6188E+1	1.6016E+1	8.60315E+1	6.2996E+1	3.607751802E-3	5.69E+2	1E+1	1.6E+1	1.8E+0	1.6162E+1	1.6015E+1	8.59957E+1	6.2996E+1	4.4E+0	1.6E+1	2.741054446E-2	1.4649E+0	-2.34E-1	8E+0	7E-1	7.001E-1
Display Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	0E+0	1.238380713E-3	1.548E-1	1.238380713E-3	3.338050296E-6	7.100732356E-6	-5.484E-1	7.100732356E-6	-6.901577145E-8	1.6164E+1	1.6001E+1	8.59957E+1	6.2996E+1	-5.365939345E-3	5.7E+2	1E+1	1.6E+1	1.8E+0	1.6188E+1	1.6016E+1	8.60315E+1	6.2996E+1	4.4E+0	1.6E+1	3.607751802E-3	1.4649E+0	-2.34E-1	9E+0	5E-1	5.001E-1
Elapsed Time{Double Float}=12790.950867	0E+0	1.23709887E-3	1.56E-1	1.23709887E-3	3.371767975E-6	4.4955049E-6	-9.6E-1	4.4955049E-6	-7.69184534E-8	1.612E+1	1.5974E+1	8.58166E+1	6.2996E+1	-3.648713231E-2	5.71E+2	1E+1	1.6E+1	1.8E+0	1.6164E+1	1.6001E+1	8.59957E+1	6.2996E+1	4.4E+0	1.6E+1	-5.365939345E-3	1.4649E+0	-2.34E-1	1E+1	3E-1	3.001E-1
File:Autodel{Boolean}=True	0E+0	1.236087707E-3	1.56E-1	1.236087707E-3	3.371767975E-6	1.876070256E-6	-2.2308E+0	1.873963078E-6	-7.42841978E-8	1.6102E+1	1.5965E+1	8.61748E+1	6.2996E+1	-2.70487871E-2	5.72E+2	1E+1	1.6E+1	1.8E+0	1.612E+1	1.5974E+1	8.58166E+1	6.2996E+1	4.4E+0	1.6E+1	-3.648713231E-2	1.4649E+0	-2.34E-1	1.1E+1	1E-1	1.001E-1
File:Autosave{Boolean}=False	0E+0	1.236087707E-3	1.56E-1	1.236087707E-3	3.371767975E-6	1.875546997E-6	-2.532E+0	1.872910903E-6	-8.482107879E-8	1.6108E+1	1.5964E+1	8.61748E+1	6.2996E+1	-2.511959709E-2	5.73E+2	1E+1	1.6E+1	1.8E+0	1.6102E+1	1.5965E+1	8.61748E+1	6.2996E+1	4.4E+0	1.6E+1	-2.70487871E-2	1.4649E+0	-2.34E-1	1.2E+1	1E-1	1E-1
File:Export Config{Boolean}=True	0E+0	1.236087707E-3	1.56E-1	1.236087707E-3	3.371767975E-6	1.74225454E-6	-2.214E+0	1.740150191E-6	-6.796212578E-8	1.6124E+1	1.5972E+1	8.62106E+1	6.2996E+1	-6.653571036E-3	5.74E+2	1E+1	1.6E+1	1.8E+0	1.6108E+1	1.5964E+1	8.61748E+1	6.2996E+1	4.4E+0	1.6E+1	-2.511959709E-2	1.4649E+0	-2.34E-1	1.3E+1	9E-2	9E-2
File:Final Autosave{Boolean}=True	0E+0	1.235919416E-3	1.56E-1	1.235919416E-3	3.371767975E-6	1.618448628E-6	-2.8872E+0	1.616867537E-6	-8.271364602E-8	1.6088E+1	1.5957E+1	8.6139E+1	6.2996E+1	-2.78380271E-2	5.75E+2	1E+1	1.6E+1	1.8E+0	1.6124E+1	1.5972E+1	8.62106E+1	6.2996E+1	4.4E+0	1.6E+1	-6.653571036E-3	1.4649E+0	-2.34E-1	1.4E+1	8E-2	8E-2
Filter:Enable{Enum U16 ((None,Analog,Digital,Analog&Digitial))}=None	0E+0	1.235919416E-3	1.56E-1	1.235919416E-3	3.371767975E-6	1.490954447E-6	-2.664E+0	1.488321181E-6	-7.059626824E-8	1.6088E+1	1.5946E+1	8.61032E+1	6.2996E+1	-4.316871241E-2	5.76E+2	1E+1	1.6E+1	1.8E+0	1.6088E+1	1.5957E+1	8.6139E+1	6.2996E+1	4.4E+0	1.6E+1	-2.78380271E-2	1.4649E+0	-2.34E-1	1.5E+1	7E-2	7E-2
Filter:Points{I32}=1	0E+0	1.235919416E-3	1.56E-1	1.235919416E-3	3.371767975E-6	1.353448765E-6	-3.51E+0	1.350814934E-6	-8.482105051E-8	1.6117E+1	1.5957E+1	8.61032E+1	6.2996E+1	-2.077061869E-2	5.77E+2	1E+1	1.6E+1	1.8E+0	1.6088E+1	1.5946E+1	8.61032E+1	6.2996E+1	4.4E+0	1.6E+1	-4.316871241E-2	1.4649E+0	-2.34E-1	1.6E+1	6E-2	6E-2
Filter:Type{U16}=1	0E+0	1.235885758E-3	1.56E-1	1.235885758E-3	3.371767975E-6	1.223317642E-6	-4.1064E+0	1.219629373E-6	-8.850889521E-8	1.6156E+1	1.5975E+1	8.60673E+1	6.2996E+1	1.775171049E-2	5.78E+2	1E+1	1.6E+1	1.8E+0	1.6117E+1	1.5957E+1	8.61032E+1	6.2996E+1	4.4E+0	1.6E+1	-2.077061869E-2	1.4649E+0	-2.34E-1	1.7E+1	5E-2	5E-2
Filter:Type.__text__{String}=Repeat	0E+0	1.235919416E-3	1.56E-1	1.235919416E-3	3.371767975E-6	1.217522195E-6	-4.368E+0	1.21488808E-6	-9.430417269E-8	1.6153E+1	1.5979E+1	8.60673E+1	6.2996E+1	2.567700483E-2	5.79E+2	1E+1	1.6E+1	1.8E+0	1.6156E+1	1.5975E+1	8.60673E+1	6.2996E+1	4.4E+0	1.6E+1	1.775171049E-2	1.4649E+0	-2.34E-1	1.8E+1	5E-2	5.01E-2
Filter:Window{Double Float}=1.000000	0E+0	1.235919416E-3	1.56E-1	1.235919416E-3	3.371767975E-6	1.159570551E-6	-3.9996E+0	1.157990026E-6	-8.271361774E-8	1.6132E+1	1.5977E+1	8.60673E+1	6.2996E+1	2.44450476E-2	5.8E+2	1E+1	1.6E+1	1.8E+0	1.6153E+1	1.5979E+1	8.60673E+1	6.2996E+1	4.4E+0	1.6E+1	2.567700483E-2	1.4649E+0	-2.34E-1	1.9E+1	4.5E-2	4.49E-2
Iterator{I32}=0	0E+0	1.235751125E-3	1.56E-1	1.235751125E-3	3.371767975E-6	1.087920835E-6	-4.2648E+0	1.085286438E-6	-8.21867949E-8	1.6107E+1	1.597E+1	8.60315E+1	6.2996E+1	1.617190614E-2	5.81E+2	1E+1	1.6E+1	1.8E+0	1.6132E+1	1.5977E+1	8.60673E+1	6.2996E+1	4.4E+0	1.6E+1	2.44450476E-2	1.4649E+0	-2.34E-1	2E+1	4E-2	4E-2
Magnet: Control Mode{Boolean}=False	0E+0	1.235751125E-3	1.56E-1	1.235751125E-3	3.371767975E-6	1.009422366E-6	-4.6308E+0	1.006261316E-6	-8.271364602E-8	1.6114E+1	1.5964E+1	8.60315E+1	6.2996E+1	5.609450396E-3	5.82E+2	1E+1	1.6E+1	1.8E+0	1.6107E+1	1.597E+1	8.60315E+1	6.2996E+1	4.4E+0	1.6E+1	1.617190614E-2	1.4649E+0	-2.34E-1	2.1E+1	3.5E-2	3.49E-2
Magnet: Final Switch Heater{Enum U8 ((False,True,Mixed))}=	0E+0	1.235751125E-3	1.56E-1	1.235751125E-3	3.371767975E-6	9.620066136E-7	-5.2512E+0	9.577922572E-7	-8.956256917E-8	1.6116E+1	1.5963E+1	8.60315E+1	6.2996E+1	-4.516903311E-3	5.83E+2	1E+1	1.6E+1	1.8E+0	1.6114E+1	1.5964E+1	8.60315E+1	6.2996E+1	4.4E+0	1.6E+1	5.609450396E-3	1.4649E+0	-2.34E-1	2.2E+1	3E-2	3E-2
Magnet: Power Supply{Enum U16 ((IPS120,LS625,PS110,Hg iPS,SMS Series,Cryomagnetics 4G,DMG Little CryoFree,DMG Big CryoFree))}=Hg iPS	0E+0	1.235751125E-3	1.56E-1	1.235751125E-3	3.371767975E-6	8.908841165E-7	-5.1552E+0	8.871964132E-7	-8.166002864E-8	1.61E+1	1.5959E+1	8.60315E+1	6.2996E+1	-1.778700389E-2	5.84E+2	1E+1	1.6E+1	1.8E+0	1.6116E+1	1.5963E+1	8.60315E+1	6.2996E+1	4.4E+0	1.6E+1	-4.516903311E-3	1.4649E+0	-2.34E-1	2.3E+1	2.5E-2	2.49E-2
Magnet: Rate{Double Float}=0.500000	0E+0	1.235751125E-3	1.524E-1	1.235751125E-3	3.270614936E-6	8.28717551E-7	-5.4696E+0	8.255567837E-7	-8.113317751E-8	1.6117E+1	1.5961E+1	8.59957E+1	6.2996E+1	-1.620171219E-2	5.85E+2	1E+1	1.6E+1	1.8E+0	1.61E+1	1.5959E+1	8.60315E+1	6.2996E+1	4.4E+0	1.6E+1	-1.778700389E-2	1.4649E+0	-2.34E-1	2.4E+1	2E-2	1.99E-2
Magnet: Setpoint{Double Float}=0.000000	0E+0	1.235582833E-3	1.56E-1	1.235582833E-3	3.371767975E-6	7.686581637E-7	-6.576E+0	7.633899354E-7	-8.903571805E-8	1.6101E+1	1.596E+1	8.60315E+1	6.2996E+1	-1.144198328E-2	5.86E+2	1E+1	1.6E+1	1.8E+0	1.6117E+1	1.5961E+1	8.59957E+1	6.2996E+1	4.4E+0	1.6E+1	-1.620171219E-2	1.4649E+0	-2.34E-1	2.5E+1	1.5E-2	1.49E-2
Magnet: Units{Enum U16 ((Field,Current))}=Field	0E+0	1.235582833E-3	1.56E-1	1.235582833E-3	3.371767975E-6	6.917405023E-7	-6.7584E+0	6.869986442E-7	-8.271364602E-8	1.6085E+1	1.595E+1	8.60315E+1	6.2996E+1	-2.053196356E-2	5.87E+2	1E+1	1.6E+1	1.8E+0	1.6101E+1	1.596E+1	8.60315E+1	6.2996E+1	4.4E+0	1.6E+1	-1.144198328E-2	1.4649E+0	-2.34E-1	2.6E+1	1E-2	1E-2
Magnet: VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	0E+0	1.235582833E-3	1.56E-1	1.235582833E-3	3.371767975E-6	6.353665556E-7	-7.8864E+0	6.290444553E-7	-8.798210066E-8	1.6077E+1	1.5941E+1	8.59957E+1	6.2996E+1	-3.034250624E-2	5.88E+2	1E+1	1.6E+1	1.8E+0	1.6085E+1	1.595E+1	8.60315E+1	6.2996E+1	4.4E+0	1.6E+1	-2.053196356E-2	1.4649E+0	-2.34E-1	2.7E+1	5E-3	5E-3
Main Screen Path{Path}=C:\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV\\\\1Code.vi	0E+0	1.235582833E-3	1.56E-1	1.235582833E-3	3.371767975E-6	5.647701459E-7	-6.7956E+0	5.605557895E-7	-6.796209749E-8	1.6071E+1	1.5932E+1	8.57808E+1	6.2996E+1	-3.989681602E-2	5.89E+2	1E+1	1.6E+1	1.8E+0	1.6077E+1	1.5941E+1	8.59957E+1	6.2996E+1	4.4E+0	1.6E+1	-3.034250624E-2	1.4649E+0	-2.34E-1	2.8E+1	0E+0	-0E+0
Measurement Timestamp{Timestamp}=<00:12:07.107 18/05/2023>T	0E+0	1.235548892E-3	1.56E-1	1.235548892E-3	3.371767975E-6	4.867986125E-7	-9.0672E+0	4.799498591E-7	-7.84989502E-8	1.6074E+1	1.593E+1	8.57808E+1	6.2996E+1	-3.965240717E-2	5.9E+2	1E+1	1.6E+1	1.8E+0	1.6071E+1	1.5932E+1	8.57808E+1	6.2996E+1	4.4E+0	1.6E+1	-3.989681602E-2	1.4649E+0	-2.34E-1	2.9E+1	-5E-3	-5.2E-3
Measurement Title{String}=	0E+0	1.235582833E-3	1.56E-1	1.235582833E-3	3.371767975E-6	4.299005583E-7	-1.12296E+1	4.20944061E-7	-8.482102222E-8	1.6087E+1	1.5935E+1	8.57092E+1	6.2996E+1	-2.639982104E-2	5.91E+2	1E+1	1.6E+1	1.8E+0	1.6074E+1	1.593E+1	8.57808E+1	6.2996E+1	4.4E+0	1.6E+1	-3.965240717E-2	1.4649E+0	-2.34E-1	3E+1	-1E-2	-1E-2
Measurment Select{U16}=4	0E+0	1.235582833E-3	1.56E-1	1.235582833E-3	3.371767975E-6	3.735288743E-7	-1.13388E+1	3.656265318E-7	-7.481104892E-8	1.6105E+1	1.5941E+1	8.58524E+1	6.2996E+1	-1.039894205E-2	5.92E+2	1E+1	1.6E+1	1.8E+0	1.6087E+1	1.5935E+1	8.57092E+1	6.2996E+1	4.4E+0	1.6E+1	-2.639982104E-2	1.4649E+0	-2.34E-1	3.1E+1	-1.5E-2	-1.51E-2
Measurment Select.__text__{String}=6221-Lockin-DAQ	0E+0	1.23565015E-3	1.56E-1	1.23565015E-3	3.371767975E-6	2.960825798E-7	-1.4196E+1	2.871266482E-7	-7.481104892E-8	1.6117E+1	1.5955E+1	8.58524E+1	6.2996E+1	1.959807612E-2	5.93E+2	1E+1	1.6E+1	1.8E+0	1.6105E+1	1.5941E+1	8.58524E+1	6.2996E+1	4.4E+0	1.6E+1	-1.039894205E-2	1.4649E+0	-2.34E-1	3.2E+1	-2E-2	-2E-2
Notes{String}=I+1A I-1E\\nrxx+1B Rxx-1C\\nRxy+1D Rxy-4A	0E+0	1.235751125E-3	1.56E-1	1.235751125E-3	3.371767975E-6	2.339160144E-7	-2.08644E+1	2.186382653E-7	-8.482096565E-8	1.6082E+1	1.5944E+1	8.57808E+1	6.2996E+1	8.23149085E-3	5.94E+2	1E+1	1.6E+1	1.8E+0	1.6117E+1	1.5955E+1	8.58524E+1	6.2996E+1	4.4E+0	1.6E+1	1.959807612E-2	1.4649E+0	-2.34E-1	3.3E+1	-2.5E-2	-2.51E-2
Offset{Double Float}=0.000000	0E+0	1.235751125E-3	1.56E-1	1.235751125E-3	3.371767975E-6	1.801790103E-7	-2.3754E+1	1.643737595E-7	-7.428422609E-8	1.6074E+1	1.5936E+1	8.6139E+1	6.2996E+1	-1.821751241E-3	5.95E+2	1E+1	1.6E+1	1.8E+0	1.6082E+1	1.5944E+1	8.57808E+1	6.2996E+1	4.4E+0	1.6E+1	8.23149085E-3	1.4649E+0	-2.34E-1	3.4E+1	-3E-2	-3.04E-2
Option: 2182 Autozero{Boolean}=True	0E+0	1.235751125E-3	1.56E-1	1.235751125E-3	3.371767975E-6	1.238070152E-7	-3.75876E+1	9.746525112E-8	-7.797209908E-8	1.6123E+1	1.5954E+1	8.6139E+1	6.2996E+1	2.272043936E-2	5.96E+2	1E+1	1.6E+1	1.8E+0	1.6074E+1	1.5936E+1	8.6139E+1	6.2996E+1	4.4E+0	1.6E+1	-1.821751241E-3	1.4649E+0	-2.34E-1	3.5E+1	-3.5E-2	-3.51E-2
Option: 2182 Front Autozero{Boolean}=True	0E+0	1.235751125E-3	1.56E-1	1.235751125E-3	3.371767975E-6	7.744513482E-8	-7.24776E+1	2.160038682E-8	-7.586460974E-8	1.6125E+1	1.5962E+1	8.60673E+1	6.2996E+1	2.892868035E-2	5.97E+2	1E+1	1.6E+1	1.8E+0	1.6123E+1	1.5954E+1	8.6139E+1	6.2996E+1	4.4E+0	1.6E+1	2.272043936E-2	1.4649E+0	-2.34E-1	3.6E+1	-4E-2	-3.99E-2
Option: 2182 Hold{Boolean}=False	0E+0	1.235751125E-3	1.56E-1	1.235751125E-3	3.371767975E-6	9.325052701E-8	-1.058568E+2	-2.792245885E-8	-9.11431791E-8	1.6118E+1	1.5963E+1	8.60673E+1	6.2996E+1	2.410332672E-2	5.98E+2	1E+1	1.6E+1	1.8E+0	1.6125E+1	1.5962E+1	8.60673E+1	6.2996E+1	4.4E+0	1.6E+1	2.892868035E-2	1.4649E+0	-2.34E-1	3.7E+1	-4.5E-2	-4.51E-2
Option: 2182 Hold Count{I32}=10	0E+0	1.235751125E-3	1.56E-1	1.235751125E-3	3.371767975E-6	1.259144762E-7	-1.428192E+2	-1.022067415E-7	-7.84989502E-8	1.6105E+1	1.5957E+1	8.60315E+1	6.2996E+1	9.512536228E-3	5.99E+2	1E+1	1.6E+1	1.8E+0	1.6118E+1	1.5963E+1	8.60673E+1	6.2996E+1	4.4E+0	1.6E+1	2.410332672E-2	1.4649E+0	-2.34E-1	3.8E+1	-5E-2	-5E-2
Option: 2182 Hold Window{Double Float}=1.000000	0E+0	1.235751125E-3	1.56E-1	1.235751125E-3	3.371767975E-6	1.195923476E-7	-1.460844E+2	-1.022067698E-7	-6.901577145E-8	1.6099E+1	1.5955E+1	8.60315E+1	6.2996E+1	6.049095187E-3	6E+2	1E+1	1.6E+1	1.8E+0	1.6105E+1	1.5957E+1	8.60315E+1	6.2996E+1	4.4E+0	1.6E+1	9.512536228E-3	1.4649E+0	-2.34E-1	3.9E+1	-5E-2	-5E-2
Option: 2182 Line Sync{Boolean}=False	0E+0	1.235852099E-3	1.56E-1	1.235852099E-3	3.371767975E-6	2.523553793E-7	-1.620168E+2	-2.423458586E-7	-7.955259587E-8	1.6066E+1	1.5938E+1	8.60315E+1	6.2996E+1	-1.950630359E-2	6.01E+2	1E+1	1.6E+1	1.8E+0	1.6099E+1	1.5955E+1	8.60315E+1	6.2996E+1	4.4E+0	1.6E+1	6.049095187E-3	1.4649E+0	-2.34E-1	4E+1	-6E-2	-5.99E-2
Option: 2182 Reference Reading{Double Float}=0.000000	0E+0	1.235919416E-3	1.56E-1	1.235919416E-3	3.371767975E-6	3.656265318E-7	-1.661964E+2	-3.566700344E-7	-8.956259745E-8	1.61E+1	1.5939E+1	8.60315E+1	6.2996E+1	-2.363701724E-2	6.02E+2	1E+1	1.6E+1	1.8E+0	1.6066E+1	1.5938E+1	8.60315E+1	6.2996E+1	4.4E+0	1.6E+1	-1.950630359E-2	1.4649E+0	-2.34E-1	4.1E+1	-7E-2	-7E-2
Option: 2182 Relative Mode{Boolean}=False	0E+0	1.235919416E-3	1.56E-1	1.235919416E-3	3.371767975E-6	5.036577353E-7	-1.686012E+2	-4.973353521E-7	-1.022067415E-7	1.6094E+1	1.5946E+1	8.60315E+1	6.2996E+1	-1.571096852E-2	6.03E+2	1E+1	1.6E+1	1.8E+0	1.61E+1	1.5939E+1	8.60315E+1	6.2996E+1	4.4E+0	1.6E+1	-2.363701724E-2	1.4649E+0	-2.34E-1	4.2E+1	-8E-2	-7.99E-2
Option: 2182 Trigger Delay{Cluster (Boolean,Double Float)}={'Auto':True,'Time(s)':0.000000}	0E+0	1.235986732E-3	1.56E-1	1.235986732E-3	3.371767975E-6	6.237759441E-7	-1.726224E+2	-6.211415471E-7	-8.113312095E-8	1.6066E+1	1.5934E+1	8.60315E+1	6.2996E+1	-2.890251391E-2	6.04E+2	1E+1	1.6E+1	1.8E+0	1.6094E+1	1.5946E+1	8.60315E+1	6.2996E+1	4.4E+0	1.6E+1	-1.571096852E-2	1.4649E+0	-2.34E-1	4.3E+1	-9E-2	-8.99E-2
Option: 2182 Trigger Source{Enum U16 ((Immediate,Timer,Manual,Bus,Trigger link))}=Bus	0E+0	1.236087707E-3	1.56E-1	1.236087707E-3	3.371767975E-6	7.486388394E-7	-1.733868E+2	-7.449505704E-7	-8.745524954E-8	1.6064E+1	1.5925E+1	8.60315E+1	6.2996E+1	-3.381681815E-2	6.05E+2	1E+1	1.6E+1	1.8E+0	1.6066E+1	1.5934E+1	8.60315E+1	6.2996E+1	4.4E+0	1.6E+1	-2.890251391E-2	1.4649E+0	-2.34E-1	4.4E+1	-1E-1	-1E-1
Option: 2182 Trigger Timer{Double Float}=0.000000	0E+0	1.236087707E-3	1.56E-1	1.236087707E-3	3.371767975E-6	7.654973964E-7	-1.741716E+2	-7.639168714E-7	-7.902577303E-8	1.606E+1	1.5923E+1	8.60315E+1	6.2996E+1	-3.250689805E-2	6.06E+2	1E+1	1.6E+1	1.8E+0	1.6064E+1	1.5925E+1	8.60315E+1	6.2996E+1	4.4E+0	1.6E+1	-3.381681815E-2	1.4649E+0	-2.34E-1	4.5E+1	-1E-1	-1E-1
Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	0E+0	1.23709887E-3	1.56E-1	1.23709887E-3	3.371767975E-6	3.359124906E-6	-1.783284E+2	-3.359650994E-6	-9.957257075E-8	1.6094E+1	1.5926E+1	8.59957E+1	6.2996E+1	-6.794394925E-3	6.07E+2	1E+1	1.6E+1	1.8E+0	1.606E+1	1.5923E+1	8.60315E+1	6.2996E+1	4.4E+0	1.6E+1	-3.250689805E-2	1.4649E+0	-2.34E-1	4.6E+1	-3E-1	-2.999E-1
Option: 560 Enabled{Boolean}=False	0E+0	1.238111447E-3	1.56E-1	1.238111447E-3	3.371767975E-6	5.946434275E-6	-1.790184E+2	-5.949067541E-6	-1.032604155E-7	1.604E+1	1.5904E+1	8.5745E+1	6.2996E+1	-2.245563455E-2	6.08E+2	1E+1	1.6E+1	1.8E+0	1.6094E+1	1.5926E+1	8.59957E+1	6.2996E+1	4.4E+0	1.6E+1	-6.794394925E-3	1.4649E+0	-2.34E-1	4.7E+1	-5E-1	-4.999E-1
Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	0E+0	1.239459192E-3	1.56E-1	1.239459192E-3	3.371767975E-6	8.549000181E-6	-1.793052E+2	-8.551639103E-6	-1.048409123E-7	1.6036E+1	1.589E+1	8.61032E+1	6.2996E+1	-2.905404568E-2	6.09E+2	1E+1	1.6E+1	1.8E+0	1.604E+1	1.5904E+1	8.5745E+1	6.2996E+1	4.4E+0	1.6E+1	-2.245563455E-2	1.4649E+0	-2.34E-1	4.8E+1	-7E-1	-6.999E-1
Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	0E+0	1.240976644E-3	1.56E-1	1.240976644E-3	3.371767975E-6	1.117004986E-5	-1.79496E+2	-1.117268312E-5	-1.000994219E-7	1.6058E+1	1.5902E+1	8.60673E+1	6.2996E+1	1.464256179E-2	6.1E+2	1E+1	1.6E+1	1.8E+0	1.6036E+1	1.589E+1	8.61032E+1	6.2996E+1	4.4E+0	1.6E+1	-2.905404568E-2	1.4649E+0	-2.34E-1	4.9E+1	-9E-1	-8.999E-1
Option: 6221 Adjust Mode{Enum U16 ((Offset,Frequency,Amplitude))}=Offset	0E+0	1.243000383E-3	1.56E-1	1.243000383E-3	3.371767975E-6	1.375628725E-5	-1.795308E+2	-1.375892052E-5	-1.137971267E-7	1.605E+1	1.5899E+1	8.59957E+1	6.2996E+1	1.70321425E-3	6.11E+2	1E+1	1.6E+1	1.8E+0	1.6058E+1	1.5902E+1	8.60673E+1	6.2996E+1	4.4E+0	1.6E+1	1.464256179E-2	1.4649E+0	-2.34E-1	5E+1	-1.1E+0	-1.1E+0
Option: 6221 Amplitude{Double Float}=1.000000E-6	0E+0	1.245022709E-3	1.56E-1	1.245022709E-3	3.371767975E-6	1.636358229E-5	-1.79592E+2	-1.636621272E-5	-1.180117943E-7	1.6086E+1	1.5922E+1	8.59957E+1	6.2996E+1	2.63832733E-2	6.12E+2	1E+1	1.6E+1	1.8E+0	1.605E+1	1.5899E+1	8.59957E+1	6.2996E+1	4.4E+0	1.6E+1	1.70321425E-3	1.4649E+0	-2.34E-1	5.1E+1	-1.3E+0	-1.3E+0
Option: 6221 Compliance{Double Float}=10.000000	0E+0	1.247551322E-3	1.56E-1	1.247551322E-3	3.371767975E-6	1.897617214E-5	-1.796208E+2	-1.897883086E-5	-1.269680653E-7	1.6066E+1	1.5916E+1	8.56375E+1	6.2996E+1	2.706173342E-3	6.13E+2	1E+1	1.6E+1	1.8E+0	1.6086E+1	1.5922E+1	8.59957E+1	6.2996E+1	4.4E+0	1.6E+1	2.63832733E-2	1.4649E+0	-2.34E-1	5.2E+1	-1.5E+0	-1.5E+0
Option: 6221 Duty Cycle{Double Float}=50.000000	0E+0	1.247551322E-3	1.56E-1	1.247551322E-3	3.371767975E-6	1.897933998E-5	-1.796088E+2	-1.898197041E-5	-1.311827612E-7	1.6062E+1	1.5913E+1	8.56375E+1	6.2996E+1	-5.589080974E-3	6.14E+2	1E+1	1.6E+1	1.8E+0	1.6066E+1	1.5916E+1	8.56375E+1	6.2996E+1	4.4E+0	1.6E+1	2.706173342E-3	1.4649E+0	-2.34E-1	5.3E+1	-1.5E+0	-1.5E+0
Option: 6221 External Trigger{Boolean}=False	0E+0	1.241989221E-3	1.56E-1	1.241989221E-3	3.371767975E-6	1.245183929E-5	-1.794408E+2	-1.245447821E-5	-1.232801641E-7	1.6112E+1	1.5952E+1	8.61032E+1	6.2996E+1	3.771406785E-2	6.15E+2	1E+1	1.6E+1	1.8E+0	1.6062E+1	1.5913E+1	8.56375E+1	6.2996E+1	4.4E+0	1.6E+1	-5.589080974E-3	1.4649E+0	-2.34E-1	5.4E+1	-1E+0	-1.0001E+0
Option: 6221 External Trigger Ignore Multiple{Boolean}=False	0E+0	1.23824608E-3	1.56E-1	1.23824608E-3	3.371767975E-6	5.942217091E-6	-1.789248E+2	-5.944324269E-6	-1.127434811E-7	1.6112E+1	1.5968E+1	8.59599E+1	6.23121E+1	-5.849490408E-4	6.16E+2	1E+1	1.6E+1	1.8E+0	1.6112E+1	1.5952E+1	8.61032E+1	6.2996E+1	4.4E+0	1.6E+1	3.771406785E-2	1.4649E+0	-2.34E-1	5.5E+1	-5E-1	-5.001E-1
Option: 6221 Frequency{Double Float}=119.770000	
Option: 6221 Function{U16}=1	
Option: 6221 Function.__text__{String}=Sine	
Option: 6221 Idle Level{Double Float}=0.000000	
Option: 6221 Input trigger Line{U8}=5	
Option: 6221 Offset{Double Float}=0.000000	
Option: 6221 Output Trigger Line{U8}=4	
Option: 6221 Pass Through{Boolean}=True	
Option: 6221 Phase Marker{Boolean}=True	
Option: 6221 Phase Marker Phase{Double Float}=0.000000	
Option: 6221 Range Level{Double Float}=2.000000E-12	
Option: 6221 Ranging{U16}=1	
Option: 6221 Ranging.__text__{String}=Best	
Option: 6221 Update Clock{Double Float}=0.000000	
Option: 6221 VISA{Visa Refnum (Void)}=GPIB0::13::INSTR	
Option: Confirm Config{Boolean}=False	
Option: Control Panel Ref{LVObjVI Refnum (Void)}=	
Option: DAQ Global Channel{Boolean}=False	
Option: DAQ Input Rate{Double Float}=10000.000000	
Option: DAQ Input Samples{I32}=200	
Option: DAQ Measurement Channels{1D Array (Cluster (UserDefinedRefnumTag Refnum (Void),\tkDAQmxPhysChanTagType Tag,\tkDAQmxScaleTagType Tag,Boolean,Double Float,String))}=[]	
Option: Differential{I32}=10106	
Option: Differential.__text__{String}=Differential	
Option: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values))}=Function Generator	
Option: Lockin Standoff Time{Double Float}=0.000000	
Option: Paranoid Save Data{Boolean}=True	
Option: Plot Autoback Path{Path}=C:\\\\TEMP\\\\XY Multiparam\\\\Backup.txt	
Option: SR830  Ref Phase{Double Float}=0.000000	
Option: SR830  Synch Filter{Boolean}=False	
Option: SR830  Time Constant{I16}=8	
Option: SR830  Time Constant.__text__{String}=100 ms	
Option: SR830 2x Line Filter{Boolean}=True	
Option: SR830 Adjust Gains{Boolean}=False	
Option: SR830 Auto Gain Lower.__text__{String}=2 nV/fA	
Option: SR830 Auto Gain Upper.__text__{String}=1 V/uA	
Option: SR830 Auto Offset 1{Boolean}=False	
Option: SR830 Auto Offset 2{Boolean}=False	
Option: SR830 Autophase{Boolean}=False	
Option: SR830 DC Coupling?{Boolean}=False	
Option: SR830 Display 1{U16}=0	
Option: SR830 Display 1.__text__{String}=X	
Option: SR830 Display 2{U16}=0	
Option: SR830 Display 2.__text__{String}=Y	
Option: SR830 Dynamic Reserve{I16}=1	
Option: SR830 Dynamic Reserve.__text__{String}=Normal	
Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Option: SR830 Filter Slope{I32}=1	
Option: SR830 Filter Slope.__text__{String}=12 dB/oct	
Option: SR830 Gain{I32}=-1	
Option: SR830 Gain.__text__{String}=Auto Gain	
Option: SR830 Ground Shield?{Boolean}=False	
Option: SR830 Harmonic{I32}=1	
Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A	
Option: SR830 Line Filter{Boolean}=True	
Option: SR830 No Reset{Boolean}=False	
Option: SR830 Offset 1{Double Float}=0.000000	
Option: SR830 Offset 2{Double Float}=0.000000	
Option: SR830 Output Channel 1{Boolean}=False	
Option: SR830 Output Channel 2{Boolean}=False	
Option: SR830 Ratio 1{U16}=0	
Option: SR830 Ratio 1.__text__{String}=None	
Option: SR830 Ratio 2{U16}=0	
Option: SR830 Ratio 2.__text__{String}=None	
Option: SR830 Ref Amplitude{Double Float}=0.100000	
Option: SR830 Ref Frequency{Double Float}=1013.000000	
Option: SR830 Ref Source{Boolean}=False	
Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta]	
Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Option: SR830 VISA{Visa Refnum (Void)}=	
Option: Sense Autorange{Boolean}=False	
Option: Sense Range Level{Double Float}=0.100000	
Option: Sense Rate{Double Float}=1.000000	
Option:560 Comport{Visa Refnum (Void)}=COM1	
Option:560 Filter High Pass{U16}=0	
Option:560 Filter High Pass.__text__{String}=0.03	
Option:560 Filter Lowpass{U16}=0	
Option:560 Filter Lowpass.__text__{String}=0.03	
Option:560 Filter Mode{U16}=0	
Option:560 Filter Mode.__text__{String}=6 dB high pass	
Option:560 Invert{Boolean}=False	
Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Option:570 Enabled{Boolean}=False	
Option:570 Filter High Pass{U16}=0	
Option:570 Filter High Pass.__text__{String}=0.03	
Option:570 Filter Lowpass{U16}=0	
Option:570 Filter Lowpass.__text__{String}=0.03	
Option:570 Filter Mode{U16}=0	
Option:570 Filter Mode.__text__{String}=6 dB high pass	
Option:570 Gain Mode{U16}=0	
Option:570 Gain Mode.__text__{String}=Low Noise	
Option:570 Input Offset{U16}=0	
Option:570 Input Offset On{Boolean}=False	
Option:570 Input Offset.__text__{String}=1pA	
Option:570 Sensitivity{U16}=0	
Option:570 Sensitivity.__text__{String}=1pA/V	
Option:Debug On{Boolean}=False	
Option:GPIB 2182{Visa Refnum (Void)}=	
Option:Parallel Config Voltage Measurers{Boolean}=True	
Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Option:SR830 Settle Time{Double Float}=5.000000	
Option:Sense Digits{I32}=8	
Output Names{1D Array (String)}=['Offset','Rxx::R','Rxx::Theta','Rxx::X','Rxx::Y','Rxy::R','Rxy::Theta','Rxy::X','Rxy::Y','temperature: T1','temperature: T2','temperature: T3','temperature: T4','temperature: dT/dt','iterator','multi[0]:iterator','multi[0]:y','multi[0]:temperature: setpoint','multi[0]:temperature: T1','multi[0]:temperature: T2','multi[0]:temperature: T3','multi[0]:temperature: T4','multi[0]:temperature: heater','multi[0]:temperature: gas','multi[0]:temperature: dT/dt','multi[0]:temperature: current temperature','multi[0]:temperature: error','multi[1]:iterator','multi[1]:y','multi[1]:Control:Magnet Output']	
Parameter Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Parameter Select{U16}=6	
Parameter Select.__text__{String}=Multi-Parameter	
Paths{U32}=0	
Plot: Column Renames{1D Array (Cluster (String,String))}=[]	
Plot: No dups{Boolean}=False	
Plot: StdDevs{Boolean}=False	
Plotting Class{String}=Parameter Plot	
Plotting Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	
Plotting Select{U16}=1	
Plotting Select.__text__{String}=Parameter Plot	
Project Code{String}=Topological_Insulators	
Ref: Temperature Window{LVObjVI Refnum (Void)}=	
Ref:Control Subpanel{LVObjUnknown Refnum (Void)}=	
Ref:Main Screen{LVObjVI Refnum (Void)}=	
Ref:Plotting Subpanel{LVObjUnknown Refnum (Void)}=	
Ref:Toolbar{LVObjUnknown Refnum (Void)}=	
Ref:XY Subpanel{LVObjUnknown Refnum (Void)}=	
Rxx::R{Double Float}=0.001238	
Rxx::Theta{Double Float}=0.156000	
Rxx::X{Double Float}=0.001238	
Rxx::Y{Double Float}=3.371768E-6	
Rxx:Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	
Rxx:Option: 560 Enabled{Boolean}=False	
Rxx:Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	
Rxx:Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	
Rxx:Option: Lockin Standoff Time{Double Float}=0.000000	
Rxx:Option: Lockin Type{Enum U16 ((SRS 830,EG&G 5302))}=SRS 830	
Rxx:Option: SR803 Full Scale Reading{Double Float}=0.000000	
Rxx:Option: SR830  Ref Phase{Double Float}=0.000000	
Rxx:Option: SR830  Synch Filter{Boolean}=False	
Rxx:Option: SR830  Time Constant{I16}=8	
Rxx:Option: SR830 2x Line Filter{Boolean}=False	
Rxx:Option: SR830 Adjust Gains{Boolean}=False	
Rxx:Option: SR830 Auto Gain Lower{I32}=0	
Rxx:Option: SR830 Auto Gain Upper{I32}=26	
Rxx:Option: SR830 Auto Offset 1{Boolean}=False	
Rxx:Option: SR830 Auto Offset 2{Boolean}=False	
Rxx:Option: SR830 Autophase{Boolean}=False	
Rxx:Option: SR830 DC Coupling?{Boolean}=False	
Rxx:Option: SR830 Display 1{U16}=0	
Rxx:Option: SR830 Display 2{U16}=0	
Rxx:Option: SR830 Dynamic Reserve{I16}=2	
Rxx:Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Rxx:Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Rxx:Option: SR830 Filter Slope{I32}=3	
Rxx:Option: SR830 Gain{I32}=18	
Rxx:Option: SR830 Ground Shield?{Boolean}=False	
Rxx:Option: SR830 Harmonic{I32}=1	
Rxx:Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A-B	
Rxx:Option: SR830 Line Filter{Boolean}=False	
Rxx:Option: SR830 No Reset{Boolean}=False	
Rxx:Option: SR830 Offset 1{Double Float}=0.000000	
Rxx:Option: SR830 Offset 2{Double Float}=0.000000	
Rxx:Option: SR830 Output Channel 1{Boolean}=False	
Rxx:Option: SR830 Output Channel 2{Boolean}=False	
Rxx:Option: SR830 Ratio 1{U16}=0	
Rxx:Option: SR830 Ratio 2{U16}=0	
Rxx:Option: SR830 Ref Amplitude{Double Float}=0.100000	
Rxx:Option: SR830 Ref Frequency{Double Float}=1013.000000	
Rxx:Option: SR830 Ref Source{Boolean}=False	
Rxx:Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta,X,Y]	
Rxx:Option: SR830 Time Constant value{Double Float}=0.000000	
Rxx:Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Rxx:Option: SR830 VISA{Visa Refnum (Void)}=GPIB0::5::INSTR	
Rxx:Option:560 Comport{Visa Refnum (Void)}=COM1	
Rxx:Option:560 Filter High Pass{U16}=0	
Rxx:Option:560 Filter Lowpass{U16}=0	
Rxx:Option:560 Filter Mode{U16}=0	
Rxx:Option:560 Invert{Boolean}=False	
Rxx:Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Rxx:Option:570 Enabled{Boolean}=False	
Rxx:Option:570 Filter High Pass{U16}=0	
Rxx:Option:570 Filter Lowpass{U16}=0	
Rxx:Option:570 Filter Mode{U16}=0	
Rxx:Option:570 Gain Mode{U16}=0	
Rxx:Option:570 Input Offset{U16}=0	
Rxx:Option:570 Input Offset On{Boolean}=False	
Rxx:Option:570 Sensitivity{U16}=0	
Rxx:Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Rxx:Option:SR830 Autogain Lower Threshold{Double Float}=0.100000	
Rxx:Option:SR830 Autogain Standoff{Double Float}=3.000000	
Rxx:Option:SR830 Autogain Upper Threshold{Double Float}=0.900000	
Rxx:Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Rxx:Option:SR830 Settle Time{Double Float}=0.000000	
Rxy::R{Double Float}=5.942217E-6	
Rxy::Theta{Double Float}=-178.924800	
Rxy::X{Double Float}=-5.944324E-6	
Rxy::Y{Double Float}=-1.127435E-7	
Rxy:Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	
Rxy:Option: 560 Enabled{Boolean}=False	
Rxy:Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	
Rxy:Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	
Rxy:Option: Lockin Standoff Time{Double Float}=0.000000	
Rxy:Option: Lockin Type{Enum U16 ((SRS 830,EG&G 5302))}=SRS 830	
Rxy:Option: SR803 Full Scale Reading{Double Float}=0.000000	
Rxy:Option: SR830  Ref Phase{Double Float}=0.000000	
Rxy:Option: SR830  Synch Filter{Boolean}=False	
Rxy:Option: SR830  Time Constant{I16}=8	
Rxy:Option: SR830 2x Line Filter{Boolean}=False	
Rxy:Option: SR830 Adjust Gains{Boolean}=False	
Rxy:Option: SR830 Auto Gain Lower{I32}=0	
Rxy:Option: SR830 Auto Gain Upper{I32}=26	
Rxy:Option: SR830 Auto Offset 1{Boolean}=False	
Rxy:Option: SR830 Auto Offset 2{Boolean}=False	
Rxy:Option: SR830 Autophase{Boolean}=False	
Rxy:Option: SR830 DC Coupling?{Boolean}=False	
Rxy:Option: SR830 Display 1{U16}=0	
Rxy:Option: SR830 Display 2{U16}=1	
Rxy:Option: SR830 Dynamic Reserve{I16}=2	
Rxy:Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Rxy:Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Rxy:Option: SR830 Filter Slope{I32}=3	
Rxy:Option: SR830 Gain{I32}=18	
Rxy:Option: SR830 Ground Shield?{Boolean}=False	
Rxy:Option: SR830 Harmonic{I32}=1	
Rxy:Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A-B	
Rxy:Option: SR830 Line Filter{Boolean}=False	
Rxy:Option: SR830 No Reset{Boolean}=False	
Rxy:Option: SR830 Offset 1{Double Float}=0.000000	
Rxy:Option: SR830 Offset 2{Double Float}=0.000000	
Rxy:Option: SR830 Output Channel 1{Boolean}=False	
Rxy:Option: SR830 Output Channel 2{Boolean}=False	
Rxy:Option: SR830 Ratio 1{U16}=0	
Rxy:Option: SR830 Ratio 2{U16}=0	
Rxy:Option: SR830 Ref Amplitude{Double Float}=0.100000	
Rxy:Option: SR830 Ref Frequency{Double Float}=1013.000000	
Rxy:Option: SR830 Ref Source{Boolean}=False	
Rxy:Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta,X,Y]	
Rxy:Option: SR830 Time Constant value{Double Float}=0.000000	
Rxy:Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Rxy:Option: SR830 VISA{Visa Refnum (Void)}=GPIB0::6::INSTR	
Rxy:Option:560 Comport{Visa Refnum (Void)}=COM1	
Rxy:Option:560 Filter High Pass{U16}=0	
Rxy:Option:560 Filter Lowpass{U16}=0	
Rxy:Option:560 Filter Mode{U16}=0	
Rxy:Option:560 Invert{Boolean}=False	
Rxy:Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Rxy:Option:570 Enabled{Boolean}=False	
Rxy:Option:570 Filter High Pass{U16}=0	
Rxy:Option:570 Filter Lowpass{U16}=0	
Rxy:Option:570 Filter Mode{U16}=0	
Rxy:Option:570 Gain Mode{U16}=0	
Rxy:Option:570 Input Offset{U16}=0	
Rxy:Option:570 Input Offset On{Boolean}=False	
Rxy:Option:570 Sensitivity{U16}=0	
Rxy:Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Rxy:Option:SR830 Autogain Lower Threshold{Double Float}=0.100000	
Rxy:Option:SR830 Autogain Standoff{Double Float}=3.000000	
Rxy:Option:SR830 Autogain Upper Threshold{Double Float}=0.900000	
Rxy:Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Rxy:Option:SR830 Settle Time{Double Float}=0.000000	
Sample ID{String}=MBE202221213_PA_D1 750C Cracker WAL	
Save:Filename{String}=${X-Y Class} ${2nd Parameter Class} ${iterator}{%04d} ${y}{%04.2g}.txt	
Save:Final Filename{String}=${X-Y Class} ${2nd Parameter Class} .txt	
Save:Final path{Path}=C:\\\\Data\\\\${Project Code}\\\\${User}\\\\${Sample ID}\\\\${Measurement Timestamp}{%Y%m%d}\\\\${X-Y Class}	
Save:Path{Path}=C:\\\\Data\\\\${Project Code}\\\\${User}\\\\${Sample ID}\\\\${Measurement Timestamp}{%Y%m%d}\\\\${X-Y Class}	
Startup path{Path}=C:\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV	
Sub Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Sweep Step{I32}=3	
T Control Measure.__text__{1D Array (String)}=['temperature: T1','temperature: T2','temperature: T3','temperature: T4','temperature: dT/dt']	
Timestamp{Timestamp}=<00:13:15.990 18/05/2023>T	
Toolbar{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Unaved Data{Boolean}=True	
Unsaved Data{Boolean}=False	
User{String}=Craig	
X-Y Class{String}=6221-Lockin-DAQ	
X-Y Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	
d(Offset){Double Float}=0.000000	
d(Rxx::R){Double Float}=7.526221E-8	
d(Rxx::Theta){Double Float}=0.000000	
d(Rxx::X){Double Float}=7.526221E-8	
d(Rxx::Y){Double Float}=4.735058E-22	
d(Rxy::R){Double Float}=1.411326E-8	
d(Rxy::Theta){Double Float}=0.092700	
d(Rxy::X){Double Float}=1.473733E-8	
d(Rxy::Y){Double Float}=9.200788E-9	
iterate result{U16}=5	
iterator{I32}=616	
multi[0]:Control: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values,Adaptive Step Ramp))}=List of Values	
multi[0]:Control: Monitor Update Timeout{Double Float}=0.010000	
multi[0]:Control: Open T Window{Boolean}=False	
multi[0]:Control: Reverse Temperature Sense{Boolean}=False	
multi[0]:Iterator{I32}=0	
multi[0]:Ref: Temperature Window{LVObjVI Refnum (Void)}=	
multi[0]:iterate result{U16}=0	
multi[0]:iterator{I32}=10	
multi[0]:temperature:  rate window{Double Float}=120.000000	
multi[0]:temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[0]:temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
multi[0]:temperature: T1{Double Float}=16.077000	
multi[0]:temperature: T2{Double Float}=15.928000	
multi[0]:temperature: T3{Double Float}=85.745000	
multi[0]:temperature: T4{Double Float}=62.312100	
multi[0]:temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
multi[0]:temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
multi[0]:temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
multi[0]:temperature: current temperature{Double Float}=1.464900	
multi[0]:temperature: current temperature 2{Double Float}=287.100000	
multi[0]:temperature: dT/dt{Double Float}=-0.010762	
multi[0]:temperature: error{Double Float}=-0.234000	
multi[0]:temperature: gas{Double Float}=16.000000	
multi[0]:temperature: gas control{Boolean}=False	
multi[0]:temperature: gas control 2{Boolean}=False	
multi[0]:temperature: gass boost{I8}=0	
multi[0]:temperature: gass boost 2{I8}=0	
multi[0]:temperature: gast flow{I16}=0	
multi[0]:temperature: gast flow 2{I16}=7	
multi[0]:temperature: heater{Double Float}=4.400000	
multi[0]:temperature: heater output{Double Float}=0.000000	
multi[0]:temperature: heater output 2{Double Float}=0.000000	
multi[0]:temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
multi[0]:temperature: monitor timeout{Double Float}=0.010000	
multi[0]:temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
multi[0]:temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
multi[0]:temperature: ramp rate{Double Float}=8.000000	
multi[0]:temperature: ramp rate 2{Double Float}=0.000000	
multi[0]:temperature: ramp target{Double Float}=20.000000	
multi[0]:temperature: ramp target 2{Double Float}=0.000000	
multi[0]:temperature: ramping{Boolean}=False	
multi[0]:temperature: setpoint{Double Float}=1.800000	
multi[0]:temperature: setpoint 2{Double Float}=287.100000	
multi[0]:temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
multi[0]:temperature: stability error{Extended Float}=0.040000	
multi[0]:temperature: stability script{String}=	
multi[0]:temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
multi[0]:temperature: temp control mode{U16}=2	
multi[0]:temperature: temp control mode 2{U16}=3	
multi[0]:temperature: temp control mode 2.__text__{String}=Open Loop	
multi[0]:temperature: temp control mode.__text__{String}=Zone	
multi[0]:temperature: temp control sensor{U16}=0	
multi[0]:temperature: temp control sensor 2{U16}=0	
multi[0]:temperature: temp control sensor 2.__text__{String}=Sensor 1	
multi[0]:temperature: temp control sensor.__text__{String}=Sensor A	
multi[0]:temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
multi[0]:temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
multi[0]:temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
multi[0]:temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
multi[0]:temperature: temp loop{U16}=0	
multi[0]:temperature: temp loop 2{U16}=0	
multi[0]:temperature: temp loop 2.__text__{String}=Heater	
multi[0]:temperature: temp loop.__text__{String}=Loop 1	
multi[0]:temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
multi[0]:temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[0]:temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[0]:temperature:error for gas boost{Double Float}=0.000000	
multi[0]:temperature:error for gas boost 2{Double Float}=0.000000	
multi[0]:temperature:heater range{U16}=2	
multi[0]:temperature:heater range 2{U16}=0	
multi[0]:temperature:heater range 2.__text__{String}=Off	
multi[0]:temperature:heater range.__text__{String}=40mW	
multi[0]:temperature:history window{Extended Float}=300.000000	
multi[0]:temperature:is stable?{Boolean}=True	
multi[0]:temperature:monitor{Boolean}=True	
multi[0]:temperature:ramping{Boolean}=False	
multi[0]:temperature:ramping on{Boolean}=False	
multi[0]:temperature:ramping on 2{Boolean}=False	
multi[0]:temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
multi[0]:temperature:stability code{U32}=6618880	
multi[0]:temperature:stability rate{Extended Float}=0.040000	
multi[0]:y{Double Float}=16.000000	
multi[1]:Control: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values,Adaptive Step Ramp))}=Multi-Segment Ramp	
multi[1]:Control: Gate delay{Double Float}=0.000000	
multi[1]:Control: Monitor Update Timeout{Double Float}=0.010000	
multi[1]:Control: Open T Window{Boolean}=False	
multi[1]:Control: Reverse Temperature Sense{Boolean}=False	
multi[1]:Control:Magnet Output{Double Float}=-0.000100	
multi[1]:Iterator{I32}=0	
multi[1]:Magnet: Final Switch Heater{Enum U8 ((False,True,Mixed))}=	
multi[1]:Magnet: Power Supply{Enum U16 ((IPS120,LS625,PS110,Hg iPS,SMS Series,Cryomagnetics 4G,DMG Little CryoFree,DMG Big CryoFree))}=Hg iPS	
multi[1]:Magnet: Rate{Double Float}=0.500000	
multi[1]:Magnet: Units{Enum U16 ((Field,Current))}=Field	
multi[1]:Magnet: VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[1]:Multi-segment_Stage{I32}=0	
multi[1]:Multi-segment_Stage_Changed{Boolean}=False	
multi[1]:Ref: Temperature Window{LVObjVI Refnum (Void)}=	
multi[1]:iterate result{U16}=4	
multi[1]:iterator{I32}=57	
multi[1]:measure point{Boolean}=False	
multi[1]:temperature:  rate window{Double Float}=120.000000	
multi[1]:temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[1]:temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
multi[1]:temperature: T1{Double Float}=1.842400	
multi[1]:temperature: T2{Double Float}=1.465600	
multi[1]:temperature: T3{Double Float}=86.318100	
multi[1]:temperature: T4{Double Float}=66.769200	
multi[1]:temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
multi[1]:temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
multi[1]:temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
multi[1]:temperature: current temperature{Double Float}=1.465600	
multi[1]:temperature: current temperature 2{Double Float}=287.100000	
multi[1]:temperature: dT/dt{Double Float}=-0.001864	
multi[1]:temperature: gas control{Boolean}=False	
multi[1]:temperature: gas control 2{Boolean}=False	
multi[1]:temperature: gass boost{I8}=0	
multi[1]:temperature: gass boost 2{I8}=0	
multi[1]:temperature: gast flow{I16}=0	
multi[1]:temperature: gast flow 2{I16}=7	
multi[1]:temperature: heater output{Double Float}=0.000000	
multi[1]:temperature: heater output 2{Double Float}=0.000000	
multi[1]:temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
multi[1]:temperature: monitor timeout{Double Float}=1.000000	
multi[1]:temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
multi[1]:temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
multi[1]:temperature: ramp rate{Double Float}=8.000000	
multi[1]:temperature: ramp rate 2{Double Float}=0.000000	
multi[1]:temperature: ramp target{Double Float}=20.000000	
multi[1]:temperature: ramp target 2{Double Float}=0.000000	
multi[1]:temperature: ramping{Boolean}=False	
multi[1]:temperature: setpoint{Double Float}=1.800000	
multi[1]:temperature: setpoint 2{Double Float}=287.100000	
multi[1]:temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
multi[1]:temperature: stability error{Extended Float}=0.040000	
multi[1]:temperature: stability script{String}=	
multi[1]:temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
multi[1]:temperature: temp control mode{U16}=2	
multi[1]:temperature: temp control mode 2{U16}=3	
multi[1]:temperature: temp control mode 2.__text__{String}=Open Loop	
multi[1]:temperature: temp control mode.__text__{String}=Zone	
multi[1]:temperature: temp control sensor{U16}=0	
multi[1]:temperature: temp control sensor 2{U16}=0	
multi[1]:temperature: temp control sensor 2.__text__{String}=Sensor 1	
multi[1]:temperature: temp control sensor.__text__{String}=Sensor A	
multi[1]:temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
multi[1]:temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
multi[1]:temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
multi[1]:temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
multi[1]:temperature: temp loop{U16}=0	
multi[1]:temperature: temp loop 2{U16}=0	
multi[1]:temperature: temp loop 2.__text__{String}=Heater	
multi[1]:temperature: temp loop.__text__{String}=Loop 1	
multi[1]:temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
multi[1]:temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[1]:temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[1]:temperature:error for gas boost{Double Float}=0.000000	
multi[1]:temperature:error for gas boost 2{Double Float}=0.000000	
multi[1]:temperature:heater range{U16}=2	
multi[1]:temperature:heater range 2{U16}=0	
multi[1]:temperature:heater range 2.__text__{String}=Off	
multi[1]:temperature:heater range.__text__{String}=40mW	
multi[1]:temperature:history window{Extended Float}=300.000000	
multi[1]:temperature:is stable?{Boolean}=True	
multi[1]:temperature:monitor{Boolean}=True	
multi[1]:temperature:ramping{Boolean}=False	
multi[1]:temperature:ramping on{Boolean}=False	
multi[1]:temperature:ramping on 2{Boolean}=False	
multi[1]:temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
multi[1]:temperature:stability code{U32}=6618880	
multi[1]:temperature:stability rate{Extended Float}=0.040000	
multi[1]:y{Double Float}=0.000000	
parameter: Termination{String}=False	
parameter: delta time{Double Float}=1.000000	
parameter: progress{Double Float}=100.000000	
temperature:  rate window{Double Float}=120.000000	
temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
temperature: T1{Double Float}=16.077000	
temperature: T2{Double Float}=15.928000	
temperature: T3{Double Float}=85.745000	
temperature: T4{Double Float}=62.312100	
temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
temperature: current temperature{Double Float}=1.464900	
temperature: current temperature 2{Double Float}=287.100000	
temperature: dT/dt{Double Float}=-0.010762	
temperature: gas control{Boolean}=False	
temperature: gas control 2{Boolean}=False	
temperature: gass boost{I8}=0	
temperature: gass boost 2{I8}=0	
temperature: gast flow{I16}=0	
temperature: gast flow 2{I16}=7	
temperature: heater output{Double Float}=0.000000	
temperature: heater output 2{Double Float}=0.000000	
temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
temperature: monitor timeout{Double Float}=0.010000	
temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
temperature: ramp rate{Double Float}=8.000000	
temperature: ramp rate 2{Double Float}=0.000000	
temperature: ramp target{Double Float}=20.000000	
temperature: ramp target 2{Double Float}=0.000000	
temperature: ramping{Boolean}=False	
temperature: setpoint{Double Float}=1.800000	
temperature: setpoint 2{Double Float}=287.100000	
temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
temperature: stability error{Extended Float}=0.040000	
temperature: stability script{String}=	
temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
temperature: temp control mode{U16}=2	
temperature: temp control mode 2{U16}=3	
temperature: temp control mode 2.__text__{String}=Open Loop	
temperature: temp control mode.__text__{String}=Zone	
temperature: temp control sensor{U16}=0	
temperature: temp control sensor 2{U16}=0	
temperature: temp control sensor 2.__text__{String}=Sensor 1	
temperature: temp control sensor.__text__{String}=Sensor A	
temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
temperature: temp loop{U16}=0	
temperature: temp loop 2{U16}=0	
temperature: temp loop 2.__text__{String}=Heater	
temperature: temp loop.__text__{String}=Loop 1	
temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
temperature:error for gas boost{Double Float}=0.000000	
temperature:error for gas boost 2{Double Float}=0.000000	
temperature:heater range{U16}=2	
temperature:heater range 2{U16}=0	
temperature:heater range 2.__text__{String}=Off	
temperature:heater range.__text__{String}=40mW	
temperature:history window{Extended Float}=300.000000	
temperature:is stable?{Boolean}=True	
temperature:monitor{Boolean}=True	
temperature:ramping{Boolean}=False	
temperature:ramping on{Boolean}=False	
temperature:ramping on 2{Boolean}=False	
temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
temperature:stability code{U32}=6618880	
temperature:stability rate{Extended Float}=0.040000	
y{Double Float}=16.000000	
