TDI Format 1.5	Offset	Rxx::R	Rxx::Theta	Rxx::X	Rxx::Y	Rxy::R	Rxy::Theta	Rxy::X	Rxy::Y	temperature: T1	temperature: T2	temperature: T3	temperature: T4	temperature: dT/dt	iterator	multi[0]:iterator	multi[0]:y	multi[0]:temperature: setpoint	multi[0]:temperature: T1	multi[0]:temperature: T2	multi[0]:temperature: T3	multi[0]:temperature: T4	multi[0]:temperature: heater	multi[0]:temperature: gas	multi[0]:temperature: dT/dt	multi[0]:temperature: current temperature	multi[0]:temperature: error	multi[1]:iterator	multi[1]:y	multi[1]:Control:Magnet Output
2nd Parameter Class{String}=Multi-Parameter	0E+0	1.269468804E-3	1.524E-1	1.269468804E-3	3.371767975E-6	6.058632323E-7	-8.4756E+0	5.995414148E-7	-9.114320738E-8	3.003E+1	3.2002E+1	8.56375E+1	6.16061E+1	6.2501885E-2	6.73E+2	1.2E+1	3E+1	3E+1	3.0031E+1	3.2002E+1	8.56375E+1	6.16061E+1	6.6E+0	3E+1	6.573075056E-2	3.0031E+1	-3.1E-2	0E+0	0E+0	1E-4
2nd Parameter Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	0E+0	1.271322838E-3	1.524E-1	1.271322838E-3	3.371767975E-6	7.070700116E-6	-5.46E-1	7.070700116E-6	-6.848892033E-8	3.0025E+1	3.2059E+1	8.60673E+1	6.16061E+1	4.711785913E-2	6.74E+2	1.2E+1	3E+1	1.8E+0	3.003E+1	3.2002E+1	8.56375E+1	6.16061E+1	6.6E+0	3E+1	6.2501885E-2	1.4649E+0	-3.1E-2	1E+0	5E-1	4.998E-1
Analysis Class{String}=Basic Plot	0E+0	1.27503232E-3	1.56E-1	1.27503232E-3	3.371767975E-6	1.35618838E-5	-1.68E-1	1.35618838E-5	-4.162024857E-8	3.0035E+1	3.2103E+1	8.59241E+1	6.16061E+1	3.847818077E-2	6.75E+2	1.2E+1	3E+1	1.8E+0	3.0025E+1	3.2059E+1	8.60673E+1	6.16061E+1	6.6E+0	3E+1	4.711785913E-2	1.4649E+0	-3.1E-2	2E+0	1E+0	9.999E-1
Analysis Class Path{Path}=C\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV\\\\plugins\\\\Plotting\\\\Plotting_Base_class\\\\Plotting_Base.lvclass	0E+0	1.280764128E-3	1.524E-1	1.280764128E-3	3.371767975E-6	2.005148356E-5	-1.332E-1	2.005148356E-5	-4.846914343E-8	3.0024E+1	3.2138E+1	8.55659E+1	6.16061E+1	2.872448787E-2	6.76E+2	1.2E+1	3E+1	1.8E+0	3.0035E+1	3.2103E+1	8.59241E+1	6.16061E+1	6.6E+0	3E+1	3.847818077E-2	1.4649E+0	-3.1E-2	3E+0	1.5E+0	1.4999E+0
Analysis.# pre-routines{I32}=5	0E+0	1.280764128E-3	1.548E-1	1.280764128E-3	3.371767975E-6	2.00440448E-5	-1.536E-1	2.00440448E-5	-5.479121546E-8	3.0025E+1	3.2141E+1	8.55659E+1	6.16061E+1	3.037758358E-2	6.77E+2	1.2E+1	3E+1	1.8E+0	3.0024E+1	3.2138E+1	8.55659E+1	6.16061E+1	6.6E+0	3E+1	2.872448787E-2	1.4649E+0	-3.1E-2	4E+0	1.5E+0	1.5E+0
Analysis:Pre[0]:T Control Measure{1D Array (I32)}=[1,2,3,4,7]	0E+0	1.278403806E-3	1.524E-1	1.278403806E-3	3.371767975E-6	1.743414195E-5	-1.428E-1	1.743414195E-5	-4.478129873E-8	3.0024E+1	3.2157E+1	8.57092E+1	6.16061E+1	2.944261022E-2	6.78E+2	1.2E+1	3E+1	1.8E+0	3.0025E+1	3.2141E+1	8.55659E+1	6.16061E+1	6.6E+0	3E+1	3.037758358E-2	1.4649E+0	-3.1E-2	5E+0	1.3E+0	1.3001E+0
Autosave Tabs{Enum U32 ((XY Measurement Save,Parameter Plot Save 2))}=Parameter Plot Save 2	0E+0	1.276380066E-3	1.512E-1	1.276380066E-3	3.371767975E-6	1.484898785E-5	-2.124E-1	1.484898785E-5	-5.637174054E-8	3.0025E+1	3.2167E+1	8.59599E+1	6.16061E+1	2.196332067E-2	6.79E+2	1.2E+1	3E+1	1.8E+0	3.0024E+1	3.2157E+1	8.57092E+1	6.16061E+1	6.6E+0	3E+1	2.944261022E-2	1.4649E+0	-3.1E-2	6E+0	1.1E+0	1.1001E+0
Control:Magnet Output{Double Float}=-0.007000	0E+0	1.274526032E-3	1.512E-1	1.274526032E-3	3.371767975E-6	1.224795212E-5	-2.7E-1	1.224795212E-5	-5.953276241E-8	3.0027E+1	3.2181E+1	8.59241E+1	6.16061E+1	2.249444835E-2	6.8E+2	1.2E+1	3E+1	1.8E+0	3.0025E+1	3.2167E+1	8.59599E+1	6.16061E+1	6.6E+0	3E+1	2.196332067E-2	1.4649E+0	-3.1E-2	7E+0	9E-1	9.001E-1
Control:Magnet Rate{Double Float}=0.500000	0E+0	1.273176872E-3	1.536E-1	1.273176872E-3	3.371767975E-6	9.652723155E-6	-3.768E-1	9.652723155E-6	-6.532801159E-8	3.0021E+1	3.2194E+1	8.58883E+1	6.16061E+1	2.224576101E-2	6.81E+2	1.2E+1	3E+1	1.8E+0	3.0027E+1	3.2181E+1	8.59241E+1	6.16061E+1	6.6E+0	3E+1	2.249444835E-2	1.4649E+0	-3.1E-2	8E+0	7E-1	7E-1
Display Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	0E+0	1.271997418E-3	1.5E-1	1.271997418E-3	3.371767975E-6	7.064907498E-6	-6.732E-1	7.064907498E-6	-8.482102222E-8	3.0018E+1	3.2203E+1	8.58883E+1	6.16061E+1	1.803190634E-2	6.82E+2	1.2E+1	3E+1	1.8E+0	3.0021E+1	3.2194E+1	8.58883E+1	6.16061E+1	6.6E+0	3E+1	2.224576101E-2	1.4649E+0	-3.1E-2	9E+0	5E-1	5.001E-1
Elapsed Time{Double Float}=12790.950867	0E+0	1.271154547E-3	1.5E-1	1.271154547E-3	3.371767975E-6	4.473383772E-6	-1.104E+0	4.473383772E-6	-8.798212894E-8	3.0018E+1	3.2213E+1	8.56375E+1	6.16061E+1	1.85593646E-2	6.83E+2	1.2E+1	3E+1	1.8E+0	3.0018E+1	3.2203E+1	8.58883E+1	6.16061E+1	6.6E+0	3E+1	1.803190634E-2	1.4649E+0	-3.1E-2	1E+1	3E-1	3E-1
File:Autodel{Boolean}=True	0E+0	1.270479967E-3	1.5E-1	1.270479967E-3	3.371767975E-6	1.866060452E-6	-2.0244E+0	1.865008278E-6	-6.690845182E-8	3.0019E+1	3.2222E+1	8.58166E+1	6.16061E+1	1.717623509E-2	6.84E+2	1.2E+1	3E+1	1.8E+0	3.0018E+1	3.2213E+1	8.56375E+1	6.16061E+1	6.6E+0	3E+1	1.85593646E-2	1.4649E+0	-3.1E-2	1.1E+1	1E-1	1.001E-1
File:Autosave{Boolean}=False	0E+0	1.270479967E-3	1.56E-1	1.270479967E-3	3.371767975E-6	1.877651347E-6	-2.5896E+0	1.875546997E-6	-8.640146245E-8	3.0018E+1	3.2224E+1	8.59957E+1	6.16061E+1	1.807773672E-2	6.85E+2	1.2E+1	3E+1	1.8E+0	3.0019E+1	3.2222E+1	8.58166E+1	6.16061E+1	6.6E+0	3E+1	1.717623509E-2	1.4649E+0	-3.1E-2	1.2E+1	1E-1	1E-1
File:Export Config{Boolean}=True	0E+0	1.270479967E-3	1.5E-1	1.270479967E-3	3.371767975E-6	1.734880831E-6	-2.7084E+0	1.73329974E-6	-8.324046886E-8	3.0018E+1	3.2226E+1	8.60315E+1	6.16061E+1	1.683806255E-2	6.86E+2	1.2E+1	3E+1	1.8E+0	3.0018E+1	3.2224E+1	8.59957E+1	6.16061E+1	6.6E+0	3E+1	1.807773672E-2	1.4649E+0	-3.1E-2	1.3E+1	9E-2	9.01E-2
File:Final Autosave{Boolean}=True	0E+0	1.270479967E-3	1.512E-1	1.270479967E-3	3.371767975E-6	1.612127094E-6	-2.6976E+0	1.609496656E-6	-7.744527624E-8	3.0018E+1	3.223E+1	8.59599E+1	6.16061E+1	1.831972227E-2	6.87E+2	1.2E+1	3E+1	1.8E+0	3.0018E+1	3.2226E+1	8.60315E+1	6.16061E+1	6.6E+0	3E+1	1.683806255E-2	1.4649E+0	-3.1E-2	1.4E+1	8E-2	8.01E-2
Filter:Enable{Enum U16 ((None,Analog,Digital,Analog&Digitial))}=None	0E+0	1.270479967E-3	1.512E-1	1.270479967E-3	3.371767975E-6	1.497275982E-6	-2.9952E+0	1.495171632E-6	-7.955262415E-8	3.0017E+1	3.2232E+1	8.59599E+1	6.16061E+1	1.736902632E-2	6.88E+2	1.2E+1	3E+1	1.8E+0	3.0018E+1	3.223E+1	8.59599E+1	6.16061E+1	6.6E+0	3E+1	1.831972227E-2	1.4649E+0	-3.1E-2	1.5E+1	7E-2	7E-2
Filter:Points{I32}=1	0E+0	1.270479967E-3	1.5E-1	1.270479967E-3	3.371767975E-6	1.364514421E-6	-3.8796E+0	1.361880024E-6	-9.377737813E-8	3.0016E+1	3.2235E+1	8.59599E+1	6.16061E+1	1.740885898E-2	6.89E+2	1.2E+1	3E+1	1.8E+0	3.0017E+1	3.2232E+1	8.59599E+1	6.16061E+1	6.6E+0	3E+1	1.736902632E-2	1.4649E+0	-3.1E-2	1.6E+1	6E-2	6.01E-2
Filter:Type{U16}=1	0E+0	1.270479967E-3	1.512E-1	1.270479967E-3	3.371767975E-6	1.236488495E-6	-3.3636E+0	1.234381034E-6	-7.42841978E-8	3.0016E+1	3.2237E+1	8.59241E+1	6.16061E+1	1.614658535E-2	6.9E+2	1.2E+1	3E+1	1.8E+0	3.0016E+1	3.2235E+1	8.59599E+1	6.16061E+1	6.6E+0	3E+1	1.740885898E-2	1.4649E+0	-3.1E-2	1.7E+1	5E-2	5.01E-2
Filter:Type.__text__{String}=Repeat	0E+0	1.270479967E-3	1.512E-1	1.270479967E-3	3.371767975E-6	1.215414733E-6	-3.8232E+0	1.212780902E-6	-8.218676662E-8	3.0017E+1	3.2239E+1	8.58883E+1	6.16061E+1	1.72874555E-2	6.91E+2	1.2E+1	3E+1	1.8E+0	3.0016E+1	3.2237E+1	8.59241E+1	6.16061E+1	6.6E+0	3E+1	1.614658535E-2	1.4649E+0	-3.1E-2	1.8E+1	5E-2	5E-2
Filter:Window{Double Float}=1.000000	0E+0	1.270479967E-3	1.536E-1	1.270479967E-3	3.371767975E-6	1.156409218E-6	-4.1784E+0	1.153248451E-6	-8.587469618E-8	3.0016E+1	3.2241E+1	8.59241E+1	6.16061E+1	1.649027131E-2	6.92E+2	1.2E+1	3E+1	1.8E+0	3.0017E+1	3.2239E+1	8.58883E+1	6.16061E+1	6.6E+0	3E+1	1.72874555E-2	1.4649E+0	-3.1E-2	1.9E+1	4.5E-2	4.49E-2
Iterator{I32}=0	0E+0	1.270547284E-3	1.5E-1	1.270547284E-3	3.371767975E-6	1.084233132E-6	-3.7596E+0	1.081598735E-6	-7.270370101E-8	3.0016E+1	3.2243E+1	8.58883E+1	6.16061E+1	1.549024135E-2	6.93E+2	1.2E+1	3E+1	1.8E+0	3.0016E+1	3.2241E+1	8.59241E+1	6.16061E+1	6.6E+0	3E+1	1.649027131E-2	1.4649E+0	-3.1E-2	2E+1	4E-2	4E-2
Magnet: Control Mode{Boolean}=False	0E+0	1.270479967E-3	1.5E-1	1.270479967E-3	3.371767975E-6	1.026807859E-6	-4.3644E+0	1.024173745E-6	-7.95525393E-8	3.0017E+1	3.2245E+1	8.58883E+1	6.16061E+1	1.4435146E-2	6.94E+2	1.2E+1	3E+1	1.8E+0	3.0016E+1	3.2243E+1	8.58883E+1	6.16061E+1	6.6E+0	3E+1	1.549024135E-2	1.4649E+0	-3.1E-2	2.1E+1	3.5E-2	3.5E-2
Magnet: Final Switch Heater{Enum U8 ((False,True,Mixed))}=	0E+0	1.270479967E-3	1.5E-1	1.270479967E-3	3.371767975E-6	9.583191931E-7	-4.788E+0	9.551578601E-7	-8.165994378E-8	3.0025E+1	3.2248E+1	8.58883E+1	6.16061E+1	1.563533768E-2	6.95E+2	1.2E+1	3E+1	1.8E+0	3.0017E+1	3.2245E+1	8.58883E+1	6.16061E+1	6.6E+0	3E+1	1.4435146E-2	1.4649E+0	-3.1E-2	2.2E+1	3E-2	3E-2
Magnet: Power Supply{Enum U16 ((IPS120,LS625,PS110,Hg iPS,SMS Series,Cryomagnetics 4G,DMG Little CryoFree,DMG Big CryoFree))}=Hg iPS	0E+0	1.270547284E-3	1.5E-1	1.270547284E-3	3.371767975E-6	9.124845316E-7	-4.7964E+0	9.093234814E-7	-7.744527624E-8	3.0022E+1	3.2252E+1	8.58883E+1	6.16061E+1	1.799326763E-2	6.96E+2	1.2E+1	3E+1	1.8E+0	3.0025E+1	3.2248E+1	8.58883E+1	6.16061E+1	6.6E+0	3E+1	1.563533768E-2	1.4649E+0	-3.1E-2	2.3E+1	2.5E-2	2.49E-2
Magnet: Rate{Double Float}=0.500000	0E+0	1.270547284E-3	1.536E-1	1.270547284E-3	3.371767975E-6	8.29244487E-7	-5.3724E+0	8.255565008E-7	-7.902568818E-8	3.0029E+1	3.225E+1	8.58883E+1	6.16061E+1	1.143235434E-2	6.97E+2	1.2E+1	3E+1	1.8E+0	3.0022E+1	3.2252E+1	8.58883E+1	6.16061E+1	6.6E+0	3E+1	1.799326763E-2	1.4649E+0	-3.1E-2	2.4E+1	2E-2	1.99E-2
Magnet: Setpoint{Double Float}=0.000000	0E+0	1.270648258E-3	1.548E-1	1.270648258E-3	3.371767975E-6	7.818290175E-7	-5.5872E+0	7.791951862E-7	-7.691836855E-8	3.004E+1	3.2253E+1	8.58883E+1	6.16061E+1	1.262372173E-2	6.98E+2	1.2E+1	3E+1	1.8E+0	3.0029E+1	3.225E+1	8.58883E+1	6.16061E+1	6.6E+0	3E+1	1.143235434E-2	1.4649E+0	-3.1E-2	2.5E+1	1.5E-2	1.48E-2
Magnet: Units{Enum U16 ((Field,Current))}=Field	0E+0	1.270513625E-3	1.56E-1	1.270513625E-3	3.371767975E-6	7.133406346E-7	-6.5868E+0	7.085990593E-7	-8.376734826E-8	3.0051E+1	3.2254E+1	8.58883E+1	6.16061E+1	1.059813797E-2	6.99E+2	1.2E+1	3E+1	1.8E+0	3.004E+1	3.2253E+1	8.58883E+1	6.16061E+1	6.6E+0	3E+1	1.262372173E-2	1.4649E+0	-3.1E-2	2.6E+1	1E-2	1E-2
Magnet: VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	0E+0	1.270648258E-3	1.5E-1	1.270648258E-3	3.371767975E-6	6.395811949E-7	-8.2908E+0	6.327321586E-7	-9.325047044E-8	3.0072E+1	3.2258E+1	8.56017E+1	6.16061E+1	1.315735281E-2	7E+2	1.2E+1	3E+1	1.8E+0	3.0051E+1	3.2254E+1	8.58883E+1	6.16061E+1	6.6E+0	3E+1	1.059813797E-2	1.4649E+0	-3.1E-2	2.7E+1	5E-3	4.9E-3
Main Screen Path{Path}=C:\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV\\\\1Code.vi	0E+0	1.270648258E-3	1.5E-1	1.270648258E-3	3.371767975E-6	5.958534287E-7	-9.126E+0	5.890046752E-7	-9.588464119E-8	3.0153E+1	3.2238E+1	8.56375E+1	6.16061E+1	-2.019691654E-2	7.01E+2	1.2E+1	3E+1	1.8E+0	3.0072E+1	3.2258E+1	8.56017E+1	6.16061E+1	6.6E+0	3E+1	1.315735281E-2	1.4649E+0	-3.1E-2	2.8E+1	0E+0	-1E-4
Measurement Timestamp{Timestamp}=<01:09:24.342 18/05/2023>T	0E+0	1.270648258E-3	1.524E-1	1.270648258E-3	3.371767975E-6	5.163013702E-7	-9.108E+0	5.089259636E-7	-8.324052543E-8	3.0225E+1	3.2245E+1	8.56375E+1	6.16061E+1	-1.047209743E-2	7.02E+2	1.2E+1	3E+1	1.8E+0	3.0153E+1	3.2238E+1	8.56375E+1	6.16061E+1	6.6E+0	3E+1	-2.019691654E-2	1.4649E+0	-3.1E-2	2.9E+1	-5E-3	-5E-3
Measurement Title{String}=	0E+0	1.270648258E-3	1.548E-1	1.270648258E-3	3.371767975E-6	4.509737546E-7	-1.03116E+1	4.441250011E-7	-8.218671005E-8	3.0245E+1	3.2263E+1	8.57092E+1	6.16061E+1	1.738925092E-2	7.03E+2	1.2E+1	3E+1	1.8E+0	3.0225E+1	3.2245E+1	8.56375E+1	6.16061E+1	6.6E+0	3E+1	-1.047209743E-2	1.4649E+0	-3.1E-2	3E+1	-1E-2	-1.01E-2
Measurment Select{U16}=4	0E+0	1.27081655E-3	1.512E-1	1.27081655E-3	3.371767975E-6	3.772165776E-7	-1.18608E+1	3.693145179E-7	-7.902571646E-8	3.0197E+1	3.2309E+1	8.5745E+1	6.16061E+1	8.571923524E-2	7.04E+2	1.2E+1	3E+1	1.8E+0	3.0245E+1	3.2263E+1	8.57092E+1	6.16061E+1	6.6E+0	3E+1	1.738925092E-2	1.4649E+0	-3.1E-2	3.1E+1	-1.5E-2	-1.5E-2
Measurment Select.__text__{String}=6221-Lockin-DAQ	0E+0	1.27081655E-3	1.524E-1	1.27081655E-3	3.371767975E-6	3.113608946E-7	-1.5192E+1	3.002975019E-7	-8.324052543E-8	2.9988E+1	3.2309E+1	8.57092E+1	6.16061E+1	8.276800066E-2	7.05E+2	1.2E+1	3E+1	1.8E+0	3.0197E+1	3.2309E+1	8.5745E+1	6.16061E+1	6.6E+0	3E+1	8.571923524E-2	1.4649E+0	-3.1E-2	3.2E+1	-2E-2	-2.01E-2
Notes{String}=I+1A I-1E\\nrxx+1B Rxx-1C\\nRxy+1D Rxy-4A	0E+0	1.270715575E-3	1.524E-1	1.270715575E-3	3.371767975E-6	2.560433655E-7	-1.73328E+1	2.449799728E-7	-7.797204251E-8	2.9759E+1	3.2273E+1	8.60315E+1	6.16061E+1	2.440401167E-2	7.06E+2	1.2E+1	3E+1	1.8E+0	2.9988E+1	3.2309E+1	8.57092E+1	6.16061E+1	6.6E+0	3E+1	8.276800066E-2	1.4649E+0	-3.1E-2	3.3E+1	-2.5E-2	-2.51E-2
Offset{Double Float}=0.000000	0E+0	1.270479967E-3	1.536E-1	1.270479967E-3	3.371767975E-6	1.849205855E-7	-2.31696E+1	1.69641705E-7	-7.428411295E-8	2.9591E+1	3.2214E+1	8.59599E+1	6.16061E+1	-7.401507348E-2	7.07E+2	1.2E+1	3E+1	1.8E+0	2.9759E+1	3.2273E+1	8.60315E+1	6.16061E+1	6.6E+0	3E+1	2.440401167E-2	1.4649E+0	-3.1E-2	3.4E+1	-3E-2	-3E-2
Option: 2182 Autozero{Boolean}=True	0E+0	1.270345334E-3	1.5E-1	1.270345334E-3	3.371767975E-6	1.327632297E-7	-4.0212E+1	1.00626273E-7	-8.90358029E-8	2.9548E+1	3.2165E+1	8.59599E+1	6.16061E+1	-1.629709452E-1	7.08E+2	1.2E+1	3E+1	1.8E+0	2.9591E+1	3.2214E+1	8.59599E+1	6.16061E+1	6.6E+0	3E+1	-7.401507348E-2	1.4649E+0	-3.1E-2	3.5E+1	-3.5E-2	-3.51E-2
Option: 2182 Front Autozero{Boolean}=True	0E+0	1.270311676E-3	1.548E-1	1.270311676E-3	3.371767975E-6	1.022067698E-7	-6.83592E+1	3.687872991E-8	-9.799207396E-8	2.9568E+1	3.2147E+1	8.59241E+1	6.16061E+1	-1.924740374E-1	7.09E+2	1.2E+1	3E+1	1.8E+0	2.9548E+1	3.2165E+1	8.59599E+1	6.16061E+1	6.6E+0	3E+1	-1.629709452E-1	1.4649E+0	-3.1E-2	3.6E+1	-4E-2	-4.04E-2
Option: 2182 Hold{Boolean}=False	0E+0	1.270311676E-3	1.548E-1	1.270311676E-3	3.371767975E-6	8.692837014E-8	-1.11864E+2	-3.4771382E-8	-8.324052543E-8	2.9626E+1	3.214E+1	8.59241E+1	6.16061E+1	-1.984475404E-1	7.1E+2	1.2E+1	3E+1	1.8E+0	2.9568E+1	3.2147E+1	8.59241E+1	6.16061E+1	6.6E+0	3E+1	-1.924740374E-1	1.4649E+0	-3.1E-2	3.7E+1	-4.5E-2	-4.52E-2
Option: 2182 Hold Count{I32}=10	0E+0	1.270311676E-3	1.512E-1	1.270311676E-3	3.371767975E-6	1.116898354E-7	-1.359324E+2	-8.271367431E-8	-7.955259587E-8	2.9684E+1	3.2142E+1	8.59241E+1	6.16061E+1	-1.749477237E-1	7.11E+2	1.2E+1	3E+1	1.8E+0	2.9626E+1	3.214E+1	8.59241E+1	6.16061E+1	6.6E+0	3E+1	-1.984475404E-1	1.4649E+0	-3.1E-2	3.8E+1	-5E-2	-5.01E-2
Option: 2182 Hold Window{Double Float}=1.000000	0E+0	1.270311676E-3	1.5E-1	1.270311676E-3	3.371767975E-6	1.127434528E-7	-1.328892E+2	-8.007953184E-8	-8.482099394E-8	2.9709E+1	3.2144E+1	8.58883E+1	6.16061E+1	-1.580028683E-1	7.12E+2	1.2E+1	3E+1	1.8E+0	2.9684E+1	3.2142E+1	8.59241E+1	6.16061E+1	6.6E+0	3E+1	-1.749477237E-1	1.4649E+0	-3.1E-2	3.9E+1	-5E-2	-5E-2
Option: 2182 Line Sync{Boolean}=False	0E+0	1.270311676E-3	1.5E-1	1.270311676E-3	3.371767975E-6	2.202187903E-7	-1.599768E+2	-2.086281788E-7	-7.691842512E-8	2.9769E+1	3.216E+1	8.58883E+1	6.16061E+1	-8.202643692E-2	7.13E+2	1.2E+1	3E+1	1.8E+0	2.9709E+1	3.2144E+1	8.58883E+1	6.16061E+1	6.6E+0	3E+1	-1.580028683E-1	1.4649E+0	-3.1E-2	4E+1	-6E-2	-5.99E-2
Option: 2182 Reference Reading{Double Float}=0.000000	0E+0	1.270345334E-3	1.524E-1	1.270345334E-3	3.371767975E-6	3.587772126E-7	-1.641132E+2	-3.477141028E-7	-9.957257075E-8	2.9815E+1	3.2179E+1	8.58883E+1	6.16061E+1	-2.766742138E-3	7.14E+2	1.2E+1	3E+1	1.8E+0	2.9769E+1	3.216E+1	8.58883E+1	6.16061E+1	6.6E+0	3E+1	-8.202643692E-2	1.4649E+0	-3.1E-2	4.1E+1	-7E-2	-7E-2
Option: 2182 Relative Mode{Boolean}=False	0E+0	1.270479967E-3	1.5E-1	1.270479967E-3	3.371767975E-6	4.873252657E-7	-1.693416E+2	-4.820573202E-7	-9.219685306E-8	2.9869E+1	3.2202E+1	8.58883E+1	6.16061E+1	6.33585602E-2	7.15E+2	1.2E+1	3E+1	1.8E+0	2.9815E+1	3.2179E+1	8.58883E+1	6.16061E+1	6.6E+0	3E+1	-2.766742138E-3	1.4649E+0	-3.1E-2	4.2E+1	-8E-2	-8E-2
Option: 2182 Trigger Delay{Cluster (Boolean,Double Float)}={'Auto':True,'Time(s)':0.000000}	0E+0	1.270648258E-3	1.536E-1	1.270648258E-3	3.371767975E-6	6.148200124E-7	-1.723956E+2	-6.121853326E-7	-8.324052543E-8	2.9897E+1	3.2226E+1	8.58524E+1	6.16061E+1	1.063928306E-1	7.16E+2	1.2E+1	3E+1	1.8E+0	2.9869E+1	3.2202E+1	8.58883E+1	6.16061E+1	6.6E+0	3E+1	6.33585602E-2	1.4649E+0	-3.1E-2	4.3E+1	-9E-2	-8.99E-2
Option: 2182 Trigger Source{Enum U16 ((Immediate,Timer,Manual,Bus,Trigger link))}=Bus	0E+0	1.270715575E-3	1.524E-1	1.270715575E-3	3.371767975E-6	7.359943559E-7	-1.726176E+2	-7.317797167E-7	-9.588475433E-8	2.9924E+1	3.2246E+1	8.58524E+1	6.16061E+1	1.246122867E-1	7.17E+2	1.2E+1	3E+1	1.8E+0	2.9897E+1	3.2226E+1	8.58524E+1	6.16061E+1	6.6E+0	3E+1	1.063928306E-1	1.4649E+0	-3.1E-2	4.4E+1	-1E-1	-1E-1
Option: 2182 Trigger Timer{Double Float}=0.000000	0E+0	1.27081655E-3	1.512E-1	1.27081655E-3	3.371767975E-6	7.359943559E-7	-1.727652E+2	-7.323066527E-7	-9.430411612E-8	2.993E+1	3.2256E+1	8.58883E+1	6.16061E+1	1.306976825E-1	7.18E+2	1.2E+1	3E+1	1.8E+0	2.9924E+1	3.2246E+1	8.58524E+1	6.16061E+1	6.6E+0	3E+1	1.246122867E-1	1.4649E+0	-3.1E-2	4.5E+1	-1E-1	-1E-1
Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	0E+0	1.271457471E-3	1.512E-1	1.271457471E-3	3.371767975E-6	3.325407226E-6	-1.78278E+2	-3.326459401E-6	-1.011530675E-7	2.9991E+1	3.2317E+1	8.58524E+1	6.16061E+1	1.201767996E-1	7.19E+2	1.2E+1	3E+1	1.8E+0	2.993E+1	3.2256E+1	8.58883E+1	6.16061E+1	6.6E+0	3E+1	1.306976825E-1	1.4649E+0	-3.1E-2	4.6E+1	-3E-1	-2.999E-1
Option: 560 Enabled{Boolean}=False	0E+0	1.272502292E-3	1.56E-1	1.272502292E-3	3.371767975E-6	5.89058981E-6	-1.789596E+2	-5.893223076E-6	-1.085287852E-7	3.0022E+1	3.2361E+1	8.56375E+1	6.16061E+1	8.849421144E-2	7.2E+2	1.2E+1	3E+1	1.8E+0	2.9991E+1	3.2317E+1	8.58524E+1	6.16061E+1	6.6E+0	3E+1	1.201767996E-1	1.4649E+0	-3.1E-2	4.7E+1	-5E-1	-4.998E-1
Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	0E+0	1.273683161E-3	1.512E-1	1.273683161E-3	3.371767975E-6	8.482093737E-6	-1.792956E+2	-8.484729831E-6	-1.053677634E-7	3.0043E+1	3.2397E+1	8.60315E+1	6.16061E+1	6.892291456E-2	7.21E+2	1.2E+1	3E+1	1.8E+0	3.0022E+1	3.2361E+1	8.56375E+1	6.16061E+1	6.6E+0	3E+1	8.849421144E-2	1.4649E+0	-3.1E-2	4.8E+1	-7E-1	-6.999E-1
Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	0E+0	1.275200612E-3	1.536E-1	1.275200612E-3	3.371767975E-6	1.106099702E-5	-1.794528E+2	-1.106362746E-5	-1.069482885E-7	3.0045E+1	3.2419E+1	8.59241E+1	6.16061E+1	4.624034464E-2	7.22E+2	1.2E+1	3E+1	1.8E+0	3.0043E+1	3.2397E+1	8.60315E+1	6.16061E+1	6.6E+0	3E+1	6.892291456E-2	1.4649E+0	-3.1E-2	4.9E+1	-9E-1	-9E-1
Option: 6221 Adjust Mode{Enum U16 ((Offset,Frequency,Amplitude))}=Offset	0E+0	1.277054646E-3	1.512E-1	1.277054646E-3	3.371767975E-6	1.363880287E-5	-1.7946E+2	-1.364143897E-5	-1.296020947E-7	3.0042E+1	3.2433E+1	8.58524E+1	6.16061E+1	2.833721414E-2	7.23E+2	1.2E+1	3E+1	1.8E+0	3.0045E+1	3.2419E+1	8.59241E+1	6.16061E+1	6.6E+0	3E+1	4.624034464E-2	1.4649E+0	-3.1E-2	5E+1	-1.1E+0	-1.0998E+0
Option: 6221 Amplitude{Double Float}=1.000000E-6	0E+0	1.279246677E-3	1.512E-1	1.279246677E-3	3.371767975E-6	1.62308442E-5	-1.795572E+2	-1.623347464E-5	-1.264411859E-7	3.0055E+1	3.2443E+1	8.58524E+1	6.16061E+1	1.932519861E-2	7.24E+2	1.2E+1	3E+1	1.8E+0	3.0042E+1	3.2433E+1	8.58524E+1	6.16061E+1	6.6E+0	3E+1	2.833721414E-2	1.4649E+0	-3.1E-2	5.1E+1	-1.3E+0	-1.2999E+0
Option: 6221 Compliance{Double Float}=10.000000	0E+0	1.281606999E-3	1.548E-1	1.281606999E-3	3.371767975E-6	1.882810398E-5	-1.795908E+2	-1.883079098E-5	-1.359241384E-7	3.0043E+1	3.245E+1	8.55301E+1	6.16061E+1	1.477081794E-2	7.25E+2	1.2E+1	3E+1	1.8E+0	3.0055E+1	3.2443E+1	8.58524E+1	6.16061E+1	6.6E+0	3E+1	1.932519861E-2	1.4649E+0	-3.1E-2	5.2E+1	-1.5E+0	-1.4998E+0
Option: 6221 Duty Cycle{Double Float}=50.000000	0E+0	1.281606999E-3	1.524E-1	1.281606999E-3	3.371767975E-6	1.8808107E-5	-1.795908E+2	-1.8810794E-5	-1.364510744E-7	3.0043E+1	3.245E+1	8.55301E+1	6.16061E+1	1.362075098E-2	7.26E+2	1.2E+1	3E+1	1.8E+0	3.0043E+1	3.245E+1	8.55301E+1	6.16061E+1	6.6E+0	3E+1	1.477081794E-2	1.4649E+0	-3.1E-2	5.3E+1	-1.5E+0	-1.4999E+0
Option: 6221 External Trigger{Boolean}=False	0E+0	1.276211775E-3	1.512E-1	1.276211775E-3	3.371767975E-6	1.235121799E-5	-1.794924E+2	-1.235385126E-5	-1.106361332E-7	3.0043E+1	3.2456E+1	8.59241E+1	6.16061E+1	4.29484155E-3	7.27E+2	1.2E+1	3E+1	1.8E+0	3.0043E+1	3.245E+1	8.55301E+1	6.16061E+1	6.6E+0	3E+1	1.362075098E-2	1.4649E+0	-3.1E-2	5.4E+1	-1E+0	-1.0001E+0
Option: 6221 External Trigger Ignore Multiple{Boolean}=False	0E+0	1.272840289E-3	1.5E-1	1.272840289E-3	3.371767975E-6	5.872677381E-6	-1.79094E+2	-5.875313475E-6	-9.430420097E-8	3.0031E+1	3.2458E+1	8.58166E+1	6.16061E+1	1.789073693E-3	7.28E+2	1.2E+1	3E+1	1.8E+0	3.0043E+1	3.2456E+1	8.59241E+1	6.16061E+1	6.6E+0	3E+1	4.29484155E-3	1.4649E+0	-3.1E-2	5.5E+1	-5E-1	-5.001E-1
Option: 6221 Frequency{Double Float}=119.770000	
Option: 6221 Function{U16}=1	
Option: 6221 Function.__text__{String}=Sine	
Option: 6221 Idle Level{Double Float}=0.000000	
Option: 6221 Input trigger Line{U8}=5	
Option: 6221 Offset{Double Float}=0.000000	
Option: 6221 Output Trigger Line{U8}=4	
Option: 6221 Pass Through{Boolean}=True	
Option: 6221 Phase Marker{Boolean}=True	
Option: 6221 Phase Marker Phase{Double Float}=0.000000	
Option: 6221 Range Level{Double Float}=2.000000E-12	
Option: 6221 Ranging{U16}=1	
Option: 6221 Ranging.__text__{String}=Best	
Option: 6221 Update Clock{Double Float}=0.000000	
Option: 6221 VISA{Visa Refnum (Void)}=GPIB0::13::INSTR	
Option: Confirm Config{Boolean}=False	
Option: Control Panel Ref{LVObjVI Refnum (Void)}=	
Option: DAQ Global Channel{Boolean}=False	
Option: DAQ Input Rate{Double Float}=10000.000000	
Option: DAQ Input Samples{I32}=200	
Option: DAQ Measurement Channels{1D Array (Cluster (UserDefinedRefnumTag Refnum (Void),\tkDAQmxPhysChanTagType Tag,\tkDAQmxScaleTagType Tag,Boolean,Double Float,String))}=[]	
Option: Differential{I32}=10106	
Option: Differential.__text__{String}=Differential	
Option: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values))}=Function Generator	
Option: Lockin Standoff Time{Double Float}=0.000000	
Option: Paranoid Save Data{Boolean}=True	
Option: Plot Autoback Path{Path}=C:\\\\TEMP\\\\XY Multiparam\\\\Backup.txt	
Option: SR830  Ref Phase{Double Float}=0.000000	
Option: SR830  Synch Filter{Boolean}=False	
Option: SR830  Time Constant{I16}=8	
Option: SR830  Time Constant.__text__{String}=100 ms	
Option: SR830 2x Line Filter{Boolean}=True	
Option: SR830 Adjust Gains{Boolean}=False	
Option: SR830 Auto Gain Lower.__text__{String}=2 nV/fA	
Option: SR830 Auto Gain Upper.__text__{String}=1 V/uA	
Option: SR830 Auto Offset 1{Boolean}=False	
Option: SR830 Auto Offset 2{Boolean}=False	
Option: SR830 Autophase{Boolean}=False	
Option: SR830 DC Coupling?{Boolean}=False	
Option: SR830 Display 1{U16}=0	
Option: SR830 Display 1.__text__{String}=X	
Option: SR830 Display 2{U16}=0	
Option: SR830 Display 2.__text__{String}=Y	
Option: SR830 Dynamic Reserve{I16}=1	
Option: SR830 Dynamic Reserve.__text__{String}=Normal	
Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Option: SR830 Filter Slope{I32}=1	
Option: SR830 Filter Slope.__text__{String}=12 dB/oct	
Option: SR830 Gain{I32}=-1	
Option: SR830 Gain.__text__{String}=Auto Gain	
Option: SR830 Ground Shield?{Boolean}=False	
Option: SR830 Harmonic{I32}=1	
Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A	
Option: SR830 Line Filter{Boolean}=True	
Option: SR830 No Reset{Boolean}=False	
Option: SR830 Offset 1{Double Float}=0.000000	
Option: SR830 Offset 2{Double Float}=0.000000	
Option: SR830 Output Channel 1{Boolean}=False	
Option: SR830 Output Channel 2{Boolean}=False	
Option: SR830 Ratio 1{U16}=0	
Option: SR830 Ratio 1.__text__{String}=None	
Option: SR830 Ratio 2{U16}=0	
Option: SR830 Ratio 2.__text__{String}=None	
Option: SR830 Ref Amplitude{Double Float}=0.100000	
Option: SR830 Ref Frequency{Double Float}=1013.000000	
Option: SR830 Ref Source{Boolean}=False	
Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta]	
Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Option: SR830 VISA{Visa Refnum (Void)}=	
Option: Sense Autorange{Boolean}=False	
Option: Sense Range Level{Double Float}=0.100000	
Option: Sense Rate{Double Float}=1.000000	
Option:560 Comport{Visa Refnum (Void)}=COM1	
Option:560 Filter High Pass{U16}=0	
Option:560 Filter High Pass.__text__{String}=0.03	
Option:560 Filter Lowpass{U16}=0	
Option:560 Filter Lowpass.__text__{String}=0.03	
Option:560 Filter Mode{U16}=0	
Option:560 Filter Mode.__text__{String}=6 dB high pass	
Option:560 Invert{Boolean}=False	
Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Option:570 Enabled{Boolean}=False	
Option:570 Filter High Pass{U16}=0	
Option:570 Filter High Pass.__text__{String}=0.03	
Option:570 Filter Lowpass{U16}=0	
Option:570 Filter Lowpass.__text__{String}=0.03	
Option:570 Filter Mode{U16}=0	
Option:570 Filter Mode.__text__{String}=6 dB high pass	
Option:570 Gain Mode{U16}=0	
Option:570 Gain Mode.__text__{String}=Low Noise	
Option:570 Input Offset{U16}=0	
Option:570 Input Offset On{Boolean}=False	
Option:570 Input Offset.__text__{String}=1pA	
Option:570 Sensitivity{U16}=0	
Option:570 Sensitivity.__text__{String}=1pA/V	
Option:Debug On{Boolean}=False	
Option:GPIB 2182{Visa Refnum (Void)}=	
Option:Parallel Config Voltage Measurers{Boolean}=True	
Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Option:SR830 Settle Time{Double Float}=5.000000	
Option:Sense Digits{I32}=8	
Output Names{1D Array (String)}=['Offset','Rxx::R','Rxx::Theta','Rxx::X','Rxx::Y','Rxy::R','Rxy::Theta','Rxy::X','Rxy::Y','temperature: T1','temperature: T2','temperature: T3','temperature: T4','temperature: dT/dt','iterator','multi[0]:iterator','multi[0]:y','multi[0]:temperature: setpoint','multi[0]:temperature: T1','multi[0]:temperature: T2','multi[0]:temperature: T3','multi[0]:temperature: T4','multi[0]:temperature: heater','multi[0]:temperature: gas','multi[0]:temperature: dT/dt','multi[0]:temperature: current temperature','multi[0]:temperature: error','multi[1]:iterator','multi[1]:y','multi[1]:Control:Magnet Output']	
Parameter Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Parameter Select{U16}=6	
Parameter Select.__text__{String}=Multi-Parameter	
Paths{U32}=0	
Plot: Column Renames{1D Array (Cluster (String,String))}=[]	
Plot: No dups{Boolean}=False	
Plot: StdDevs{Boolean}=False	
Plotting Class{String}=Parameter Plot	
Plotting Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	
Plotting Select{U16}=1	
Plotting Select.__text__{String}=Parameter Plot	
Project Code{String}=Topological_Insulators	
Ref: Temperature Window{LVObjVI Refnum (Void)}=	
Ref:Control Subpanel{LVObjUnknown Refnum (Void)}=	
Ref:Main Screen{LVObjVI Refnum (Void)}=	
Ref:Plotting Subpanel{LVObjUnknown Refnum (Void)}=	
Ref:Toolbar{LVObjUnknown Refnum (Void)}=	
Ref:XY Subpanel{LVObjUnknown Refnum (Void)}=	
Rxx::R{Double Float}=0.001273	
Rxx::Theta{Double Float}=0.150000	
Rxx::X{Double Float}=0.001273	
Rxx::Y{Double Float}=3.371768E-6	
Rxx:Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	
Rxx:Option: 560 Enabled{Boolean}=False	
Rxx:Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	
Rxx:Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	
Rxx:Option: Lockin Standoff Time{Double Float}=0.000000	
Rxx:Option: Lockin Type{Enum U16 ((SRS 830,EG&G 5302))}=SRS 830	
Rxx:Option: SR803 Full Scale Reading{Double Float}=0.000000	
Rxx:Option: SR830  Ref Phase{Double Float}=0.000000	
Rxx:Option: SR830  Synch Filter{Boolean}=False	
Rxx:Option: SR830  Time Constant{I16}=8	
Rxx:Option: SR830 2x Line Filter{Boolean}=False	
Rxx:Option: SR830 Adjust Gains{Boolean}=False	
Rxx:Option: SR830 Auto Gain Lower{I32}=0	
Rxx:Option: SR830 Auto Gain Upper{I32}=26	
Rxx:Option: SR830 Auto Offset 1{Boolean}=False	
Rxx:Option: SR830 Auto Offset 2{Boolean}=False	
Rxx:Option: SR830 Autophase{Boolean}=False	
Rxx:Option: SR830 DC Coupling?{Boolean}=False	
Rxx:Option: SR830 Display 1{U16}=0	
Rxx:Option: SR830 Display 2{U16}=0	
Rxx:Option: SR830 Dynamic Reserve{I16}=2	
Rxx:Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Rxx:Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Rxx:Option: SR830 Filter Slope{I32}=3	
Rxx:Option: SR830 Gain{I32}=18	
Rxx:Option: SR830 Ground Shield?{Boolean}=False	
Rxx:Option: SR830 Harmonic{I32}=1	
Rxx:Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A-B	
Rxx:Option: SR830 Line Filter{Boolean}=False	
Rxx:Option: SR830 No Reset{Boolean}=False	
Rxx:Option: SR830 Offset 1{Double Float}=0.000000	
Rxx:Option: SR830 Offset 2{Double Float}=0.000000	
Rxx:Option: SR830 Output Channel 1{Boolean}=False	
Rxx:Option: SR830 Output Channel 2{Boolean}=False	
Rxx:Option: SR830 Ratio 1{U16}=0	
Rxx:Option: SR830 Ratio 2{U16}=0	
Rxx:Option: SR830 Ref Amplitude{Double Float}=0.100000	
Rxx:Option: SR830 Ref Frequency{Double Float}=1013.000000	
Rxx:Option: SR830 Ref Source{Boolean}=False	
Rxx:Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta,X,Y]	
Rxx:Option: SR830 Time Constant value{Double Float}=0.000000	
Rxx:Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Rxx:Option: SR830 VISA{Visa Refnum (Void)}=GPIB0::5::INSTR	
Rxx:Option:560 Comport{Visa Refnum (Void)}=COM1	
Rxx:Option:560 Filter High Pass{U16}=0	
Rxx:Option:560 Filter Lowpass{U16}=0	
Rxx:Option:560 Filter Mode{U16}=0	
Rxx:Option:560 Invert{Boolean}=False	
Rxx:Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Rxx:Option:570 Enabled{Boolean}=False	
Rxx:Option:570 Filter High Pass{U16}=0	
Rxx:Option:570 Filter Lowpass{U16}=0	
Rxx:Option:570 Filter Mode{U16}=0	
Rxx:Option:570 Gain Mode{U16}=0	
Rxx:Option:570 Input Offset{U16}=0	
Rxx:Option:570 Input Offset On{Boolean}=False	
Rxx:Option:570 Sensitivity{U16}=0	
Rxx:Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Rxx:Option:SR830 Autogain Lower Threshold{Double Float}=0.100000	
Rxx:Option:SR830 Autogain Standoff{Double Float}=3.000000	
Rxx:Option:SR830 Autogain Upper Threshold{Double Float}=0.900000	
Rxx:Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Rxx:Option:SR830 Settle Time{Double Float}=0.000000	
Rxy::R{Double Float}=5.872677E-6	
Rxy::Theta{Double Float}=-179.094000	
Rxy::X{Double Float}=-5.875313E-6	
Rxy::Y{Double Float}=-9.430420E-8	
Rxy:Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	
Rxy:Option: 560 Enabled{Boolean}=False	
Rxy:Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	
Rxy:Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	
Rxy:Option: Lockin Standoff Time{Double Float}=0.000000	
Rxy:Option: Lockin Type{Enum U16 ((SRS 830,EG&G 5302))}=SRS 830	
Rxy:Option: SR803 Full Scale Reading{Double Float}=0.000000	
Rxy:Option: SR830  Ref Phase{Double Float}=0.000000	
Rxy:Option: SR830  Synch Filter{Boolean}=False	
Rxy:Option: SR830  Time Constant{I16}=8	
Rxy:Option: SR830 2x Line Filter{Boolean}=False	
Rxy:Option: SR830 Adjust Gains{Boolean}=False	
Rxy:Option: SR830 Auto Gain Lower{I32}=0	
Rxy:Option: SR830 Auto Gain Upper{I32}=26	
Rxy:Option: SR830 Auto Offset 1{Boolean}=False	
Rxy:Option: SR830 Auto Offset 2{Boolean}=False	
Rxy:Option: SR830 Autophase{Boolean}=False	
Rxy:Option: SR830 DC Coupling?{Boolean}=False	
Rxy:Option: SR830 Display 1{U16}=0	
Rxy:Option: SR830 Display 2{U16}=1	
Rxy:Option: SR830 Dynamic Reserve{I16}=2	
Rxy:Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Rxy:Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Rxy:Option: SR830 Filter Slope{I32}=3	
Rxy:Option: SR830 Gain{I32}=18	
Rxy:Option: SR830 Ground Shield?{Boolean}=False	
Rxy:Option: SR830 Harmonic{I32}=1	
Rxy:Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A-B	
Rxy:Option: SR830 Line Filter{Boolean}=False	
Rxy:Option: SR830 No Reset{Boolean}=False	
Rxy:Option: SR830 Offset 1{Double Float}=0.000000	
Rxy:Option: SR830 Offset 2{Double Float}=0.000000	
Rxy:Option: SR830 Output Channel 1{Boolean}=False	
Rxy:Option: SR830 Output Channel 2{Boolean}=False	
Rxy:Option: SR830 Ratio 1{U16}=0	
Rxy:Option: SR830 Ratio 2{U16}=0	
Rxy:Option: SR830 Ref Amplitude{Double Float}=0.100000	
Rxy:Option: SR830 Ref Frequency{Double Float}=1013.000000	
Rxy:Option: SR830 Ref Source{Boolean}=False	
Rxy:Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta,X,Y]	
Rxy:Option: SR830 Time Constant value{Double Float}=0.000000	
Rxy:Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Rxy:Option: SR830 VISA{Visa Refnum (Void)}=GPIB0::6::INSTR	
Rxy:Option:560 Comport{Visa Refnum (Void)}=COM1	
Rxy:Option:560 Filter High Pass{U16}=0	
Rxy:Option:560 Filter Lowpass{U16}=0	
Rxy:Option:560 Filter Mode{U16}=0	
Rxy:Option:560 Invert{Boolean}=False	
Rxy:Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Rxy:Option:570 Enabled{Boolean}=False	
Rxy:Option:570 Filter High Pass{U16}=0	
Rxy:Option:570 Filter Lowpass{U16}=0	
Rxy:Option:570 Filter Mode{U16}=0	
Rxy:Option:570 Gain Mode{U16}=0	
Rxy:Option:570 Input Offset{U16}=0	
Rxy:Option:570 Input Offset On{Boolean}=False	
Rxy:Option:570 Sensitivity{U16}=0	
Rxy:Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Rxy:Option:SR830 Autogain Lower Threshold{Double Float}=0.100000	
Rxy:Option:SR830 Autogain Standoff{Double Float}=3.000000	
Rxy:Option:SR830 Autogain Upper Threshold{Double Float}=0.900000	
Rxy:Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Rxy:Option:SR830 Settle Time{Double Float}=0.000000	
Sample ID{String}=MBE202221213_PA_D1 750C Cracker WAL	
Save:Filename{String}=${X-Y Class} ${2nd Parameter Class} ${iterator}{%04d} ${y}{%04.2g}.txt	
Save:Final Filename{String}=${X-Y Class} ${2nd Parameter Class} .txt	
Save:Final path{Path}=C:\\\\Data\\\\${Project Code}\\\\${User}\\\\${Sample ID}\\\\${Measurement Timestamp}{%Y%m%d}\\\\${X-Y Class}	
Save:Path{Path}=C:\\\\Data\\\\${Project Code}\\\\${User}\\\\${Sample ID}\\\\${Measurement Timestamp}{%Y%m%d}\\\\${X-Y Class}	
Startup path{Path}=C:\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV	
Sub Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Sweep Step{I32}=3	
T Control Measure.__text__{1D Array (String)}=['temperature: T1','temperature: T2','temperature: T3','temperature: T4','temperature: dT/dt']	
Timestamp{Timestamp}=<01:10:36.196 18/05/2023>T	
Toolbar{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Unaved Data{Boolean}=True	
Unsaved Data{Boolean}=False	
User{String}=Craig	
X-Y Class{String}=6221-Lockin-DAQ	
X-Y Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	
d(Offset){Double Float}=0.000000	
d(Rxx::R){Double Float}=0.000000	
d(Rxx::Theta){Double Float}=0.000000	
d(Rxx::X){Double Float}=0.000000	
d(Rxx::Y){Double Float}=4.735058E-22	
d(Rxy::R){Double Float}=1.216127E-8	
d(Rxy::Theta){Double Float}=0.061628	
d(Rxy::X){Double Float}=1.215683E-8	
d(Rxy::Y){Double Float}=5.710780E-9	
iterate result{U16}=5	
iterator{I32}=728	
multi[0]:Control: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values,Adaptive Step Ramp))}=List of Values	
multi[0]:Control: Monitor Update Timeout{Double Float}=0.010000	
multi[0]:Control: Open T Window{Boolean}=False	
multi[0]:Control: Reverse Temperature Sense{Boolean}=False	
multi[0]:Iterator{I32}=0	
multi[0]:Ref: Temperature Window{LVObjVI Refnum (Void)}=	
multi[0]:iterate result{U16}=0	
multi[0]:iterator{I32}=12	
multi[0]:temperature:  rate window{Double Float}=120.000000	
multi[0]:temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[0]:temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
multi[0]:temperature: T1{Double Float}=30.025000	
multi[0]:temperature: T2{Double Float}=32.458000	
multi[0]:temperature: T3{Double Float}=85.601700	
multi[0]:temperature: T4{Double Float}=61.606100	
multi[0]:temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
multi[0]:temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
multi[0]:temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
multi[0]:temperature: current temperature{Double Float}=1.464900	
multi[0]:temperature: current temperature 2{Double Float}=287.100000	
multi[0]:temperature: dT/dt{Double Float}=-8.971590E-5	
multi[0]:temperature: error{Double Float}=-0.031000	
multi[0]:temperature: gas{Double Float}=30.000000	
multi[0]:temperature: gas control{Boolean}=False	
multi[0]:temperature: gas control 2{Boolean}=False	
multi[0]:temperature: gass boost{I8}=0	
multi[0]:temperature: gass boost 2{I8}=0	
multi[0]:temperature: gast flow{I16}=0	
multi[0]:temperature: gast flow 2{I16}=7	
multi[0]:temperature: heater{Double Float}=6.600000	
multi[0]:temperature: heater output{Double Float}=0.000000	
multi[0]:temperature: heater output 2{Double Float}=0.000000	
multi[0]:temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
multi[0]:temperature: monitor timeout{Double Float}=0.010000	
multi[0]:temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
multi[0]:temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
multi[0]:temperature: ramp rate{Double Float}=8.000000	
multi[0]:temperature: ramp rate 2{Double Float}=0.000000	
multi[0]:temperature: ramp target{Double Float}=20.000000	
multi[0]:temperature: ramp target 2{Double Float}=0.000000	
multi[0]:temperature: ramping{Boolean}=False	
multi[0]:temperature: setpoint{Double Float}=1.800000	
multi[0]:temperature: setpoint 2{Double Float}=287.100000	
multi[0]:temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
multi[0]:temperature: stability error{Extended Float}=0.040000	
multi[0]:temperature: stability script{String}=	
multi[0]:temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
multi[0]:temperature: temp control mode{U16}=2	
multi[0]:temperature: temp control mode 2{U16}=3	
multi[0]:temperature: temp control mode 2.__text__{String}=Open Loop	
multi[0]:temperature: temp control mode.__text__{String}=Zone	
multi[0]:temperature: temp control sensor{U16}=0	
multi[0]:temperature: temp control sensor 2{U16}=0	
multi[0]:temperature: temp control sensor 2.__text__{String}=Sensor 1	
multi[0]:temperature: temp control sensor.__text__{String}=Sensor A	
multi[0]:temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
multi[0]:temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
multi[0]:temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
multi[0]:temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
multi[0]:temperature: temp loop{U16}=0	
multi[0]:temperature: temp loop 2{U16}=0	
multi[0]:temperature: temp loop 2.__text__{String}=Heater	
multi[0]:temperature: temp loop.__text__{String}=Loop 1	
multi[0]:temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
multi[0]:temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[0]:temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[0]:temperature:error for gas boost{Double Float}=0.000000	
multi[0]:temperature:error for gas boost 2{Double Float}=0.000000	
multi[0]:temperature:heater range{U16}=2	
multi[0]:temperature:heater range 2{U16}=0	
multi[0]:temperature:heater range 2.__text__{String}=Off	
multi[0]:temperature:heater range.__text__{String}=40mW	
multi[0]:temperature:history window{Extended Float}=300.000000	
multi[0]:temperature:is stable?{Boolean}=True	
multi[0]:temperature:monitor{Boolean}=True	
multi[0]:temperature:ramping{Boolean}=False	
multi[0]:temperature:ramping on{Boolean}=False	
multi[0]:temperature:ramping on 2{Boolean}=False	
multi[0]:temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
multi[0]:temperature:stability code{U32}=6618880	
multi[0]:temperature:stability rate{Extended Float}=0.040000	
multi[0]:y{Double Float}=30.000000	
multi[1]:Control: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values,Adaptive Step Ramp))}=Multi-Segment Ramp	
multi[1]:Control: Gate delay{Double Float}=0.000000	
multi[1]:Control: Monitor Update Timeout{Double Float}=0.010000	
multi[1]:Control: Open T Window{Boolean}=False	
multi[1]:Control: Reverse Temperature Sense{Boolean}=False	
multi[1]:Control:Magnet Output{Double Float}=-0.000000	
multi[1]:Iterator{I32}=0	
multi[1]:Magnet: Final Switch Heater{Enum U8 ((False,True,Mixed))}=	
multi[1]:Magnet: Power Supply{Enum U16 ((IPS120,LS625,PS110,Hg iPS,SMS Series,Cryomagnetics 4G,DMG Little CryoFree,DMG Big CryoFree))}=Hg iPS	
multi[1]:Magnet: Rate{Double Float}=0.500000	
multi[1]:Magnet: Units{Enum U16 ((Field,Current))}=Field	
multi[1]:Magnet: VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[1]:Multi-segment_Stage{I32}=0	
multi[1]:Multi-segment_Stage_Changed{Boolean}=False	
multi[1]:Ref: Temperature Window{LVObjVI Refnum (Void)}=	
multi[1]:iterate result{U16}=4	
multi[1]:iterator{I32}=57	
multi[1]:measure point{Boolean}=False	
multi[1]:temperature:  rate window{Double Float}=120.000000	
multi[1]:temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[1]:temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
multi[1]:temperature: T1{Double Float}=1.842400	
multi[1]:temperature: T2{Double Float}=1.465600	
multi[1]:temperature: T3{Double Float}=86.318100	
multi[1]:temperature: T4{Double Float}=66.769200	
multi[1]:temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
multi[1]:temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
multi[1]:temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
multi[1]:temperature: current temperature{Double Float}=1.465600	
multi[1]:temperature: current temperature 2{Double Float}=287.100000	
multi[1]:temperature: dT/dt{Double Float}=-0.001864	
multi[1]:temperature: gas control{Boolean}=False	
multi[1]:temperature: gas control 2{Boolean}=False	
multi[1]:temperature: gass boost{I8}=0	
multi[1]:temperature: gass boost 2{I8}=0	
multi[1]:temperature: gast flow{I16}=0	
multi[1]:temperature: gast flow 2{I16}=7	
multi[1]:temperature: heater output{Double Float}=0.000000	
multi[1]:temperature: heater output 2{Double Float}=0.000000	
multi[1]:temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
multi[1]:temperature: monitor timeout{Double Float}=1.000000	
multi[1]:temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
multi[1]:temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
multi[1]:temperature: ramp rate{Double Float}=8.000000	
multi[1]:temperature: ramp rate 2{Double Float}=0.000000	
multi[1]:temperature: ramp target{Double Float}=20.000000	
multi[1]:temperature: ramp target 2{Double Float}=0.000000	
multi[1]:temperature: ramping{Boolean}=False	
multi[1]:temperature: setpoint{Double Float}=1.800000	
multi[1]:temperature: setpoint 2{Double Float}=287.100000	
multi[1]:temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
multi[1]:temperature: stability error{Extended Float}=0.040000	
multi[1]:temperature: stability script{String}=	
multi[1]:temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
multi[1]:temperature: temp control mode{U16}=2	
multi[1]:temperature: temp control mode 2{U16}=3	
multi[1]:temperature: temp control mode 2.__text__{String}=Open Loop	
multi[1]:temperature: temp control mode.__text__{String}=Zone	
multi[1]:temperature: temp control sensor{U16}=0	
multi[1]:temperature: temp control sensor 2{U16}=0	
multi[1]:temperature: temp control sensor 2.__text__{String}=Sensor 1	
multi[1]:temperature: temp control sensor.__text__{String}=Sensor A	
multi[1]:temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
multi[1]:temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
multi[1]:temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
multi[1]:temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
multi[1]:temperature: temp loop{U16}=0	
multi[1]:temperature: temp loop 2{U16}=0	
multi[1]:temperature: temp loop 2.__text__{String}=Heater	
multi[1]:temperature: temp loop.__text__{String}=Loop 1	
multi[1]:temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
multi[1]:temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[1]:temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[1]:temperature:error for gas boost{Double Float}=0.000000	
multi[1]:temperature:error for gas boost 2{Double Float}=0.000000	
multi[1]:temperature:heater range{U16}=2	
multi[1]:temperature:heater range 2{U16}=0	
multi[1]:temperature:heater range 2.__text__{String}=Off	
multi[1]:temperature:heater range.__text__{String}=40mW	
multi[1]:temperature:history window{Extended Float}=300.000000	
multi[1]:temperature:is stable?{Boolean}=True	
multi[1]:temperature:monitor{Boolean}=True	
multi[1]:temperature:ramping{Boolean}=False	
multi[1]:temperature:ramping on{Boolean}=False	
multi[1]:temperature:ramping on 2{Boolean}=False	
multi[1]:temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
multi[1]:temperature:stability code{U32}=6618880	
multi[1]:temperature:stability rate{Extended Float}=0.040000	
multi[1]:y{Double Float}=0.000000	
parameter: Termination{String}=False	
parameter: delta time{Double Float}=1.000000	
parameter: progress{Double Float}=100.000000	
temperature:  rate window{Double Float}=120.000000	
temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
temperature: T1{Double Float}=30.025000	
temperature: T2{Double Float}=32.458000	
temperature: T3{Double Float}=85.601700	
temperature: T4{Double Float}=61.606100	
temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
temperature: current temperature{Double Float}=1.464900	
temperature: current temperature 2{Double Float}=287.100000	
temperature: dT/dt{Double Float}=-8.971590E-5	
temperature: gas control{Boolean}=False	
temperature: gas control 2{Boolean}=False	
temperature: gass boost{I8}=0	
temperature: gass boost 2{I8}=0	
temperature: gast flow{I16}=0	
temperature: gast flow 2{I16}=7	
temperature: heater output{Double Float}=0.000000	
temperature: heater output 2{Double Float}=0.000000	
temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
temperature: monitor timeout{Double Float}=0.010000	
temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
temperature: ramp rate{Double Float}=8.000000	
temperature: ramp rate 2{Double Float}=0.000000	
temperature: ramp target{Double Float}=20.000000	
temperature: ramp target 2{Double Float}=0.000000	
temperature: ramping{Boolean}=False	
temperature: setpoint{Double Float}=1.800000	
temperature: setpoint 2{Double Float}=287.100000	
temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
temperature: stability error{Extended Float}=0.040000	
temperature: stability script{String}=	
temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
temperature: temp control mode{U16}=2	
temperature: temp control mode 2{U16}=3	
temperature: temp control mode 2.__text__{String}=Open Loop	
temperature: temp control mode.__text__{String}=Zone	
temperature: temp control sensor{U16}=0	
temperature: temp control sensor 2{U16}=0	
temperature: temp control sensor 2.__text__{String}=Sensor 1	
temperature: temp control sensor.__text__{String}=Sensor A	
temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
temperature: temp loop{U16}=0	
temperature: temp loop 2{U16}=0	
temperature: temp loop 2.__text__{String}=Heater	
temperature: temp loop.__text__{String}=Loop 1	
temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
temperature:error for gas boost{Double Float}=0.000000	
temperature:error for gas boost 2{Double Float}=0.000000	
temperature:heater range{U16}=2	
temperature:heater range 2{U16}=0	
temperature:heater range 2.__text__{String}=Off	
temperature:heater range.__text__{String}=40mW	
temperature:history window{Extended Float}=300.000000	
temperature:is stable?{Boolean}=True	
temperature:monitor{Boolean}=True	
temperature:ramping{Boolean}=False	
temperature:ramping on{Boolean}=False	
temperature:ramping on 2{Boolean}=False	
temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
temperature:stability code{U32}=6618880	
temperature:stability rate{Extended Float}=0.040000	
y{Double Float}=30.000000	
