TDI Format 1.5	Offset	Rxx::R	Rxx::Theta	Rxx::X	Rxx::Y	Rxy::R	Rxy::Theta	Rxy::X	Rxy::Y	temperature: T1	temperature: T2	temperature: T3	temperature: T4	temperature: dT/dt	iterator	multi[0]:iterator	multi[0]:y	multi[0]:temperature: setpoint	multi[0]:temperature: T1	multi[0]:temperature: T2	multi[0]:temperature: T3	multi[0]:temperature: T4	multi[0]:temperature: heater	multi[0]:temperature: gas	multi[0]:temperature: dT/dt	multi[0]:temperature: current temperature	multi[0]:temperature: error	multi[1]:iterator	multi[1]:y	multi[1]:Control:Magnet Output
2nd Parameter Class{String}=Multi-Parameter	0E+0	1.2303559E-3	1.56E-1	1.2303559E-3	3.371767975E-6	5.779412825E-7	-6.5544E+0	5.747802324E-7	-6.690845182E-8	1.2E+1	1.1908E+1	8.56017E+1	6.35264E+1	3.463027999E-2	5.05E+2	9E+0	1.2E+1	1.2E+1	1.2003E+1	1.1909E+1	8.55301E+1	6.35264E+1	1.7E+0	1.2E+1	3.778541088E-2	1.2003E+1	-3E-3	0E+0	0E+0	1E-4
2nd Parameter Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	0E+0	1.233727385E-3	1.548E-1	1.233727385E-3	3.338050296E-6	7.1233824E-6	-4.452E-1	7.1233824E-6	-5.689856337E-8	1.2004E+1	1.1933E+1	8.63539E+1	6.35264E+1	1.711800508E-2	5.06E+2	9E+0	1.2E+1	1.8E+0	1.2E+1	1.1908E+1	8.56017E+1	6.35264E+1	1.7E+0	1.2E+1	3.463027999E-2	1.4649E+0	-3E-3	1E+0	5E-1	4.999E-1
Analysis Class{String}=Basic Plot	0E+0	1.23777345E-3	1.56E-1	1.23777345E-3	3.371767975E-6	1.366725119E-5	-2.388E-1	1.366725119E-5	-5.847906016E-8	1.2E+1	1.1944E+1	8.62822E+1	6.35264E+1	6.810193881E-3	5.07E+2	9E+0	1.2E+1	1.8E+0	1.2004E+1	1.1933E+1	8.63539E+1	6.35264E+1	1.7E+0	1.2E+1	1.711800508E-2	1.4649E+0	-3E-3	2E+0	1E+0	9.999E-1
Analysis Class Path{Path}=C\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV\\\\plugins\\\\Plotting\\\\Plotting_Base_class\\\\Plotting_Base.lvclass	0E+0	1.243505257E-3	1.56E-1	1.243505257E-3	3.371767975E-6	2.023847088E-5	-6.12E-2	2.023847088E-5	-2.265410038E-8	1.2002E+1	1.1953E+1	8.59957E+1	6.35264E+1	5.718370434E-3	5.08E+2	9E+0	1.2E+1	1.8E+0	1.2E+1	1.1944E+1	8.62822E+1	6.35264E+1	1.7E+0	1.2E+1	6.810193881E-3	1.4649E+0	-3E-3	3E+0	1.5E+0	1.5E+0
Analysis.# pre-routines{I32}=5	0E+0	1.243505257E-3	1.56E-1	1.243505257E-3	3.371767975E-6	2.025323527E-5	-1.14E-1	2.025323527E-5	-4.214709969E-8	1.2002E+1	1.1953E+1	8.59241E+1	6.35264E+1	4.673474003E-3	5.09E+2	9E+0	1.2E+1	1.8E+0	1.2002E+1	1.1953E+1	8.59957E+1	6.35264E+1	1.7E+0	1.2E+1	5.718370434E-3	1.4649E+0	-3E-3	4E+0	1.5E+0	1.5E+0
Analysis:Pre[0]:T Control Measure{1D Array (I32)}=[1,2,3,4,7]	0E+0	1.240976644E-3	1.56E-1	1.240976644E-3	3.371767975E-6	1.760851449E-5	-1.608E-1	1.760851449E-5	-5.057649135E-8	1.2395E+1	1.2101E+1	8.63897E+1	6.35264E+1	2.185745388E-1	5.1E+2	9E+0	1.2E+1	1.8E+0	1.2002E+1	1.1953E+1	8.59241E+1	6.35264E+1	1.7E+0	1.2E+1	4.673474003E-3	1.4649E+0	-3E-3	5E+0	1.3E+0	1.3001E+0
Autosave Tabs{Enum U32 ((XY Measurement Save,Parameter Plot Save 2))}=Parameter Plot Save 2	0E+0	1.23844803E-3	1.56E-1	1.23844803E-3	3.371767975E-6	1.499015464E-5	-2.472E-1	1.499015464E-5	-6.63816007E-8	1.1319E+1	1.15E+1	8.62822E+1	6.35264E+1	-7.73462832E-1	5.11E+2	9E+0	1.2E+1	1.8E+0	1.2395E+1	1.2101E+1	8.63897E+1	6.35264E+1	1.7E+0	1.2E+1	2.185745388E-1	1.4649E+0	-3E-3	6E+0	1.1E+0	1.1E+0
Control:Magnet Output{Double Float}=-0.007000	0E+0	1.236627654E-3	1.56E-1	1.236627654E-3	3.371767975E-6	1.237176369E-5	-2.364E-1	1.237176369E-5	-5.268386754E-8	1.1923E+1	1.182E+1	8.62106E+1	6.35264E+1	-2.221655659E-2	5.12E+2	9E+0	1.2E+1	1.8E+0	1.1319E+1	1.15E+1	8.62822E+1	6.35264E+1	1.7E+0	1.2E+1	-7.73462832E-1	1.4649E+0	-3E-3	7E+0	9E-1	9.001E-1
Control:Magnet Rate{Double Float}=0.500000	0E+0	1.235076545E-3	1.56E-1	1.235076545E-3	3.371767975E-6	9.752295104E-6	-2.868E-1	9.752295104E-6	-5.057651963E-8	1.1987E+1	1.1934E+1	8.62106E+1	6.35264E+1	3.256395459E-1	5.13E+2	9E+0	1.2E+1	1.8E+0	1.1923E+1	1.182E+1	8.62106E+1	6.35264E+1	1.7E+0	1.2E+1	-2.221655659E-2	1.4649E+0	-3E-3	8E+0	7E-1	7.002E-1
Display Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	0E+0	1.233727385E-3	1.56E-1	1.233727385E-3	3.371767975E-6	7.132340029E-6	-5.52E-1	7.132340029E-6	-7.006944541E-8	1.2019E+1	1.1959E+1	8.59241E+1	6.35264E+1	7.975147665E-2	5.14E+2	9E+0	1.2E+1	1.8E+0	1.1987E+1	1.1934E+1	8.62106E+1	6.35264E+1	1.7E+0	1.2E+1	3.256395459E-1	1.4649E+0	-3E-3	9E+0	5E-1	5E-1
Elapsed Time{Double Float}=12790.950867	0E+0	1.232547931E-3	1.56E-1	1.232547931E-3	3.371767975E-6	4.497612079E-6	-8.88E-1	4.497612079E-6	-7.059635309E-8	1.2021E+1	1.197E+1	8.56734E+1	6.35264E+1	2.669183537E-2	5.15E+2	9E+0	1.2E+1	1.8E+0	1.2019E+1	1.1959E+1	8.59241E+1	6.35264E+1	1.7E+0	1.2E+1	7.975147665E-2	1.4649E+0	-3E-3	1E+1	3E-1	3.001E-1
File:Autodel{Boolean}=True	0E+0	1.231198771E-3	1.56E-1	1.231198771E-3	3.371767975E-6	1.885027885E-6	-2.3928E+0	1.882394619E-6	-7.955262415E-8	1.1977E+1	1.1961E+1	8.62822E+1	6.35264E+1	-6.517963484E-3	5.16E+2	9E+0	1.2E+1	1.8E+0	1.2021E+1	1.197E+1	8.56734E+1	6.35264E+1	1.7E+0	1.2E+1	2.669183537E-2	1.4649E+0	-3E-3	1.1E+1	1E-1	1.001E-1
File:Autosave{Boolean}=False	0E+0	1.231198771E-3	1.56E-1	1.231198771E-3	3.371767975E-6	1.871858728E-6	-2.7708E+0	1.869222634E-6	-9.167000194E-8	1.2026E+1	1.1969E+1	8.62822E+1	6.35264E+1	3.409213154E-3	5.17E+2	9E+0	1.2E+1	1.8E+0	1.1977E+1	1.1961E+1	8.62822E+1	6.35264E+1	1.7E+0	1.2E+1	-6.517963484E-3	1.4649E+0	-3E-3	1.2E+1	1E-1	1E-1
File:Export Config{Boolean}=True	0E+0	1.231165113E-3	1.56E-1	1.231165113E-3	3.371767975E-6	1.741731281E-6	-2.388E+0	1.740150191E-6	-7.428425437E-8	1.2022E+1	1.198E+1	8.62106E+1	6.35264E+1	1.395003777E-2	5.18E+2	9E+0	1.2E+1	1.8E+0	1.2026E+1	1.1969E+1	8.62822E+1	6.35264E+1	1.7E+0	1.2E+1	3.409213154E-3	1.4649E+0	-3E-3	1.3E+1	9E-2	9E-2
File:Final Autosave{Boolean}=True	0E+0	1.23103048E-3	1.56E-1	1.23103048E-3	3.371767975E-6	1.618977544E-6	-2.9508E+0	1.616870366E-6	-8.534784506E-8	1.2006E+1	1.1974E+1	8.62106E+1	6.35264E+1	8.256997098E-4	5.19E+2	9E+0	1.2E+1	1.8E+0	1.2022E+1	1.198E+1	8.62106E+1	6.35264E+1	1.7E+0	1.2E+1	1.395003777E-2	1.4649E+0	-3E-3	1.4E+1	8E-2	8.01E-2
Filter:Enable{Enum U16 ((None,Analog,Digital,Analog&Digitial))}=None	0E+0	1.23103048E-3	1.56E-1	1.23103048E-3	3.371767975E-6	1.478311378E-6	-3.1224E+0	1.476207028E-6	-8.166002864E-8	1.2023E+1	1.1977E+1	8.62464E+1	6.35264E+1	2.680080011E-3	5.2E+2	9E+0	1.2E+1	1.8E+0	1.2006E+1	1.1974E+1	8.62106E+1	6.35264E+1	1.7E+0	1.2E+1	8.256997098E-4	1.4649E+0	-3E-3	1.5E+1	7E-2	7E-2
Filter:Points{I32}=1	0E+0	1.230862188E-3	1.56E-1	1.230862188E-3	3.371767975E-6	1.353449897E-6	-3.372E+0	1.350816065E-6	-8.113317751E-8	1.2021E+1	1.1974E+1	8.62106E+1	6.35264E+1	-3.632940818E-3	5.21E+2	9E+0	1.2E+1	1.8E+0	1.2023E+1	1.1977E+1	8.62464E+1	6.35264E+1	1.7E+0	1.2E+1	2.680080011E-3	1.4649E+0	-3E-3	1.6E+1	6E-2	6.01E-2
Filter:Type{U16}=1	0E+0	1.230693897E-3	1.56E-1	1.230693897E-3	3.270614936E-6	1.212253683E-6	-3.9876E+0	1.209092916E-6	-8.534787334E-8	1.2021E+1	1.1979E+1	8.61748E+1	6.35264E+1	4.540704191E-3	5.22E+2	9E+0	1.2E+1	1.8E+0	1.2021E+1	1.1974E+1	8.62106E+1	6.35264E+1	1.7E+0	1.2E+1	-3.632940818E-3	1.4649E+0	-3E-3	1.7E+1	5E-2	5E-2
Filter:Type.__text__{String}=Repeat	0E+0	1.230693897E-3	1.56E-1	1.230693897E-3	3.371767975E-6	1.214360862E-6	-4.0032E+0	1.21172703E-6	-8.692848327E-8	1.2023E+1	1.1982E+1	8.61748E+1	6.35264E+1	1.139783114E-2	5.23E+2	9E+0	1.2E+1	1.8E+0	1.2021E+1	1.1979E+1	8.61748E+1	6.35264E+1	1.7E+0	1.2E+1	4.540704191E-3	1.4649E+0	-3E-3	1.8E+1	5E-2	5E-2
Filter:Window{Double Float}=1.000000	0E+0	1.230693897E-3	1.56E-1	1.230693897E-3	3.371767975E-6	1.152194579E-6	-3.4908E+0	1.149560748E-6	-7.112317593E-8	1.2029E+1	1.1982E+1	8.61748E+1	6.35264E+1	7.00042909E-3	5.24E+2	9E+0	1.2E+1	1.8E+0	1.2023E+1	1.1982E+1	8.61748E+1	6.35264E+1	1.7E+0	1.2E+1	1.139783114E-2	1.4649E+0	-3E-3	1.9E+1	4.5E-2	4.5E-2
Iterator{I32}=0	0E+0	1.230693897E-3	1.56E-1	1.230693897E-3	3.304332616E-6	1.082652324E-6	-3.8916E+0	1.080017927E-6	-7.481102064E-8	1.2043E+1	1.1992E+1	8.6139E+1	6.35264E+1	2.301933616E-2	5.25E+2	9E+0	1.2E+1	1.8E+0	1.2029E+1	1.1982E+1	8.61748E+1	6.35264E+1	1.7E+0	1.2E+1	7.00042909E-3	1.4649E+0	-3E-3	2E+1	4E-2	3.99E-2
Magnet: Control Mode{Boolean}=False	0E+0	1.230524191E-3	1.56E-1	1.230524191E-3	3.338050296E-6	1.020486041E-6	-4.8708E+0	1.016270836E-6	-8.850900835E-8	1.1989E+1	1.1976E+1	8.61748E+1	6.35264E+1	-7.713058149E-4	5.26E+2	9E+0	1.2E+1	1.8E+0	1.2043E+1	1.1992E+1	8.6139E+1	6.35264E+1	1.7E+0	1.2E+1	2.301933616E-2	1.4649E+0	-3E-3	2.1E+1	3.5E-2	3.5E-2
Magnet: Final Switch Heater{Enum U8 ((False,True,Mixed))}=	0E+0	1.230524191E-3	1.56E-1	1.230524191E-3	3.371767975E-6	9.419875721E-7	-4.842E+0	9.388259562E-7	-8.113303609E-8	1.1986E+1	1.1963E+1	8.61748E+1	6.35264E+1	-2.238929458E-2	5.27E+2	9E+0	1.2E+1	1.8E+0	1.1989E+1	1.1976E+1	8.61748E+1	6.35264E+1	1.7E+0	1.2E+1	-7.713058149E-4	1.4649E+0	-3E-3	2.2E+1	3E-2	2.99E-2
Magnet: Power Supply{Enum U16 ((IPS120,LS625,PS110,Hg iPS,SMS Series,Cryomagnetics 4G,DMG Little CryoFree,DMG Big CryoFree))}=Hg iPS	0E+0	1.230524191E-3	1.56E-1	1.230524191E-3	3.371767975E-6	8.887769383E-7	-4.5288E+0	8.856156053E-7	-7.165002705E-8	1.2018E+1	1.1974E+1	8.61748E+1	6.35264E+1	-8.660981432E-3	5.28E+2	9E+0	1.2E+1	1.8E+0	1.1986E+1	1.1963E+1	8.61748E+1	6.35264E+1	1.7E+0	1.2E+1	-2.238929458E-2	1.4649E+0	-3E-3	2.3E+1	2.5E-2	2.5E-2
Magnet: Rate{Double Float}=0.500000	0E+0	1.230524191E-3	1.56E-1	1.230524191E-3	3.371767975E-6	8.166005692E-7	-5.4924E+0	8.123853643E-7	-7.902577303E-8	1.2027E+1	1.1989E+1	8.61032E+1	6.35264E+1	1.123839896E-2	5.29E+2	9E+0	1.2E+1	1.8E+0	1.2018E+1	1.1974E+1	8.61748E+1	6.35264E+1	1.7E+0	1.2E+1	-8.660981432E-3	1.4649E+0	-3E-3	2.4E+1	2E-2	1.99E-2
Magnet: Setpoint{Double Float}=0.000000	0E+0	1.2303559E-3	1.56E-1	1.2303559E-3	3.270614936E-6	7.517993239E-7	-5.898E+0	7.475852503E-7	-7.902577303E-8	1.2026E+1	1.1985E+1	8.58883E+1	6.35264E+1	4.86266613E-3	5.3E+2	9E+0	1.2E+1	1.8E+0	1.2027E+1	1.1989E+1	8.61032E+1	6.35264E+1	1.7E+0	1.2E+1	1.123839896E-2	1.4649E+0	-3E-3	2.5E+1	1.5E-2	1.49E-2
Magnet: Units{Enum U16 ((Field,Current))}=Field	0E+0	1.2303559E-3	1.56E-1	1.2303559E-3	3.371767975E-6	7.075451874E-7	-6.9888E+0	7.02276959E-7	-8.798215723E-8	1.1992E+1	1.1972E+1	8.57808E+1	6.35264E+1	-1.491058245E-2	5.31E+2	9E+0	1.2E+1	1.8E+0	1.2026E+1	1.1985E+1	8.58883E+1	6.35264E+1	1.7E+0	1.2E+1	4.86266613E-3	1.4649E+0	-3E-3	2.6E+1	1E-2	1E-2
Magnet: VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	0E+0	1.2303559E-3	1.56E-1	1.2303559E-3	3.304332616E-6	6.206146111E-7	-7.3296E+0	6.142925108E-7	-7.955259587E-8	1.2038E+1	1.198E+1	8.59241E+1	6.35264E+1	2.278627595E-3	5.32E+2	9E+0	1.2E+1	1.8E+0	1.1992E+1	1.1972E+1	8.57808E+1	6.35264E+1	1.7E+0	1.2E+1	-1.491058245E-2	1.4649E+0	-3E-3	2.7E+1	5E-3	4.9E-3
Main Screen Path{Path}=C:\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV\\\\1Code.vi	0E+0	1.2303559E-3	1.56E-1	1.2303559E-3	3.371767975E-6	5.652973647E-7	-7.3116E+0	5.605557895E-7	-7.323043899E-8	1.2016E+1	1.1991E+1	8.59241E+1	6.35264E+1	2.143363655E-2	5.33E+2	9E+0	1.2E+1	1.8E+0	1.2038E+1	1.198E+1	8.59241E+1	6.35264E+1	1.7E+0	1.2E+1	2.278627595E-3	1.4649E+0	-3E-3	2.8E+1	0E+0	-1E-4
Measurement Timestamp{Timestamp}=<23:47:04.540 17/05/2023>T	0E+0	1.2303559E-3	1.56E-1	1.2303559E-3	3.371767975E-6	4.878522016E-7	-8.6472E+0	4.825842561E-7	-7.481096407E-8	1.1994E+1	1.196E+1	8.57808E+1	6.35264E+1	-3.26035656E-2	5.34E+2	9E+0	1.2E+1	1.8E+0	1.2016E+1	1.1991E+1	8.59241E+1	6.35264E+1	1.7E+0	1.2E+1	2.143363655E-2	1.4649E+0	-3E-3	2.9E+1	-5E-3	-5.1E-3
Measurement Title{String}=	0E+0	1.2303559E-3	1.56E-1	1.2303559E-3	3.371767975E-6	4.341154804E-7	-1.11132E+1	4.251589831E-7	-8.534792991E-8	1.2034E+1	1.1995E+1	8.59241E+1	6.35264E+1	2.052432299E-2	5.35E+2	9E+0	1.2E+1	1.8E+0	1.1994E+1	1.196E+1	8.57808E+1	6.35264E+1	1.7E+0	1.2E+1	-3.26035656E-2	1.4649E+0	-3E-3	3E+1	-1E-2	-1E-2
Measurment Select{U16}=4	0E+0	1.2303559E-3	1.56E-1	1.2303559E-3	3.371767975E-6	3.687875819E-7	-1.20852E+1	3.598316503E-7	-7.902571646E-8	1.1991E+1	1.197E+1	8.62822E+1	6.35264E+1	-1.418302953E-2	5.36E+2	9E+0	1.2E+1	1.8E+0	1.2034E+1	1.1995E+1	8.59241E+1	6.35264E+1	1.7E+0	1.2E+1	2.052432299E-2	1.4649E+0	-3E-3	3.1E+1	-1.5E-2	-1.51E-2
Measurment Select.__text__{String}=6221-Lockin-DAQ	0E+0	1.230524191E-3	1.56E-1	1.230524191E-3	3.371767975E-6	2.960831455E-7	-1.35708E+1	2.876535842E-7	-7.112311936E-8	1.2019E+1	1.1982E+1	8.62464E+1	6.35264E+1	5.481996108E-3	5.37E+2	9E+0	1.2E+1	1.8E+0	1.1991E+1	1.197E+1	8.62822E+1	6.35264E+1	1.7E+0	1.2E+1	-1.418302953E-2	1.4649E+0	-3E-3	3.2E+1	-2E-2	-2.01E-2
Notes{String}=I+1A I-1E\\nrxx+1B Rxx-1C\\nRxy+1D Rxy-4A	0E+0	1.230524191E-3	1.56E-1	1.230524191E-3	3.371767975E-6	2.365506943E-7	-1.64964E+1	2.270675438E-7	-6.90158563E-8	1.2035E+1	1.1982E+1	8.62106E+1	6.35264E+1	1.152377692E-3	5.38E+2	9E+0	1.2E+1	1.8E+0	1.2019E+1	1.1982E+1	8.62464E+1	6.35264E+1	1.7E+0	1.2E+1	5.481996108E-3	1.4649E+0	-3E-3	3.3E+1	-2.5E-2	-2.51E-2
Offset{Double Float}=0.000000	0E+0	1.230524191E-3	1.56E-1	1.230524191E-3	3.338050296E-6	1.870277637E-7	-3.01416E+1	1.601582717E-7	-9.483096724E-8	1.1995E+1	1.1981E+1	8.61748E+1	6.35264E+1	3.836388933E-3	5.39E+2	9E+0	1.2E+1	1.8E+0	1.2035E+1	1.1982E+1	8.62106E+1	6.35264E+1	1.7E+0	1.2E+1	1.152377692E-3	1.4649E+0	-3E-3	3.4E+1	-3E-2	-3E-2
Option: 2182 Autozero{Boolean}=True	0E+0	1.230524191E-3	1.56E-1	1.230524191E-3	3.371767975E-6	1.343438679E-7	-4.04184E+1	1.022067698E-7	-8.903568976E-8	1.2022E+1	1.1984E+1	8.61748E+1	6.35264E+1	9.71653033E-3	5.4E+2	9E+0	1.2E+1	1.8E+0	1.1995E+1	1.1981E+1	8.61748E+1	6.35264E+1	1.7E+0	1.2E+1	3.836388933E-3	1.4649E+0	-3E-3	3.5E+1	-3.5E-2	-3.51E-2
Option: 2182 Front Autozero{Boolean}=True	0E+0	1.230524191E-3	1.56E-1	1.230524191E-3	3.371767975E-6	8.798204409E-8	-7.81824E+1	1.738569665E-8	-8.850886693E-8	1.1991E+1	1.1974E+1	8.6139E+1	6.35264E+1	-1.050012E-2	5.41E+2	9E+0	1.2E+1	1.8E+0	1.2022E+1	1.1984E+1	8.61748E+1	6.35264E+1	1.7E+0	1.2E+1	9.71653033E-3	1.4649E+0	-3E-3	3.6E+1	-4E-2	-4.01E-2
Option: 2182 Hold{Boolean}=False	0E+0	1.230693897E-3	1.56E-1	1.230693897E-3	3.371767975E-6	8.798207238E-8	-1.16172E+2	-4.056657462E-8	-8.11332058E-8	1.1993E+1	1.1968E+1	8.6139E+1	6.35264E+1	-1.563045941E-2	5.42E+2	9E+0	1.2E+1	1.8E+0	1.1991E+1	1.1974E+1	8.6139E+1	6.35264E+1	1.7E+0	1.2E+1	-1.050012E-2	1.4649E+0	-3E-3	3.7E+1	-4.5E-2	-4.51E-2
Option: 2182 Hold Count{I32}=10	0E+0	1.230693897E-3	1.56E-1	1.230693897E-3	3.371767975E-6	1.14850829E-7	-1.458504E+2	-9.746522284E-8	-6.638162898E-8	1.204E+1	1.1985E+1	8.61032E+1	6.35264E+1	6.883034483E-3	5.43E+2	9E+0	1.2E+1	1.8E+0	1.1993E+1	1.1968E+1	8.6139E+1	6.35264E+1	1.7E+0	1.2E+1	-1.563045941E-2	1.4649E+0	-3E-3	3.8E+1	-5E-2	-5.01E-2
Option: 2182 Hold Window{Double Float}=1.000000	0E+0	1.230693897E-3	1.56E-1	1.230693897E-3	3.371767975E-6	1.343437265E-7	-1.441812E+2	-1.10109282E-7	-8.060626983E-8	1.2047E+1	1.1994E+1	8.6139E+1	6.35264E+1	2.061288804E-2	5.44E+2	9E+0	1.2E+1	1.8E+0	1.204E+1	1.1985E+1	8.61032E+1	6.35264E+1	1.7E+0	1.2E+1	6.883034483E-3	1.4649E+0	-3E-3	3.9E+1	-5E-2	-5E-2
Option: 2182 Line Sync{Boolean}=False	0E+0	1.230862188E-3	1.56E-1	1.230862188E-3	3.371767975E-6	2.507745714E-7	-1.609164E+2	-2.397114616E-7	-8.482110707E-8	1.2008E+1	1.1981E+1	8.61032E+1	6.35264E+1	-7.915797323E-5	5.45E+2	9E+0	1.2E+1	1.8E+0	1.2047E+1	1.1994E+1	8.6139E+1	6.35264E+1	1.7E+0	1.2E+1	2.061288804E-2	1.4649E+0	-3E-3	4E+1	-6E-2	-5.99E-2
Option: 2182 Reference Reading{Double Float}=0.000000	0E+0	1.230996821E-3	1.56E-1	1.230996821E-3	3.371767975E-6	3.772165776E-7	-1.690728E+2	-3.724752852E-7	-7.323046728E-8	1.201E+1	1.1977E+1	8.61032E+1	6.35264E+1	-1.242906088E-3	5.46E+2	9E+0	1.2E+1	1.8E+0	1.2008E+1	1.1981E+1	8.61032E+1	6.35264E+1	1.7E+0	1.2E+1	-7.915797323E-5	1.4649E+0	-3E-3	4.1E+1	-7E-2	-7E-2
Option: 2182 Relative Mode{Boolean}=False	0E+0	1.23103048E-3	1.56E-1	1.23103048E-3	3.338050296E-6	5.026032976E-7	-1.702692E+2	-4.983889412E-7	-8.69284267E-8	1.1998E+1	1.1976E+1	8.61032E+1	6.35264E+1	-2.23034434E-3	5.47E+2	9E+0	1.2E+1	1.8E+0	1.201E+1	1.1977E+1	8.61032E+1	6.35264E+1	1.7E+0	1.2E+1	-1.242906088E-3	1.4649E+0	-3E-3	4.2E+1	-8E-2	-8E-2
Option: 2182 Trigger Delay{Cluster (Boolean,Double Float)}={'Auto':True,'Time(s)':0.000000}	0E+0	1.23103048E-3	1.56E-1	1.23103048E-3	3.371767975E-6	6.390542589E-7	-1.730304E+2	-6.369467978E-7	-7.902577303E-8	1.2004E+1	1.1977E+1	8.61032E+1	6.35264E+1	5.326131359E-4	5.48E+2	9E+0	1.2E+1	1.8E+0	1.1998E+1	1.1976E+1	8.61032E+1	6.35264E+1	1.7E+0	1.2E+1	-2.23034434E-3	1.4649E+0	-3E-3	4.3E+1	-9E-2	-8.99E-2
Option: 2182 Trigger Source{Enum U16 ((Immediate,Timer,Manual,Bus,Trigger link))}=Bus	0E+0	1.231198771E-3	1.56E-1	1.231198771E-3	3.371767975E-6	7.660240496E-7	-1.740732E+2	-7.639168714E-7	-8.113317751E-8	1.2012E+1	1.1978E+1	8.61032E+1	6.35264E+1	-2.203031443E-3	5.49E+2	9E+0	1.2E+1	1.8E+0	1.2004E+1	1.1977E+1	8.61032E+1	6.35264E+1	1.7E+0	1.2E+1	5.326131359E-4	1.4649E+0	-3E-3	4.4E+1	-1E-1	-1E-1
Option: 2182 Trigger Timer{Double Float}=0.000000	0E+0	1.231198771E-3	1.56E-1	1.231198771E-3	3.338050296E-6	7.665509855E-7	-1.740168E+2	-7.649704605E-7	-8.113306438E-8	1.2022E+1	1.1982E+1	8.61032E+1	6.35264E+1	1.83546741E-3	5.5E+2	9E+0	1.2E+1	1.8E+0	1.2012E+1	1.1978E+1	8.61032E+1	6.35264E+1	1.7E+0	1.2E+1	-2.203031443E-3	1.4649E+0	-3E-3	4.5E+1	-1E-1	-1E-1
Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	0E+0	1.232379639E-3	1.56E-1	1.232379639E-3	3.371767975E-6	3.363868178E-6	-1.785708E+2	-3.365975357E-6	-8.534784506E-8	1.2006E+1	1.1977E+1	8.5745E+1	6.2996E+1	-1.730625401E-3	5.51E+2	9E+0	1.2E+1	1.8E+0	1.2022E+1	1.1982E+1	8.61032E+1	6.35264E+1	1.7E+0	1.2E+1	1.83546741E-3	1.4649E+0	-3E-3	4.6E+1	-3E-1	-2.999E-1
Option: 560 Enabled{Boolean}=False	0E+0	1.233559093E-3	1.56E-1	1.233559093E-3	3.371767975E-6	5.983314137E-6	-1.791384E+2	-5.985947402E-6	-9.166994537E-8	1.1996E+1	1.1972E+1	8.58524E+1	6.2996E+1	-1.456389204E-2	5.52E+2	9E+0	1.2E+1	1.8E+0	1.2006E+1	1.1977E+1	8.5745E+1	6.2996E+1	1.7E+0	1.2E+1	-1.730625401E-3	1.4649E+0	-3E-3	4.7E+1	-5E-1	-4.999E-1
Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	0E+0	1.234908253E-3	1.56E-1	1.234908253E-3	3.371767975E-6	8.57903242E-6	-1.792356E+2	-8.581662857E-6	-1.159044747E-7	1.1988E+1	1.1987E+1	8.61748E+1	6.2996E+1	1.118894946E-2	5.53E+2	9E+0	1.2E+1	1.8E+0	1.1996E+1	1.1972E+1	8.58524E+1	6.2996E+1	1.7E+0	1.2E+1	-1.456389204E-2	1.4649E+0	-3E-3	4.8E+1	-7E-1	-6.999E-1
Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	0E+0	1.236593996E-3	1.56E-1	1.236593996E-3	3.371767975E-6	1.118795946E-5	-1.79472E+2	-1.119059838E-5	-1.048409405E-7	1.2016E+1	1.1982E+1	8.60673E+1	6.2996E+1	4.899398424E-3	5.54E+2	9E+0	1.2E+1	1.8E+0	1.1988E+1	1.1987E+1	8.61748E+1	6.2996E+1	1.7E+0	1.2E+1	1.118894946E-2	1.4649E+0	-3E-3	4.9E+1	-9E-1	-8.998E-1
Option: 6221 Adjust Mode{Enum U16 ((Offset,Frequency,Amplitude))}=Offset	0E+0	1.23844803E-3	1.56E-1	1.23844803E-3	3.371767975E-6	1.379948582E-5	-1.795296E+2	-1.380212474E-5	-1.14850829E-7	1.2014E+1	1.1984E+1	8.60673E+1	6.2996E+1	1.813882031E-2	5.55E+2	9E+0	1.2E+1	1.8E+0	1.2016E+1	1.1982E+1	8.60673E+1	6.2996E+1	1.7E+0	1.2E+1	4.899398424E-3	1.4649E+0	-3E-3	5E+1	-1.1E+0	-1.0998E+0
Option: 6221 Amplitude{Double Float}=1.000000E-6	0E+0	1.240640061E-3	1.56E-1	1.240640061E-3	3.371767975E-6	1.641206153E-5	-1.7955E+2	-1.641469197E-5	-1.301290306E-7	1.2015E+1	1.198E+1	8.57808E+1	6.2996E+1	2.677898621E-3	5.56E+2	9E+0	1.2E+1	1.8E+0	1.2014E+1	1.1984E+1	8.60673E+1	6.2996E+1	1.7E+0	1.2E+1	1.813882031E-2	1.4649E+0	-3E-3	5.1E+1	-1.3E+0	-1.2999E+0
Option: 6221 Compliance{Double Float}=10.000000	0E+0	1.243168675E-3	1.56E-1	1.243168675E-3	3.371767975E-6	1.904411096E-5	-1.795896E+2	-1.904679796E-5	-1.380315146E-7	1.2008E+1	1.1976E+1	8.58166E+1	6.2996E+1	4.285530653E-3	5.57E+2	9E+0	1.2E+1	1.8E+0	1.2015E+1	1.198E+1	8.57808E+1	6.2996E+1	1.7E+0	1.2E+1	2.677898621E-3	1.4649E+0	-3E-3	5.2E+1	-1.5E+0	-1.4999E+0
Option: 6221 Duty Cycle{Double Float}=50.000000	0E+0	1.243168675E-3	1.56E-1	1.243168675E-3	3.371767975E-6	1.904886272E-5	-1.796424E+2	-1.905149315E-5	-1.195923194E-7	1.2006E+1	1.1975E+1	8.58166E+1	6.2996E+1	3.045605728E-3	5.58E+2	9E+0	1.2E+1	1.8E+0	1.2008E+1	1.1976E+1	8.58166E+1	6.2996E+1	1.7E+0	1.2E+1	4.285530653E-3	1.4649E+0	-3E-3	5.3E+1	-1.5E+0	-1.5E+0
Option: 6221 External Trigger{Boolean}=False	0E+0	1.237605158E-3	1.56E-1	1.237605158E-3	3.371767975E-6	1.24918785E-5	-1.79538E+2	-1.249451743E-5	-1.022067698E-7	1.2271E+1	1.2136E+1	8.60673E+1	6.2996E+1	2.003584653E-1	5.59E+2	9E+0	1.2E+1	1.8E+0	1.2006E+1	1.1975E+1	8.58166E+1	6.2996E+1	1.7E+0	1.2E+1	3.045605728E-3	1.4649E+0	-3E-3	5.4E+1	-1E+0	-1.0001E+0
Option: 6221 External Trigger Ignore Multiple{Boolean}=False	0E+0	1.233559093E-3	1.548E-1	1.233559093E-3	3.338050296E-6	5.973304333E-6	-1.790184E+2	-5.975937599E-6	-1.037872383E-7	1.1971E+1	1.1892E+1	8.57808E+1	6.2996E+1	3.696641922E-1	5.6E+2	9E+0	1.2E+1	1.8E+0	1.2271E+1	1.2136E+1	8.60673E+1	6.2996E+1	1.7E+0	1.2E+1	2.003584653E-1	1.4649E+0	-3E-3	5.5E+1	-5E-1	-5.001E-1
Option: 6221 Frequency{Double Float}=119.770000	
Option: 6221 Function{U16}=1	
Option: 6221 Function.__text__{String}=Sine	
Option: 6221 Idle Level{Double Float}=0.000000	
Option: 6221 Input trigger Line{U8}=5	
Option: 6221 Offset{Double Float}=0.000000	
Option: 6221 Output Trigger Line{U8}=4	
Option: 6221 Pass Through{Boolean}=True	
Option: 6221 Phase Marker{Boolean}=True	
Option: 6221 Phase Marker Phase{Double Float}=0.000000	
Option: 6221 Range Level{Double Float}=2.000000E-12	
Option: 6221 Ranging{U16}=1	
Option: 6221 Ranging.__text__{String}=Best	
Option: 6221 Update Clock{Double Float}=0.000000	
Option: 6221 VISA{Visa Refnum (Void)}=GPIB0::13::INSTR	
Option: Confirm Config{Boolean}=False	
Option: Control Panel Ref{LVObjVI Refnum (Void)}=	
Option: DAQ Global Channel{Boolean}=False	
Option: DAQ Input Rate{Double Float}=10000.000000	
Option: DAQ Input Samples{I32}=200	
Option: DAQ Measurement Channels{1D Array (Cluster (UserDefinedRefnumTag Refnum (Void),\tkDAQmxPhysChanTagType Tag,\tkDAQmxScaleTagType Tag,Boolean,Double Float,String))}=[]	
Option: Differential{I32}=10106	
Option: Differential.__text__{String}=Differential	
Option: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values))}=Function Generator	
Option: Lockin Standoff Time{Double Float}=0.000000	
Option: Paranoid Save Data{Boolean}=True	
Option: Plot Autoback Path{Path}=C:\\\\TEMP\\\\XY Multiparam\\\\Backup.txt	
Option: SR830  Ref Phase{Double Float}=0.000000	
Option: SR830  Synch Filter{Boolean}=False	
Option: SR830  Time Constant{I16}=8	
Option: SR830  Time Constant.__text__{String}=100 ms	
Option: SR830 2x Line Filter{Boolean}=True	
Option: SR830 Adjust Gains{Boolean}=False	
Option: SR830 Auto Gain Lower.__text__{String}=2 nV/fA	
Option: SR830 Auto Gain Upper.__text__{String}=1 V/uA	
Option: SR830 Auto Offset 1{Boolean}=False	
Option: SR830 Auto Offset 2{Boolean}=False	
Option: SR830 Autophase{Boolean}=False	
Option: SR830 DC Coupling?{Boolean}=False	
Option: SR830 Display 1{U16}=0	
Option: SR830 Display 1.__text__{String}=X	
Option: SR830 Display 2{U16}=0	
Option: SR830 Display 2.__text__{String}=Y	
Option: SR830 Dynamic Reserve{I16}=1	
Option: SR830 Dynamic Reserve.__text__{String}=Normal	
Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Option: SR830 Filter Slope{I32}=1	
Option: SR830 Filter Slope.__text__{String}=12 dB/oct	
Option: SR830 Gain{I32}=-1	
Option: SR830 Gain.__text__{String}=Auto Gain	
Option: SR830 Ground Shield?{Boolean}=False	
Option: SR830 Harmonic{I32}=1	
Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A	
Option: SR830 Line Filter{Boolean}=True	
Option: SR830 No Reset{Boolean}=False	
Option: SR830 Offset 1{Double Float}=0.000000	
Option: SR830 Offset 2{Double Float}=0.000000	
Option: SR830 Output Channel 1{Boolean}=False	
Option: SR830 Output Channel 2{Boolean}=False	
Option: SR830 Ratio 1{U16}=0	
Option: SR830 Ratio 1.__text__{String}=None	
Option: SR830 Ratio 2{U16}=0	
Option: SR830 Ratio 2.__text__{String}=None	
Option: SR830 Ref Amplitude{Double Float}=0.100000	
Option: SR830 Ref Frequency{Double Float}=1013.000000	
Option: SR830 Ref Source{Boolean}=False	
Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta]	
Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Option: SR830 VISA{Visa Refnum (Void)}=	
Option: Sense Autorange{Boolean}=False	
Option: Sense Range Level{Double Float}=0.100000	
Option: Sense Rate{Double Float}=1.000000	
Option:560 Comport{Visa Refnum (Void)}=COM1	
Option:560 Filter High Pass{U16}=0	
Option:560 Filter High Pass.__text__{String}=0.03	
Option:560 Filter Lowpass{U16}=0	
Option:560 Filter Lowpass.__text__{String}=0.03	
Option:560 Filter Mode{U16}=0	
Option:560 Filter Mode.__text__{String}=6 dB high pass	
Option:560 Invert{Boolean}=False	
Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Option:570 Enabled{Boolean}=False	
Option:570 Filter High Pass{U16}=0	
Option:570 Filter High Pass.__text__{String}=0.03	
Option:570 Filter Lowpass{U16}=0	
Option:570 Filter Lowpass.__text__{String}=0.03	
Option:570 Filter Mode{U16}=0	
Option:570 Filter Mode.__text__{String}=6 dB high pass	
Option:570 Gain Mode{U16}=0	
Option:570 Gain Mode.__text__{String}=Low Noise	
Option:570 Input Offset{U16}=0	
Option:570 Input Offset On{Boolean}=False	
Option:570 Input Offset.__text__{String}=1pA	
Option:570 Sensitivity{U16}=0	
Option:570 Sensitivity.__text__{String}=1pA/V	
Option:Debug On{Boolean}=False	
Option:GPIB 2182{Visa Refnum (Void)}=	
Option:Parallel Config Voltage Measurers{Boolean}=True	
Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Option:SR830 Settle Time{Double Float}=5.000000	
Option:Sense Digits{I32}=8	
Output Names{1D Array (String)}=['Offset','Rxx::R','Rxx::Theta','Rxx::X','Rxx::Y','Rxy::R','Rxy::Theta','Rxy::X','Rxy::Y','temperature: T1','temperature: T2','temperature: T3','temperature: T4','temperature: dT/dt','iterator','multi[0]:iterator','multi[0]:y','multi[0]:temperature: setpoint','multi[0]:temperature: T1','multi[0]:temperature: T2','multi[0]:temperature: T3','multi[0]:temperature: T4','multi[0]:temperature: heater','multi[0]:temperature: gas','multi[0]:temperature: dT/dt','multi[0]:temperature: current temperature','multi[0]:temperature: error','multi[1]:iterator','multi[1]:y','multi[1]:Control:Magnet Output']	
Parameter Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Parameter Select{U16}=6	
Parameter Select.__text__{String}=Multi-Parameter	
Paths{U32}=0	
Plot: Column Renames{1D Array (Cluster (String,String))}=[]	
Plot: No dups{Boolean}=False	
Plot: StdDevs{Boolean}=False	
Plotting Class{String}=Parameter Plot	
Plotting Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	
Plotting Select{U16}=1	
Plotting Select.__text__{String}=Parameter Plot	
Project Code{String}=Topological_Insulators	
Ref: Temperature Window{LVObjVI Refnum (Void)}=	
Ref:Control Subpanel{LVObjUnknown Refnum (Void)}=	
Ref:Main Screen{LVObjVI Refnum (Void)}=	
Ref:Plotting Subpanel{LVObjUnknown Refnum (Void)}=	
Ref:Toolbar{LVObjUnknown Refnum (Void)}=	
Ref:XY Subpanel{LVObjUnknown Refnum (Void)}=	
Rxx::R{Double Float}=0.001234	
Rxx::Theta{Double Float}=0.154800	
Rxx::X{Double Float}=0.001234	
Rxx::Y{Double Float}=3.338050E-6	
Rxx:Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	
Rxx:Option: 560 Enabled{Boolean}=False	
Rxx:Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	
Rxx:Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	
Rxx:Option: Lockin Standoff Time{Double Float}=0.000000	
Rxx:Option: Lockin Type{Enum U16 ((SRS 830,EG&G 5302))}=SRS 830	
Rxx:Option: SR803 Full Scale Reading{Double Float}=0.000000	
Rxx:Option: SR830  Ref Phase{Double Float}=0.000000	
Rxx:Option: SR830  Synch Filter{Boolean}=False	
Rxx:Option: SR830  Time Constant{I16}=8	
Rxx:Option: SR830 2x Line Filter{Boolean}=False	
Rxx:Option: SR830 Adjust Gains{Boolean}=False	
Rxx:Option: SR830 Auto Gain Lower{I32}=0	
Rxx:Option: SR830 Auto Gain Upper{I32}=26	
Rxx:Option: SR830 Auto Offset 1{Boolean}=False	
Rxx:Option: SR830 Auto Offset 2{Boolean}=False	
Rxx:Option: SR830 Autophase{Boolean}=False	
Rxx:Option: SR830 DC Coupling?{Boolean}=False	
Rxx:Option: SR830 Display 1{U16}=0	
Rxx:Option: SR830 Display 2{U16}=0	
Rxx:Option: SR830 Dynamic Reserve{I16}=2	
Rxx:Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Rxx:Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Rxx:Option: SR830 Filter Slope{I32}=3	
Rxx:Option: SR830 Gain{I32}=18	
Rxx:Option: SR830 Ground Shield?{Boolean}=False	
Rxx:Option: SR830 Harmonic{I32}=1	
Rxx:Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A-B	
Rxx:Option: SR830 Line Filter{Boolean}=False	
Rxx:Option: SR830 No Reset{Boolean}=False	
Rxx:Option: SR830 Offset 1{Double Float}=0.000000	
Rxx:Option: SR830 Offset 2{Double Float}=0.000000	
Rxx:Option: SR830 Output Channel 1{Boolean}=False	
Rxx:Option: SR830 Output Channel 2{Boolean}=False	
Rxx:Option: SR830 Ratio 1{U16}=0	
Rxx:Option: SR830 Ratio 2{U16}=0	
Rxx:Option: SR830 Ref Amplitude{Double Float}=0.100000	
Rxx:Option: SR830 Ref Frequency{Double Float}=1013.000000	
Rxx:Option: SR830 Ref Source{Boolean}=False	
Rxx:Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta,X,Y]	
Rxx:Option: SR830 Time Constant value{Double Float}=0.000000	
Rxx:Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Rxx:Option: SR830 VISA{Visa Refnum (Void)}=GPIB0::5::INSTR	
Rxx:Option:560 Comport{Visa Refnum (Void)}=COM1	
Rxx:Option:560 Filter High Pass{U16}=0	
Rxx:Option:560 Filter Lowpass{U16}=0	
Rxx:Option:560 Filter Mode{U16}=0	
Rxx:Option:560 Invert{Boolean}=False	
Rxx:Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Rxx:Option:570 Enabled{Boolean}=False	
Rxx:Option:570 Filter High Pass{U16}=0	
Rxx:Option:570 Filter Lowpass{U16}=0	
Rxx:Option:570 Filter Mode{U16}=0	
Rxx:Option:570 Gain Mode{U16}=0	
Rxx:Option:570 Input Offset{U16}=0	
Rxx:Option:570 Input Offset On{Boolean}=False	
Rxx:Option:570 Sensitivity{U16}=0	
Rxx:Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Rxx:Option:SR830 Autogain Lower Threshold{Double Float}=0.100000	
Rxx:Option:SR830 Autogain Standoff{Double Float}=3.000000	
Rxx:Option:SR830 Autogain Upper Threshold{Double Float}=0.900000	
Rxx:Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Rxx:Option:SR830 Settle Time{Double Float}=0.000000	
Rxy::R{Double Float}=5.973304E-6	
Rxy::Theta{Double Float}=-179.018400	
Rxy::X{Double Float}=-5.975938E-6	
Rxy::Y{Double Float}=-1.037872E-7	
Rxy:Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	
Rxy:Option: 560 Enabled{Boolean}=False	
Rxy:Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	
Rxy:Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	
Rxy:Option: Lockin Standoff Time{Double Float}=0.000000	
Rxy:Option: Lockin Type{Enum U16 ((SRS 830,EG&G 5302))}=SRS 830	
Rxy:Option: SR803 Full Scale Reading{Double Float}=0.000000	
Rxy:Option: SR830  Ref Phase{Double Float}=0.000000	
Rxy:Option: SR830  Synch Filter{Boolean}=False	
Rxy:Option: SR830  Time Constant{I16}=8	
Rxy:Option: SR830 2x Line Filter{Boolean}=False	
Rxy:Option: SR830 Adjust Gains{Boolean}=False	
Rxy:Option: SR830 Auto Gain Lower{I32}=0	
Rxy:Option: SR830 Auto Gain Upper{I32}=26	
Rxy:Option: SR830 Auto Offset 1{Boolean}=False	
Rxy:Option: SR830 Auto Offset 2{Boolean}=False	
Rxy:Option: SR830 Autophase{Boolean}=False	
Rxy:Option: SR830 DC Coupling?{Boolean}=False	
Rxy:Option: SR830 Display 1{U16}=0	
Rxy:Option: SR830 Display 2{U16}=1	
Rxy:Option: SR830 Dynamic Reserve{I16}=2	
Rxy:Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Rxy:Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Rxy:Option: SR830 Filter Slope{I32}=3	
Rxy:Option: SR830 Gain{I32}=18	
Rxy:Option: SR830 Ground Shield?{Boolean}=False	
Rxy:Option: SR830 Harmonic{I32}=1	
Rxy:Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A-B	
Rxy:Option: SR830 Line Filter{Boolean}=False	
Rxy:Option: SR830 No Reset{Boolean}=False	
Rxy:Option: SR830 Offset 1{Double Float}=0.000000	
Rxy:Option: SR830 Offset 2{Double Float}=0.000000	
Rxy:Option: SR830 Output Channel 1{Boolean}=False	
Rxy:Option: SR830 Output Channel 2{Boolean}=False	
Rxy:Option: SR830 Ratio 1{U16}=0	
Rxy:Option: SR830 Ratio 2{U16}=0	
Rxy:Option: SR830 Ref Amplitude{Double Float}=0.100000	
Rxy:Option: SR830 Ref Frequency{Double Float}=1013.000000	
Rxy:Option: SR830 Ref Source{Boolean}=False	
Rxy:Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta,X,Y]	
Rxy:Option: SR830 Time Constant value{Double Float}=0.000000	
Rxy:Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Rxy:Option: SR830 VISA{Visa Refnum (Void)}=GPIB0::6::INSTR	
Rxy:Option:560 Comport{Visa Refnum (Void)}=COM1	
Rxy:Option:560 Filter High Pass{U16}=0	
Rxy:Option:560 Filter Lowpass{U16}=0	
Rxy:Option:560 Filter Mode{U16}=0	
Rxy:Option:560 Invert{Boolean}=False	
Rxy:Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Rxy:Option:570 Enabled{Boolean}=False	
Rxy:Option:570 Filter High Pass{U16}=0	
Rxy:Option:570 Filter Lowpass{U16}=0	
Rxy:Option:570 Filter Mode{U16}=0	
Rxy:Option:570 Gain Mode{U16}=0	
Rxy:Option:570 Input Offset{U16}=0	
Rxy:Option:570 Input Offset On{Boolean}=False	
Rxy:Option:570 Sensitivity{U16}=0	
Rxy:Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Rxy:Option:SR830 Autogain Lower Threshold{Double Float}=0.100000	
Rxy:Option:SR830 Autogain Standoff{Double Float}=3.000000	
Rxy:Option:SR830 Autogain Upper Threshold{Double Float}=0.900000	
Rxy:Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Rxy:Option:SR830 Settle Time{Double Float}=0.000000	
Sample ID{String}=MBE202221213_PA_D1 750C Cracker WAL	
Save:Filename{String}=${X-Y Class} ${2nd Parameter Class} ${iterator}{%04d} ${y}{%04.2g}.txt	
Save:Final Filename{String}=${X-Y Class} ${2nd Parameter Class} .txt	
Save:Final path{Path}=C:\\\\Data\\\\${Project Code}\\\\${User}\\\\${Sample ID}\\\\${Measurement Timestamp}{%Y%m%d}\\\\${X-Y Class}	
Save:Path{Path}=C:\\\\Data\\\\${Project Code}\\\\${User}\\\\${Sample ID}\\\\${Measurement Timestamp}{%Y%m%d}\\\\${X-Y Class}	
Startup path{Path}=C:\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV	
Sub Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Sweep Step{I32}=3	
T Control Measure.__text__{1D Array (String)}=['temperature: T1','temperature: T2','temperature: T3','temperature: T4','temperature: dT/dt']	
Timestamp{Timestamp}=<23:48:13.155 17/05/2023>T	
Toolbar{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Unaved Data{Boolean}=True	
Unsaved Data{Boolean}=False	
User{String}=Craig	
X-Y Class{String}=6221-Lockin-DAQ	
X-Y Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	
d(Offset){Double Float}=0.000000	
d(Rxx::R){Double Float}=0.000000	
d(Rxx::Theta){Double Float}=0.002683	
d(Rxx::X){Double Float}=0.000000	
d(Rxx::Y){Double Float}=7.539502E-8	
d(Rxy::R){Double Float}=1.095581E-8	
d(Rxy::Theta){Double Float}=0.067162	
d(Rxy::X){Double Float}=1.095785E-8	
d(Rxy::Y){Double Float}=7.814255E-9	
iterate result{U16}=5	
iterator{I32}=560	
multi[0]:Control: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values,Adaptive Step Ramp))}=List of Values	
multi[0]:Control: Monitor Update Timeout{Double Float}=0.010000	
multi[0]:Control: Open T Window{Boolean}=False	
multi[0]:Control: Reverse Temperature Sense{Boolean}=False	
multi[0]:Iterator{I32}=0	
multi[0]:Ref: Temperature Window{LVObjVI Refnum (Void)}=	
multi[0]:iterate result{U16}=0	
multi[0]:iterator{I32}=9	
multi[0]:temperature:  rate window{Double Float}=120.000000	
multi[0]:temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[0]:temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
multi[0]:temperature: T1{Double Float}=12.011000	
multi[0]:temperature: T2{Double Float}=11.966000	
multi[0]:temperature: T3{Double Float}=86.210600	
multi[0]:temperature: T4{Double Float}=62.996000	
multi[0]:temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
multi[0]:temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
multi[0]:temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
multi[0]:temperature: current temperature{Double Float}=1.464900	
multi[0]:temperature: current temperature 2{Double Float}=287.100000	
multi[0]:temperature: dT/dt{Double Float}=0.038443	
multi[0]:temperature: error{Double Float}=-0.003000	
multi[0]:temperature: gas{Double Float}=12.000000	
multi[0]:temperature: gas control{Boolean}=False	
multi[0]:temperature: gas control 2{Boolean}=False	
multi[0]:temperature: gass boost{I8}=0	
multi[0]:temperature: gass boost 2{I8}=0	
multi[0]:temperature: gast flow{I16}=0	
multi[0]:temperature: gast flow 2{I16}=7	
multi[0]:temperature: heater{Double Float}=1.700000	
multi[0]:temperature: heater output{Double Float}=0.000000	
multi[0]:temperature: heater output 2{Double Float}=0.000000	
multi[0]:temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
multi[0]:temperature: monitor timeout{Double Float}=0.010000	
multi[0]:temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
multi[0]:temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
multi[0]:temperature: ramp rate{Double Float}=8.000000	
multi[0]:temperature: ramp rate 2{Double Float}=0.000000	
multi[0]:temperature: ramp target{Double Float}=20.000000	
multi[0]:temperature: ramp target 2{Double Float}=0.000000	
multi[0]:temperature: ramping{Boolean}=False	
multi[0]:temperature: setpoint{Double Float}=1.800000	
multi[0]:temperature: setpoint 2{Double Float}=287.100000	
multi[0]:temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
multi[0]:temperature: stability error{Extended Float}=0.040000	
multi[0]:temperature: stability script{String}=	
multi[0]:temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
multi[0]:temperature: temp control mode{U16}=2	
multi[0]:temperature: temp control mode 2{U16}=3	
multi[0]:temperature: temp control mode 2.__text__{String}=Open Loop	
multi[0]:temperature: temp control mode.__text__{String}=Zone	
multi[0]:temperature: temp control sensor{U16}=0	
multi[0]:temperature: temp control sensor 2{U16}=0	
multi[0]:temperature: temp control sensor 2.__text__{String}=Sensor 1	
multi[0]:temperature: temp control sensor.__text__{String}=Sensor A	
multi[0]:temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
multi[0]:temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
multi[0]:temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
multi[0]:temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
multi[0]:temperature: temp loop{U16}=0	
multi[0]:temperature: temp loop 2{U16}=0	
multi[0]:temperature: temp loop 2.__text__{String}=Heater	
multi[0]:temperature: temp loop.__text__{String}=Loop 1	
multi[0]:temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
multi[0]:temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[0]:temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[0]:temperature:error for gas boost{Double Float}=0.000000	
multi[0]:temperature:error for gas boost 2{Double Float}=0.000000	
multi[0]:temperature:heater range{U16}=2	
multi[0]:temperature:heater range 2{U16}=0	
multi[0]:temperature:heater range 2.__text__{String}=Off	
multi[0]:temperature:heater range.__text__{String}=40mW	
multi[0]:temperature:history window{Extended Float}=300.000000	
multi[0]:temperature:is stable?{Boolean}=False	
multi[0]:temperature:monitor{Boolean}=True	
multi[0]:temperature:ramping{Boolean}=False	
multi[0]:temperature:ramping on{Boolean}=False	
multi[0]:temperature:ramping on 2{Boolean}=False	
multi[0]:temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
multi[0]:temperature:stability code{U32}=6618880	
multi[0]:temperature:stability rate{Extended Float}=0.040000	
multi[0]:y{Double Float}=12.000000	
multi[1]:Control: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values,Adaptive Step Ramp))}=Multi-Segment Ramp	
multi[1]:Control: Gate delay{Double Float}=0.000000	
multi[1]:Control: Monitor Update Timeout{Double Float}=0.010000	
multi[1]:Control: Open T Window{Boolean}=False	
multi[1]:Control: Reverse Temperature Sense{Boolean}=False	
multi[1]:Control:Magnet Output{Double Float}=-0.000000	
multi[1]:Iterator{I32}=0	
multi[1]:Magnet: Final Switch Heater{Enum U8 ((False,True,Mixed))}=	
multi[1]:Magnet: Power Supply{Enum U16 ((IPS120,LS625,PS110,Hg iPS,SMS Series,Cryomagnetics 4G,DMG Little CryoFree,DMG Big CryoFree))}=Hg iPS	
multi[1]:Magnet: Rate{Double Float}=0.500000	
multi[1]:Magnet: Units{Enum U16 ((Field,Current))}=Field	
multi[1]:Magnet: VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[1]:Multi-segment_Stage{I32}=0	
multi[1]:Multi-segment_Stage_Changed{Boolean}=False	
multi[1]:Ref: Temperature Window{LVObjVI Refnum (Void)}=	
multi[1]:iterate result{U16}=4	
multi[1]:iterator{I32}=57	
multi[1]:measure point{Boolean}=False	
multi[1]:temperature:  rate window{Double Float}=120.000000	
multi[1]:temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[1]:temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
multi[1]:temperature: T1{Double Float}=1.842400	
multi[1]:temperature: T2{Double Float}=1.465600	
multi[1]:temperature: T3{Double Float}=86.318100	
multi[1]:temperature: T4{Double Float}=66.769200	
multi[1]:temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
multi[1]:temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
multi[1]:temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
multi[1]:temperature: current temperature{Double Float}=1.465600	
multi[1]:temperature: current temperature 2{Double Float}=287.100000	
multi[1]:temperature: dT/dt{Double Float}=-0.001864	
multi[1]:temperature: gas control{Boolean}=False	
multi[1]:temperature: gas control 2{Boolean}=False	
multi[1]:temperature: gass boost{I8}=0	
multi[1]:temperature: gass boost 2{I8}=0	
multi[1]:temperature: gast flow{I16}=0	
multi[1]:temperature: gast flow 2{I16}=7	
multi[1]:temperature: heater output{Double Float}=0.000000	
multi[1]:temperature: heater output 2{Double Float}=0.000000	
multi[1]:temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
multi[1]:temperature: monitor timeout{Double Float}=1.000000	
multi[1]:temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
multi[1]:temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
multi[1]:temperature: ramp rate{Double Float}=8.000000	
multi[1]:temperature: ramp rate 2{Double Float}=0.000000	
multi[1]:temperature: ramp target{Double Float}=20.000000	
multi[1]:temperature: ramp target 2{Double Float}=0.000000	
multi[1]:temperature: ramping{Boolean}=False	
multi[1]:temperature: setpoint{Double Float}=1.800000	
multi[1]:temperature: setpoint 2{Double Float}=287.100000	
multi[1]:temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
multi[1]:temperature: stability error{Extended Float}=0.040000	
multi[1]:temperature: stability script{String}=	
multi[1]:temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
multi[1]:temperature: temp control mode{U16}=2	
multi[1]:temperature: temp control mode 2{U16}=3	
multi[1]:temperature: temp control mode 2.__text__{String}=Open Loop	
multi[1]:temperature: temp control mode.__text__{String}=Zone	
multi[1]:temperature: temp control sensor{U16}=0	
multi[1]:temperature: temp control sensor 2{U16}=0	
multi[1]:temperature: temp control sensor 2.__text__{String}=Sensor 1	
multi[1]:temperature: temp control sensor.__text__{String}=Sensor A	
multi[1]:temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
multi[1]:temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
multi[1]:temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
multi[1]:temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
multi[1]:temperature: temp loop{U16}=0	
multi[1]:temperature: temp loop 2{U16}=0	
multi[1]:temperature: temp loop 2.__text__{String}=Heater	
multi[1]:temperature: temp loop.__text__{String}=Loop 1	
multi[1]:temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
multi[1]:temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[1]:temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[1]:temperature:error for gas boost{Double Float}=0.000000	
multi[1]:temperature:error for gas boost 2{Double Float}=0.000000	
multi[1]:temperature:heater range{U16}=2	
multi[1]:temperature:heater range 2{U16}=0	
multi[1]:temperature:heater range 2.__text__{String}=Off	
multi[1]:temperature:heater range.__text__{String}=40mW	
multi[1]:temperature:history window{Extended Float}=300.000000	
multi[1]:temperature:is stable?{Boolean}=True	
multi[1]:temperature:monitor{Boolean}=True	
multi[1]:temperature:ramping{Boolean}=False	
multi[1]:temperature:ramping on{Boolean}=False	
multi[1]:temperature:ramping on 2{Boolean}=False	
multi[1]:temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
multi[1]:temperature:stability code{U32}=6618880	
multi[1]:temperature:stability rate{Extended Float}=0.040000	
multi[1]:y{Double Float}=0.000000	
parameter: Termination{String}=False	
parameter: delta time{Double Float}=1.000000	
parameter: progress{Double Float}=100.000000	
temperature:  rate window{Double Float}=120.000000	
temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
temperature: T1{Double Float}=12.011000	
temperature: T2{Double Float}=11.966000	
temperature: T3{Double Float}=86.210600	
temperature: T4{Double Float}=62.996000	
temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
temperature: current temperature{Double Float}=1.464900	
temperature: current temperature 2{Double Float}=287.100000	
temperature: dT/dt{Double Float}=0.038443	
temperature: gas control{Boolean}=False	
temperature: gas control 2{Boolean}=False	
temperature: gass boost{I8}=0	
temperature: gass boost 2{I8}=0	
temperature: gast flow{I16}=0	
temperature: gast flow 2{I16}=7	
temperature: heater output{Double Float}=0.000000	
temperature: heater output 2{Double Float}=0.000000	
temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
temperature: monitor timeout{Double Float}=0.010000	
temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
temperature: ramp rate{Double Float}=8.000000	
temperature: ramp rate 2{Double Float}=0.000000	
temperature: ramp target{Double Float}=20.000000	
temperature: ramp target 2{Double Float}=0.000000	
temperature: ramping{Boolean}=False	
temperature: setpoint{Double Float}=1.800000	
temperature: setpoint 2{Double Float}=287.100000	
temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
temperature: stability error{Extended Float}=0.040000	
temperature: stability script{String}=	
temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
temperature: temp control mode{U16}=2	
temperature: temp control mode 2{U16}=3	
temperature: temp control mode 2.__text__{String}=Open Loop	
temperature: temp control mode.__text__{String}=Zone	
temperature: temp control sensor{U16}=0	
temperature: temp control sensor 2{U16}=0	
temperature: temp control sensor 2.__text__{String}=Sensor 1	
temperature: temp control sensor.__text__{String}=Sensor A	
temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
temperature: temp loop{U16}=0	
temperature: temp loop 2{U16}=0	
temperature: temp loop 2.__text__{String}=Heater	
temperature: temp loop.__text__{String}=Loop 1	
temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
temperature:error for gas boost{Double Float}=0.000000	
temperature:error for gas boost 2{Double Float}=0.000000	
temperature:heater range{U16}=2	
temperature:heater range 2{U16}=0	
temperature:heater range 2.__text__{String}=Off	
temperature:heater range.__text__{String}=40mW	
temperature:history window{Extended Float}=300.000000	
temperature:is stable?{Boolean}=False	
temperature:monitor{Boolean}=True	
temperature:ramping{Boolean}=False	
temperature:ramping on{Boolean}=False	
temperature:ramping on 2{Boolean}=False	
temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
temperature:stability code{U32}=6618880	
temperature:stability rate{Extended Float}=0.040000	
y{Double Float}=12.000000	
