TDI Format 1.5	Offset	Rxx::R	Rxx::Theta	Rxx::X	Rxx::Y	Rxy::R	Rxy::Theta	Rxy::X	Rxy::Y	temperature: T1	temperature: T2	temperature: T3	temperature: T4	temperature: dT/dt	iterator	multi[0]:iterator	multi[0]:y	multi[0]:temperature: setpoint	multi[0]:temperature: T1	multi[0]:temperature: T2	multi[0]:temperature: T3	multi[0]:temperature: T4	multi[0]:temperature: heater	multi[0]:temperature: gas	multi[0]:temperature: dT/dt	multi[0]:temperature: current temperature	multi[0]:temperature: error	multi[1]:iterator	multi[1]:y	multi[1]:Control:Magnet Output
2nd Parameter Class{String}=Multi-Parameter	0E+0	1.226647832E-3	1.56E-1	1.226647832E-3	3.203179577E-6	5.905852003E-7	-7.5492E+0	5.84790036E-7	-7.902568818E-8	2.4611E+0	2.5326E+0	8.60315E+1	6.52378E+1	6.412574649E-2	2.25E+2	4E+0	2.4E+0	2.4E+0	2.4381E+0	2.4921E+0	8.60673E+1	6.52378E+1	2.7E+0	2.4E+0	5.423092283E-3	2.4419E+0	-4.19E-2	0E+0	0E+0	0E+0
2nd Parameter Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	0E+0	1.233727385E-3	1.56E-1	1.233727385E-3	3.371767975E-6	7.20451866E-6	-5.22E-1	7.20451866E-6	-6.690850839E-8	2.3504E+0	2.5185E+0	8.62464E+1	6.52378E+1	1.93477869E-2	2.26E+2	4E+0	2.4E+0	1.8E+0	2.4611E+0	2.5326E+0	8.60315E+1	6.52378E+1	2.7E+0	2.4E+0	6.412574649E-2	1.4649E+0	-4.19E-2	1E+0	5E-1	4.999E-1
Analysis Class{String}=Basic Plot	0E+0	1.23777345E-3	1.56E-1	1.23777345E-3	3.371767975E-6	1.379843082E-5	-1.752E-1	1.379843082E-5	-4.267392253E-8	2.3554E+0	2.4953E+0	8.60673E+1	6.52378E+1	7.820194587E-3	2.27E+2	4E+0	2.4E+0	1.8E+0	2.3504E+0	2.5185E+0	8.62464E+1	6.52378E+1	2.7E+0	2.4E+0	1.93477869E-2	1.4649E+0	-4.19E-2	2E+0	1E+0	9.999E-1
Analysis Class Path{Path}=C\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV\\\\plugins\\\\Plotting\\\\Plotting_Base_class\\\\Plotting_Base.lvclass	0E+0	1.243674963E-3	1.56E-1	1.243674963E-3	3.371767975E-6	2.041705777E-5	-8.16E-2	2.041705777E-5	-3.055660132E-8	2.452E+0	2.5259E+0	8.59957E+1	6.52378E+1	5.255256966E-2	2.28E+2	4E+0	2.4E+0	1.8E+0	2.3554E+0	2.4953E+0	8.60673E+1	6.52378E+1	2.7E+0	2.4E+0	7.820194587E-3	1.4649E+0	-4.19E-2	3E+0	1.5E+0	1.4999E+0
Analysis.# pre-routines{I32}=5	0E+0	1.243708621E-3	1.56E-1	1.243708621E-3	3.371767975E-6	2.042127212E-5	-9.72E-2	2.042127212E-5	-3.63518505E-8	2.337E+0	2.478E+0	8.5745E+1	6.52378E+1	-1.612171531E-2	2.29E+2	4E+0	2.4E+0	1.8E+0	2.452E+0	2.5259E+0	8.59957E+1	6.52378E+1	2.7E+0	2.4E+0	5.255256966E-2	1.4649E+0	-4.19E-2	4E+0	1.5E+0	1.5E+0
Analysis:Pre[0]:T Control Measure{1D Array (I32)}=[1,2,3,4,7]	0E+0	1.240976644E-3	1.56E-1	1.240976644E-3	3.371767975E-6	1.777233699E-5	-1.044E-1	1.777233699E-5	-3.424450259E-8	2.3455E+0	2.4848E+0	8.57808E+1	6.52378E+1	-1.687754877E-2	2.3E+2	4E+0	2.4E+0	1.8E+0	2.337E+0	2.478E+0	8.5745E+1	6.52378E+1	2.7E+0	2.4E+0	-1.612171531E-2	1.4649E+0	-4.19E-2	5E+0	1.3E+0	1.3002E+0
Autosave Tabs{Enum U32 ((XY Measurement Save,Parameter Plot Save 2))}=Parameter Plot Save 2	0E+0	1.238786027E-3	1.548E-1	1.238786027E-3	3.338050296E-6	1.510920314E-5	-2.16E-1	1.510920314E-5	-5.847908845E-8	2.3506E+0	2.4585E+0	8.61748E+1	6.52378E+1	-6.41720444E-2	2.31E+2	4E+0	2.4E+0	1.8E+0	2.3455E+0	2.4848E+0	8.57808E+1	6.52378E+1	2.7E+0	2.4E+0	-1.687754877E-2	1.4649E+0	-4.19E-2	6E+0	1.1E+0	1.1001E+0
Control:Magnet Output{Double Float}=-0.007000	0E+0	1.236762287E-3	1.56E-1	1.236762287E-3	3.371767975E-6	1.24729139E-5	-2.364E-1	1.24729139E-5	-5.268383926E-8	2.4329E+0	2.5102E+0	8.60673E+1	6.52378E+1	1.827870496E-2	2.32E+2	4E+0	2.4E+0	1.8E+0	2.3506E+0	2.4585E+0	8.61748E+1	6.52378E+1	2.7E+0	2.4E+0	-6.41720444E-2	1.4649E+0	-4.19E-2	7E+0	9E-1	9E-1
Control:Magnet Rate{Double Float}=0.500000	0E+0	1.235177519E-3	1.56E-1	1.235177519E-3	3.371767975E-6	9.836587889E-6	-3.96E-1	9.836587889E-6	-6.954262257E-8	2.3183E+0	2.4239E+0	8.60673E+1	6.52378E+1	-9.899234772E-2	2.33E+2	4E+0	2.4E+0	1.8E+0	2.4329E+0	2.5102E+0	8.60673E+1	6.52378E+1	2.7E+0	2.4E+0	1.827870496E-2	1.4649E+0	-4.19E-2	8E+0	7E-1	7.002E-1
Display Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	0E+0	1.233660068E-3	1.56E-1	1.233660068E-3	3.371767975E-6	7.178177519E-6	-4.728E-1	7.178177519E-6	-6.058643636E-8	2.3555E+0	2.4289E+0	8.60315E+1	6.52378E+1	-9.60592106E-2	2.34E+2	4E+0	2.4E+0	1.8E+0	2.3183E+0	2.4239E+0	8.60673E+1	6.52378E+1	2.7E+0	2.4E+0	-9.899234772E-2	1.4649E+0	-4.19E-2	9E+0	5E-1	5E-1
Elapsed Time{Double Float}=12790.950867	0E+0	1.232243875E-3	1.56E-1	1.232243875E-3	3.371767975E-6	4.530803671E-6	-1.008E+0	4.530803671E-6	-8.113312095E-8	2.3481E+0	2.4099E+0	8.60673E+1	6.52378E+1	-1.06895946E-1	2.35E+2	4E+0	2.4E+0	1.8E+0	2.3555E+0	2.4289E+0	8.60315E+1	6.52378E+1	2.7E+0	2.4E+0	-9.60592106E-2	1.4649E+0	-4.19E-2	1E+1	3E-1	3.001E-1
File:Autodel{Boolean}=True	0E+0	1.230490533E-3	1.56E-1	1.230490533E-3	3.371767975E-6	1.882917878E-6	-2.4804E+0	1.880287441E-6	-8.324052543E-8	2.4001E+0	2.4818E+0	8.58524E+1	6.52378E+1	-7.504609879E-3	2.36E+2	4E+0	2.4E+0	1.8E+0	2.3481E+0	2.4099E+0	8.60673E+1	6.52378E+1	2.7E+0	2.4E+0	-1.06895946E-1	1.4649E+0	-4.19E-2	1.1E+1	1E-1	1E-1
File:Autosave{Boolean}=False	0E+0	1.230524191E-3	1.56E-1	1.230524191E-3	3.371767975E-6	1.897673782E-6	-2.178E+0	1.89503486E-6	-7.270361616E-8	2.3371E+0	2.4701E+0	8.57808E+1	6.52378E+1	-2.246081829E-2	2.37E+2	4E+0	2.4E+0	1.8E+0	2.4001E+0	2.4818E+0	8.58524E+1	6.52378E+1	2.7E+0	2.4E+0	-7.504609879E-3	1.4649E+0	-4.19E-2	1.2E+1	1E-1	1E-1
File:Export Config{Boolean}=True	0E+0	1.2303559E-3	1.56E-1	1.2303559E-3	3.371767975E-6	1.754900438E-6	-2.2896E+0	1.753842606E-6	-7.165005534E-8	2.4382E+0	2.5126E+0	8.59599E+1	6.52378E+1	4.917355999E-2	2.38E+2	4E+0	2.4E+0	1.8E+0	2.3371E+0	2.4701E+0	8.57808E+1	6.52378E+1	2.7E+0	2.4E+0	-2.246081829E-2	1.4649E+0	-4.19E-2	1.3E+1	9E-2	9.01E-2
File:Final Autosave{Boolean}=True	0E+0	1.230187608E-3	1.56E-1	1.230187608E-3	3.371767975E-6	1.608441653E-6	-2.9028E+0	1.606337303E-6	-8.271361774E-8	2.4237E+0	2.4844E+0	8.59957E+1	6.52378E+1	-5.91142755E-3	2.39E+2	4E+0	2.4E+0	1.8E+0	2.4382E+0	2.5126E+0	8.59599E+1	6.52378E+1	2.7E+0	2.4E+0	4.917355999E-2	1.4649E+0	-4.19E-2	1.4E+1	8E-2	8.01E-2
Filter:Enable{Enum U16 ((None,Analog,Digital,Analog&Digitial))}=None	0E+0	1.229985376E-3	1.56E-1	1.229985376E-3	3.338050296E-6	1.49042836E-6	-3.1896E+0	1.487792266E-6	-8.482105051E-8	2.3509E+0	2.4514E+0	8.62106E+1	6.52378E+1	-5.884662271E-2	2.4E+2	4E+0	2.4E+0	1.8E+0	2.4237E+0	2.4844E+0	8.59957E+1	6.52378E+1	2.7E+0	2.4E+0	-5.91142755E-3	1.4649E+0	-4.19E-2	1.5E+1	7E-2	7E-2
Filter:Points{I32}=1	0E+0	1.229714978E-3	1.56E-1	1.229714978E-3	3.371767975E-6	1.350287998E-6	-3.24E+0	1.347653601E-6	-7.84989502E-8	2.4543E+0	2.5244E+0	8.61748E+1	6.52378E+1	5.216040462E-2	2.41E+2	4E+0	2.4E+0	1.8E+0	2.3509E+0	2.4514E+0	8.62106E+1	6.52378E+1	2.7E+0	2.4E+0	-5.884662271E-2	1.4649E+0	-4.19E-2	1.6E+1	6E-2	6.01E-2
Filter:Type{U16}=1	0E+0	1.229513028E-3	1.56E-1	1.229513028E-3	3.371767975E-6	1.220156592E-6	-3.6948E+0	1.217521912E-6	-8.007944699E-8	2.4308E+0	2.4625E+0	8.6139E+1	6.52378E+1	-2.849177644E-2	2.42E+2	4E+0	2.4E+0	1.8E+0	2.4543E+0	2.5244E+0	8.61748E+1	6.52378E+1	2.7E+0	2.4E+0	5.216040462E-2	1.4649E+0	-4.19E-2	1.7E+1	5E-2	5.01E-2
Filter:Type.__text__{String}=Repeat	0E+0	1.229513028E-3	1.56E-1	1.229513028E-3	3.338050296E-6	1.218048848E-6	-3.7428E+0	1.215941669E-6	-8.113306438E-8	2.4597E+0	2.5294E+0	8.6139E+1	6.52378E+1	7.212246209E-2	2.43E+2	4E+0	2.4E+0	1.8E+0	2.4308E+0	2.4625E+0	8.6139E+1	6.52378E+1	2.7E+0	2.4E+0	-2.849177644E-2	1.4649E+0	-4.19E-2	1.8E+1	5E-2	5E-2
Filter:Window{Double Float}=1.000000	0E+0	1.229344737E-3	1.56E-1	1.229344737E-3	3.371767975E-6	1.159570268E-6	-4.0956E+0	1.157462807E-6	-8.482105051E-8	2.3998E+0	2.4915E+0	8.6139E+1	6.52378E+1	2.295802347E-2	2.44E+2	4E+0	2.4E+0	1.8E+0	2.4597E+0	2.5294E+0	8.6139E+1	6.52378E+1	2.7E+0	2.4E+0	7.212246209E-2	1.4649E+0	-4.19E-2	1.9E+1	4.5E-2	4.5E-2
Iterator{I32}=0	0E+0	1.229344737E-3	1.56E-1	1.229344737E-3	3.304332616E-6	1.085813657E-6	-3.9552E+0	1.084232849E-6	-7.639163057E-8	2.3505E+0	2.458E+0	8.6139E+1	6.52378E+1	-4.176889732E-2	2.45E+2	4E+0	2.4E+0	1.8E+0	2.3998E+0	2.4915E+0	8.6139E+1	6.52378E+1	2.7E+0	2.4E+0	2.295802347E-2	1.4649E+0	-4.19E-2	2E+1	4E-2	3.99E-2
Magnet: Control Mode{Boolean}=False	0E+0	1.22900674E-3	1.56E-1	1.22900674E-3	3.371767975E-6	1.02891532E-6	-4.9656E+0	1.024700398E-6	-9.11431791E-8	2.428E+0	2.4892E+0	8.61032E+1	6.52378E+1	5.963979289E-3	2.46E+2	4E+0	2.4E+0	1.8E+0	2.3505E+0	2.458E+0	8.6139E+1	6.52378E+1	2.7E+0	2.4E+0	-4.176889732E-2	1.4649E+0	-4.19E-2	2.1E+1	3.5E-2	3.5E-2
Magnet: Final Switch Heater{Enum U8 ((False,True,Mixed))}=	0E+0	1.228703815E-3	1.56E-1	1.228703815E-3	3.371767975E-6	9.583186274E-7	-4.2276E+0	9.556850789E-7	-7.164997048E-8	2.4341E+0	2.4951E+0	8.60673E+1	6.52378E+1	1.42636802E-2	2.47E+2	4E+0	2.4E+0	1.8E+0	2.428E+0	2.4892E+0	8.61032E+1	6.52378E+1	2.7E+0	2.4E+0	5.963979289E-3	1.4649E+0	-4.19E-2	2.2E+1	3E-2	2.97E-2
Magnet: Power Supply{Enum U16 ((IPS120,LS625,PS110,Hg iPS,SMS Series,Cryomagnetics 4G,DMG Little CryoFree,DMG Big CryoFree))}=Hg iPS	0E+0	1.228535524E-3	1.56E-1	1.228535524E-3	3.371767975E-6	8.845620162E-7	-5.6832E+0	8.798204409E-7	-8.90358029E-8	2.4399E+0	2.5172E+0	8.61032E+1	6.52378E+1	4.655489698E-2	2.48E+2	4E+0	2.4E+0	1.8E+0	2.4341E+0	2.4951E+0	8.60673E+1	6.52378E+1	2.7E+0	2.4E+0	1.42636802E-2	1.4649E+0	-4.19E-2	2.3E+1	2.5E-2	2.5E-2
Magnet: Rate{Double Float}=0.500000	0E+0	1.228299633E-3	1.56E-1	1.228299633E-3	3.371767975E-6	8.260834368E-7	-5.082E+0	8.218687976E-7	-7.428431094E-8	2.3539E+0	2.4577E+0	8.60673E+1	6.52378E+1	-5.319289118E-2	2.49E+2	4E+0	2.4E+0	1.8E+0	2.4399E+0	2.5172E+0	8.61032E+1	6.52378E+1	2.7E+0	2.4E+0	4.655489698E-2	1.4649E+0	-4.19E-2	2.4E+1	2E-2	1.99E-2
Magnet: Setpoint{Double Float}=0.000000	0E+0	1.227995577E-3	1.56E-1	1.227995577E-3	3.371767975E-6	7.597022321E-7	-6.48E+0	7.554870272E-7	-8.745527782E-8	2.3468E+0	2.4532E+0	8.60673E+1	6.52378E+1	-6.11115545E-2	2.5E+2	4E+0	2.4E+0	1.8E+0	2.3539E+0	2.4577E+0	8.60673E+1	6.52378E+1	2.7E+0	2.4E+0	-5.319289118E-2	1.4649E+0	-4.19E-2	2.5E+1	1.5E-2	1.49E-2
Magnet: Units{Enum U16 ((Field,Current))}=Field	0E+0	1.227490703E-3	1.56E-1	1.227490703E-3	3.371767975E-6	6.732991574E-7	-5.6544E+0	6.69611737E-7	-6.796218234E-8	2.3676E+0	2.4563E+0	8.60673E+1	6.52378E+1	-4.498647526E-2	2.51E+2	4E+0	2.4E+0	1.8E+0	2.3468E+0	2.4532E+0	8.60673E+1	6.52378E+1	2.7E+0	2.4E+0	-6.11115545E-2	1.4649E+0	-4.19E-2	2.6E+1	1E-2	9.9E-3
Magnet: VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	0E+0	1.226984415E-3	1.56E-1	1.226984415E-3	3.371767975E-6	6.132392045E-7	-6.3732E+0	6.100781544E-7	-7.006950197E-8	2.3953E+0	2.5209E+0	8.60673E+1	6.52378E+1	6.36934191E-2	2.52E+2	4E+0	2.4E+0	1.8E+0	2.3676E+0	2.4563E+0	8.60673E+1	6.52378E+1	2.7E+0	2.4E+0	-4.498647526E-2	1.4649E+0	-4.19E-2	2.7E+1	5E-3	4.6E-3
Main Screen Path{Path}=C:\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV\\\\1Code.vi	0E+0	1.226647832E-3	1.56E-1	1.226647832E-3	3.338050296E-6	5.54233972E-7	-8.2812E+0	5.48965178E-7	-8.113306438E-8	2.3696E+0	2.4618E+0	8.60673E+1	6.52378E+1	-4.124575481E-2	2.53E+2	4E+0	2.4E+0	1.8E+0	2.3953E+0	2.5209E+0	8.60673E+1	6.52378E+1	2.7E+0	2.4E+0	6.36934191E-2	1.4649E+0	-4.19E-2	2.8E+1	0E+0	-1E-4
Measurement Timestamp{Timestamp}=<21:41:39.749 17/05/2023>T	0E+0	1.227152706E-3	1.56E-1	1.227152706E-3	3.338050296E-6	4.894330096E-7	-9.9096E+0	4.810034482E-7	-8.587469618E-8	2.3867E+0	2.4277E+0	8.60315E+1	6.52378E+1	-9.632791579E-2	2.54E+2	4E+0	2.4E+0	1.8E+0	2.3696E+0	2.4618E+0	8.60673E+1	6.52378E+1	2.7E+0	2.4E+0	-4.124575481E-2	1.4649E+0	-4.19E-2	2.9E+1	-5E-3	-4.9E-3
Measurement Title{String}=	0E+0	1.227524361E-3	1.56E-1	1.227524361E-3	3.371767975E-6	4.188371656E-7	-9.876E+0	4.125147824E-7	-7.323052384E-8	2.4543E+0	2.5291E+0	8.57808E+1	6.52378E+1	5.329291895E-2	2.55E+2	4E+0	2.4E+0	1.8E+0	2.3867E+0	2.4277E+0	8.60315E+1	6.52378E+1	2.7E+0	2.4E+0	-9.632791579E-2	1.4649E+0	-4.19E-2	3E+1	-1E-2	-1.02E-2
Measurment Select{U16}=4	0E+0	1.227995577E-3	1.56E-1	1.227995577E-3	3.371767975E-6	3.535092671E-7	-1.1466E+1	3.466602308E-7	-7.165002705E-8	2.4115E+0	2.4742E+0	8.57808E+1	6.52378E+1	-2.531948499E-2	2.56E+2	4E+0	2.4E+0	1.8E+0	2.4543E+0	2.5291E+0	8.57808E+1	6.52378E+1	2.7E+0	2.4E+0	5.329291895E-2	1.4649E+0	-4.19E-2	3.1E+1	-1.5E-2	-1.52E-2
Measurment Select.__text__{String}=6221-Lockin-DAQ	0E+0	1.228333574E-3	1.56E-1	1.228333574E-3	3.371767975E-6	2.960825798E-7	-1.46172E+1	2.860733419E-7	-7.586460974E-8	2.4193E+0	2.4996E+0	8.5745E+1	6.52378E+1	1.27447648E-2	2.57E+2	4E+0	2.4E+0	1.8E+0	2.4115E+0	2.4742E+0	8.57808E+1	6.52378E+1	2.7E+0	2.4E+0	-2.531948499E-2	1.4649E+0	-4.19E-2	3.2E+1	-2E-2	-2.01E-2
Notes{String}=I+1A I-1E\\nrxx+1B Rxx-1C\\nRxy+1D Rxy-4A	0E+0	1.228670157E-3	1.56E-1	1.228670157E-3	3.338050296E-6	2.29701658E-7	-1.98828E+1	2.160041511E-7	-7.955259587E-8	2.4708E+0	2.5385E+0	8.58883E+1	6.52378E+1	7.409267128E-2	2.58E+2	4E+0	2.4E+0	1.8E+0	2.4193E+0	2.4996E+0	8.5745E+1	6.52378E+1	2.7E+0	2.4E+0	1.27447648E-2	1.4649E+0	-4.19E-2	3.3E+1	-2.5E-2	-2.5E-2
Offset{Double Float}=0.000000	0E+0	1.228838449E-3	1.56E-1	1.228838449E-3	3.371767975E-6	1.838667136E-7	-3.09648E+1	1.569977873E-7	-9.69384E-8	2.3761E+0	2.4427E+0	8.58883E+1	6.52378E+1	-7.331901044E-2	2.59E+2	4E+0	2.4E+0	1.8E+0	2.4708E+0	2.5385E+0	8.58883E+1	6.52378E+1	2.7E+0	2.4E+0	7.409267128E-2	1.4649E+0	-4.19E-2	3.4E+1	-3E-2	-3.01E-2
Option: 2182 Autozero{Boolean}=True	0E+0	1.22900674E-3	1.56E-1	1.22900674E-3	3.371767975E-6	1.074751113E-7	-4.50648E+1	7.586475116E-8	-7.849900677E-8	2.3905E+0	2.4844E+0	8.59241E+1	6.52378E+1	-7.662055083E-3	2.6E+2	4E+0	2.4E+0	1.8E+0	2.3761E+0	2.4427E+0	8.58883E+1	6.52378E+1	2.7E+0	2.4E+0	-7.331901044E-2	1.4649E+0	-4.19E-2	3.5E+1	-3.5E-2	-3.54E-2
Option: 2182 Front Autozero{Boolean}=True	0E+0	1.229311079E-3	1.56E-1	1.229311079E-3	3.371767975E-6	8.113312095E-8	-6.72732E+1	3.002980111E-8	-7.691834027E-8	2.3586E+0	2.4859E+0	8.58883E+1	6.52378E+1	-7.649732754E-3	2.61E+2	4E+0	2.4E+0	1.8E+0	2.3905E+0	2.4844E+0	8.59241E+1	6.52378E+1	2.7E+0	2.4E+0	-7.662055083E-3	1.4649E+0	-4.19E-2	3.6E+1	-4E-2	-4.01E-2
Option: 2182 Hold{Boolean}=False	0E+0	1.229513028E-3	1.56E-1	1.229513028E-3	3.338050296E-6	9.166997365E-8	-1.289124E+2	-5.953273412E-8	-7.323049556E-8	2.3767E+0	2.4718E+0	8.62464E+1	6.52378E+1	-3.287266567E-2	2.62E+2	4E+0	2.4E+0	1.8E+0	2.3586E+0	2.4859E+0	8.58883E+1	6.52378E+1	2.7E+0	2.4E+0	-7.649732754E-3	1.4649E+0	-4.19E-2	3.7E+1	-4.5E-2	-4.5E-2
Option: 2182 Hold Count{I32}=10	0E+0	1.229513028E-3	1.56E-1	1.229513028E-3	3.371767975E-6	1.232801641E-7	-1.426716E+2	-1.011530958E-7	-7.744519139E-8	2.4083E+0	2.4966E+0	8.62106E+1	6.52378E+1	-1.925673918E-3	2.63E+2	4E+0	2.4E+0	1.8E+0	2.3767E+0	2.4718E+0	8.62464E+1	6.52378E+1	2.7E+0	2.4E+0	-3.287266567E-2	1.4649E+0	-4.19E-2	3.8E+1	-5E-2	-5.01E-2
Option: 2182 Hold Window{Double Float}=1.000000	0E+0	1.229513028E-3	1.56E-1	1.229513028E-3	3.338050296E-6	1.417191896E-7	-1.433796E+2	-1.159044464E-7	-8.69284267E-8	2.4289E+0	2.5115E+0	8.62106E+1	6.52378E+1	1.945870183E-2	2.64E+2	4E+0	2.4E+0	1.8E+0	2.4083E+0	2.4966E+0	8.62106E+1	6.52378E+1	2.7E+0	2.4E+0	-1.925673918E-3	1.4649E+0	-4.19E-2	3.9E+1	-5E-2	-5E-2
Option: 2182 Line Sync{Boolean}=False	0E+0	1.229849611E-3	1.56E-1	1.229849611E-3	3.371767975E-6	2.581505437E-7	-1.605432E+2	-2.455069087E-7	-8.798210066E-8	2.3956E+0	2.485E+0	8.61748E+1	6.52378E+1	-1.472474169E-2	2.65E+2	4E+0	2.4E+0	1.8E+0	2.4289E+0	2.5115E+0	8.62106E+1	6.52378E+1	2.7E+0	2.4E+0	1.945870183E-2	1.4649E+0	-4.19E-2	4E+1	-6E-2	-6E-2
Option: 2182 Reference Reading{Double Float}=0.000000	0E+0	1.229849611E-3	1.56E-1	1.229849611E-3	3.338050296E-6	3.946023535E-7	-1.687344E+2	-3.893338422E-7	-7.902580132E-8	2.4576E+0	2.5352E+0	8.61032E+1	6.52378E+1	7.301738113E-2	2.66E+2	4E+0	2.4E+0	1.8E+0	2.3956E+0	2.485E+0	8.61748E+1	6.52378E+1	2.7E+0	2.4E+0	-1.472474169E-2	1.4649E+0	-4.19E-2	4.1E+1	-7E-2	-7E-2
Option: 2182 Relative Mode{Boolean}=False	0E+0	1.230187608E-3	1.56E-1	1.230187608E-3	3.371767975E-6	5.089259636E-7	-1.711788E+2	-5.057646306E-7	-7.955259587E-8	2.4252E+0	2.5093E+0	8.6139E+1	6.52378E+1	1.994600892E-2	2.67E+2	4E+0	2.4E+0	1.8E+0	2.4576E+0	2.5352E+0	8.61032E+1	6.52378E+1	2.7E+0	2.4E+0	7.301738113E-2	1.4649E+0	-4.19E-2	4.2E+1	-8E-2	-8E-2
Option: 2182 Trigger Delay{Cluster (Boolean,Double Float)}={'Auto':True,'Time(s)':0.000000}	0E+0	1.2303559E-3	1.56E-1	1.2303559E-3	3.371767975E-6	6.516984595E-7	-1.732812E+2	-6.495907156E-7	-7.744527624E-8	2.4032E+0	2.4947E+0	8.60673E+1	6.52378E+1	-8.805575198E-4	2.68E+2	4E+0	2.4E+0	1.8E+0	2.4252E+0	2.5093E+0	8.6139E+1	6.52378E+1	2.7E+0	2.4E+0	1.994600892E-2	1.4649E+0	-4.19E-2	4.3E+1	-9E-2	-9E-2
Option: 2182 Trigger Source{Enum U16 ((Immediate,Timer,Manual,Bus,Trigger link))}=Bus	0E+0	1.230456875E-3	1.56E-1	1.230456875E-3	3.371767975E-6	7.791949033E-7	-1.7421E+2	-7.776146611E-7	-8.007947527E-8	2.4326E+0	2.5101E+0	8.60673E+1	6.52378E+1	2.519327588E-2	2.69E+2	4E+0	2.4E+0	1.8E+0	2.4032E+0	2.4947E+0	8.60673E+1	6.52378E+1	2.7E+0	2.4E+0	-8.805575198E-4	1.4649E+0	-4.19E-2	4.4E+1	-1E-1	-1E-1
Option: 2182 Trigger Timer{Double Float}=0.000000	0E+0	1.230490533E-3	1.56E-1	1.230490533E-3	3.371767975E-6	7.691850997E-7	-1.729368E+2	-7.654973964E-7	-9.641154888E-8	2.4368E+0	2.5177E+0	8.60673E+1	6.52378E+1	3.395805508E-2	2.7E+2	4E+0	2.4E+0	1.8E+0	2.4326E+0	2.5101E+0	8.60673E+1	6.52378E+1	2.7E+0	2.4E+0	2.519327588E-2	1.4649E+0	-4.19E-2	4.5E+1	-1E-1	-9.99E-2
Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	0E+0	1.232209934E-3	1.56E-1	1.232209934E-3	3.371767975E-6	3.400216295E-6	-1.784832E+2	-3.402320645E-6	-9.166991708E-8	2.3765E+0	2.4641E+0	8.60673E+1	6.52378E+1	-6.166083366E-2	2.71E+2	4E+0	2.4E+0	1.8E+0	2.4368E+0	2.5177E+0	8.60673E+1	6.52378E+1	2.7E+0	2.4E+0	3.395805508E-2	1.4649E+0	-4.19E-2	4.6E+1	-3E-1	-2.998E-1
Option: 560 Enabled{Boolean}=False	0E+0	1.233390802E-3	1.56E-1	1.233390802E-3	3.371767975E-6	6.03599642E-6	-1.790292E+2	-6.038629686E-6	-1.032604437E-7	2.6099E+0	2.6468E+0	8.5745E+1	6.52378E+1	1.975286603E-1	2.72E+2	4E+0	2.4E+0	1.8E+0	2.3765E+0	2.4641E+0	8.60673E+1	6.52378E+1	2.7E+0	2.4E+0	-6.166083366E-2	1.4649E+0	-4.19E-2	4.7E+1	-5E-1	-4.998E-1
Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	0E+0	1.233390802E-3	1.56E-1	1.233390802E-3	3.371767975E-6	8.651208223E-6	-1.792788E+2	-8.653847146E-6	-1.10109282E-7	4.5031E+0	4.2579E+0	8.58166E+1	6.52378E+1	2.429947376E+0	2.73E+2	4E+0	2.4E+0	1.8E+0	2.6099E+0	2.6468E+0	8.5745E+1	6.52378E+1	2.7E+0	2.4E+0	1.975286603E-1	1.4649E+0	-4.19E-2	4.8E+1	-7E-1	-6.999E-1
Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	0E+0	1.23709887E-3	1.56E-1	1.23709887E-3	3.371767975E-6	1.130650167E-5	-1.794636E+2	-1.13091321E-5	-1.074751396E-7	2.0803E+0	2.1678E+0	8.61748E+1	6.52378E+1	-1.761847496E+0	2.74E+2	4E+0	2.4E+0	1.8E+0	4.5031E+0	4.2579E+0	8.58166E+1	6.52378E+1	2.7E+0	2.4E+0	2.429947376E+0	1.4649E+0	-4.19E-2	4.9E+1	-9E-1	-8.999E-1
Option: 6221 Adjust Mode{Enum U16 ((Offset,Frequency,Amplitude))}=Offset	0E+0	1.238616321E-3	1.56E-1	1.238616321E-3	3.371767975E-6	1.394015199E-5	-1.795296E+2	-1.394278525E-5	-1.159044464E-7	2.3921E+0	2.4582E+0	8.60673E+1	6.52378E+1	-1.1133641E-1	2.75E+2	4E+0	2.4E+0	1.8E+0	2.0803E+0	2.1678E+0	8.61748E+1	6.52378E+1	2.7E+0	2.4E+0	-1.761847496E+0	1.4649E+0	-4.19E-2	5E+1	-1.1E+0	-1.0999E+0
Option: 6221 Amplitude{Double Float}=1.000000E-6	0E+0	1.240808352E-3	1.56E-1	1.240808352E-3	3.371767975E-6	1.658434102E-5	-1.795476E+2	-1.658697146E-5	-1.322362937E-7	2.374E+0	2.4664E+0	8.59957E+1	6.52378E+1	1.321350485E-1	2.76E+2	4E+0	2.4E+0	1.8E+0	2.3921E+0	2.4582E+0	8.60673E+1	6.52378E+1	2.7E+0	2.4E+0	-1.1133641E-1	1.4649E+0	-4.19E-2	5.1E+1	-1.3E+0	-1.2999E+0
Option: 6221 Compliance{Double Float}=10.000000	0E+0	1.243336966E-3	1.56E-1	1.243336966E-3	3.371767975E-6	1.922382922E-5	-1.795956E+2	-1.922640309E-5	-1.369778689E-7	2.3846E+0	2.4801E+0	8.59957E+1	6.52378E+1	-2.722180914E-3	2.77E+2	4E+0	2.4E+0	1.8E+0	2.374E+0	2.4664E+0	8.59957E+1	6.52378E+1	2.7E+0	2.4E+0	1.321350485E-1	1.4649E+0	-4.19E-2	5.2E+1	-1.5E+0	-1.4999E+0
Option: 6221 Duty Cycle{Double Float}=50.000000	0E+0	1.243202333E-3	1.56E-1	1.243202333E-3	3.371767975E-6	1.920589699E-5	-1.795812E+2	-1.920849914E-5	-1.432998561E-7	2.4107E+0	2.4869E+0	8.59957E+1	6.52378E+1	2.870513825E-3	2.78E+2	4E+0	2.4E+0	1.8E+0	2.3846E+0	2.4801E+0	8.59957E+1	6.52378E+1	2.7E+0	2.4E+0	-2.722180914E-3	1.4649E+0	-4.19E-2	5.3E+1	-1.5E+0	-1.5E+0
Option: 6221 External Trigger{Boolean}=False	0E+0	1.237605158E-3	1.56E-1	1.237605158E-3	3.371767975E-6	1.26209566E-5	-1.795392E+2	-1.262358987E-5	-1.022067415E-7	2.4292E+0	2.5508E+0	8.6139E+1	6.47381E+1	6.547442824E-2	2.79E+2	4E+0	2.4E+0	1.8E+0	2.4107E+0	2.4869E+0	8.59957E+1	6.52378E+1	2.7E+0	2.4E+0	2.870513825E-3	1.4649E+0	-4.19E-2	5.4E+1	-1E+0	-1.0001E+0
Option: 6221 External Trigger Ignore Multiple{Boolean}=False	0E+0	1.233458119E-3	1.56E-1	1.233458119E-3	3.371767975E-6	6.020720085E-6	-1.792956E+2	-6.023353351E-6	-7.533787176E-8	2.4674E+0	2.5345E+0	8.60315E+1	6.47381E+1	5.600174144E-2	2.8E+2	4E+0	2.4E+0	1.8E+0	2.4292E+0	2.5508E+0	8.6139E+1	6.47381E+1	2.7E+0	2.4E+0	6.547442824E-2	1.4649E+0	-4.19E-2	5.5E+1	-5E-1	-5.001E-1
Option: 6221 Frequency{Double Float}=119.770000	
Option: 6221 Function{U16}=1	
Option: 6221 Function.__text__{String}=Sine	
Option: 6221 Idle Level{Double Float}=0.000000	
Option: 6221 Input trigger Line{U8}=5	
Option: 6221 Offset{Double Float}=0.000000	
Option: 6221 Output Trigger Line{U8}=4	
Option: 6221 Pass Through{Boolean}=True	
Option: 6221 Phase Marker{Boolean}=True	
Option: 6221 Phase Marker Phase{Double Float}=0.000000	
Option: 6221 Range Level{Double Float}=2.000000E-12	
Option: 6221 Ranging{U16}=1	
Option: 6221 Ranging.__text__{String}=Best	
Option: 6221 Update Clock{Double Float}=0.000000	
Option: 6221 VISA{Visa Refnum (Void)}=GPIB0::13::INSTR	
Option: Confirm Config{Boolean}=False	
Option: Control Panel Ref{LVObjVI Refnum (Void)}=	
Option: DAQ Global Channel{Boolean}=False	
Option: DAQ Input Rate{Double Float}=10000.000000	
Option: DAQ Input Samples{I32}=200	
Option: DAQ Measurement Channels{1D Array (Cluster (UserDefinedRefnumTag Refnum (Void),\tkDAQmxPhysChanTagType Tag,\tkDAQmxScaleTagType Tag,Boolean,Double Float,String))}=[]	
Option: Differential{I32}=10106	
Option: Differential.__text__{String}=Differential	
Option: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values))}=Function Generator	
Option: Lockin Standoff Time{Double Float}=0.000000	
Option: Paranoid Save Data{Boolean}=True	
Option: Plot Autoback Path{Path}=C:\\\\TEMP\\\\XY Multiparam\\\\Backup.txt	
Option: SR830  Ref Phase{Double Float}=0.000000	
Option: SR830  Synch Filter{Boolean}=False	
Option: SR830  Time Constant{I16}=8	
Option: SR830  Time Constant.__text__{String}=100 ms	
Option: SR830 2x Line Filter{Boolean}=True	
Option: SR830 Adjust Gains{Boolean}=False	
Option: SR830 Auto Gain Lower.__text__{String}=2 nV/fA	
Option: SR830 Auto Gain Upper.__text__{String}=1 V/uA	
Option: SR830 Auto Offset 1{Boolean}=False	
Option: SR830 Auto Offset 2{Boolean}=False	
Option: SR830 Autophase{Boolean}=False	
Option: SR830 DC Coupling?{Boolean}=False	
Option: SR830 Display 1{U16}=0	
Option: SR830 Display 1.__text__{String}=X	
Option: SR830 Display 2{U16}=0	
Option: SR830 Display 2.__text__{String}=Y	
Option: SR830 Dynamic Reserve{I16}=1	
Option: SR830 Dynamic Reserve.__text__{String}=Normal	
Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Option: SR830 Filter Slope{I32}=1	
Option: SR830 Filter Slope.__text__{String}=12 dB/oct	
Option: SR830 Gain{I32}=-1	
Option: SR830 Gain.__text__{String}=Auto Gain	
Option: SR830 Ground Shield?{Boolean}=False	
Option: SR830 Harmonic{I32}=1	
Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A	
Option: SR830 Line Filter{Boolean}=True	
Option: SR830 No Reset{Boolean}=False	
Option: SR830 Offset 1{Double Float}=0.000000	
Option: SR830 Offset 2{Double Float}=0.000000	
Option: SR830 Output Channel 1{Boolean}=False	
Option: SR830 Output Channel 2{Boolean}=False	
Option: SR830 Ratio 1{U16}=0	
Option: SR830 Ratio 1.__text__{String}=None	
Option: SR830 Ratio 2{U16}=0	
Option: SR830 Ratio 2.__text__{String}=None	
Option: SR830 Ref Amplitude{Double Float}=0.100000	
Option: SR830 Ref Frequency{Double Float}=1013.000000	
Option: SR830 Ref Source{Boolean}=False	
Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta]	
Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Option: SR830 VISA{Visa Refnum (Void)}=	
Option: Sense Autorange{Boolean}=False	
Option: Sense Range Level{Double Float}=0.100000	
Option: Sense Rate{Double Float}=1.000000	
Option:560 Comport{Visa Refnum (Void)}=COM1	
Option:560 Filter High Pass{U16}=0	
Option:560 Filter High Pass.__text__{String}=0.03	
Option:560 Filter Lowpass{U16}=0	
Option:560 Filter Lowpass.__text__{String}=0.03	
Option:560 Filter Mode{U16}=0	
Option:560 Filter Mode.__text__{String}=6 dB high pass	
Option:560 Invert{Boolean}=False	
Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Option:570 Enabled{Boolean}=False	
Option:570 Filter High Pass{U16}=0	
Option:570 Filter High Pass.__text__{String}=0.03	
Option:570 Filter Lowpass{U16}=0	
Option:570 Filter Lowpass.__text__{String}=0.03	
Option:570 Filter Mode{U16}=0	
Option:570 Filter Mode.__text__{String}=6 dB high pass	
Option:570 Gain Mode{U16}=0	
Option:570 Gain Mode.__text__{String}=Low Noise	
Option:570 Input Offset{U16}=0	
Option:570 Input Offset On{Boolean}=False	
Option:570 Input Offset.__text__{String}=1pA	
Option:570 Sensitivity{U16}=0	
Option:570 Sensitivity.__text__{String}=1pA/V	
Option:Debug On{Boolean}=False	
Option:GPIB 2182{Visa Refnum (Void)}=	
Option:Parallel Config Voltage Measurers{Boolean}=True	
Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Option:SR830 Settle Time{Double Float}=5.000000	
Option:Sense Digits{I32}=8	
Output Names{1D Array (String)}=['Offset','Rxx::R','Rxx::Theta','Rxx::X','Rxx::Y','Rxy::R','Rxy::Theta','Rxy::X','Rxy::Y','temperature: T1','temperature: T2','temperature: T3','temperature: T4','temperature: dT/dt','iterator','multi[0]:iterator','multi[0]:y','multi[0]:temperature: setpoint','multi[0]:temperature: T1','multi[0]:temperature: T2','multi[0]:temperature: T3','multi[0]:temperature: T4','multi[0]:temperature: heater','multi[0]:temperature: gas','multi[0]:temperature: dT/dt','multi[0]:temperature: current temperature','multi[0]:temperature: error','multi[1]:iterator','multi[1]:y','multi[1]:Control:Magnet Output']	
Parameter Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Parameter Select{U16}=6	
Parameter Select.__text__{String}=Multi-Parameter	
Paths{U32}=0	
Plot: Column Renames{1D Array (Cluster (String,String))}=[]	
Plot: No dups{Boolean}=False	
Plot: StdDevs{Boolean}=False	
Plotting Class{String}=Parameter Plot	
Plotting Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	
Plotting Select{U16}=1	
Plotting Select.__text__{String}=Parameter Plot	
Project Code{String}=Topological_Insulators	
Ref: Temperature Window{LVObjVI Refnum (Void)}=	
Ref:Control Subpanel{LVObjUnknown Refnum (Void)}=	
Ref:Main Screen{LVObjVI Refnum (Void)}=	
Ref:Plotting Subpanel{LVObjUnknown Refnum (Void)}=	
Ref:Toolbar{LVObjUnknown Refnum (Void)}=	
Ref:XY Subpanel{LVObjUnknown Refnum (Void)}=	
Rxx::R{Double Float}=0.001233	
Rxx::Theta{Double Float}=0.156000	
Rxx::X{Double Float}=0.001233	
Rxx::Y{Double Float}=3.371768E-6	
Rxx:Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	
Rxx:Option: 560 Enabled{Boolean}=False	
Rxx:Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	
Rxx:Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	
Rxx:Option: Lockin Standoff Time{Double Float}=0.000000	
Rxx:Option: Lockin Type{Enum U16 ((SRS 830,EG&G 5302))}=SRS 830	
Rxx:Option: SR803 Full Scale Reading{Double Float}=0.000000	
Rxx:Option: SR830  Ref Phase{Double Float}=0.000000	
Rxx:Option: SR830  Synch Filter{Boolean}=False	
Rxx:Option: SR830  Time Constant{I16}=8	
Rxx:Option: SR830 2x Line Filter{Boolean}=False	
Rxx:Option: SR830 Adjust Gains{Boolean}=False	
Rxx:Option: SR830 Auto Gain Lower{I32}=0	
Rxx:Option: SR830 Auto Gain Upper{I32}=26	
Rxx:Option: SR830 Auto Offset 1{Boolean}=False	
Rxx:Option: SR830 Auto Offset 2{Boolean}=False	
Rxx:Option: SR830 Autophase{Boolean}=False	
Rxx:Option: SR830 DC Coupling?{Boolean}=False	
Rxx:Option: SR830 Display 1{U16}=0	
Rxx:Option: SR830 Display 2{U16}=0	
Rxx:Option: SR830 Dynamic Reserve{I16}=2	
Rxx:Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Rxx:Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Rxx:Option: SR830 Filter Slope{I32}=3	
Rxx:Option: SR830 Gain{I32}=18	
Rxx:Option: SR830 Ground Shield?{Boolean}=False	
Rxx:Option: SR830 Harmonic{I32}=1	
Rxx:Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A-B	
Rxx:Option: SR830 Line Filter{Boolean}=False	
Rxx:Option: SR830 No Reset{Boolean}=False	
Rxx:Option: SR830 Offset 1{Double Float}=0.000000	
Rxx:Option: SR830 Offset 2{Double Float}=0.000000	
Rxx:Option: SR830 Output Channel 1{Boolean}=False	
Rxx:Option: SR830 Output Channel 2{Boolean}=False	
Rxx:Option: SR830 Ratio 1{U16}=0	
Rxx:Option: SR830 Ratio 2{U16}=0	
Rxx:Option: SR830 Ref Amplitude{Double Float}=0.100000	
Rxx:Option: SR830 Ref Frequency{Double Float}=1013.000000	
Rxx:Option: SR830 Ref Source{Boolean}=False	
Rxx:Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta,X,Y]	
Rxx:Option: SR830 Time Constant value{Double Float}=0.000000	
Rxx:Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Rxx:Option: SR830 VISA{Visa Refnum (Void)}=GPIB0::5::INSTR	
Rxx:Option:560 Comport{Visa Refnum (Void)}=COM1	
Rxx:Option:560 Filter High Pass{U16}=0	
Rxx:Option:560 Filter Lowpass{U16}=0	
Rxx:Option:560 Filter Mode{U16}=0	
Rxx:Option:560 Invert{Boolean}=False	
Rxx:Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Rxx:Option:570 Enabled{Boolean}=False	
Rxx:Option:570 Filter High Pass{U16}=0	
Rxx:Option:570 Filter Lowpass{U16}=0	
Rxx:Option:570 Filter Mode{U16}=0	
Rxx:Option:570 Gain Mode{U16}=0	
Rxx:Option:570 Input Offset{U16}=0	
Rxx:Option:570 Input Offset On{Boolean}=False	
Rxx:Option:570 Sensitivity{U16}=0	
Rxx:Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Rxx:Option:SR830 Autogain Lower Threshold{Double Float}=0.100000	
Rxx:Option:SR830 Autogain Standoff{Double Float}=3.000000	
Rxx:Option:SR830 Autogain Upper Threshold{Double Float}=0.900000	
Rxx:Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Rxx:Option:SR830 Settle Time{Double Float}=0.000000	
Rxy::R{Double Float}=6.020720E-6	
Rxy::Theta{Double Float}=-179.295600	
Rxy::X{Double Float}=-6.023353E-6	
Rxy::Y{Double Float}=-7.533787E-8	
Rxy:Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	
Rxy:Option: 560 Enabled{Boolean}=False	
Rxy:Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	
Rxy:Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	
Rxy:Option: Lockin Standoff Time{Double Float}=0.000000	
Rxy:Option: Lockin Type{Enum U16 ((SRS 830,EG&G 5302))}=SRS 830	
Rxy:Option: SR803 Full Scale Reading{Double Float}=0.000000	
Rxy:Option: SR830  Ref Phase{Double Float}=0.000000	
Rxy:Option: SR830  Synch Filter{Boolean}=False	
Rxy:Option: SR830  Time Constant{I16}=8	
Rxy:Option: SR830 2x Line Filter{Boolean}=False	
Rxy:Option: SR830 Adjust Gains{Boolean}=False	
Rxy:Option: SR830 Auto Gain Lower{I32}=0	
Rxy:Option: SR830 Auto Gain Upper{I32}=26	
Rxy:Option: SR830 Auto Offset 1{Boolean}=False	
Rxy:Option: SR830 Auto Offset 2{Boolean}=False	
Rxy:Option: SR830 Autophase{Boolean}=False	
Rxy:Option: SR830 DC Coupling?{Boolean}=False	
Rxy:Option: SR830 Display 1{U16}=0	
Rxy:Option: SR830 Display 2{U16}=1	
Rxy:Option: SR830 Dynamic Reserve{I16}=2	
Rxy:Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Rxy:Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Rxy:Option: SR830 Filter Slope{I32}=3	
Rxy:Option: SR830 Gain{I32}=18	
Rxy:Option: SR830 Ground Shield?{Boolean}=False	
Rxy:Option: SR830 Harmonic{I32}=1	
Rxy:Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A-B	
Rxy:Option: SR830 Line Filter{Boolean}=False	
Rxy:Option: SR830 No Reset{Boolean}=False	
Rxy:Option: SR830 Offset 1{Double Float}=0.000000	
Rxy:Option: SR830 Offset 2{Double Float}=0.000000	
Rxy:Option: SR830 Output Channel 1{Boolean}=False	
Rxy:Option: SR830 Output Channel 2{Boolean}=False	
Rxy:Option: SR830 Ratio 1{U16}=0	
Rxy:Option: SR830 Ratio 2{U16}=0	
Rxy:Option: SR830 Ref Amplitude{Double Float}=0.100000	
Rxy:Option: SR830 Ref Frequency{Double Float}=1013.000000	
Rxy:Option: SR830 Ref Source{Boolean}=False	
Rxy:Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta,X,Y]	
Rxy:Option: SR830 Time Constant value{Double Float}=0.000000	
Rxy:Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Rxy:Option: SR830 VISA{Visa Refnum (Void)}=GPIB0::6::INSTR	
Rxy:Option:560 Comport{Visa Refnum (Void)}=COM1	
Rxy:Option:560 Filter High Pass{U16}=0	
Rxy:Option:560 Filter Lowpass{U16}=0	
Rxy:Option:560 Filter Mode{U16}=0	
Rxy:Option:560 Invert{Boolean}=False	
Rxy:Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Rxy:Option:570 Enabled{Boolean}=False	
Rxy:Option:570 Filter High Pass{U16}=0	
Rxy:Option:570 Filter Lowpass{U16}=0	
Rxy:Option:570 Filter Mode{U16}=0	
Rxy:Option:570 Gain Mode{U16}=0	
Rxy:Option:570 Input Offset{U16}=0	
Rxy:Option:570 Input Offset On{Boolean}=False	
Rxy:Option:570 Sensitivity{U16}=0	
Rxy:Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Rxy:Option:SR830 Autogain Lower Threshold{Double Float}=0.100000	
Rxy:Option:SR830 Autogain Standoff{Double Float}=3.000000	
Rxy:Option:SR830 Autogain Upper Threshold{Double Float}=0.900000	
Rxy:Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Rxy:Option:SR830 Settle Time{Double Float}=0.000000	
Sample ID{String}=MBE202221213_PA_D1 750C Cracker WAL	
Save:Filename{String}=${X-Y Class} ${2nd Parameter Class} ${iterator}{%04d} ${y}{%04.2g}.txt	
Save:Final Filename{String}=${X-Y Class} ${2nd Parameter Class} .txt	
Save:Final path{Path}=C:\\\\Data\\\\${Project Code}\\\\${User}\\\\${Sample ID}\\\\${Measurement Timestamp}{%Y%m%d}\\\\${X-Y Class}	
Save:Path{Path}=C:\\\\Data\\\\${Project Code}\\\\${User}\\\\${Sample ID}\\\\${Measurement Timestamp}{%Y%m%d}\\\\${X-Y Class}	
Startup path{Path}=C:\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV	
Sub Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Sweep Step{I32}=3	
T Control Measure.__text__{1D Array (String)}=['temperature: T1','temperature: T2','temperature: T3','temperature: T4','temperature: dT/dt']	
Timestamp{Timestamp}=<21:42:48.616 17/05/2023>T	
Toolbar{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Unaved Data{Boolean}=True	
Unsaved Data{Boolean}=False	
User{String}=Craig	
X-Y Class{String}=6221-Lockin-DAQ	
X-Y Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	
d(Offset){Double Float}=0.000000	
d(Rxx::R){Double Float}=9.217700E-8	
d(Rxx::Theta){Double Float}=0.000000	
d(Rxx::X){Double Float}=9.217700E-8	
d(Rxx::Y){Double Float}=4.735058E-22	
d(Rxy::R){Double Float}=1.244279E-8	
d(Rxy::Theta){Double Float}=0.079214	
d(Rxy::X){Double Float}=1.243710E-8	
d(Rxy::Y){Double Float}=8.246366E-9	
iterate result{U16}=5	
iterator{I32}=280	
multi[0]:Control: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values,Adaptive Step Ramp))}=List of Values	
multi[0]:Control: Monitor Update Timeout{Double Float}=0.010000	
multi[0]:Control: Open T Window{Boolean}=False	
multi[0]:Control: Reverse Temperature Sense{Boolean}=False	
multi[0]:Iterator{I32}=0	
multi[0]:Ref: Temperature Window{LVObjVI Refnum (Void)}=	
multi[0]:iterate result{U16}=0	
multi[0]:iterator{I32}=4	
multi[0]:temperature:  rate window{Double Float}=120.000000	
multi[0]:temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[0]:temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
multi[0]:temperature: T1{Double Float}=2.388000	
multi[0]:temperature: T2{Double Float}=2.475200	
multi[0]:temperature: T3{Double Float}=85.780800	
multi[0]:temperature: T4{Double Float}=64.738100	
multi[0]:temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
multi[0]:temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
multi[0]:temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
multi[0]:temperature: current temperature{Double Float}=1.464900	
multi[0]:temperature: current temperature 2{Double Float}=287.100000	
multi[0]:temperature: dT/dt{Double Float}=-0.029201	
multi[0]:temperature: error{Double Float}=-0.041900	
multi[0]:temperature: gas{Double Float}=2.400000	
multi[0]:temperature: gas control{Boolean}=False	
multi[0]:temperature: gas control 2{Boolean}=False	
multi[0]:temperature: gass boost{I8}=0	
multi[0]:temperature: gass boost 2{I8}=0	
multi[0]:temperature: gast flow{I16}=0	
multi[0]:temperature: gast flow 2{I16}=7	
multi[0]:temperature: heater{Double Float}=2.700000	
multi[0]:temperature: heater output{Double Float}=0.000000	
multi[0]:temperature: heater output 2{Double Float}=0.000000	
multi[0]:temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
multi[0]:temperature: monitor timeout{Double Float}=0.010000	
multi[0]:temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
multi[0]:temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
multi[0]:temperature: ramp rate{Double Float}=8.000000	
multi[0]:temperature: ramp rate 2{Double Float}=0.000000	
multi[0]:temperature: ramp target{Double Float}=20.000000	
multi[0]:temperature: ramp target 2{Double Float}=0.000000	
multi[0]:temperature: ramping{Boolean}=False	
multi[0]:temperature: setpoint{Double Float}=1.800000	
multi[0]:temperature: setpoint 2{Double Float}=287.100000	
multi[0]:temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
multi[0]:temperature: stability error{Extended Float}=0.040000	
multi[0]:temperature: stability script{String}=	
multi[0]:temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
multi[0]:temperature: temp control mode{U16}=2	
multi[0]:temperature: temp control mode 2{U16}=3	
multi[0]:temperature: temp control mode 2.__text__{String}=Open Loop	
multi[0]:temperature: temp control mode.__text__{String}=Zone	
multi[0]:temperature: temp control sensor{U16}=0	
multi[0]:temperature: temp control sensor 2{U16}=0	
multi[0]:temperature: temp control sensor 2.__text__{String}=Sensor 1	
multi[0]:temperature: temp control sensor.__text__{String}=Sensor A	
multi[0]:temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
multi[0]:temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
multi[0]:temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
multi[0]:temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
multi[0]:temperature: temp loop{U16}=0	
multi[0]:temperature: temp loop 2{U16}=0	
multi[0]:temperature: temp loop 2.__text__{String}=Heater	
multi[0]:temperature: temp loop.__text__{String}=Loop 1	
multi[0]:temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
multi[0]:temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[0]:temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[0]:temperature:error for gas boost{Double Float}=0.000000	
multi[0]:temperature:error for gas boost 2{Double Float}=0.000000	
multi[0]:temperature:heater range{U16}=2	
multi[0]:temperature:heater range 2{U16}=0	
multi[0]:temperature:heater range 2.__text__{String}=Off	
multi[0]:temperature:heater range.__text__{String}=40mW	
multi[0]:temperature:history window{Extended Float}=300.000000	
multi[0]:temperature:is stable?{Boolean}=False	
multi[0]:temperature:monitor{Boolean}=True	
multi[0]:temperature:ramping{Boolean}=False	
multi[0]:temperature:ramping on{Boolean}=False	
multi[0]:temperature:ramping on 2{Boolean}=False	
multi[0]:temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
multi[0]:temperature:stability code{U32}=6618880	
multi[0]:temperature:stability rate{Extended Float}=0.040000	
multi[0]:y{Double Float}=2.400000	
multi[1]:Control: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values,Adaptive Step Ramp))}=Multi-Segment Ramp	
multi[1]:Control: Gate delay{Double Float}=0.000000	
multi[1]:Control: Monitor Update Timeout{Double Float}=0.010000	
multi[1]:Control: Open T Window{Boolean}=False	
multi[1]:Control: Reverse Temperature Sense{Boolean}=False	
multi[1]:Control:Magnet Output{Double Float}=-0.000100	
multi[1]:Iterator{I32}=0	
multi[1]:Magnet: Final Switch Heater{Enum U8 ((False,True,Mixed))}=	
multi[1]:Magnet: Power Supply{Enum U16 ((IPS120,LS625,PS110,Hg iPS,SMS Series,Cryomagnetics 4G,DMG Little CryoFree,DMG Big CryoFree))}=Hg iPS	
multi[1]:Magnet: Rate{Double Float}=0.500000	
multi[1]:Magnet: Units{Enum U16 ((Field,Current))}=Field	
multi[1]:Magnet: VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[1]:Multi-segment_Stage{I32}=0	
multi[1]:Multi-segment_Stage_Changed{Boolean}=False	
multi[1]:Ref: Temperature Window{LVObjVI Refnum (Void)}=	
multi[1]:iterate result{U16}=4	
multi[1]:iterator{I32}=57	
multi[1]:measure point{Boolean}=False	
multi[1]:temperature:  rate window{Double Float}=120.000000	
multi[1]:temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[1]:temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
multi[1]:temperature: T1{Double Float}=1.842400	
multi[1]:temperature: T2{Double Float}=1.465600	
multi[1]:temperature: T3{Double Float}=86.318100	
multi[1]:temperature: T4{Double Float}=66.769200	
multi[1]:temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
multi[1]:temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
multi[1]:temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
multi[1]:temperature: current temperature{Double Float}=1.465600	
multi[1]:temperature: current temperature 2{Double Float}=287.100000	
multi[1]:temperature: dT/dt{Double Float}=-0.001864	
multi[1]:temperature: gas control{Boolean}=False	
multi[1]:temperature: gas control 2{Boolean}=False	
multi[1]:temperature: gass boost{I8}=0	
multi[1]:temperature: gass boost 2{I8}=0	
multi[1]:temperature: gast flow{I16}=0	
multi[1]:temperature: gast flow 2{I16}=7	
multi[1]:temperature: heater output{Double Float}=0.000000	
multi[1]:temperature: heater output 2{Double Float}=0.000000	
multi[1]:temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
multi[1]:temperature: monitor timeout{Double Float}=1.000000	
multi[1]:temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
multi[1]:temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
multi[1]:temperature: ramp rate{Double Float}=8.000000	
multi[1]:temperature: ramp rate 2{Double Float}=0.000000	
multi[1]:temperature: ramp target{Double Float}=20.000000	
multi[1]:temperature: ramp target 2{Double Float}=0.000000	
multi[1]:temperature: ramping{Boolean}=False	
multi[1]:temperature: setpoint{Double Float}=1.800000	
multi[1]:temperature: setpoint 2{Double Float}=287.100000	
multi[1]:temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
multi[1]:temperature: stability error{Extended Float}=0.040000	
multi[1]:temperature: stability script{String}=	
multi[1]:temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
multi[1]:temperature: temp control mode{U16}=2	
multi[1]:temperature: temp control mode 2{U16}=3	
multi[1]:temperature: temp control mode 2.__text__{String}=Open Loop	
multi[1]:temperature: temp control mode.__text__{String}=Zone	
multi[1]:temperature: temp control sensor{U16}=0	
multi[1]:temperature: temp control sensor 2{U16}=0	
multi[1]:temperature: temp control sensor 2.__text__{String}=Sensor 1	
multi[1]:temperature: temp control sensor.__text__{String}=Sensor A	
multi[1]:temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
multi[1]:temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
multi[1]:temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
multi[1]:temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
multi[1]:temperature: temp loop{U16}=0	
multi[1]:temperature: temp loop 2{U16}=0	
multi[1]:temperature: temp loop 2.__text__{String}=Heater	
multi[1]:temperature: temp loop.__text__{String}=Loop 1	
multi[1]:temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
multi[1]:temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[1]:temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[1]:temperature:error for gas boost{Double Float}=0.000000	
multi[1]:temperature:error for gas boost 2{Double Float}=0.000000	
multi[1]:temperature:heater range{U16}=2	
multi[1]:temperature:heater range 2{U16}=0	
multi[1]:temperature:heater range 2.__text__{String}=Off	
multi[1]:temperature:heater range.__text__{String}=40mW	
multi[1]:temperature:history window{Extended Float}=300.000000	
multi[1]:temperature:is stable?{Boolean}=True	
multi[1]:temperature:monitor{Boolean}=True	
multi[1]:temperature:ramping{Boolean}=False	
multi[1]:temperature:ramping on{Boolean}=False	
multi[1]:temperature:ramping on 2{Boolean}=False	
multi[1]:temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
multi[1]:temperature:stability code{U32}=6618880	
multi[1]:temperature:stability rate{Extended Float}=0.040000	
multi[1]:y{Double Float}=0.000000	
parameter: Termination{String}=False	
parameter: delta time{Double Float}=1.000000	
parameter: progress{Double Float}=100.000000	
temperature:  rate window{Double Float}=120.000000	
temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
temperature: T1{Double Float}=2.388000	
temperature: T2{Double Float}=2.475200	
temperature: T3{Double Float}=85.780800	
temperature: T4{Double Float}=64.738100	
temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
temperature: current temperature{Double Float}=1.464900	
temperature: current temperature 2{Double Float}=287.100000	
temperature: dT/dt{Double Float}=-0.029201	
temperature: gas control{Boolean}=False	
temperature: gas control 2{Boolean}=False	
temperature: gass boost{I8}=0	
temperature: gass boost 2{I8}=0	
temperature: gast flow{I16}=0	
temperature: gast flow 2{I16}=7	
temperature: heater output{Double Float}=0.000000	
temperature: heater output 2{Double Float}=0.000000	
temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
temperature: monitor timeout{Double Float}=0.010000	
temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
temperature: ramp rate{Double Float}=8.000000	
temperature: ramp rate 2{Double Float}=0.000000	
temperature: ramp target{Double Float}=20.000000	
temperature: ramp target 2{Double Float}=0.000000	
temperature: ramping{Boolean}=False	
temperature: setpoint{Double Float}=1.800000	
temperature: setpoint 2{Double Float}=287.100000	
temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
temperature: stability error{Extended Float}=0.040000	
temperature: stability script{String}=	
temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
temperature: temp control mode{U16}=2	
temperature: temp control mode 2{U16}=3	
temperature: temp control mode 2.__text__{String}=Open Loop	
temperature: temp control mode.__text__{String}=Zone	
temperature: temp control sensor{U16}=0	
temperature: temp control sensor 2{U16}=0	
temperature: temp control sensor 2.__text__{String}=Sensor 1	
temperature: temp control sensor.__text__{String}=Sensor A	
temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
temperature: temp loop{U16}=0	
temperature: temp loop 2{U16}=0	
temperature: temp loop 2.__text__{String}=Heater	
temperature: temp loop.__text__{String}=Loop 1	
temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
temperature:error for gas boost{Double Float}=0.000000	
temperature:error for gas boost 2{Double Float}=0.000000	
temperature:heater range{U16}=2	
temperature:heater range 2{U16}=0	
temperature:heater range 2.__text__{String}=Off	
temperature:heater range.__text__{String}=40mW	
temperature:history window{Extended Float}=300.000000	
temperature:is stable?{Boolean}=False	
temperature:monitor{Boolean}=True	
temperature:ramping{Boolean}=False	
temperature:ramping on{Boolean}=False	
temperature:ramping on 2{Boolean}=False	
temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
temperature:stability code{U32}=6618880	
temperature:stability rate{Extended Float}=0.040000	
y{Double Float}=2.400000	
