TDI Format 1.5	Offset	Rxx::R	Rxx::Theta	Rxx::X	Rxx::Y	Rxy::R	Rxy::Theta	Rxy::X	Rxy::Y	temperature: T1	temperature: T2	temperature: T3	temperature: T4	temperature: dT/dt	iterator	multi[0]:iterator	multi[0]:y	multi[0]:temperature: setpoint	multi[0]:temperature: T1	multi[0]:temperature: T2	multi[0]:temperature: T3	multi[0]:temperature: T4	multi[0]:temperature: heater	multi[0]:temperature: gas	multi[0]:temperature: dT/dt	multi[0]:temperature: current temperature	multi[0]:temperature: error	multi[1]:iterator	multi[1]:y	multi[1]:Control:Magnet Output
2nd Parameter Class{String}=Multi-Parameter	0E+0	1.226748807E-3	1.56E-1	1.226748807E-3	3.371767975E-6	5.753068855E-7	-7.4292E+0	5.700386571E-7	-7.533787176E-8	2.2098E+0	2.3188E+0	8.60315E+1	6.6564E+1	3.601363627E-3	1.13E+2	2E+0	2.2E+0	2.2E+0	2.1993E+0	2.3105E+0	8.60315E+1	6.6564E+1	4E-1	2.2E+0	-9.132997133E-3	2.1998E+0	2E-4	0E+0	0E+0	-1E-4
2nd Parameter Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	0E+0	1.233727385E-3	1.56E-1	1.233727385E-3	3.371767975E-6	7.182391875E-6	-4.104E-1	7.182391875E-6	-5.215704471E-8	2.2823E+0	2.4049E+0	8.63539E+1	6.6564E+1	6.838323921E-2	1.14E+2	2E+0	2.2E+0	1.8E+0	2.2098E+0	2.3188E+0	8.60315E+1	6.6564E+1	4E-1	2.2E+0	3.601363627E-3	1.4649E+0	2E-4	1E+0	5E-1	4.999E-1
Analysis Class{String}=Basic Plot	0E+0	1.23844803E-3	1.56E-1	1.23844803E-3	3.371767975E-6	1.381213172E-5	-1.656E-1	1.381213172E-5	-4.056657462E-8	1.9312E+0	2.0092E+0	8.62464E+1	6.6564E+1	-1.969987035E+0	1.15E+2	2E+0	2.2E+0	1.8E+0	2.2823E+0	2.4049E+0	8.63539E+1	6.6564E+1	4E-1	2.2E+0	6.838323921E-2	1.4649E+0	2E-4	2E+0	1E+0	9.999E-1
Analysis Class Path{Path}=C\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV\\\\plugins\\\\Plotting\\\\Plotting_Base_class\\\\Plotting_Base.lvclass	0E+0	1.243876913E-3	1.56E-1	1.243876913E-3	3.371767975E-6	2.043442431E-5	-7.44E-2	2.043442431E-5	-2.844926472E-8	2.2528E+0	2.3365E+0	8.59957E+1	6.6564E+1	1.48031652E-1	1.16E+2	2E+0	2.2E+0	1.8E+0	1.9312E+0	2.0092E+0	8.62464E+1	6.6564E+1	4E-1	2.2E+0	-1.969987035E+0	1.4649E+0	2E-4	3E+0	1.5E+0	1.4999E+0
Analysis.# pre-routines{I32}=5	0E+0	1.243843255E-3	1.56E-1	1.243843255E-3	3.371767975E-6	2.042859775E-5	-4.2E-2	2.042859775E-5	-1.580516592E-8	2.2048E+0	2.2651E+0	8.59957E+1	6.6564E+1	1.830841228E-2	1.17E+2	2E+0	2.2E+0	1.8E+0	2.2528E+0	2.3365E+0	8.59957E+1	6.6564E+1	4E-1	2.2E+0	1.48031652E-1	1.4649E+0	2E-4	4E+0	1.5E+0	1.5E+0
Analysis:Pre[0]:T Control Measure{1D Array (I32)}=[1,2,3,4,7]	0E+0	1.241314641E-3	1.56E-1	1.241314641E-3	3.371767975E-6	1.775652608E-5	-1.44E-1	1.775652608E-5	-4.583500097E-8	2.1887E+0	2.3122E+0	8.63539E+1	6.6564E+1	-1.319389325E-2	1.18E+2	2E+0	2.2E+0	1.8E+0	2.2048E+0	2.2651E+0	8.59957E+1	6.6564E+1	4E-1	2.2E+0	1.830841228E-2	1.4649E+0	2E-4	5E+0	1.3E+0	1.3001E+0
Autosave Tabs{Enum U32 ((XY Measurement Save,Parameter Plot Save 2))}=Parameter Plot Save 2	0E+0	1.239088951E-3	1.56E-1	1.239088951E-3	3.371767975E-6	1.511604794E-5	-2.028E-1	1.511604794E-5	-5.426439262E-8	2.1966E+0	2.3272E+0	8.62464E+1	6.6564E+1	-1.526937727E-2	1.19E+2	2E+0	2.2E+0	1.8E+0	2.1887E+0	2.3122E+0	8.63539E+1	6.6564E+1	4E-1	2.2E+0	-1.319389325E-2	1.4649E+0	2E-4	6E+0	1.1E+0	1.1E+0
Control:Magnet Output{Double Float}=-0.007000	0E+0	1.23709887E-3	1.56E-1	1.23709887E-3	3.371767975E-6	1.246712128E-5	-2.22E-1	1.246712128E-5	-4.952284567E-8	2.0965E+0	2.2439E+0	8.62106E+1	6.6564E+1	-1.080671921E-1	1.2E+2	2E+0	2.2E+0	1.8E+0	2.1966E+0	2.3272E+0	8.62464E+1	6.6564E+1	4E-1	2.2E+0	-1.526937727E-2	1.4649E+0	2E-4	7E+0	9E-1	9.001E-1
Control:Magnet Rate{Double Float}=0.500000	0E+0	1.235244836E-3	1.56E-1	1.235244836E-3	3.371767975E-6	9.832376361E-6	-3.636E-1	9.832376361E-6	-6.427428107E-8	2.2086E+0	2.3147E+0	8.62106E+1	6.6564E+1	-2.162193693E-2	1.21E+2	2E+0	2.2E+0	1.8E+0	2.0965E+0	2.2439E+0	8.62106E+1	6.6564E+1	4E-1	2.2E+0	-1.080671921E-1	1.4649E+0	2E-4	8E+0	7E-1	7.001E-1
Display Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	0E+0	1.233795267E-3	1.56E-1	1.233795267E-3	3.371767975E-6	7.192927766E-6	-6.336E-1	7.192927766E-6	-8.113303609E-8	2.184E+0	2.2967E+0	8.58883E+1	6.58035E+1	-5.144612491E-2	1.22E+2	2E+0	2.2E+0	1.8E+0	2.2086E+0	2.3147E+0	8.62106E+1	6.6564E+1	4E-1	2.2E+0	-2.162193693E-2	1.4649E+0	2E-4	9E+0	5E-1	5.001E-1
Elapsed Time{Double Float}=12790.950867	0E+0	1.232547931E-3	1.56E-1	1.232547931E-3	3.371767975E-6	4.554514376E-6	-7.716E-1	4.554514376E-6	-6.269372771E-8	2.1939E+0	2.3054E+0	8.60673E+1	6.58035E+1	-3.593948111E-2	1.23E+2	2E+0	2.2E+0	1.8E+0	2.184E+0	2.2967E+0	8.58883E+1	6.58035E+1	4E-1	2.2E+0	-5.144612491E-2	1.4649E+0	2E-4	1E+1	3E-1	3.001E-1
File:Autodel{Boolean}=True	0E+0	1.230693897E-3	1.56E-1	1.230693897E-3	3.371767975E-6	1.88714072E-6	-2.2476E+0	1.885553972E-6	-7.533781519E-8	2.1972E+0	2.3137E+0	8.63897E+1	6.58035E+1	-2.102421038E-2	1.24E+2	2E+0	2.2E+0	1.8E+0	2.1939E+0	2.3054E+0	8.60673E+1	6.58035E+1	4E-1	2.2E+0	-3.593948111E-2	1.4649E+0	2E-4	1.1E+1	1E-1	1.001E-1
File:Autosave{Boolean}=False	0E+0	1.230693897E-3	1.56E-1	1.230693897E-3	3.371767975E-6	1.887137891E-6	-2.1324E+0	1.885556801E-6	-7.112311936E-8	2.1205E+0	2.2313E+0	8.63897E+1	6.58035E+1	-1.555364579E-1	1.25E+2	2E+0	2.2E+0	1.8E+0	2.1972E+0	2.3137E+0	8.63897E+1	6.58035E+1	4E-1	2.2E+0	-2.102421038E-2	1.4649E+0	2E-4	1.2E+1	1E-1	1E-1
File:Export Config{Boolean}=True	0E+0	1.230524191E-3	1.56E-1	1.230524191E-3	3.371767975E-6	1.765436329E-6	-2.658E+0	1.763855238E-6	-8.324055371E-8	2.2299E+0	2.3389E+0	8.63181E+1	6.58035E+1	2.981721424E-2	1.26E+2	2E+0	2.2E+0	1.8E+0	2.1205E+0	2.2313E+0	8.63897E+1	6.58035E+1	4E-1	2.2E+0	-1.555364579E-1	1.4649E+0	2E-4	1.3E+1	9E-2	9E-2
File:Final Autosave{Boolean}=True	0E+0	1.2303559E-3	1.56E-1	1.2303559E-3	3.338050296E-6	1.6231919E-6	-2.826E+0	1.621084722E-6	-8.166002864E-8	2.2018E+0	2.3161E+0	8.63181E+1	6.58035E+1	4.13257163E-3	1.27E+2	2E+0	2.2E+0	1.8E+0	2.2299E+0	2.3389E+0	8.63181E+1	6.58035E+1	4E-1	2.2E+0	2.981721424E-2	1.4649E+0	2E-4	1.4E+1	8E-2	8E-2
Filter:Enable{Enum U16 ((None,Analog,Digital,Analog&Digitial))}=None	0E+0	1.230187608E-3	1.56E-1	1.230187608E-3	3.338050296E-6	1.479363553E-6	-2.7936E+0	1.476733116E-6	-7.323046728E-8	2.1393E+0	2.2806E+0	8.63181E+1	6.58035E+1	-4.542713985E-2	1.28E+2	2E+0	2.2E+0	1.8E+0	2.2018E+0	2.3161E+0	8.63181E+1	6.58035E+1	4E-1	2.2E+0	4.13257163E-3	1.4649E+0	2E-4	1.5E+1	7E-2	7E-2
Filter:Points{I32}=1	0E+0	1.229849611E-3	1.56E-1	1.229849611E-3	3.371767975E-6	1.348706342E-6	-3.3444E+0	1.346599163E-6	-8.007944699E-8	2.2231E+0	2.3374E+0	8.62822E+1	6.58035E+1	4.69814688E-2	1.29E+2	2E+0	2.2E+0	1.8E+0	2.1393E+0	2.2806E+0	8.63181E+1	6.58035E+1	4E-1	2.2E+0	-4.542713985E-2	1.4649E+0	2E-4	1.6E+1	6E-2	6E-2
Filter:Type{U16}=1	0E+0	1.22968132E-3	1.56E-1	1.22968132E-3	3.371767975E-6	1.232800509E-6	-3.5472E+0	1.230166395E-6	-7.74451631E-8	2.2044E+0	2.3203E+0	8.62822E+1	6.58035E+1	2.904360369E-2	1.3E+2	2E+0	2.2E+0	1.8E+0	2.2231E+0	2.3374E+0	8.62822E+1	6.58035E+1	4E-1	2.2E+0	4.69814688E-2	1.4649E+0	2E-4	1.7E+1	5E-2	5.01E-2
Filter:Type.__text__{String}=Repeat	0E+0	1.22968132E-3	1.56E-1	1.22968132E-3	3.338050296E-6	1.226478409E-6	-3.5856E+0	1.224370948E-6	-7.849889363E-8	2.2203E+0	2.3294E+0	8.62464E+1	6.58035E+1	3.640046716E-2	1.31E+2	2E+0	2.2E+0	1.8E+0	2.2044E+0	2.3203E+0	8.62822E+1	6.58035E+1	4E-1	2.2E+0	2.904360369E-2	1.4649E+0	2E-4	1.8E+1	5E-2	5E-2
Filter:Window{Double Float}=1.000000	0E+0	1.229513028E-3	1.56E-1	1.229513028E-3	3.371767975E-6	1.167472894E-6	-3.8628E+0	1.16483878E-6	-8.007936214E-8	2.214E+0	2.3278E+0	8.62464E+1	6.58035E+1	2.91151423E-2	1.32E+2	2E+0	2.2E+0	1.8E+0	2.2203E+0	2.3294E+0	8.62464E+1	6.58035E+1	4E-1	2.2E+0	3.640046716E-2	1.4649E+0	2E-4	1.9E+1	4.5E-2	4.5E-2
Iterator{I32}=0	0E+0	1.229513028E-3	1.56E-1	1.229513028E-3	3.371767975E-6	1.081072082E-6	-3.9444E+0	1.077911032E-6	-7.586475116E-8	2.1173E+0	2.2534E+0	8.62464E+1	6.58035E+1	-9.354202449E-2	1.33E+2	2E+0	2.2E+0	1.8E+0	2.214E+0	2.3278E+0	8.62464E+1	6.58035E+1	4E-1	2.2E+0	2.91151423E-2	1.4649E+0	2E-4	2E+1	4E-2	3.95E-2
Magnet: Control Mode{Boolean}=False	0E+0	1.229210104E-3	1.56E-1	1.229210104E-3	3.371767975E-6	1.012056197E-6	-4.5396E+0	1.008368494E-6	-8.166000035E-8	2.1956E+0	2.3102E+0	8.62464E+1	6.58035E+1	-7.197399158E-3	1.34E+2	2E+0	2.2E+0	1.8E+0	2.1173E+0	2.2534E+0	8.62464E+1	6.58035E+1	4E-1	2.2E+0	-9.354202449E-2	1.4649E+0	2E-4	2.1E+1	3.5E-2	3.49E-2
Magnet: Final Switch Heater{Enum U8 ((False,True,Mixed))}=	0E+0	1.22900674E-3	1.56E-1	1.22900674E-3	3.371767975E-6	9.567389509E-7	-4.686E+0	9.530503991E-7	-8.007941871E-8	2.2125E+0	2.3251E+0	8.62464E+1	6.58035E+1	9.648990817E-3	1.35E+2	2E+0	2.2E+0	1.8E+0	2.1956E+0	2.3102E+0	8.62464E+1	6.58035E+1	4E-1	2.2E+0	-7.197399158E-3	1.4649E+0	2E-4	2.2E+1	3E-2	2.99E-2
Magnet: Power Supply{Enum U16 ((IPS120,LS625,PS110,Hg iPS,SMS Series,Cryomagnetics 4G,DMG Little CryoFree,DMG Big CryoFree))}=Hg iPS	0E+0	1.228737474E-3	1.56E-1	1.228737474E-3	3.371767975E-6	8.808743129E-7	-4.5768E+0	8.777132627E-7	-7.164997048E-8	2.1876E+0	2.3006E+0	8.62464E+1	6.58035E+1	-3.744139895E-2	1.36E+2	2E+0	2.2E+0	1.8E+0	2.2125E+0	2.3251E+0	8.62464E+1	6.58035E+1	4E-1	2.2E+0	9.648990817E-3	1.4649E+0	2E-4	2.3E+1	2.5E-2	2.46E-2
Magnet: Rate{Double Float}=0.500000	0E+0	1.228333574E-3	1.56E-1	1.228333574E-3	3.371767975E-6	8.271367431E-7	-5.8104E+0	8.239759758E-7	-8.534784506E-8	2.2224E+0	2.33E+0	8.62106E+1	6.58035E+1	2.046822757E-2	1.37E+2	2E+0	2.2E+0	1.8E+0	2.1876E+0	2.3006E+0	8.62464E+1	6.58035E+1	4E-1	2.2E+0	-3.744139895E-2	1.4649E+0	2E-4	2.4E+1	2E-2	1.99E-2
Magnet: Setpoint{Double Float}=0.000000	0E+0	1.227995577E-3	1.56E-1	1.227995577E-3	3.371767975E-6	7.412628671E-7	-6.3084E+0	7.365212919E-7	-8.271361774E-8	2.2461E+0	2.3476E+0	8.62106E+1	6.58035E+1	5.349865928E-2	1.38E+2	2E+0	2.2E+0	1.8E+0	2.2224E+0	2.33E+0	8.62106E+1	6.58035E+1	4E-1	2.2E+0	2.046822757E-2	1.4649E+0	2E-4	2.5E+1	1.5E-2	1.49E-2
Magnet: Units{Enum U16 ((Field,Current))}=Field	0E+0	1.227658995E-3	1.56E-1	1.227658995E-3	3.371767975E-6	6.764610561E-7	-6.8436E+0	6.711919792E-7	-8.165985893E-8	2.1766E+0	2.3196E+0	8.62106E+1	6.58035E+1	2.546025626E-2	1.39E+2	2E+0	2.2E+0	1.8E+0	2.2461E+0	2.3476E+0	8.62106E+1	6.58035E+1	4E-1	2.2E+0	5.349865928E-2	1.4649E+0	2E-4	2.6E+1	1E-2	1E-2
Magnet: VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	0E+0	1.227085389E-3	1.56E-1	1.227085389E-3	3.371767975E-6	6.237759441E-7	-6.5904E+0	6.195607391E-7	-7.270367272E-8	2.2177E+0	2.331E+0	8.59599E+1	6.58035E+1	3.705522045E-2	1.4E+2	2E+0	2.2E+0	1.8E+0	2.1766E+0	2.3196E+0	8.62106E+1	6.58035E+1	4E-1	2.2E+0	2.546025626E-2	1.4649E+0	2E-4	2.7E+1	5E-3	4.9E-3
Main Screen Path{Path}=C:\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV\\\\1Code.vi	0E+0	1.226647832E-3	1.56E-1	1.226647832E-3	3.371767975E-6	5.747802324E-7	-7.674E+0	5.69512004E-7	-7.84989502E-8	2.2008E+0	2.3091E+0	8.59241E+1	6.58035E+1	5.536372773E-3	1.41E+2	2E+0	2.2E+0	1.8E+0	2.2177E+0	2.331E+0	8.59599E+1	6.58035E+1	4E-1	2.2E+0	3.705522045E-2	1.4649E+0	2E-4	2.8E+1	0E+0	0E+0
Measurement Timestamp{Timestamp}=<20:51:26.631 17/05/2023>T	0E+0	1.227287339E-3	1.56E-1	1.227287339E-3	3.371767975E-6	4.799498591E-7	-1.02012E+1	4.736277588E-7	-8.692839842E-8	2.2328E+0	2.3382E+0	8.58883E+1	6.58035E+1	4.924055561E-2	1.42E+2	2E+0	2.2E+0	1.8E+0	2.2008E+0	2.3091E+0	8.59241E+1	6.58035E+1	4E-1	2.2E+0	5.536372773E-3	1.4649E+0	2E-4	2.9E+1	-5E-3	-5.3E-3
Measurement Title{String}=	0E+0	1.227827286E-3	1.56E-1	1.227827286E-3	3.371767975E-6	4.251587002E-7	-1.20228E+1	4.151491795E-7	-9.008947686E-8	2.2079E+0	2.3235E+0	8.58883E+1	6.58035E+1	2.664026059E-2	1.43E+2	2E+0	2.2E+0	1.8E+0	2.2328E+0	2.3382E+0	8.58883E+1	6.58035E+1	4E-1	2.2E+0	4.924055561E-2	1.4649E+0	2E-4	3E+1	-1E-2	-1.01E-2
Measurment Select{U16}=4	0E+0	1.228163869E-3	1.56E-1	1.228163869E-3	3.338050296E-6	3.550900751E-7	-1.35408E+1	3.450797058E-7	-8.534798648E-8	2.2041E+0	2.3172E+0	8.60673E+1	6.58035E+1	4.917859915E-4	1.44E+2	2E+0	2.2E+0	1.8E+0	2.2079E+0	2.3235E+0	8.58883E+1	6.58035E+1	4E-1	2.2E+0	2.664026059E-2	1.4649E+0	2E-4	3.1E+1	-1.5E-2	-1.5E-2
Measurment Select.__text__{String}=6221-Lockin-DAQ	0E+0	1.228501866E-3	1.56E-1	1.228501866E-3	3.371767975E-6	2.902874155E-7	-1.64484E+1	2.765901915E-7	-8.37672917E-8	2.1944E+0	2.3001E+0	8.60673E+1	6.58035E+1	-2.670836635E-2	1.45E+2	2E+0	2.2E+0	1.8E+0	2.2041E+0	2.3172E+0	8.60673E+1	6.58035E+1	4E-1	2.2E+0	4.917859915E-4	1.4649E+0	2E-4	3.2E+1	-2E-2	-2.01E-2
Notes{String}=I+1A I-1E\\nrxx+1B Rxx-1C\\nRxy+1D Rxy-4A	0E+0	1.228838449E-3	1.56E-1	1.228838449E-3	3.338050296E-6	2.370773474E-7	-1.96764E+1	2.228529045E-7	-8.165994378E-8	2.1418E+0	2.2566E+0	8.63539E+1	6.58035E+1	-8.260057122E-2	1.46E+2	2E+0	2.2E+0	1.8E+0	2.1944E+0	2.3001E+0	8.60673E+1	6.58035E+1	4E-1	2.2E+0	-2.670836635E-2	1.4649E+0	2E-4	3.3E+1	-2.5E-2	-2.51E-2
Offset{Double Float}=0.000000	0E+0	1.22900674E-3	1.56E-1	1.22900674E-3	3.371767975E-6	1.685886816E-7	-2.94252E+1	1.464607648E-7	-8.482102222E-8	2.2354E+0	2.3479E+0	8.63539E+1	6.58035E+1	6.180777401E-2	1.47E+2	2E+0	2.2E+0	1.8E+0	2.1418E+0	2.2566E+0	8.63539E+1	6.58035E+1	4E-1	2.2E+0	-8.260057122E-2	1.4649E+0	2E-4	3.4E+1	-3E-2	-3.04E-2
Option: 2182 Autozero{Boolean}=True	0E+0	1.229277421E-3	1.56E-1	1.229277421E-3	3.371767975E-6	1.180118226E-7	-4.68612E+1	8.007950356E-8	-8.798212894E-8	2.2278E+0	2.3354E+0	8.63539E+1	6.58035E+1	4.000630602E-2	1.48E+2	2E+0	2.2E+0	1.8E+0	2.2354E+0	2.3479E+0	8.63539E+1	6.58035E+1	4E-1	2.2E+0	6.180777401E-2	1.4649E+0	2E-4	3.5E+1	-3.5E-2	-3.51E-2
Option: 2182 Front Autozero{Boolean}=True	0E+0	1.229344737E-3	1.56E-1	1.229344737E-3	3.371767975E-6	9.061629969E-8	-7.92864E+1	1.475150328E-8	-9.114309425E-8	2.2227E+0	2.3303E+0	8.63539E+1	6.58035E+1	3.636550903E-2	1.49E+2	2E+0	2.2E+0	1.8E+0	2.2278E+0	2.3354E+0	8.63539E+1	6.58035E+1	4E-1	2.2E+0	4.000630602E-2	1.4649E+0	2E-4	3.6E+1	-4E-2	-4.04E-2
Option: 2182 Hold{Boolean}=False	0E+0	1.229513028E-3	1.56E-1	1.229513028E-3	3.371767975E-6	9.851892508E-8	-1.248804E+2	-5.900593957E-8	-8.324046886E-8	2.2084E+0	2.3243E+0	8.63181E+1	6.58035E+1	3.890296817E-2	1.5E+2	2E+0	2.2E+0	1.8E+0	2.2227E+0	2.3303E+0	8.63539E+1	6.58035E+1	4E-1	2.2E+0	3.636550903E-2	1.4649E+0	2E-4	3.7E+1	-4.5E-2	-4.51E-2
Option: 2182 Hold Count{I32}=10	0E+0	1.22968132E-3	1.56E-1	1.22968132E-3	3.371767975E-6	1.475146651E-7	-1.52616E+2	-1.327631731E-7	-6.954262257E-8	2.1927E+0	2.2639E+0	8.62464E+1	6.58035E+1	-5.3141132E-2	1.51E+2	2E+0	2.2E+0	1.8E+0	2.2084E+0	2.3243E+0	8.63181E+1	6.58035E+1	4E-1	2.2E+0	3.890296817E-2	1.4649E+0	2E-4	3.8E+1	-5E-2	-5.02E-2
Option: 2182 Hold Window{Double Float}=1.000000	0E+0	1.22968132E-3	1.56E-1	1.22968132E-3	3.371767975E-6	1.49621815E-7	-1.448148E+2	-1.238070152E-7	-8.745527782E-8	2.1723E+0	2.2841E+0	8.62822E+1	6.58035E+1	-3.541325778E-2	1.52E+2	2E+0	2.2E+0	1.8E+0	2.1927E+0	2.2639E+0	8.62464E+1	6.58035E+1	4E-1	2.2E+0	-5.3141132E-2	1.4649E+0	2E-4	3.9E+1	-5E-2	-5E-2
Option: 2182 Line Sync{Boolean}=False	0E+0	1.229917494E-3	1.56E-1	1.229917494E-3	3.371767975E-6	2.623654658E-7	-1.656744E+2	-2.560433655E-7	-6.69084801E-8	2.1985E+0	2.3163E+0	8.62822E+1	6.58035E+1	-4.184823483E-3	1.53E+2	2E+0	2.2E+0	1.8E+0	2.1723E+0	2.2841E+0	8.62822E+1	6.58035E+1	4E-1	2.2E+0	-3.541325778E-2	1.4649E+0	2E-4	4E+1	-6E-2	-5.99E-2
Option: 2182 Reference Reading{Double Float}=0.000000	0E+0	1.230187608E-3	1.56E-1	1.230187608E-3	3.371767975E-6	3.793243215E-7	-1.666644E+2	-3.714216961E-7	-8.956259745E-8	2.2067E+0	2.325E+0	8.62464E+1	6.58035E+1	7.636111695E-3	1.54E+2	2E+0	2.2E+0	1.8E+0	2.1985E+0	2.3163E+0	8.62822E+1	6.58035E+1	4E-1	2.2E+0	-4.184823483E-3	1.4649E+0	2E-4	4.1E+1	-7E-2	-7E-2
Option: 2182 Relative Mode{Boolean}=False	0E+0	1.2303559E-3	1.56E-1	1.2303559E-3	3.338050296E-6	5.163013702E-7	-1.699668E+2	-5.10505923E-7	-9.166997365E-8	2.1758E+0	2.2946E+0	8.62106E+1	6.58035E+1	-3.272817284E-2	1.55E+2	2E+0	2.2E+0	1.8E+0	2.2067E+0	2.325E+0	8.62464E+1	6.58035E+1	4E-1	2.2E+0	7.636111695E-3	1.4649E+0	2E-4	4.2E+1	-8E-2	-7.99E-2
Option: 2182 Trigger Delay{Cluster (Boolean,Double Float)}={'Auto':True,'Time(s)':0.000000}	0E+0	1.230524191E-3	1.56E-1	1.230524191E-3	3.371767975E-6	6.448494232E-7	-1.73454E+2	-6.42742245E-7	-7.481102064E-8	2.1147E+0	2.2434E+0	8.61748E+1	6.58035E+1	-1.067558676E-1	1.56E+2	2E+0	2.2E+0	1.8E+0	2.1758E+0	2.2946E+0	8.62106E+1	6.58035E+1	4E-1	2.2E+0	-3.272817284E-2	1.4649E+0	2E-4	4.3E+1	-9E-2	-8.99E-2
Option: 2182 Trigger Source{Enum U16 ((Immediate,Timer,Manual,Bus,Trigger link))}=Bus	0E+0	1.230524191E-3	1.56E-1	1.230524191E-3	3.371767975E-6	7.855172865E-7	-1.730196E+2	-7.823559535E-7	-9.746519456E-8	2.2176E+0	2.3228E+0	8.62464E+1	6.58035E+1	2.408455312E-2	1.57E+2	2E+0	2.2E+0	1.8E+0	2.1147E+0	2.2434E+0	8.61748E+1	6.58035E+1	4E-1	2.2E+0	-1.067558676E-1	1.4649E+0	2E-4	4.4E+1	-1E-1	-1E-1
Option: 2182 Trigger Timer{Double Float}=0.000000	0E+0	1.230524191E-3	1.56E-1	1.230524191E-3	3.371767975E-6	7.881514006E-7	-1.73694E+2	-7.849903505E-7	-8.85089235E-8	2.2351E+0	2.3404E+0	8.62106E+1	6.58035E+1	5.333566293E-2	1.58E+2	2E+0	2.2E+0	1.8E+0	2.2176E+0	2.3228E+0	8.62464E+1	6.58035E+1	4E-1	2.2E+0	2.408455312E-2	1.4649E+0	2E-4	4.5E+1	-1E-1	-1E-1
Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	0E+0	1.232379639E-3	1.548E-1	1.232379639E-3	3.338050296E-6	3.412862193E-6	-1.7841E+2	-3.413914368E-6	-9.641157717E-8	2.1977E+0	2.3117E+0	8.62464E+1	6.58035E+1	8.534165099E-3	1.59E+2	2E+0	2.2E+0	1.8E+0	2.2351E+0	2.3404E+0	8.62106E+1	6.58035E+1	4E-1	2.2E+0	5.333566293E-2	1.4649E+0	2E-4	4.6E+1	-3E-1	-2.998E-1
Option: 560 Enabled{Boolean}=False	0E+0	1.233727385E-3	1.56E-1	1.233727385E-3	3.371767975E-6	6.040213605E-6	-1.790028E+2	-6.042846871E-6	-1.058946145E-7	2.1265E+0	2.245E+0	8.60315E+1	6.58035E+1	-1.182488799E-1	1.6E+2	2E+0	2.2E+0	1.8E+0	2.1977E+0	2.3117E+0	8.62464E+1	6.58035E+1	4E-1	2.2E+0	8.534165099E-3	1.4649E+0	2E-4	4.7E+1	-5E-1	-4.999E-1
Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	0E+0	1.235244836E-3	1.548E-1	1.235244836E-3	3.338050296E-6	8.660694768E-6	-1.792764E+2	-8.663325205E-6	-1.10109282E-7	2.1083E+0	2.2657E+0	8.63897E+1	6.58035E+1	-8.846797794E-2	1.61E+2	2E+0	2.2E+0	1.8E+0	2.1265E+0	2.245E+0	8.60315E+1	6.58035E+1	4E-1	2.2E+0	-1.182488799E-1	1.4649E+0	2E-4	4.8E+1	-7E-1	-6.999E-1
Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	0E+0	1.236863262E-3	1.56E-1	1.236863262E-3	3.371767975E-6	1.129754404E-5	-1.794756E+2	-1.130018013E-5	-1.043141177E-7	2.1752E+0	2.2879E+0	8.62822E+1	6.58035E+1	-3.596531972E-2	1.62E+2	2E+0	2.2E+0	1.8E+0	2.1083E+0	2.2657E+0	8.63897E+1	6.58035E+1	4E-1	2.2E+0	-8.846797794E-2	1.4649E+0	2E-4	4.9E+1	-9E-1	-8.999E-1
Option: 6221 Adjust Mode{Enum U16 ((Offset,Frequency,Amplitude))}=Offset	0E+0	1.238650262E-3	1.56E-1	1.238650262E-3	3.371767975E-6	1.394173025E-5	-1.795224E+2	-1.394436917E-5	-1.174849997E-7	2.1909E+0	2.2904E+0	8.61748E+1	6.58035E+1	-4.801206663E-2	1.63E+2	2E+0	2.2E+0	1.8E+0	2.1752E+0	2.2879E+0	8.62822E+1	6.58035E+1	4E-1	2.2E+0	-3.596531972E-2	1.4649E+0	2E-4	5E+1	-1.1E+0	-1.0999E+0
Option: 6221 Amplitude{Double Float}=1.000000E-6	0E+0	1.240976644E-3	1.56E-1	1.240976644E-3	3.371767975E-6	1.658436931E-5	-1.79556E+2	-1.658694318E-5	-1.301290589E-7	2.1675E+0	2.2898E+0	8.61748E+1	6.58035E+1	-6.206809729E-2	1.64E+2	2E+0	2.2E+0	1.8E+0	2.1909E+0	2.2904E+0	8.61748E+1	6.58035E+1	4E-1	2.2E+0	-4.801206663E-2	1.4649E+0	2E-4	5.1E+1	-1.3E+0	-1.2999E+0
Option: 6221 Compliance{Double Float}=10.000000	0E+0	1.243505257E-3	1.56E-1	1.243505257E-3	3.371767975E-6	1.922747789E-5	-1.796376E+2	-1.923010833E-5	-1.232801924E-7	2.1953E+0	2.3216E+0	8.6139E+1	6.58035E+1	-1.64391892E-3	1.65E+2	2E+0	2.2E+0	1.8E+0	2.1675E+0	2.2898E+0	8.61748E+1	6.58035E+1	4E-1	2.2E+0	-6.206809729E-2	1.4649E+0	2E-4	5.2E+1	-1.5E+0	-1.4999E+0
Option: 6221 Duty Cycle{Double Float}=50.000000	0E+0	1.243505257E-3	1.548E-1	1.243505257E-3	3.338050296E-6	1.922643137E-5	-1.795992E+2	-1.922906181E-5	-1.359242516E-7	2.2154E+0	2.3359E+0	8.58524E+1	6.58035E+1	2.75554359E-2	1.66E+2	2E+0	2.2E+0	1.8E+0	2.1953E+0	2.3216E+0	8.6139E+1	6.58035E+1	4E-1	2.2E+0	-1.64391892E-3	1.4649E+0	2E-4	5.3E+1	-1.5E+0	-1.5E+0
Option: 6221 External Trigger{Boolean}=False	0E+0	1.23777345E-3	1.56E-1	1.23777345E-3	3.371767975E-6	1.261094963E-5	-1.793856E+2	-1.261358289E-5	-1.369779255E-7	2.192E+0	2.3158E+0	8.62822E+1	6.58035E+1	-2.495272085E-2	1.67E+2	2E+0	2.2E+0	1.8E+0	2.2154E+0	2.3359E+0	8.58524E+1	6.58035E+1	4E-1	2.2E+0	2.75554359E-2	1.4649E+0	2E-4	5.4E+1	-1E+0	-1.0001E+0
Option: 6221 External Trigger Ignore Multiple{Boolean}=False	0E+0	1.233727385E-3	1.56E-1	1.233727385E-3	3.371767975E-6	6.021243344E-6	-1.789764E+2	-6.023353351E-6	-1.090556364E-7	2.1814E+0	2.3033E+0	8.61748E+1	6.58035E+1	-2.353528887E-2	1.68E+2	2E+0	2.2E+0	1.8E+0	2.192E+0	2.3158E+0	8.62822E+1	6.58035E+1	4E-1	2.2E+0	-2.495272085E-2	1.4649E+0	2E-4	5.5E+1	-5E-1	-5.001E-1
Option: 6221 Frequency{Double Float}=119.770000	
Option: 6221 Function{U16}=1	
Option: 6221 Function.__text__{String}=Sine	
Option: 6221 Idle Level{Double Float}=0.000000	
Option: 6221 Input trigger Line{U8}=5	
Option: 6221 Offset{Double Float}=0.000000	
Option: 6221 Output Trigger Line{U8}=4	
Option: 6221 Pass Through{Boolean}=True	
Option: 6221 Phase Marker{Boolean}=True	
Option: 6221 Phase Marker Phase{Double Float}=0.000000	
Option: 6221 Range Level{Double Float}=2.000000E-12	
Option: 6221 Ranging{U16}=1	
Option: 6221 Ranging.__text__{String}=Best	
Option: 6221 Update Clock{Double Float}=0.000000	
Option: 6221 VISA{Visa Refnum (Void)}=GPIB0::13::INSTR	
Option: Confirm Config{Boolean}=False	
Option: Control Panel Ref{LVObjVI Refnum (Void)}=	
Option: DAQ Global Channel{Boolean}=False	
Option: DAQ Input Rate{Double Float}=10000.000000	
Option: DAQ Input Samples{I32}=200	
Option: DAQ Measurement Channels{1D Array (Cluster (UserDefinedRefnumTag Refnum (Void),\tkDAQmxPhysChanTagType Tag,\tkDAQmxScaleTagType Tag,Boolean,Double Float,String))}=[]	
Option: Differential{I32}=10106	
Option: Differential.__text__{String}=Differential	
Option: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values))}=Function Generator	
Option: Lockin Standoff Time{Double Float}=0.000000	
Option: Paranoid Save Data{Boolean}=True	
Option: Plot Autoback Path{Path}=C:\\\\TEMP\\\\XY Multiparam\\\\Backup.txt	
Option: SR830  Ref Phase{Double Float}=0.000000	
Option: SR830  Synch Filter{Boolean}=False	
Option: SR830  Time Constant{I16}=8	
Option: SR830  Time Constant.__text__{String}=100 ms	
Option: SR830 2x Line Filter{Boolean}=True	
Option: SR830 Adjust Gains{Boolean}=False	
Option: SR830 Auto Gain Lower.__text__{String}=2 nV/fA	
Option: SR830 Auto Gain Upper.__text__{String}=1 V/uA	
Option: SR830 Auto Offset 1{Boolean}=False	
Option: SR830 Auto Offset 2{Boolean}=False	
Option: SR830 Autophase{Boolean}=False	
Option: SR830 DC Coupling?{Boolean}=False	
Option: SR830 Display 1{U16}=0	
Option: SR830 Display 1.__text__{String}=X	
Option: SR830 Display 2{U16}=0	
Option: SR830 Display 2.__text__{String}=Y	
Option: SR830 Dynamic Reserve{I16}=1	
Option: SR830 Dynamic Reserve.__text__{String}=Normal	
Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Option: SR830 Filter Slope{I32}=1	
Option: SR830 Filter Slope.__text__{String}=12 dB/oct	
Option: SR830 Gain{I32}=-1	
Option: SR830 Gain.__text__{String}=Auto Gain	
Option: SR830 Ground Shield?{Boolean}=False	
Option: SR830 Harmonic{I32}=1	
Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A	
Option: SR830 Line Filter{Boolean}=True	
Option: SR830 No Reset{Boolean}=False	
Option: SR830 Offset 1{Double Float}=0.000000	
Option: SR830 Offset 2{Double Float}=0.000000	
Option: SR830 Output Channel 1{Boolean}=False	
Option: SR830 Output Channel 2{Boolean}=False	
Option: SR830 Ratio 1{U16}=0	
Option: SR830 Ratio 1.__text__{String}=None	
Option: SR830 Ratio 2{U16}=0	
Option: SR830 Ratio 2.__text__{String}=None	
Option: SR830 Ref Amplitude{Double Float}=0.100000	
Option: SR830 Ref Frequency{Double Float}=1013.000000	
Option: SR830 Ref Source{Boolean}=False	
Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta]	
Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Option: SR830 VISA{Visa Refnum (Void)}=	
Option: Sense Autorange{Boolean}=False	
Option: Sense Range Level{Double Float}=0.100000	
Option: Sense Rate{Double Float}=1.000000	
Option:560 Comport{Visa Refnum (Void)}=COM1	
Option:560 Filter High Pass{U16}=0	
Option:560 Filter High Pass.__text__{String}=0.03	
Option:560 Filter Lowpass{U16}=0	
Option:560 Filter Lowpass.__text__{String}=0.03	
Option:560 Filter Mode{U16}=0	
Option:560 Filter Mode.__text__{String}=6 dB high pass	
Option:560 Invert{Boolean}=False	
Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Option:570 Enabled{Boolean}=False	
Option:570 Filter High Pass{U16}=0	
Option:570 Filter High Pass.__text__{String}=0.03	
Option:570 Filter Lowpass{U16}=0	
Option:570 Filter Lowpass.__text__{String}=0.03	
Option:570 Filter Mode{U16}=0	
Option:570 Filter Mode.__text__{String}=6 dB high pass	
Option:570 Gain Mode{U16}=0	
Option:570 Gain Mode.__text__{String}=Low Noise	
Option:570 Input Offset{U16}=0	
Option:570 Input Offset On{Boolean}=False	
Option:570 Input Offset.__text__{String}=1pA	
Option:570 Sensitivity{U16}=0	
Option:570 Sensitivity.__text__{String}=1pA/V	
Option:Debug On{Boolean}=False	
Option:GPIB 2182{Visa Refnum (Void)}=	
Option:Parallel Config Voltage Measurers{Boolean}=True	
Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Option:SR830 Settle Time{Double Float}=5.000000	
Option:Sense Digits{I32}=8	
Output Names{1D Array (String)}=['Offset','Rxx::R','Rxx::Theta','Rxx::X','Rxx::Y','Rxy::R','Rxy::Theta','Rxy::X','Rxy::Y','temperature: T1','temperature: T2','temperature: T3','temperature: T4','temperature: dT/dt','iterator','multi[0]:iterator','multi[0]:y','multi[0]:temperature: setpoint','multi[0]:temperature: T1','multi[0]:temperature: T2','multi[0]:temperature: T3','multi[0]:temperature: T4','multi[0]:temperature: heater','multi[0]:temperature: gas','multi[0]:temperature: dT/dt','multi[0]:temperature: current temperature','multi[0]:temperature: error','multi[1]:iterator','multi[1]:y','multi[1]:Control:Magnet Output']	
Parameter Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Parameter Select{U16}=6	
Parameter Select.__text__{String}=Multi-Parameter	
Paths{U32}=0	
Plot: Column Renames{1D Array (Cluster (String,String))}=[]	
Plot: No dups{Boolean}=False	
Plot: StdDevs{Boolean}=False	
Plotting Class{String}=Parameter Plot	
Plotting Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	
Plotting Select{U16}=1	
Plotting Select.__text__{String}=Parameter Plot	
Project Code{String}=Topological_Insulators	
Ref: Temperature Window{LVObjVI Refnum (Void)}=	
Ref:Control Subpanel{LVObjUnknown Refnum (Void)}=	
Ref:Main Screen{LVObjVI Refnum (Void)}=	
Ref:Plotting Subpanel{LVObjUnknown Refnum (Void)}=	
Ref:Toolbar{LVObjUnknown Refnum (Void)}=	
Ref:XY Subpanel{LVObjUnknown Refnum (Void)}=	
Rxx::R{Double Float}=0.001234	
Rxx::Theta{Double Float}=0.156000	
Rxx::X{Double Float}=0.001234	
Rxx::Y{Double Float}=3.371768E-6	
Rxx:Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	
Rxx:Option: 560 Enabled{Boolean}=False	
Rxx:Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	
Rxx:Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	
Rxx:Option: Lockin Standoff Time{Double Float}=0.000000	
Rxx:Option: Lockin Type{Enum U16 ((SRS 830,EG&G 5302))}=SRS 830	
Rxx:Option: SR803 Full Scale Reading{Double Float}=0.000000	
Rxx:Option: SR830  Ref Phase{Double Float}=0.000000	
Rxx:Option: SR830  Synch Filter{Boolean}=False	
Rxx:Option: SR830  Time Constant{I16}=8	
Rxx:Option: SR830 2x Line Filter{Boolean}=False	
Rxx:Option: SR830 Adjust Gains{Boolean}=False	
Rxx:Option: SR830 Auto Gain Lower{I32}=0	
Rxx:Option: SR830 Auto Gain Upper{I32}=26	
Rxx:Option: SR830 Auto Offset 1{Boolean}=False	
Rxx:Option: SR830 Auto Offset 2{Boolean}=False	
Rxx:Option: SR830 Autophase{Boolean}=False	
Rxx:Option: SR830 DC Coupling?{Boolean}=False	
Rxx:Option: SR830 Display 1{U16}=0	
Rxx:Option: SR830 Display 2{U16}=0	
Rxx:Option: SR830 Dynamic Reserve{I16}=2	
Rxx:Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Rxx:Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Rxx:Option: SR830 Filter Slope{I32}=3	
Rxx:Option: SR830 Gain{I32}=18	
Rxx:Option: SR830 Ground Shield?{Boolean}=False	
Rxx:Option: SR830 Harmonic{I32}=1	
Rxx:Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A-B	
Rxx:Option: SR830 Line Filter{Boolean}=False	
Rxx:Option: SR830 No Reset{Boolean}=False	
Rxx:Option: SR830 Offset 1{Double Float}=0.000000	
Rxx:Option: SR830 Offset 2{Double Float}=0.000000	
Rxx:Option: SR830 Output Channel 1{Boolean}=False	
Rxx:Option: SR830 Output Channel 2{Boolean}=False	
Rxx:Option: SR830 Ratio 1{U16}=0	
Rxx:Option: SR830 Ratio 2{U16}=0	
Rxx:Option: SR830 Ref Amplitude{Double Float}=0.100000	
Rxx:Option: SR830 Ref Frequency{Double Float}=1013.000000	
Rxx:Option: SR830 Ref Source{Boolean}=False	
Rxx:Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta,X,Y]	
Rxx:Option: SR830 Time Constant value{Double Float}=0.000000	
Rxx:Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Rxx:Option: SR830 VISA{Visa Refnum (Void)}=GPIB0::5::INSTR	
Rxx:Option:560 Comport{Visa Refnum (Void)}=COM1	
Rxx:Option:560 Filter High Pass{U16}=0	
Rxx:Option:560 Filter Lowpass{U16}=0	
Rxx:Option:560 Filter Mode{U16}=0	
Rxx:Option:560 Invert{Boolean}=False	
Rxx:Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Rxx:Option:570 Enabled{Boolean}=False	
Rxx:Option:570 Filter High Pass{U16}=0	
Rxx:Option:570 Filter Lowpass{U16}=0	
Rxx:Option:570 Filter Mode{U16}=0	
Rxx:Option:570 Gain Mode{U16}=0	
Rxx:Option:570 Input Offset{U16}=0	
Rxx:Option:570 Input Offset On{Boolean}=False	
Rxx:Option:570 Sensitivity{U16}=0	
Rxx:Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Rxx:Option:SR830 Autogain Lower Threshold{Double Float}=0.100000	
Rxx:Option:SR830 Autogain Standoff{Double Float}=3.000000	
Rxx:Option:SR830 Autogain Upper Threshold{Double Float}=0.900000	
Rxx:Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Rxx:Option:SR830 Settle Time{Double Float}=0.000000	
Rxy::R{Double Float}=6.021243E-6	
Rxy::Theta{Double Float}=-178.976400	
Rxy::X{Double Float}=-6.023353E-6	
Rxy::Y{Double Float}=-1.090556E-7	
Rxy:Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	
Rxy:Option: 560 Enabled{Boolean}=False	
Rxy:Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	
Rxy:Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	
Rxy:Option: Lockin Standoff Time{Double Float}=0.000000	
Rxy:Option: Lockin Type{Enum U16 ((SRS 830,EG&G 5302))}=SRS 830	
Rxy:Option: SR803 Full Scale Reading{Double Float}=0.000000	
Rxy:Option: SR830  Ref Phase{Double Float}=0.000000	
Rxy:Option: SR830  Synch Filter{Boolean}=False	
Rxy:Option: SR830  Time Constant{I16}=8	
Rxy:Option: SR830 2x Line Filter{Boolean}=False	
Rxy:Option: SR830 Adjust Gains{Boolean}=False	
Rxy:Option: SR830 Auto Gain Lower{I32}=0	
Rxy:Option: SR830 Auto Gain Upper{I32}=26	
Rxy:Option: SR830 Auto Offset 1{Boolean}=False	
Rxy:Option: SR830 Auto Offset 2{Boolean}=False	
Rxy:Option: SR830 Autophase{Boolean}=False	
Rxy:Option: SR830 DC Coupling?{Boolean}=False	
Rxy:Option: SR830 Display 1{U16}=0	
Rxy:Option: SR830 Display 2{U16}=1	
Rxy:Option: SR830 Dynamic Reserve{I16}=2	
Rxy:Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Rxy:Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Rxy:Option: SR830 Filter Slope{I32}=3	
Rxy:Option: SR830 Gain{I32}=18	
Rxy:Option: SR830 Ground Shield?{Boolean}=False	
Rxy:Option: SR830 Harmonic{I32}=1	
Rxy:Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A-B	
Rxy:Option: SR830 Line Filter{Boolean}=False	
Rxy:Option: SR830 No Reset{Boolean}=False	
Rxy:Option: SR830 Offset 1{Double Float}=0.000000	
Rxy:Option: SR830 Offset 2{Double Float}=0.000000	
Rxy:Option: SR830 Output Channel 1{Boolean}=False	
Rxy:Option: SR830 Output Channel 2{Boolean}=False	
Rxy:Option: SR830 Ratio 1{U16}=0	
Rxy:Option: SR830 Ratio 2{U16}=0	
Rxy:Option: SR830 Ref Amplitude{Double Float}=0.100000	
Rxy:Option: SR830 Ref Frequency{Double Float}=1013.000000	
Rxy:Option: SR830 Ref Source{Boolean}=False	
Rxy:Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta,X,Y]	
Rxy:Option: SR830 Time Constant value{Double Float}=0.000000	
Rxy:Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Rxy:Option: SR830 VISA{Visa Refnum (Void)}=GPIB0::6::INSTR	
Rxy:Option:560 Comport{Visa Refnum (Void)}=COM1	
Rxy:Option:560 Filter High Pass{U16}=0	
Rxy:Option:560 Filter Lowpass{U16}=0	
Rxy:Option:560 Filter Mode{U16}=0	
Rxy:Option:560 Invert{Boolean}=False	
Rxy:Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Rxy:Option:570 Enabled{Boolean}=False	
Rxy:Option:570 Filter High Pass{U16}=0	
Rxy:Option:570 Filter Lowpass{U16}=0	
Rxy:Option:570 Filter Mode{U16}=0	
Rxy:Option:570 Gain Mode{U16}=0	
Rxy:Option:570 Input Offset{U16}=0	
Rxy:Option:570 Input Offset On{Boolean}=False	
Rxy:Option:570 Sensitivity{U16}=0	
Rxy:Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Rxy:Option:SR830 Autogain Lower Threshold{Double Float}=0.100000	
Rxy:Option:SR830 Autogain Standoff{Double Float}=3.000000	
Rxy:Option:SR830 Autogain Upper Threshold{Double Float}=0.900000	
Rxy:Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Rxy:Option:SR830 Settle Time{Double Float}=0.000000	
Sample ID{String}=MBE202221213_PA_D1 750C Cracker WAL	
Save:Filename{String}=${X-Y Class} ${2nd Parameter Class} ${iterator}{%04d} ${y}{%04.2g}.txt	
Save:Final Filename{String}=${X-Y Class} ${2nd Parameter Class} .txt	
Save:Final path{Path}=C:\\\\Data\\\\${Project Code}\\\\${User}\\\\${Sample ID}\\\\${Measurement Timestamp}{%Y%m%d}\\\\${X-Y Class}	
Save:Path{Path}=C:\\\\Data\\\\${Project Code}\\\\${User}\\\\${Sample ID}\\\\${Measurement Timestamp}{%Y%m%d}\\\\${X-Y Class}	
Startup path{Path}=C:\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV	
Sub Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Sweep Step{I32}=3	
T Control Measure.__text__{1D Array (String)}=['temperature: T1','temperature: T2','temperature: T3','temperature: T4','temperature: dT/dt']	
Timestamp{Timestamp}=<20:52:35.663 17/05/2023>T	
Toolbar{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Unaved Data{Boolean}=True	
Unsaved Data{Boolean}=False	
User{String}=Craig	
X-Y Class{String}=6221-Lockin-DAQ	
X-Y Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	
d(Offset){Double Float}=0.000000	
d(Rxx::R){Double Float}=0.000000	
d(Rxx::Theta){Double Float}=0.000000	
d(Rxx::X){Double Float}=0.000000	
d(Rxx::Y){Double Float}=4.735058E-22	
d(Rxy::R){Double Float}=1.169375E-8	
d(Rxy::Theta){Double Float}=0.154469	
d(Rxy::X){Double Float}=1.243935E-8	
d(Rxy::Y){Double Float}=1.608792E-8	
iterate result{U16}=5	
iterator{I32}=168	
multi[0]:Control: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values,Adaptive Step Ramp))}=List of Values	
multi[0]:Control: Monitor Update Timeout{Double Float}=0.010000	
multi[0]:Control: Open T Window{Boolean}=False	
multi[0]:Control: Reverse Temperature Sense{Boolean}=False	
multi[0]:Iterator{I32}=0	
multi[0]:Ref: Temperature Window{LVObjVI Refnum (Void)}=	
multi[0]:iterate result{U16}=0	
multi[0]:iterator{I32}=2	
multi[0]:temperature:  rate window{Double Float}=120.000000	
multi[0]:temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[0]:temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
multi[0]:temperature: T1{Double Float}=2.143000	
multi[0]:temperature: T2{Double Float}=2.258700	
multi[0]:temperature: T3{Double Float}=85.888300	
multi[0]:temperature: T4{Double Float}=65.803500	
multi[0]:temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
multi[0]:temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
multi[0]:temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
multi[0]:temperature: current temperature{Double Float}=1.464900	
multi[0]:temperature: current temperature 2{Double Float}=287.100000	
multi[0]:temperature: dT/dt{Double Float}=-0.102580	
multi[0]:temperature: error{Double Float}=0.000200	
multi[0]:temperature: gas{Double Float}=2.200000	
multi[0]:temperature: gas control{Boolean}=False	
multi[0]:temperature: gas control 2{Boolean}=False	
multi[0]:temperature: gass boost{I8}=0	
multi[0]:temperature: gass boost 2{I8}=0	
multi[0]:temperature: gast flow{I16}=0	
multi[0]:temperature: gast flow 2{I16}=7	
multi[0]:temperature: heater{Double Float}=0.400000	
multi[0]:temperature: heater output{Double Float}=0.000000	
multi[0]:temperature: heater output 2{Double Float}=0.000000	
multi[0]:temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
multi[0]:temperature: monitor timeout{Double Float}=0.010000	
multi[0]:temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
multi[0]:temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
multi[0]:temperature: ramp rate{Double Float}=8.000000	
multi[0]:temperature: ramp rate 2{Double Float}=0.000000	
multi[0]:temperature: ramp target{Double Float}=20.000000	
multi[0]:temperature: ramp target 2{Double Float}=0.000000	
multi[0]:temperature: ramping{Boolean}=False	
multi[0]:temperature: setpoint{Double Float}=1.800000	
multi[0]:temperature: setpoint 2{Double Float}=287.100000	
multi[0]:temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
multi[0]:temperature: stability error{Extended Float}=0.040000	
multi[0]:temperature: stability script{String}=	
multi[0]:temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
multi[0]:temperature: temp control mode{U16}=2	
multi[0]:temperature: temp control mode 2{U16}=3	
multi[0]:temperature: temp control mode 2.__text__{String}=Open Loop	
multi[0]:temperature: temp control mode.__text__{String}=Zone	
multi[0]:temperature: temp control sensor{U16}=0	
multi[0]:temperature: temp control sensor 2{U16}=0	
multi[0]:temperature: temp control sensor 2.__text__{String}=Sensor 1	
multi[0]:temperature: temp control sensor.__text__{String}=Sensor A	
multi[0]:temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
multi[0]:temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
multi[0]:temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
multi[0]:temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
multi[0]:temperature: temp loop{U16}=0	
multi[0]:temperature: temp loop 2{U16}=0	
multi[0]:temperature: temp loop 2.__text__{String}=Heater	
multi[0]:temperature: temp loop.__text__{String}=Loop 1	
multi[0]:temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
multi[0]:temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[0]:temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[0]:temperature:error for gas boost{Double Float}=0.000000	
multi[0]:temperature:error for gas boost 2{Double Float}=0.000000	
multi[0]:temperature:heater range{U16}=2	
multi[0]:temperature:heater range 2{U16}=0	
multi[0]:temperature:heater range 2.__text__{String}=Off	
multi[0]:temperature:heater range.__text__{String}=40mW	
multi[0]:temperature:history window{Extended Float}=300.000000	
multi[0]:temperature:is stable?{Boolean}=True	
multi[0]:temperature:monitor{Boolean}=True	
multi[0]:temperature:ramping{Boolean}=False	
multi[0]:temperature:ramping on{Boolean}=False	
multi[0]:temperature:ramping on 2{Boolean}=False	
multi[0]:temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
multi[0]:temperature:stability code{U32}=6618880	
multi[0]:temperature:stability rate{Extended Float}=0.040000	
multi[0]:y{Double Float}=2.200000	
multi[1]:Control: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values,Adaptive Step Ramp))}=Multi-Segment Ramp	
multi[1]:Control: Gate delay{Double Float}=0.000000	
multi[1]:Control: Monitor Update Timeout{Double Float}=0.010000	
multi[1]:Control: Open T Window{Boolean}=False	
multi[1]:Control: Reverse Temperature Sense{Boolean}=False	
multi[1]:Control:Magnet Output{Double Float}=-0.000100	
multi[1]:Iterator{I32}=0	
multi[1]:Magnet: Final Switch Heater{Enum U8 ((False,True,Mixed))}=	
multi[1]:Magnet: Power Supply{Enum U16 ((IPS120,LS625,PS110,Hg iPS,SMS Series,Cryomagnetics 4G,DMG Little CryoFree,DMG Big CryoFree))}=Hg iPS	
multi[1]:Magnet: Rate{Double Float}=0.500000	
multi[1]:Magnet: Units{Enum U16 ((Field,Current))}=Field	
multi[1]:Magnet: VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[1]:Multi-segment_Stage{I32}=0	
multi[1]:Multi-segment_Stage_Changed{Boolean}=False	
multi[1]:Ref: Temperature Window{LVObjVI Refnum (Void)}=	
multi[1]:iterate result{U16}=4	
multi[1]:iterator{I32}=57	
multi[1]:measure point{Boolean}=False	
multi[1]:temperature:  rate window{Double Float}=120.000000	
multi[1]:temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[1]:temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
multi[1]:temperature: T1{Double Float}=1.842400	
multi[1]:temperature: T2{Double Float}=1.465600	
multi[1]:temperature: T3{Double Float}=86.318100	
multi[1]:temperature: T4{Double Float}=66.769200	
multi[1]:temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
multi[1]:temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
multi[1]:temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
multi[1]:temperature: current temperature{Double Float}=1.465600	
multi[1]:temperature: current temperature 2{Double Float}=287.100000	
multi[1]:temperature: dT/dt{Double Float}=-0.001864	
multi[1]:temperature: gas control{Boolean}=False	
multi[1]:temperature: gas control 2{Boolean}=False	
multi[1]:temperature: gass boost{I8}=0	
multi[1]:temperature: gass boost 2{I8}=0	
multi[1]:temperature: gast flow{I16}=0	
multi[1]:temperature: gast flow 2{I16}=7	
multi[1]:temperature: heater output{Double Float}=0.000000	
multi[1]:temperature: heater output 2{Double Float}=0.000000	
multi[1]:temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
multi[1]:temperature: monitor timeout{Double Float}=1.000000	
multi[1]:temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
multi[1]:temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
multi[1]:temperature: ramp rate{Double Float}=8.000000	
multi[1]:temperature: ramp rate 2{Double Float}=0.000000	
multi[1]:temperature: ramp target{Double Float}=20.000000	
multi[1]:temperature: ramp target 2{Double Float}=0.000000	
multi[1]:temperature: ramping{Boolean}=False	
multi[1]:temperature: setpoint{Double Float}=1.800000	
multi[1]:temperature: setpoint 2{Double Float}=287.100000	
multi[1]:temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
multi[1]:temperature: stability error{Extended Float}=0.040000	
multi[1]:temperature: stability script{String}=	
multi[1]:temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
multi[1]:temperature: temp control mode{U16}=2	
multi[1]:temperature: temp control mode 2{U16}=3	
multi[1]:temperature: temp control mode 2.__text__{String}=Open Loop	
multi[1]:temperature: temp control mode.__text__{String}=Zone	
multi[1]:temperature: temp control sensor{U16}=0	
multi[1]:temperature: temp control sensor 2{U16}=0	
multi[1]:temperature: temp control sensor 2.__text__{String}=Sensor 1	
multi[1]:temperature: temp control sensor.__text__{String}=Sensor A	
multi[1]:temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
multi[1]:temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
multi[1]:temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
multi[1]:temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
multi[1]:temperature: temp loop{U16}=0	
multi[1]:temperature: temp loop 2{U16}=0	
multi[1]:temperature: temp loop 2.__text__{String}=Heater	
multi[1]:temperature: temp loop.__text__{String}=Loop 1	
multi[1]:temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
multi[1]:temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[1]:temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[1]:temperature:error for gas boost{Double Float}=0.000000	
multi[1]:temperature:error for gas boost 2{Double Float}=0.000000	
multi[1]:temperature:heater range{U16}=2	
multi[1]:temperature:heater range 2{U16}=0	
multi[1]:temperature:heater range 2.__text__{String}=Off	
multi[1]:temperature:heater range.__text__{String}=40mW	
multi[1]:temperature:history window{Extended Float}=300.000000	
multi[1]:temperature:is stable?{Boolean}=True	
multi[1]:temperature:monitor{Boolean}=True	
multi[1]:temperature:ramping{Boolean}=False	
multi[1]:temperature:ramping on{Boolean}=False	
multi[1]:temperature:ramping on 2{Boolean}=False	
multi[1]:temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
multi[1]:temperature:stability code{U32}=6618880	
multi[1]:temperature:stability rate{Extended Float}=0.040000	
multi[1]:y{Double Float}=0.000000	
parameter: Termination{String}=False	
parameter: delta time{Double Float}=1.000000	
parameter: progress{Double Float}=100.000000	
temperature:  rate window{Double Float}=120.000000	
temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
temperature: T1{Double Float}=2.143000	
temperature: T2{Double Float}=2.258700	
temperature: T3{Double Float}=85.888300	
temperature: T4{Double Float}=65.803500	
temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
temperature: current temperature{Double Float}=1.464900	
temperature: current temperature 2{Double Float}=287.100000	
temperature: dT/dt{Double Float}=-0.102580	
temperature: gas control{Boolean}=False	
temperature: gas control 2{Boolean}=False	
temperature: gass boost{I8}=0	
temperature: gass boost 2{I8}=0	
temperature: gast flow{I16}=0	
temperature: gast flow 2{I16}=7	
temperature: heater output{Double Float}=0.000000	
temperature: heater output 2{Double Float}=0.000000	
temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
temperature: monitor timeout{Double Float}=0.010000	
temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
temperature: ramp rate{Double Float}=8.000000	
temperature: ramp rate 2{Double Float}=0.000000	
temperature: ramp target{Double Float}=20.000000	
temperature: ramp target 2{Double Float}=0.000000	
temperature: ramping{Boolean}=False	
temperature: setpoint{Double Float}=1.800000	
temperature: setpoint 2{Double Float}=287.100000	
temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
temperature: stability error{Extended Float}=0.040000	
temperature: stability script{String}=	
temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
temperature: temp control mode{U16}=2	
temperature: temp control mode 2{U16}=3	
temperature: temp control mode 2.__text__{String}=Open Loop	
temperature: temp control mode.__text__{String}=Zone	
temperature: temp control sensor{U16}=0	
temperature: temp control sensor 2{U16}=0	
temperature: temp control sensor 2.__text__{String}=Sensor 1	
temperature: temp control sensor.__text__{String}=Sensor A	
temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
temperature: temp loop{U16}=0	
temperature: temp loop 2{U16}=0	
temperature: temp loop 2.__text__{String}=Heater	
temperature: temp loop.__text__{String}=Loop 1	
temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
temperature:error for gas boost{Double Float}=0.000000	
temperature:error for gas boost 2{Double Float}=0.000000	
temperature:heater range{U16}=2	
temperature:heater range 2{U16}=0	
temperature:heater range 2.__text__{String}=Off	
temperature:heater range.__text__{String}=40mW	
temperature:history window{Extended Float}=300.000000	
temperature:is stable?{Boolean}=True	
temperature:monitor{Boolean}=True	
temperature:ramping{Boolean}=False	
temperature:ramping on{Boolean}=False	
temperature:ramping on 2{Boolean}=False	
temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
temperature:stability code{U32}=6618880	
temperature:stability rate{Extended Float}=0.040000	
y{Double Float}=2.200000	
