TDI Format 1.5	Offset	Rxx::R	Rxx::Theta	Rxx::X	Rxx::Y	Rxy::R	Rxy::Theta	Rxy::X	Rxy::Y	temperature: T1	temperature: T2	temperature: T3	temperature: T4	temperature: dT/dt	iterator	multi[0]:iterator	multi[0]:y	multi[0]:temperature: setpoint	multi[0]:temperature: T1	multi[0]:temperature: T2	multi[0]:temperature: T3	multi[0]:temperature: T4	multi[0]:temperature: heater	multi[0]:temperature: gas	multi[0]:temperature: dT/dt	multi[0]:temperature: current temperature	multi[0]:temperature: error	multi[1]:iterator	multi[1]:y	multi[1]:Control:Magnet Output
2nd Parameter Class{String}=Multi-Parameter	0E+0	1.305040518E-3	1.5E-1	1.305040518E-3	3.371767975E-6	6.032294009E-7	-8.2104E+0	5.974345194E-7	-8.745522126E-8	4.0052E+1	4.1174E+1	8.58166E+1	6.09242E+1	5.798124149E-2	7.29E+2	1.3E+1	4E+1	4E+1	4.0053E+1	4.1173E+1	8.58166E+1	6.09242E+1	7.5E+0	4E+1	5.938305706E-2	4.0053E+1	-5.3E-2	0E+0	0E+0	0E+0
2nd Parameter Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	0E+0	1.306557969E-3	1.5E-1	1.306557969E-3	3.371767975E-6	7.079657745E-6	-6.6E-1	7.079657745E-6	-8.324052543E-8	4.0037E+1	4.123E+1	8.56375E+1	6.09242E+1	4.588691518E-2	7.3E+2	1.3E+1	4E+1	1.8E+0	4.0052E+1	4.1174E+1	8.58166E+1	6.09242E+1	7.5E+0	4E+1	5.798124149E-2	1.4649E+0	-5.3E-2	1E+0	5E-1	5E-1
Analysis Class{String}=Basic Plot	0E+0	1.310097746E-3	1.5E-1	1.310097746E-3	3.371767975E-6	1.353870201E-5	-2.676E-1	1.353870201E-5	-6.427430935E-8	4.0029E+1	4.1278E+1	8.58883E+1	6.09242E+1	3.958750144E-2	7.31E+2	1.3E+1	4E+1	1.8E+0	4.0037E+1	4.123E+1	8.56375E+1	6.09242E+1	7.5E+0	4E+1	4.588691518E-2	1.4649E+0	-5.3E-2	2E+0	1E+0	9.999E-1
Analysis Class Path{Path}=C\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV\\\\plugins\\\\Plotting\\\\Plotting_Base_class\\\\Plotting_Base.lvclass	0E+0	1.315661262E-3	1.5E-1	1.315661262E-3	3.371767975E-6	2.004463877E-5	-1.344E-1	2.004463877E-5	-4.899599455E-8	4.0025E+1	4.1326E+1	8.58524E+1	6.09242E+1	4.022453353E-2	7.32E+2	1.3E+1	4E+1	1.8E+0	4.0029E+1	4.1278E+1	8.58883E+1	6.09242E+1	7.5E+0	4E+1	3.958750144E-2	1.4649E+0	-5.3E-2	3E+0	1.5E+0	1.4998E+0
Analysis.# pre-routines{I32}=5	0E+0	1.315661262E-3	1.5E-1	1.315661262E-3	3.371767975E-6	2.003352305E-5	-1.284E-1	2.003352305E-5	-4.63618238E-8	4.0024E+1	4.1327E+1	8.58524E+1	6.09242E+1	3.731762245E-2	7.33E+2	1.3E+1	4E+1	1.8E+0	4.0025E+1	4.1326E+1	8.58524E+1	6.09242E+1	7.5E+0	4E+1	4.022453353E-2	1.4649E+0	-5.3E-2	4E+0	1.5E+0	1.5E+0
Analysis:Pre[0]:T Control Measure{1D Array (I32)}=[1,2,3,4,7]	0E+0	1.313469231E-3	1.5E-1	1.313469231E-3	3.371767975E-6	1.741728453E-5	-1.68E-1	1.741728453E-5	-5.268383926E-8	4.0033E+1	4.1344E+1	8.55659E+1	6.09242E+1	3.333971649E-2	7.34E+2	1.3E+1	4E+1	1.8E+0	4.0024E+1	4.1327E+1	8.58524E+1	6.09242E+1	7.5E+0	4E+1	3.731762245E-2	1.4649E+0	-5.3E-2	5E+0	1.3E+0	1.3001E+0
Autosave Tabs{Enum U32 ((XY Measurement Save,Parameter Plot Save 2))}=Parameter Plot Save 2	0E+0	1.311615197E-3	1.5E-1	1.311615197E-3	3.371767975E-6	1.483261125E-5	-2.448E-1	1.483261125E-5	-6.480110391E-8	4.0038E+1	4.1358E+1	8.56375E+1	6.09242E+1	2.978177741E-2	7.35E+2	1.3E+1	4E+1	1.8E+0	4.0033E+1	4.1344E+1	8.55659E+1	6.09242E+1	7.5E+0	4E+1	3.333971649E-2	1.4649E+0	-5.3E-2	6E+0	1.1E+0	1.1001E+0
Control:Magnet Output{Double Float}=-0.007000	0E+0	1.309761163E-3	1.5E-1	1.309761163E-3	3.371767975E-6	1.222530208E-5	-2.736E-1	1.222530208E-5	-6.005961353E-8	4.0155E+1	4.13E+1	8.59241E+1	6.09242E+1	-7.637035102E-2	7.36E+2	1.3E+1	4E+1	1.8E+0	4.0038E+1	4.1358E+1	8.56375E+1	6.09242E+1	7.5E+0	4E+1	2.978177741E-2	1.4649E+0	-5.3E-2	7E+0	9E-1	9.001E-1
Control:Magnet Rate{Double Float}=0.500000	0E+0	1.308580295E-3	1.5E-1	1.308580295E-3	3.371767975E-6	9.646404449E-6	-3.828E-1	9.646404449E-6	-6.585474958E-8	4.0016E+1	4.1448E+1	8.58883E+1	6.09242E+1	1.72405377E-1	7.37E+2	1.3E+1	4E+1	1.8E+0	4.0155E+1	4.13E+1	8.59241E+1	6.09242E+1	7.5E+0	4E+1	-7.637035102E-2	1.4649E+0	-5.3E-2	8E+0	7E-1	7.001E-1
Display Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	0E+0	1.307737423E-3	1.5E-1	1.307737423E-3	3.371767975E-6	7.073333382E-6	-4.656E-1	7.073333382E-6	-5.847906016E-8	3.9609E+1	4.1447E+1	8.58524E+1	6.09242E+1	8.780152351E-2	7.38E+2	1.3E+1	4E+1	1.8E+0	4.0016E+1	4.1448E+1	8.58883E+1	6.09242E+1	7.5E+0	4E+1	1.72405377E-1	1.4649E+0	-5.3E-2	9E+0	5E-1	5.001E-1
Elapsed Time{Double Float}=12790.950867	0E+0	1.306894552E-3	1.5E-1	1.306894552E-3	3.371767975E-6	4.487079016E-6	-1.1124E+0	4.487079016E-6	-8.903583119E-8	3.9655E+1	4.144E+1	8.58166E+1	6.09242E+1	-1.749652252E-2	7.39E+2	1.3E+1	4E+1	1.8E+0	3.9609E+1	4.1447E+1	8.58524E+1	6.09242E+1	7.5E+0	4E+1	8.780152351E-2	1.4649E+0	-5.3E-2	1E+1	3E-1	3.001E-1
File:Autodel{Boolean}=True	0E+0	1.306726261E-3	1.5E-1	1.306726261E-3	3.371767975E-6	1.885553972E-6	-2.6916E+0	1.883449622E-6	-9.008944857E-8	3.9857E+1	4.1501E+1	8.56375E+1	6.09242E+1	8.52426067E-2	7.4E+2	1.3E+1	4E+1	1.8E+0	3.9655E+1	4.144E+1	8.58166E+1	6.09242E+1	7.5E+0	4E+1	-1.749652252E-2	1.4649E+0	-5.3E-2	1.1E+1	1E-1	1.001E-1
File:Autosave{Boolean}=False	0E+0	1.306726261E-3	1.5E-1	1.306726261E-3	3.371767975E-6	1.879235266E-6	-2.7864E+0	1.877128088E-6	-9.325049873E-8	3.9882E+1	4.1512E+1	8.56017E+1	6.09242E+1	9.704770148E-2	7.41E+2	1.3E+1	4E+1	1.8E+0	3.9857E+1	4.1501E+1	8.56375E+1	6.09242E+1	7.5E+0	4E+1	8.52426067E-2	1.4649E+0	-5.3E-2	1.2E+1	1E-1	1E-1
File:Export Config{Boolean}=True	0E+0	1.306894552E-3	1.5E-1	1.306894552E-3	3.371767975E-6	1.740676278E-6	-3.1176E+0	1.738566271E-6	-9.588472605E-8	3.9923E+1	4.1539E+1	8.56375E+1	6.09242E+1	1.231752411E-1	7.42E+2	1.3E+1	4E+1	1.8E+0	3.9882E+1	4.1512E+1	8.56017E+1	6.09242E+1	7.5E+0	4E+1	9.704770148E-2	1.4649E+0	-5.3E-2	1.3E+1	9E-2	9E-2
File:Final Autosave{Boolean}=True	0E+0	1.306894552E-3	1.5E-1	1.306894552E-3	3.371767975E-6	1.626351254E-6	-2.8212E+0	1.624246904E-6	-8.113312095E-8	3.9958E+1	4.156E+1	8.57092E+1	6.09242E+1	1.34063825E-1	7.43E+2	1.3E+1	4E+1	1.8E+0	3.9923E+1	4.1539E+1	8.56375E+1	6.09242E+1	7.5E+0	4E+1	1.231752411E-1	1.4649E+0	-5.3E-2	1.4E+1	8E-2	8.01E-2
Filter:Enable{Enum U16 ((None,Analog,Digital,Analog&Digitial))}=None	0E+0	1.307062843E-3	1.5E-1	1.307062843E-3	3.371767975E-6	1.508869705E-6	-3.0252E+0	1.506230782E-6	-8.113312095E-8	3.9997E+1	4.158E+1	8.56375E+1	6.09242E+1	1.371471882E-1	7.44E+2	1.3E+1	4E+1	1.8E+0	3.9958E+1	4.156E+1	8.57092E+1	6.09242E+1	7.5E+0	4E+1	1.34063825E-1	1.4649E+0	-5.3E-2	1.5E+1	7E-2	7.01E-2
Filter:Points{I32}=1	0E+0	1.307062843E-3	1.5E-1	1.307062843E-3	3.371767975E-6	1.370309868E-6	-3.5256E+0	1.367148535E-6	-8.587469618E-8	4.0017E+1	4.1608E+1	8.59599E+1	6.09242E+1	1.478310972E-1	7.45E+2	1.3E+1	4E+1	1.8E+0	3.9997E+1	4.158E+1	8.56375E+1	6.09242E+1	7.5E+0	4E+1	1.371471882E-1	1.4649E+0	-5.3E-2	1.6E+1	6E-2	6.01E-2
Filter:Type{U16}=1	0E+0	1.307232549E-3	1.5E-1	1.307232549E-3	3.371767975E-6	1.248078824E-6	-4.3728E+0	1.243864185E-6	-9.641157717E-8	4.0034E+1	4.1627E+1	8.59599E+1	6.09242E+1	1.426941603E-1	7.46E+2	1.3E+1	4E+1	1.8E+0	4.0017E+1	4.1608E+1	8.59599E+1	6.09242E+1	7.5E+0	4E+1	1.478310972E-1	1.4649E+0	-5.3E-2	1.7E+1	5E-2	5E-2
Filter:Type.__text__{String}=Repeat	0E+0	1.307232549E-3	1.5E-1	1.307232549E-3	3.371767975E-6	1.231747203E-6	-4.0332E+0	1.229112523E-6	-8.850889521E-8	4.0039E+1	4.1637E+1	8.59599E+1	6.09242E+1	1.434859633E-1	7.47E+2	1.3E+1	4E+1	1.8E+0	4.0034E+1	4.1627E+1	8.59599E+1	6.09242E+1	7.5E+0	4E+1	1.426941603E-1	1.4649E+0	-5.3E-2	1.8E+1	5E-2	5E-2
Filter:Window{Double Float}=1.000000	0E+0	1.30740084E-3	1.5E-1	1.30740084E-3	3.371767975E-6	1.16799983E-6	-3.8832E+0	1.165365716E-6	-8.11332058E-8	4.0051E+1	4.1654E+1	8.59241E+1	6.09242E+1	1.345063448E-1	7.48E+2	1.3E+1	4E+1	1.8E+0	4.0039E+1	4.1637E+1	8.59599E+1	6.09242E+1	7.5E+0	4E+1	1.434859633E-1	1.4649E+0	-5.3E-2	1.9E+1	4.5E-2	4.49E-2
Iterator{I32}=0	0E+0	1.30740084E-3	1.5E-1	1.30740084E-3	3.371767975E-6	1.097403703E-6	-5.3184E+0	1.092135475E-6	-1.032604437E-7	4.0066E+1	4.1669E+1	8.58883E+1	6.09242E+1	1.236833334E-1	7.49E+2	1.3E+1	4E+1	1.8E+0	4.0051E+1	4.1654E+1	8.59241E+1	6.09242E+1	7.5E+0	4E+1	1.345063448E-1	1.4649E+0	-5.3E-2	2E+1	4E-2	3.98E-2
Magnet: Control Mode{Boolean}=False	0E+0	1.307569132E-3	1.5E-1	1.307569132E-3	3.371767975E-6	1.041032019E-6	-5.4792E+0	1.036291009E-6	-1.006261599E-7	4.007E+1	4.1688E+1	8.58883E+1	6.09242E+1	1.19410418E-1	7.5E+2	1.3E+1	4E+1	1.8E+0	4.0066E+1	4.1669E+1	8.58883E+1	6.09242E+1	7.5E+0	4E+1	1.236833334E-1	1.4649E+0	-5.3E-2	2.1E+1	3.5E-2	3.49E-2
Magnet: Final Switch Heater{Enum U8 ((False,True,Mixed))}=	0E+0	1.307569132E-3	1.5E-1	1.307569132E-3	3.371767975E-6	9.604260885E-7	-4.56E+0	9.56738668E-7	-7.744524796E-8	4.0076E+1	4.17E+1	8.58524E+1	6.09242E+1	1.045876518E-1	7.51E+2	1.3E+1	4E+1	1.8E+0	4.007E+1	4.1688E+1	8.58883E+1	6.09242E+1	7.5E+0	4E+1	1.19410418E-1	1.4649E+0	-5.3E-2	2.2E+1	3E-2	2.99E-2
Magnet: Power Supply{Enum U16 ((IPS120,LS625,PS110,Hg iPS,SMS Series,Cryomagnetics 4G,DMG Little CryoFree,DMG Big CryoFree))}=Hg iPS	0E+0	1.307569132E-3	1.5E-1	1.307569132E-3	3.371767975E-6	9.114306596E-7	-5.9916E+0	9.056357781E-7	-9.641157717E-8	4.0081E+1	4.1713E+1	8.58524E+1	6.09242E+1	9.534128755E-2	7.52E+2	1.3E+1	4E+1	1.8E+0	4.0076E+1	4.17E+1	8.58524E+1	6.09242E+1	7.5E+0	4E+1	1.045876518E-1	1.4649E+0	-5.3E-2	2.3E+1	2.5E-2	2.49E-2
Magnet: Rate{Double Float}=0.500000	0E+0	1.307737423E-3	1.5E-1	1.307737423E-3	3.371767975E-6	8.545326054E-7	-5.9784E+0	8.508446192E-7	-9.061632798E-8	4.0089E+1	4.1722E+1	8.58524E+1	6.09242E+1	8.397766948E-2	7.53E+2	1.3E+1	4E+1	1.8E+0	4.0081E+1	4.1713E+1	8.58524E+1	6.09242E+1	7.5E+0	4E+1	9.534128755E-2	1.4649E+0	-5.3E-2	2.4E+1	2E-2	2E-2
Magnet: Setpoint{Double Float}=0.000000	0E+0	1.307737423E-3	1.5E-1	1.307737423E-3	3.371767975E-6	7.791946205E-7	-5.97E+0	7.744536109E-7	-8.271364602E-8	4.0089E+1	4.1734E+1	8.58524E+1	6.09242E+1	7.983419299E-2	7.54E+2	1.3E+1	4E+1	1.8E+0	4.0089E+1	4.1722E+1	8.58524E+1	6.09242E+1	7.5E+0	4E+1	8.397766948E-2	1.4649E+0	-5.3E-2	2.5E+1	1.5E-2	1.49E-2
Magnet: Units{Enum U16 ((Field,Current))}=Field	0E+0	1.307737423E-3	1.5E-1	1.307737423E-3	3.371767975E-6	7.080721234E-7	-7.7184E+0	7.017503059E-7	-9.641154888E-8	4.0086E+1	4.1743E+1	8.58166E+1	6.09242E+1	7.132910937E-2	7.55E+2	1.3E+1	4E+1	1.8E+0	4.0089E+1	4.1734E+1	8.58524E+1	6.09242E+1	7.5E+0	4E+1	7.983419299E-2	1.4649E+0	-5.3E-2	2.6E+1	1E-2	9.9E-3
Magnet: VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	0E+0	1.307737423E-3	1.5E-1	1.307737423E-3	3.371767975E-6	6.522251126E-7	-9.0096E+0	6.437958341E-7	-1.032604437E-7	4.0084E+1	4.1754E+1	8.58524E+1	6.09242E+1	6.684663892E-2	7.56E+2	1.3E+1	4E+1	1.8E+0	4.0086E+1	4.1743E+1	8.58166E+1	6.09242E+1	7.5E+0	4E+1	7.132910937E-2	1.4649E+0	-5.3E-2	2.7E+1	5E-3	5E-3
Main Screen Path{Path}=C:\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV\\\\1Code.vi	0E+0	1.307905715E-3	1.5E-1	1.307905715E-3	3.371767975E-6	5.83209228E-7	-8.3868E+0	5.768876934E-7	-8.64015473E-8	4.0078E+1	4.176E+1	8.58524E+1	6.09242E+1	5.925079063E-2	7.57E+2	1.3E+1	4E+1	1.8E+0	4.0084E+1	4.1754E+1	8.58524E+1	6.09242E+1	7.5E+0	4E+1	6.684663892E-2	1.4649E+0	-5.3E-2	2.8E+1	0E+0	-2E-4
Measurement Timestamp{Timestamp}=<01:40:57.863 18/05/2023>T	0E+0	1.307905715E-3	1.5E-1	1.307905715E-3	3.371767975E-6	5.215698814E-7	-1.06668E+1	5.115600778E-7	-9.851884023E-8	4.0075E+1	4.1765E+1	8.58524E+1	6.09242E+1	5.07286936E-2	7.58E+2	1.3E+1	4E+1	1.8E+0	4.0078E+1	4.176E+1	8.58524E+1	6.09242E+1	7.5E+0	4E+1	5.925079063E-2	1.4649E+0	-5.3E-2	2.9E+1	-5E-3	-5.1E-3
Measurement Title{String}=	0E+0	1.307905715E-3	1.5E-1	1.307905715E-3	3.371767975E-6	4.583497268E-7	-1.01568E+1	4.515006906E-7	-8.218676662E-8	4.0073E+1	4.1773E+1	8.5745E+1	6.09242E+1	4.684615135E-2	7.59E+2	1.3E+1	4E+1	1.8E+0	4.0075E+1	4.1765E+1	8.58524E+1	6.09242E+1	7.5E+0	4E+1	5.07286936E-2	1.4649E+0	-5.3E-2	3E+1	-1E-2	-1.01E-2
Measurment Select{U16}=4	0E+0	1.307905715E-3	1.5E-1	1.307905715E-3	3.371767975E-6	4.019783257E-7	-1.20144E+1	3.930218284E-7	-8.534787334E-8	4.0069E+1	4.1774E+1	8.56017E+1	6.09242E+1	3.529654071E-2	7.6E+2	1.3E+1	4E+1	1.8E+0	4.0073E+1	4.1773E+1	8.5745E+1	6.09242E+1	7.5E+0	4E+1	4.684615135E-2	1.4649E+0	-5.3E-2	3.1E+1	-1.5E-2	-1.51E-2
Measurment Select.__text__{String}=6221-Lockin-DAQ	0E+0	1.307905715E-3	1.5E-1	1.307905715E-3	3.371767975E-6	3.298008253E-7	-1.6704E+1	3.161027527E-7	-9.693837172E-8	4.0072E+1	4.1781E+1	8.56375E+1	6.09242E+1	3.405437246E-2	7.61E+2	1.3E+1	4E+1	1.8E+0	4.0069E+1	4.1774E+1	8.56017E+1	6.09242E+1	7.5E+0	4E+1	3.529654071E-2	1.4649E+0	-5.3E-2	3.2E+1	-2E-2	-2E-2
Notes{String}=I+1A I-1E\\nrxx+1B Rxx-1C\\nRxy+1D Rxy-4A	0E+0	1.307905715E-3	1.5E-1	1.307905715E-3	3.371767975E-6	2.63418772E-7	-2.0328E+1	2.47087151E-7	-9.325047044E-8	4.0065E+1	4.1786E+1	8.56734E+1	6.09242E+1	3.175126761E-2	7.62E+2	1.3E+1	4E+1	1.8E+0	4.0072E+1	4.1781E+1	8.56375E+1	6.09242E+1	7.5E+0	4E+1	3.405437246E-2	1.4649E+0	-5.3E-2	3.3E+1	-2.5E-2	-2.51E-2
Offset{Double Float}=0.000000	0E+0	1.307905715E-3	1.5E-1	1.307905715E-3	3.371767975E-6	2.123158821E-7	-2.53764E+1	1.912426858E-7	-9.272364761E-8	4.0063E+1	4.1785E+1	8.57092E+1	6.09242E+1	2.532603592E-2	7.63E+2	1.3E+1	4E+1	1.8E+0	4.0065E+1	4.1786E+1	8.56734E+1	6.09242E+1	7.5E+0	4E+1	3.175126761E-2	1.4649E+0	-5.3E-2	3.4E+1	-3E-2	-3.02E-2
Option: 2182 Autozero{Boolean}=True	0E+0	1.307939656E-3	1.5E-1	1.307939656E-3	3.371767975E-6	1.580513764E-7	-3.5406E+1	1.290753001E-7	-9.430420097E-8	4.0069E+1	4.1788E+1	8.56734E+1	6.09242E+1	2.199007012E-2	7.64E+2	1.3E+1	4E+1	1.8E+0	4.0063E+1	4.1785E+1	8.57092E+1	6.09242E+1	7.5E+0	4E+1	2.532603592E-2	1.4649E+0	-5.3E-2	3.5E+1	-3.5E-2	-3.51E-2
Option: 2182 Front Autozero{Boolean}=True	0E+0	1.30807542E-3	1.5E-1	1.30807542E-3	3.371767975E-6	1.164313541E-7	-5.50776E+1	6.585483443E-8	-9.693834344E-8	4.0065E+1	4.1793E+1	8.60315E+1	6.09242E+1	2.252699062E-2	7.65E+2	1.3E+1	4E+1	1.8E+0	4.0069E+1	4.1788E+1	8.56734E+1	6.09242E+1	7.5E+0	4E+1	2.199007012E-2	1.4649E+0	-5.3E-2	3.6E+1	-4E-2	-4.01E-2
Option: 2182 Hold{Boolean}=False	0E+0	1.30807542E-3	1.5E-1	1.30807542E-3	3.371767975E-6	8.745530611E-8	-9.69108E+1	-1.211728162E-8	-8.903577462E-8	4.006E+1	4.1796E+1	8.59957E+1	6.09242E+1	2.158832364E-2	7.66E+2	1.3E+1	4E+1	1.8E+0	4.0065E+1	4.1793E+1	8.60315E+1	6.09242E+1	7.5E+0	4E+1	2.252699062E-2	1.4649E+0	-5.3E-2	3.7E+1	-4.5E-2	-4.5E-2
Option: 2182 Hold Count{I32}=10	0E+0	1.30807542E-3	1.5E-1	1.30807542E-3	3.371767975E-6	1.174849715E-7	-1.291344E+2	-7.639160228E-8	-9.325052701E-8	4.0057E+1	4.1797E+1	8.59957E+1	6.09242E+1	1.766118035E-2	7.67E+2	1.3E+1	4E+1	1.8E+0	4.006E+1	4.1796E+1	8.59957E+1	6.09242E+1	7.5E+0	4E+1	2.158832364E-2	1.4649E+0	-5.3E-2	3.8E+1	-5E-2	-5.02E-2
Option: 2182 Hold Window{Double Float}=1.000000	0E+0	1.308109079E-3	1.5E-1	1.308109079E-3	3.371767975E-6	1.159045029E-7	-1.305012E+2	-7.691839683E-8	-9.061629969E-8	4.0057E+1	4.1798E+1	8.59957E+1	6.09242E+1	1.740164123E-2	7.68E+2	1.3E+1	4E+1	1.8E+0	4.0057E+1	4.1797E+1	8.59957E+1	6.09242E+1	7.5E+0	4E+1	1.766118035E-2	1.4649E+0	-5.3E-2	3.9E+1	-5E-2	-5E-2
Option: 2182 Line Sync{Boolean}=False	0E+0	1.308243712E-3	1.5E-1	1.308243712E-3	3.371767975E-6	2.244331468E-7	-1.569396E+2	-2.091551148E-7	-8.956259745E-8	4.0054E+1	4.1803E+1	8.59599E+1	6.09242E+1	2.008714341E-2	7.69E+2	1.3E+1	4E+1	1.8E+0	4.0057E+1	4.1798E+1	8.59957E+1	6.09242E+1	7.5E+0	4E+1	1.740164123E-2	1.4649E+0	-5.3E-2	4E+1	-6E-2	-6E-2
Option: 2182 Reference Reading{Double Float}=0.000000	0E+0	1.308243712E-3	1.5E-1	1.308243712E-3	3.371767975E-6	3.440258338E-7	-1.641924E+2	-3.334890943E-7	-9.483102381E-8	4.0049E+1	4.1802E+1	8.59241E+1	6.09242E+1	1.442255918E-2	7.7E+2	1.3E+1	4E+1	1.8E+0	4.0054E+1	4.1803E+1	8.59599E+1	6.09242E+1	7.5E+0	4E+1	2.008714341E-2	1.4649E+0	-5.3E-2	4.1E+1	-7E-2	-7E-2
Option: 2182 Relative Mode{Boolean}=False	0E+0	1.308243712E-3	1.5E-1	1.308243712E-3	3.371767975E-6	4.746816307E-7	-1.695216E+2	-4.699403383E-7	-8.798210066E-8	4.0046E+1	4.1806E+1	8.58883E+1	6.09242E+1	1.506344695E-2	7.71E+2	1.3E+1	4E+1	1.8E+0	4.0049E+1	4.1802E+1	8.59241E+1	6.09242E+1	7.5E+0	4E+1	1.442255918E-2	1.4649E+0	-5.3E-2	4.2E+1	-8E-2	-7.99E-2
Option: 2182 Trigger Delay{Cluster (Boolean,Double Float)}={'Auto':True,'Time(s)':0.000000}	0E+0	1.308243712E-3	1.5E-1	1.308243712E-3	3.371767975E-6	5.995416976E-7	-1.711908E+2	-5.953267755E-7	-9.325047044E-8	4.0045E+1	4.1805E+1	8.59241E+1	6.09242E+1	9.703860618E-3	7.72E+2	1.3E+1	4E+1	1.8E+0	4.0046E+1	4.1806E+1	8.58883E+1	6.09242E+1	7.5E+0	4E+1	1.506344695E-2	1.4649E+0	-5.3E-2	4.3E+1	-9E-2	-8.99E-2
Option: 2182 Trigger Source{Enum U16 ((Immediate,Timer,Manual,Bus,Trigger link))}=Bus	0E+0	1.308243712E-3	1.5E-1	1.308243712E-3	3.371767975E-6	7.249306804E-7	-1.71594E+2	-7.19662452E-7	-1.069482602E-7	4.0045E+1	4.1809E+1	8.58883E+1	6.09242E+1	1.300007943E-2	7.73E+2	1.3E+1	4E+1	1.8E+0	4.0045E+1	4.1805E+1	8.59241E+1	6.09242E+1	7.5E+0	4E+1	9.703860618E-3	1.4649E+0	-5.3E-2	4.4E+1	-1E-1	-1E-1
Option: 2182 Trigger Timer{Double Float}=0.000000	0E+0	1.308243712E-3	1.5E-1	1.308243712E-3	3.371767975E-6	7.386290358E-7	-1.726032E+2	-7.354677028E-7	-9.641154888E-8	4.0041E+1	4.1812E+1	8.58883E+1	6.09242E+1	1.618024707E-2	7.74E+2	1.3E+1	4E+1	1.8E+0	4.0045E+1	4.1809E+1	8.58883E+1	6.09242E+1	7.5E+0	4E+1	1.300007943E-2	1.4649E+0	-5.3E-2	4.5E+1	-1E-1	-1E-1
Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	0E+0	1.308580295E-3	1.5E-1	1.308580295E-3	3.371767975E-6	3.299063256E-6	-1.784532E+2	-3.300118259E-6	-9.061629969E-8	4.0041E+1	4.1815E+1	8.58524E+1	6.09242E+1	1.129005291E-2	7.75E+2	1.3E+1	4E+1	1.8E+0	4.0041E+1	4.1812E+1	8.58883E+1	6.09242E+1	7.5E+0	4E+1	1.618024707E-2	1.4649E+0	-5.3E-2	4.6E+1	-3E-1	-2.999E-1
Option: 560 Enabled{Boolean}=False	0E+0	1.309423166E-3	1.5E-1	1.309423166E-3	3.371767975E-6	5.875313475E-6	-1.790136E+2	-5.877943913E-6	-1.027335926E-7	4.0032E+1	4.1819E+1	8.55659E+1	6.09242E+1	9.776269086E-3	7.76E+2	1.3E+1	4E+1	1.8E+0	4.0041E+1	4.1815E+1	8.58524E+1	6.09242E+1	7.5E+0	4E+1	1.129005291E-2	1.4649E+0	-5.3E-2	4.7E+1	-5E-1	-4.998E-1
Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	0E+0	1.310604034E-3	1.5E-1	1.310604034E-3	3.371767975E-6	8.455229336E-6	-1.793316E+2	-8.457859773E-6	-9.957259904E-8	4.0029E+1	4.1824E+1	8.56734E+1	6.09242E+1	7.855493575E-3	7.77E+2	1.3E+1	4E+1	1.8E+0	4.0032E+1	4.1819E+1	8.55659E+1	6.09242E+1	7.5E+0	4E+1	9.776269086E-3	1.4649E+0	-5.3E-2	4.8E+1	-7E-1	-6.999E-1
Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	0E+0	1.31195178E-3	1.5E-1	1.31195178E-3	3.371767975E-6	1.103623414E-5	-1.793412E+2	-1.103886741E-5	-1.280216544E-7	4.0026E+1	4.183E+1	8.59599E+1	6.09242E+1	8.63133464E-3	7.78E+2	1.3E+1	4E+1	1.8E+0	4.0029E+1	4.1824E+1	8.56734E+1	6.09242E+1	7.5E+0	4E+1	7.855493575E-3	1.4649E+0	-5.3E-2	4.9E+1	-9E-1	-8.998E-1
Option: 6221 Adjust Mode{Enum U16 ((Offset,Frequency,Amplitude))}=Offset	0E+0	1.313638936E-3	1.5E-1	1.313638936E-3	3.371767975E-6	1.361140956E-5	-1.795104E+2	-1.361404E-5	-1.180118226E-7	4.0025E+1	4.1836E+1	8.58883E+1	6.09242E+1	9.12334118E-3	7.79E+2	1.3E+1	4E+1	1.8E+0	4.0026E+1	4.183E+1	8.59599E+1	6.09242E+1	7.5E+0	4E+1	8.63133464E-3	1.4649E+0	-5.3E-2	5E+1	-1.1E+0	-1.0998E+0
Option: 6221 Amplitude{Double Float}=1.000000E-6	0E+0	1.315661262E-3	1.5E-1	1.315661262E-3	3.371767975E-6	1.620394586E-5	-1.795632E+2	-1.620660458E-5	-1.248606891E-7	4.0026E+1	4.1843E+1	8.58524E+1	6.09242E+1	1.090034563E-2	7.8E+2	1.3E+1	4E+1	1.8E+0	4.0025E+1	4.1836E+1	8.58883E+1	6.09242E+1	7.5E+0	4E+1	9.12334118E-3	1.4649E+0	-5.3E-2	5.1E+1	-1.3E+0	-1.2999E+0
Option: 6221 Compliance{Double Float}=10.000000	0E+0	1.318021584E-3	1.5E-1	1.318021584E-3	3.371767975E-6	1.879438913E-5	-1.79538E+2	-1.879704785E-5	-1.52783148E-7	4.0034E+1	4.1848E+1	8.58166E+1	6.09242E+1	9.32162255E-3	7.81E+2	1.3E+1	4E+1	1.8E+0	4.0026E+1	4.1843E+1	8.58524E+1	6.09242E+1	7.5E+0	4E+1	1.090034563E-2	1.4649E+0	-5.3E-2	5.2E+1	-1.5E+0	-1.4998E+0
Option: 6221 Duty Cycle{Double Float}=50.000000	0E+0	1.318021584E-3	1.5E-1	1.318021584E-3	3.371767975E-6	1.879492653E-5	-1.7955E+2	-1.879758525E-5	-1.49095077E-7	4.0034E+1	4.1849E+1	8.58166E+1	6.09242E+1	9.760603309E-3	7.82E+2	1.3E+1	4E+1	1.8E+0	4.0034E+1	4.1848E+1	8.58166E+1	6.09242E+1	7.5E+0	4E+1	9.32162255E-3	1.4649E+0	-5.3E-2	5.3E+1	-1.5E+0	-1.5E+0
Option: 6221 External Trigger{Boolean}=False	0E+0	1.312964357E-3	1.5E-1	1.312964357E-3	3.371767975E-6	1.231222813E-5	-1.793772E+2	-1.231486139E-5	-1.359243364E-7	4.0037E+1	4.1906E+1	8.59957E+1	6.09242E+1	1.104953066E-1	7.83E+2	1.3E+1	4E+1	1.8E+0	4.0034E+1	4.1849E+1	8.58166E+1	6.09242E+1	7.5E+0	4E+1	9.760603309E-3	1.4649E+0	-5.3E-2	5.4E+1	-1E+0	-1.0001E+0
Option: 6221 External Trigger Ignore Multiple{Boolean}=False	0E+0	1.309423166E-3	1.5E-1	1.309423166E-3	3.371767975E-6	5.853712777E-6	-1.789848E+2	-5.856346043E-6	-1.048409123E-7	3.9657E+1	4.1814E+1	8.58524E+1	6.09242E+1	-7.610604912E-2	7.84E+2	1.3E+1	4E+1	1.8E+0	4.0037E+1	4.1906E+1	8.59957E+1	6.09242E+1	7.5E+0	4E+1	1.104953066E-1	1.4649E+0	-5.3E-2	5.5E+1	-5E-1	-5.001E-1
Option: 6221 Frequency{Double Float}=119.770000	
Option: 6221 Function{U16}=1	
Option: 6221 Function.__text__{String}=Sine	
Option: 6221 Idle Level{Double Float}=0.000000	
Option: 6221 Input trigger Line{U8}=5	
Option: 6221 Offset{Double Float}=0.000000	
Option: 6221 Output Trigger Line{U8}=4	
Option: 6221 Pass Through{Boolean}=True	
Option: 6221 Phase Marker{Boolean}=True	
Option: 6221 Phase Marker Phase{Double Float}=0.000000	
Option: 6221 Range Level{Double Float}=2.000000E-12	
Option: 6221 Ranging{U16}=1	
Option: 6221 Ranging.__text__{String}=Best	
Option: 6221 Update Clock{Double Float}=0.000000	
Option: 6221 VISA{Visa Refnum (Void)}=GPIB0::13::INSTR	
Option: Confirm Config{Boolean}=False	
Option: Control Panel Ref{LVObjVI Refnum (Void)}=	
Option: DAQ Global Channel{Boolean}=False	
Option: DAQ Input Rate{Double Float}=10000.000000	
Option: DAQ Input Samples{I32}=200	
Option: DAQ Measurement Channels{1D Array (Cluster (UserDefinedRefnumTag Refnum (Void),\tkDAQmxPhysChanTagType Tag,\tkDAQmxScaleTagType Tag,Boolean,Double Float,String))}=[]	
Option: Differential{I32}=10106	
Option: Differential.__text__{String}=Differential	
Option: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values))}=Function Generator	
Option: Lockin Standoff Time{Double Float}=0.000000	
Option: Paranoid Save Data{Boolean}=True	
Option: Plot Autoback Path{Path}=C:\\\\TEMP\\\\XY Multiparam\\\\Backup.txt	
Option: SR830  Ref Phase{Double Float}=0.000000	
Option: SR830  Synch Filter{Boolean}=False	
Option: SR830  Time Constant{I16}=8	
Option: SR830  Time Constant.__text__{String}=100 ms	
Option: SR830 2x Line Filter{Boolean}=True	
Option: SR830 Adjust Gains{Boolean}=False	
Option: SR830 Auto Gain Lower.__text__{String}=2 nV/fA	
Option: SR830 Auto Gain Upper.__text__{String}=1 V/uA	
Option: SR830 Auto Offset 1{Boolean}=False	
Option: SR830 Auto Offset 2{Boolean}=False	
Option: SR830 Autophase{Boolean}=False	
Option: SR830 DC Coupling?{Boolean}=False	
Option: SR830 Display 1{U16}=0	
Option: SR830 Display 1.__text__{String}=X	
Option: SR830 Display 2{U16}=0	
Option: SR830 Display 2.__text__{String}=Y	
Option: SR830 Dynamic Reserve{I16}=1	
Option: SR830 Dynamic Reserve.__text__{String}=Normal	
Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Option: SR830 Filter Slope{I32}=1	
Option: SR830 Filter Slope.__text__{String}=12 dB/oct	
Option: SR830 Gain{I32}=-1	
Option: SR830 Gain.__text__{String}=Auto Gain	
Option: SR830 Ground Shield?{Boolean}=False	
Option: SR830 Harmonic{I32}=1	
Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A	
Option: SR830 Line Filter{Boolean}=True	
Option: SR830 No Reset{Boolean}=False	
Option: SR830 Offset 1{Double Float}=0.000000	
Option: SR830 Offset 2{Double Float}=0.000000	
Option: SR830 Output Channel 1{Boolean}=False	
Option: SR830 Output Channel 2{Boolean}=False	
Option: SR830 Ratio 1{U16}=0	
Option: SR830 Ratio 1.__text__{String}=None	
Option: SR830 Ratio 2{U16}=0	
Option: SR830 Ratio 2.__text__{String}=None	
Option: SR830 Ref Amplitude{Double Float}=0.100000	
Option: SR830 Ref Frequency{Double Float}=1013.000000	
Option: SR830 Ref Source{Boolean}=False	
Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta]	
Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Option: SR830 VISA{Visa Refnum (Void)}=	
Option: Sense Autorange{Boolean}=False	
Option: Sense Range Level{Double Float}=0.100000	
Option: Sense Rate{Double Float}=1.000000	
Option:560 Comport{Visa Refnum (Void)}=COM1	
Option:560 Filter High Pass{U16}=0	
Option:560 Filter High Pass.__text__{String}=0.03	
Option:560 Filter Lowpass{U16}=0	
Option:560 Filter Lowpass.__text__{String}=0.03	
Option:560 Filter Mode{U16}=0	
Option:560 Filter Mode.__text__{String}=6 dB high pass	
Option:560 Invert{Boolean}=False	
Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Option:570 Enabled{Boolean}=False	
Option:570 Filter High Pass{U16}=0	
Option:570 Filter High Pass.__text__{String}=0.03	
Option:570 Filter Lowpass{U16}=0	
Option:570 Filter Lowpass.__text__{String}=0.03	
Option:570 Filter Mode{U16}=0	
Option:570 Filter Mode.__text__{String}=6 dB high pass	
Option:570 Gain Mode{U16}=0	
Option:570 Gain Mode.__text__{String}=Low Noise	
Option:570 Input Offset{U16}=0	
Option:570 Input Offset On{Boolean}=False	
Option:570 Input Offset.__text__{String}=1pA	
Option:570 Sensitivity{U16}=0	
Option:570 Sensitivity.__text__{String}=1pA/V	
Option:Debug On{Boolean}=False	
Option:GPIB 2182{Visa Refnum (Void)}=	
Option:Parallel Config Voltage Measurers{Boolean}=True	
Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Option:SR830 Settle Time{Double Float}=5.000000	
Option:Sense Digits{I32}=8	
Output Names{1D Array (String)}=['Offset','Rxx::R','Rxx::Theta','Rxx::X','Rxx::Y','Rxy::R','Rxy::Theta','Rxy::X','Rxy::Y','temperature: T1','temperature: T2','temperature: T3','temperature: T4','temperature: dT/dt','iterator','multi[0]:iterator','multi[0]:y','multi[0]:temperature: setpoint','multi[0]:temperature: T1','multi[0]:temperature: T2','multi[0]:temperature: T3','multi[0]:temperature: T4','multi[0]:temperature: heater','multi[0]:temperature: gas','multi[0]:temperature: dT/dt','multi[0]:temperature: current temperature','multi[0]:temperature: error','multi[1]:iterator','multi[1]:y','multi[1]:Control:Magnet Output']	
Parameter Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Parameter Select{U16}=6	
Parameter Select.__text__{String}=Multi-Parameter	
Paths{U32}=0	
Plot: Column Renames{1D Array (Cluster (String,String))}=[]	
Plot: No dups{Boolean}=False	
Plot: StdDevs{Boolean}=False	
Plotting Class{String}=Parameter Plot	
Plotting Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	
Plotting Select{U16}=1	
Plotting Select.__text__{String}=Parameter Plot	
Project Code{String}=Topological_Insulators	
Ref: Temperature Window{LVObjVI Refnum (Void)}=	
Ref:Control Subpanel{LVObjUnknown Refnum (Void)}=	
Ref:Main Screen{LVObjVI Refnum (Void)}=	
Ref:Plotting Subpanel{LVObjUnknown Refnum (Void)}=	
Ref:Toolbar{LVObjUnknown Refnum (Void)}=	
Ref:XY Subpanel{LVObjUnknown Refnum (Void)}=	
Rxx::R{Double Float}=0.001309	
Rxx::Theta{Double Float}=0.150000	
Rxx::X{Double Float}=0.001309	
Rxx::Y{Double Float}=3.371768E-6	
Rxx:Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	
Rxx:Option: 560 Enabled{Boolean}=False	
Rxx:Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	
Rxx:Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	
Rxx:Option: Lockin Standoff Time{Double Float}=0.000000	
Rxx:Option: Lockin Type{Enum U16 ((SRS 830,EG&G 5302))}=SRS 830	
Rxx:Option: SR803 Full Scale Reading{Double Float}=0.000000	
Rxx:Option: SR830  Ref Phase{Double Float}=0.000000	
Rxx:Option: SR830  Synch Filter{Boolean}=False	
Rxx:Option: SR830  Time Constant{I16}=8	
Rxx:Option: SR830 2x Line Filter{Boolean}=False	
Rxx:Option: SR830 Adjust Gains{Boolean}=False	
Rxx:Option: SR830 Auto Gain Lower{I32}=0	
Rxx:Option: SR830 Auto Gain Upper{I32}=26	
Rxx:Option: SR830 Auto Offset 1{Boolean}=False	
Rxx:Option: SR830 Auto Offset 2{Boolean}=False	
Rxx:Option: SR830 Autophase{Boolean}=False	
Rxx:Option: SR830 DC Coupling?{Boolean}=False	
Rxx:Option: SR830 Display 1{U16}=0	
Rxx:Option: SR830 Display 2{U16}=0	
Rxx:Option: SR830 Dynamic Reserve{I16}=2	
Rxx:Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Rxx:Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Rxx:Option: SR830 Filter Slope{I32}=3	
Rxx:Option: SR830 Gain{I32}=18	
Rxx:Option: SR830 Ground Shield?{Boolean}=False	
Rxx:Option: SR830 Harmonic{I32}=1	
Rxx:Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A-B	
Rxx:Option: SR830 Line Filter{Boolean}=False	
Rxx:Option: SR830 No Reset{Boolean}=False	
Rxx:Option: SR830 Offset 1{Double Float}=0.000000	
Rxx:Option: SR830 Offset 2{Double Float}=0.000000	
Rxx:Option: SR830 Output Channel 1{Boolean}=False	
Rxx:Option: SR830 Output Channel 2{Boolean}=False	
Rxx:Option: SR830 Ratio 1{U16}=0	
Rxx:Option: SR830 Ratio 2{U16}=0	
Rxx:Option: SR830 Ref Amplitude{Double Float}=0.100000	
Rxx:Option: SR830 Ref Frequency{Double Float}=1013.000000	
Rxx:Option: SR830 Ref Source{Boolean}=False	
Rxx:Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta,X,Y]	
Rxx:Option: SR830 Time Constant value{Double Float}=0.000000	
Rxx:Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Rxx:Option: SR830 VISA{Visa Refnum (Void)}=GPIB0::5::INSTR	
Rxx:Option:560 Comport{Visa Refnum (Void)}=COM1	
Rxx:Option:560 Filter High Pass{U16}=0	
Rxx:Option:560 Filter Lowpass{U16}=0	
Rxx:Option:560 Filter Mode{U16}=0	
Rxx:Option:560 Invert{Boolean}=False	
Rxx:Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Rxx:Option:570 Enabled{Boolean}=False	
Rxx:Option:570 Filter High Pass{U16}=0	
Rxx:Option:570 Filter Lowpass{U16}=0	
Rxx:Option:570 Filter Mode{U16}=0	
Rxx:Option:570 Gain Mode{U16}=0	
Rxx:Option:570 Input Offset{U16}=0	
Rxx:Option:570 Input Offset On{Boolean}=False	
Rxx:Option:570 Sensitivity{U16}=0	
Rxx:Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Rxx:Option:SR830 Autogain Lower Threshold{Double Float}=0.100000	
Rxx:Option:SR830 Autogain Standoff{Double Float}=3.000000	
Rxx:Option:SR830 Autogain Upper Threshold{Double Float}=0.900000	
Rxx:Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Rxx:Option:SR830 Settle Time{Double Float}=0.000000	
Rxy::R{Double Float}=5.853713E-6	
Rxy::Theta{Double Float}=-178.984800	
Rxy::X{Double Float}=-5.856346E-6	
Rxy::Y{Double Float}=-1.048409E-7	
Rxy:Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	
Rxy:Option: 560 Enabled{Boolean}=False	
Rxy:Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	
Rxy:Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	
Rxy:Option: Lockin Standoff Time{Double Float}=0.000000	
Rxy:Option: Lockin Type{Enum U16 ((SRS 830,EG&G 5302))}=SRS 830	
Rxy:Option: SR803 Full Scale Reading{Double Float}=0.000000	
Rxy:Option: SR830  Ref Phase{Double Float}=0.000000	
Rxy:Option: SR830  Synch Filter{Boolean}=False	
Rxy:Option: SR830  Time Constant{I16}=8	
Rxy:Option: SR830 2x Line Filter{Boolean}=False	
Rxy:Option: SR830 Adjust Gains{Boolean}=False	
Rxy:Option: SR830 Auto Gain Lower{I32}=0	
Rxy:Option: SR830 Auto Gain Upper{I32}=26	
Rxy:Option: SR830 Auto Offset 1{Boolean}=False	
Rxy:Option: SR830 Auto Offset 2{Boolean}=False	
Rxy:Option: SR830 Autophase{Boolean}=False	
Rxy:Option: SR830 DC Coupling?{Boolean}=False	
Rxy:Option: SR830 Display 1{U16}=0	
Rxy:Option: SR830 Display 2{U16}=1	
Rxy:Option: SR830 Dynamic Reserve{I16}=2	
Rxy:Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Rxy:Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Rxy:Option: SR830 Filter Slope{I32}=3	
Rxy:Option: SR830 Gain{I32}=18	
Rxy:Option: SR830 Ground Shield?{Boolean}=False	
Rxy:Option: SR830 Harmonic{I32}=1	
Rxy:Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A-B	
Rxy:Option: SR830 Line Filter{Boolean}=False	
Rxy:Option: SR830 No Reset{Boolean}=False	
Rxy:Option: SR830 Offset 1{Double Float}=0.000000	
Rxy:Option: SR830 Offset 2{Double Float}=0.000000	
Rxy:Option: SR830 Output Channel 1{Boolean}=False	
Rxy:Option: SR830 Output Channel 2{Boolean}=False	
Rxy:Option: SR830 Ratio 1{U16}=0	
Rxy:Option: SR830 Ratio 2{U16}=0	
Rxy:Option: SR830 Ref Amplitude{Double Float}=0.100000	
Rxy:Option: SR830 Ref Frequency{Double Float}=1013.000000	
Rxy:Option: SR830 Ref Source{Boolean}=False	
Rxy:Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta,X,Y]	
Rxy:Option: SR830 Time Constant value{Double Float}=0.000000	
Rxy:Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Rxy:Option: SR830 VISA{Visa Refnum (Void)}=GPIB0::6::INSTR	
Rxy:Option:560 Comport{Visa Refnum (Void)}=COM1	
Rxy:Option:560 Filter High Pass{U16}=0	
Rxy:Option:560 Filter Lowpass{U16}=0	
Rxy:Option:560 Filter Mode{U16}=0	
Rxy:Option:560 Invert{Boolean}=False	
Rxy:Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Rxy:Option:570 Enabled{Boolean}=False	
Rxy:Option:570 Filter High Pass{U16}=0	
Rxy:Option:570 Filter Lowpass{U16}=0	
Rxy:Option:570 Filter Mode{U16}=0	
Rxy:Option:570 Gain Mode{U16}=0	
Rxy:Option:570 Input Offset{U16}=0	
Rxy:Option:570 Input Offset On{Boolean}=False	
Rxy:Option:570 Sensitivity{U16}=0	
Rxy:Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Rxy:Option:SR830 Autogain Lower Threshold{Double Float}=0.100000	
Rxy:Option:SR830 Autogain Standoff{Double Float}=3.000000	
Rxy:Option:SR830 Autogain Upper Threshold{Double Float}=0.900000	
Rxy:Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Rxy:Option:SR830 Settle Time{Double Float}=0.000000	
Sample ID{String}=MBE202221213_PA_D1 750C Cracker WAL	
Save:Filename{String}=${X-Y Class} ${2nd Parameter Class} ${iterator}{%04d} ${y}{%04.2g}.txt	
Save:Final Filename{String}=${X-Y Class} ${2nd Parameter Class} .txt	
Save:Final path{Path}=C:\\\\Data\\\\${Project Code}\\\\${User}\\\\${Sample ID}\\\\${Measurement Timestamp}{%Y%m%d}\\\\${X-Y Class}	
Save:Path{Path}=C:\\\\Data\\\\${Project Code}\\\\${User}\\\\${Sample ID}\\\\${Measurement Timestamp}{%Y%m%d}\\\\${X-Y Class}	
Startup path{Path}=C:\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV	
Sub Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Sweep Step{I32}=3	
T Control Measure.__text__{1D Array (String)}=['temperature: T1','temperature: T2','temperature: T3','temperature: T4','temperature: dT/dt']	
Timestamp{Timestamp}=<01:42:06.264 18/05/2023>T	
Toolbar{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Unaved Data{Boolean}=True	
Unsaved Data{Boolean}=False	
User{String}=Craig	
X-Y Class{String}=6221-Lockin-DAQ	
X-Y Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	
d(Offset){Double Float}=0.000000	
d(Rxx::R){Double Float}=0.000000	
d(Rxx::Theta){Double Float}=0.000000	
d(Rxx::X){Double Float}=0.000000	
d(Rxx::Y){Double Float}=4.735058E-22	
d(Rxy::R){Double Float}=1.076087E-8	
d(Rxy::Theta){Double Float}=0.127731	
d(Rxy::X){Double Float}=1.076329E-8	
d(Rxy::Y){Double Float}=1.255040E-8	
iterate result{U16}=5	
iterator{I32}=784	
multi[0]:Control: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values,Adaptive Step Ramp))}=List of Values	
multi[0]:Control: Monitor Update Timeout{Double Float}=0.010000	
multi[0]:Control: Open T Window{Boolean}=False	
multi[0]:Control: Reverse Temperature Sense{Boolean}=False	
multi[0]:Iterator{I32}=0	
multi[0]:Ref: Temperature Window{LVObjVI Refnum (Void)}=	
multi[0]:iterate result{U16}=0	
multi[0]:iterator{I32}=13	
multi[0]:temperature:  rate window{Double Float}=120.000000	
multi[0]:temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[0]:temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
multi[0]:temperature: T1{Double Float}=40.006000	
multi[0]:temperature: T2{Double Float}=41.926000	
multi[0]:temperature: T3{Double Float}=85.601700	
multi[0]:temperature: T4{Double Float}=60.924200	
multi[0]:temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
multi[0]:temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
multi[0]:temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
multi[0]:temperature: current temperature{Double Float}=1.464900	
multi[0]:temperature: current temperature 2{Double Float}=287.100000	
multi[0]:temperature: dT/dt{Double Float}=0.114328	
multi[0]:temperature: error{Double Float}=-0.053000	
multi[0]:temperature: gas{Double Float}=40.000000	
multi[0]:temperature: gas control{Boolean}=False	
multi[0]:temperature: gas control 2{Boolean}=False	
multi[0]:temperature: gass boost{I8}=0	
multi[0]:temperature: gass boost 2{I8}=0	
multi[0]:temperature: gast flow{I16}=0	
multi[0]:temperature: gast flow 2{I16}=7	
multi[0]:temperature: heater{Double Float}=7.500000	
multi[0]:temperature: heater output{Double Float}=0.000000	
multi[0]:temperature: heater output 2{Double Float}=0.000000	
multi[0]:temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
multi[0]:temperature: monitor timeout{Double Float}=0.010000	
multi[0]:temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
multi[0]:temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
multi[0]:temperature: ramp rate{Double Float}=8.000000	
multi[0]:temperature: ramp rate 2{Double Float}=0.000000	
multi[0]:temperature: ramp target{Double Float}=20.000000	
multi[0]:temperature: ramp target 2{Double Float}=0.000000	
multi[0]:temperature: ramping{Boolean}=False	
multi[0]:temperature: setpoint{Double Float}=1.800000	
multi[0]:temperature: setpoint 2{Double Float}=287.100000	
multi[0]:temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
multi[0]:temperature: stability error{Extended Float}=0.040000	
multi[0]:temperature: stability script{String}=	
multi[0]:temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
multi[0]:temperature: temp control mode{U16}=2	
multi[0]:temperature: temp control mode 2{U16}=3	
multi[0]:temperature: temp control mode 2.__text__{String}=Open Loop	
multi[0]:temperature: temp control mode.__text__{String}=Zone	
multi[0]:temperature: temp control sensor{U16}=0	
multi[0]:temperature: temp control sensor 2{U16}=0	
multi[0]:temperature: temp control sensor 2.__text__{String}=Sensor 1	
multi[0]:temperature: temp control sensor.__text__{String}=Sensor A	
multi[0]:temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
multi[0]:temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
multi[0]:temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
multi[0]:temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
multi[0]:temperature: temp loop{U16}=0	
multi[0]:temperature: temp loop 2{U16}=0	
multi[0]:temperature: temp loop 2.__text__{String}=Heater	
multi[0]:temperature: temp loop.__text__{String}=Loop 1	
multi[0]:temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
multi[0]:temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[0]:temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[0]:temperature:error for gas boost{Double Float}=0.000000	
multi[0]:temperature:error for gas boost 2{Double Float}=0.000000	
multi[0]:temperature:heater range{U16}=2	
multi[0]:temperature:heater range 2{U16}=0	
multi[0]:temperature:heater range 2.__text__{String}=Off	
multi[0]:temperature:heater range.__text__{String}=40mW	
multi[0]:temperature:history window{Extended Float}=300.000000	
multi[0]:temperature:is stable?{Boolean}=True	
multi[0]:temperature:monitor{Boolean}=True	
multi[0]:temperature:ramping{Boolean}=False	
multi[0]:temperature:ramping on{Boolean}=False	
multi[0]:temperature:ramping on 2{Boolean}=False	
multi[0]:temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
multi[0]:temperature:stability code{U32}=6618880	
multi[0]:temperature:stability rate{Extended Float}=0.040000	
multi[0]:y{Double Float}=40.000000	
multi[1]:Control: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values,Adaptive Step Ramp))}=Multi-Segment Ramp	
multi[1]:Control: Gate delay{Double Float}=0.000000	
multi[1]:Control: Monitor Update Timeout{Double Float}=0.010000	
multi[1]:Control: Open T Window{Boolean}=False	
multi[1]:Control: Reverse Temperature Sense{Boolean}=False	
multi[1]:Control:Magnet Output{Double Float}=-0.000100	
multi[1]:Iterator{I32}=0	
multi[1]:Magnet: Final Switch Heater{Enum U8 ((False,True,Mixed))}=	
multi[1]:Magnet: Power Supply{Enum U16 ((IPS120,LS625,PS110,Hg iPS,SMS Series,Cryomagnetics 4G,DMG Little CryoFree,DMG Big CryoFree))}=Hg iPS	
multi[1]:Magnet: Rate{Double Float}=0.500000	
multi[1]:Magnet: Units{Enum U16 ((Field,Current))}=Field	
multi[1]:Magnet: VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[1]:Multi-segment_Stage{I32}=0	
multi[1]:Multi-segment_Stage_Changed{Boolean}=False	
multi[1]:Ref: Temperature Window{LVObjVI Refnum (Void)}=	
multi[1]:iterate result{U16}=4	
multi[1]:iterator{I32}=57	
multi[1]:measure point{Boolean}=False	
multi[1]:temperature:  rate window{Double Float}=120.000000	
multi[1]:temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[1]:temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
multi[1]:temperature: T1{Double Float}=1.842400	
multi[1]:temperature: T2{Double Float}=1.465600	
multi[1]:temperature: T3{Double Float}=86.318100	
multi[1]:temperature: T4{Double Float}=66.769200	
multi[1]:temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
multi[1]:temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
multi[1]:temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
multi[1]:temperature: current temperature{Double Float}=1.465600	
multi[1]:temperature: current temperature 2{Double Float}=287.100000	
multi[1]:temperature: dT/dt{Double Float}=-0.001864	
multi[1]:temperature: gas control{Boolean}=False	
multi[1]:temperature: gas control 2{Boolean}=False	
multi[1]:temperature: gass boost{I8}=0	
multi[1]:temperature: gass boost 2{I8}=0	
multi[1]:temperature: gast flow{I16}=0	
multi[1]:temperature: gast flow 2{I16}=7	
multi[1]:temperature: heater output{Double Float}=0.000000	
multi[1]:temperature: heater output 2{Double Float}=0.000000	
multi[1]:temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
multi[1]:temperature: monitor timeout{Double Float}=1.000000	
multi[1]:temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
multi[1]:temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
multi[1]:temperature: ramp rate{Double Float}=8.000000	
multi[1]:temperature: ramp rate 2{Double Float}=0.000000	
multi[1]:temperature: ramp target{Double Float}=20.000000	
multi[1]:temperature: ramp target 2{Double Float}=0.000000	
multi[1]:temperature: ramping{Boolean}=False	
multi[1]:temperature: setpoint{Double Float}=1.800000	
multi[1]:temperature: setpoint 2{Double Float}=287.100000	
multi[1]:temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
multi[1]:temperature: stability error{Extended Float}=0.040000	
multi[1]:temperature: stability script{String}=	
multi[1]:temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
multi[1]:temperature: temp control mode{U16}=2	
multi[1]:temperature: temp control mode 2{U16}=3	
multi[1]:temperature: temp control mode 2.__text__{String}=Open Loop	
multi[1]:temperature: temp control mode.__text__{String}=Zone	
multi[1]:temperature: temp control sensor{U16}=0	
multi[1]:temperature: temp control sensor 2{U16}=0	
multi[1]:temperature: temp control sensor 2.__text__{String}=Sensor 1	
multi[1]:temperature: temp control sensor.__text__{String}=Sensor A	
multi[1]:temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
multi[1]:temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
multi[1]:temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
multi[1]:temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
multi[1]:temperature: temp loop{U16}=0	
multi[1]:temperature: temp loop 2{U16}=0	
multi[1]:temperature: temp loop 2.__text__{String}=Heater	
multi[1]:temperature: temp loop.__text__{String}=Loop 1	
multi[1]:temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
multi[1]:temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[1]:temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[1]:temperature:error for gas boost{Double Float}=0.000000	
multi[1]:temperature:error for gas boost 2{Double Float}=0.000000	
multi[1]:temperature:heater range{U16}=2	
multi[1]:temperature:heater range 2{U16}=0	
multi[1]:temperature:heater range 2.__text__{String}=Off	
multi[1]:temperature:heater range.__text__{String}=40mW	
multi[1]:temperature:history window{Extended Float}=300.000000	
multi[1]:temperature:is stable?{Boolean}=True	
multi[1]:temperature:monitor{Boolean}=True	
multi[1]:temperature:ramping{Boolean}=False	
multi[1]:temperature:ramping on{Boolean}=False	
multi[1]:temperature:ramping on 2{Boolean}=False	
multi[1]:temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
multi[1]:temperature:stability code{U32}=6618880	
multi[1]:temperature:stability rate{Extended Float}=0.040000	
multi[1]:y{Double Float}=0.000000	
parameter: Termination{String}=False	
parameter: delta time{Double Float}=1.000000	
parameter: progress{Double Float}=100.000000	
temperature:  rate window{Double Float}=120.000000	
temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
temperature: T1{Double Float}=40.006000	
temperature: T2{Double Float}=41.926000	
temperature: T3{Double Float}=85.601700	
temperature: T4{Double Float}=60.924200	
temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
temperature: current temperature{Double Float}=1.464900	
temperature: current temperature 2{Double Float}=287.100000	
temperature: dT/dt{Double Float}=0.114328	
temperature: gas control{Boolean}=False	
temperature: gas control 2{Boolean}=False	
temperature: gass boost{I8}=0	
temperature: gass boost 2{I8}=0	
temperature: gast flow{I16}=0	
temperature: gast flow 2{I16}=7	
temperature: heater output{Double Float}=0.000000	
temperature: heater output 2{Double Float}=0.000000	
temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
temperature: monitor timeout{Double Float}=0.010000	
temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
temperature: ramp rate{Double Float}=8.000000	
temperature: ramp rate 2{Double Float}=0.000000	
temperature: ramp target{Double Float}=20.000000	
temperature: ramp target 2{Double Float}=0.000000	
temperature: ramping{Boolean}=False	
temperature: setpoint{Double Float}=1.800000	
temperature: setpoint 2{Double Float}=287.100000	
temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
temperature: stability error{Extended Float}=0.040000	
temperature: stability script{String}=	
temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
temperature: temp control mode{U16}=2	
temperature: temp control mode 2{U16}=3	
temperature: temp control mode 2.__text__{String}=Open Loop	
temperature: temp control mode.__text__{String}=Zone	
temperature: temp control sensor{U16}=0	
temperature: temp control sensor 2{U16}=0	
temperature: temp control sensor 2.__text__{String}=Sensor 1	
temperature: temp control sensor.__text__{String}=Sensor A	
temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
temperature: temp loop{U16}=0	
temperature: temp loop 2{U16}=0	
temperature: temp loop 2.__text__{String}=Heater	
temperature: temp loop.__text__{String}=Loop 1	
temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
temperature:error for gas boost{Double Float}=0.000000	
temperature:error for gas boost 2{Double Float}=0.000000	
temperature:heater range{U16}=2	
temperature:heater range 2{U16}=0	
temperature:heater range 2.__text__{String}=Off	
temperature:heater range.__text__{String}=40mW	
temperature:history window{Extended Float}=300.000000	
temperature:is stable?{Boolean}=True	
temperature:monitor{Boolean}=True	
temperature:ramping{Boolean}=False	
temperature:ramping on{Boolean}=False	
temperature:ramping on 2{Boolean}=False	
temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
temperature:stability code{U32}=6618880	
temperature:stability rate{Extended Float}=0.040000	
y{Double Float}=40.000000	
