TDI Format 1.5	Offset	Rxx::R	Rxx::Theta	Rxx::X	Rxx::Y	Rxy::R	Rxy::Theta	Rxy::X	Rxy::Y	temperature: T1	temperature: T2	temperature: T3	temperature: T4	temperature: dT/dt	iterator	multi[0]:iterator	multi[0]:y	multi[0]:temperature: setpoint	multi[0]:temperature: T1	multi[0]:temperature: T2	multi[0]:temperature: T3	multi[0]:temperature: T4	multi[0]:temperature: heater	multi[0]:temperature: gas	multi[0]:temperature: dT/dt	multi[0]:temperature: current temperature	multi[0]:temperature: error	multi[1]:iterator	multi[1]:y	multi[1]:Control:Magnet Output
2nd Parameter Class{String}=Multi-Parameter	0E+0	1.227152706E-3	1.56E-1	1.227152706E-3	3.304332616E-6	5.900585472E-7	-8.2404E+0	5.842628171E-7	-8.640146245E-8	8.0161E+0	8.0843E+0	8.67479E+1	6.8541E+1	5.455103237E-3	5.7E+1	1E+0	8E+0	8E+0	7.9968E+0	8.0755E+0	8.67479E+1	6.8541E+1	1.6E+0	8E+0	-6.804257631E-3	7.9987E+0	1.3E-3	0E+0	0E+0	1E-4
2nd Parameter Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	0E+0	1.231570426E-3	1.56E-1	1.231570426E-3	3.371767975E-6	7.14972637E-6	-5.136E-1	7.14972637E-6	-6.532801159E-8	8.0138E+0	8.0736E+0	8.68195E+1	6.8541E+1	-1.302679814E-2	5.8E+1	1E+0	8E+0	1.8E+0	8.0161E+0	8.0843E+0	8.67479E+1	6.8541E+1	1.6E+0	8E+0	5.455103237E-3	1.4649E+0	1.3E-3	1E+0	5E-1	4.999E-1
Analysis Class{String}=Basic Plot	0E+0	1.235717466E-3	1.56E-1	1.235717466E-3	3.371767975E-6	1.372046239E-5	-2.028E-1	1.372046239E-5	-4.952281739E-8	8.005E+0	8.079E+0	8.56734E+1	6.8541E+1	-8.298812434E-3	5.9E+1	1E+0	8E+0	1.8E+0	8.0138E+0	8.0736E+0	8.68195E+1	6.8541E+1	1.6E+0	8E+0	-1.302679814E-2	1.4649E+0	1.3E-3	2E+0	1E+0	9.999E-1
Analysis Class Path{Path}=C\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV\\\\plugins\\\\Plotting\\\\Plotting_Base_class\\\\Plotting_Base.lvclass	0E+0	1.241482932E-3	1.56E-1	1.241482932E-3	3.371767975E-6	2.031645062E-5	-7.08E-2	2.031645062E-5	-2.686877358E-8	7.9999E+0	8.0776E+0	8.67837E+1	6.8541E+1	-3.672970226E-3	6E+1	1E+0	8E+0	1.8E+0	8.005E+0	8.079E+0	8.56734E+1	6.8541E+1	1.6E+0	8E+0	-8.298812434E-3	1.4649E+0	1.3E-3	3E+0	1.5E+0	1.4999E+0
Analysis.# pre-routines{I32}=5	0E+0	1.241482932E-3	1.56E-1	1.241482932E-3	3.371767975E-6	2.032224889E-5	-1.008E-1	2.032224889E-5	-3.740555274E-8	7.9975E+0	8.0759E+0	8.67479E+1	6.8541E+1	-5.648694467E-3	6.1E+1	1E+0	8E+0	1.8E+0	7.9999E+0	8.0776E+0	8.67837E+1	6.8541E+1	1.6E+0	8E+0	-3.672970226E-3	1.4649E+0	1.3E-3	4E+0	1.5E+0	1.5E+0
Analysis:Pre[0]:T Control Measure{1D Array (I32)}=[1,2,3,4,7]	0E+0	1.238954318E-3	1.56E-1	1.238954318E-3	3.371767975E-6	1.765648461E-5	-1.62E-1	1.765648461E-5	-5.163019359E-8	7.9963E+0	8.0778E+0	8.6712E+1	6.8541E+1	5.13179414E-3	6.2E+1	1E+0	8E+0	1.8E+0	7.9975E+0	8.0759E+0	8.67479E+1	6.8541E+1	1.6E+0	8E+0	-5.648694467E-3	1.4649E+0	1.3E-3	5E+0	1.3E+0	1.3001E+0
Autosave Tabs{Enum U32 ((XY Measurement Save,Parameter Plot Save 2))}=Parameter Plot Save 2	0E+0	1.236593996E-3	1.56E-1	1.236593996E-3	3.371767975E-6	1.50396804E-5	-1.536E-1	1.50396804E-5	-4.214707141E-8	7.9577E+0	8.051E+0	8.6712E+1	6.8541E+1	-2.647345327E-2	6.3E+1	1E+0	8E+0	1.8E+0	7.9963E+0	8.0778E+0	8.6712E+1	6.8541E+1	1.6E+0	8E+0	5.13179414E-3	1.4649E+0	1.3E-3	6E+0	1.1E+0	1.1001E+0
Control:Magnet Output{Double Float}=-0.007000	0E+0	1.234604197E-3	1.56E-1	1.234604197E-3	3.371767975E-6	1.240495245E-5	-2.292E-1	1.240495245E-5	-5.16301653E-8	8.0122E+0	8.0845E+0	8.57808E+1	6.8541E+1	2.148127183E-2	6.4E+1	1E+0	8E+0	1.8E+0	7.9577E+0	8.051E+0	8.6712E+1	6.8541E+1	1.6E+0	8E+0	-2.647345327E-2	1.4649E+0	1.3E-3	7E+0	9E-1	9.001E-1
Control:Magnet Rate{Double Float}=0.500000	0E+0	1.233052805E-3	1.536E-1	1.233052805E-3	3.304332616E-6	9.780746252E-6	-3.24E-1	9.780746252E-6	-5.637168397E-8	8.0053E+0	8.079E+0	8.68553E+1	6.8541E+1	6.030605175E-3	6.5E+1	1E+0	8E+0	1.8E+0	8.0122E+0	8.0845E+0	8.57808E+1	6.8541E+1	1.6E+0	8E+0	2.148127183E-2	1.4649E+0	1.3E-3	8E+0	7E-1	7E-1
Display Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	0E+0	1.231570426E-3	1.56E-1	1.231570426E-3	3.371767975E-6	7.144985926E-6	-4.74E-1	7.144985926E-6	-6.058643636E-8	7.9972E+0	8.0787E+0	8.68911E+1	6.8541E+1	1.269882917E-2	6.6E+1	1E+0	8E+0	1.8E+0	8.0053E+0	8.079E+0	8.68553E+1	6.8541E+1	1.6E+0	8E+0	6.030605175E-3	1.4649E+0	1.3E-3	9E+0	5E-1	5.001E-1
Elapsed Time{Double Float}=12790.950867	0E+0	1.230322241E-3	1.56E-1	1.230322241E-3	3.371767975E-6	4.526063227E-6	-8.124E-1	4.526063227E-6	-6.480110391E-8	8.0229E+0	8.0904E+0	8.67837E+1	6.8541E+1	3.506113961E-2	6.7E+1	1E+0	8E+0	1.8E+0	7.9972E+0	8.0787E+0	8.68911E+1	6.8541E+1	1.6E+0	8E+0	1.269882917E-2	1.4649E+0	1.3E-3	1E+1	3E-1	3.002E-1
File:Autodel{Boolean}=True	0E+0	1.228670157E-3	1.56E-1	1.228670157E-3	3.371767975E-6	1.882394619E-6	-2.5248E+0	1.880287441E-6	-8.482107879E-8	8.0145E+0	8.0775E+0	8.6712E+1	6.8541E+1	9.643551894E-3	6.8E+1	1E+0	8E+0	1.8E+0	8.0229E+0	8.0904E+0	8.67837E+1	6.8541E+1	1.6E+0	8E+0	3.506113961E-2	1.4649E+0	1.3E-3	1.1E+1	1E-1	1E-1
File:Autosave{Boolean}=False	0E+0	1.228670157E-3	1.56E-1	1.228670157E-3	3.371767975E-6	1.878703522E-6	-2.3748E+0	1.876073084E-6	-7.902571646E-8	7.9656E+0	8.0542E+0	8.6712E+1	6.8541E+1	-2.649862505E-2	6.9E+1	1E+0	8E+0	1.8E+0	8.0145E+0	8.0775E+0	8.6712E+1	6.8541E+1	1.6E+0	8E+0	9.643551894E-3	1.4649E+0	1.3E-3	1.2E+1	1E-1	1E-1
File:Export Config{Boolean}=True	0E+0	1.228670157E-3	1.56E-1	1.228670157E-3	3.304332616E-6	1.744887806E-6	-2.3676E+0	1.744361719E-6	-7.375729011E-8	8.0361E+0	8.0896E+0	8.66762E+1	6.8541E+1	2.735222504E-2	7E+1	1E+0	8E+0	1.8E+0	7.9656E+0	8.0542E+0	8.6712E+1	6.8541E+1	1.6E+0	8E+0	-2.649862505E-2	1.4649E+0	1.3E-3	1.3E+1	9E-2	9E-2
File:Final Autosave{Boolean}=True	0E+0	1.228468208E-3	1.56E-1	1.228468208E-3	3.338050296E-6	1.621084722E-6	-3.4332E+0	1.617922541E-6	-9.90457762E-8	8.0134E+0	8.0884E+0	8.66762E+1	6.8541E+1	2.313079312E-2	7.1E+1	1E+0	8E+0	1.8E+0	8.0361E+0	8.0896E+0	8.66762E+1	6.8541E+1	1.6E+0	8E+0	2.735222504E-2	1.4649E+0	1.3E-3	1.4E+1	8E-2	8.01E-2
Filter:Enable{Enum U16 ((None,Analog,Digital,Analog&Digitial))}=None	0E+0	1.228333574E-3	1.56E-1	1.228333574E-3	3.338050296E-6	1.492535538E-6	-2.9676E+0	1.489899444E-6	-7.902577303E-8	8.0238E+0	8.0749E+0	8.66762E+1	6.8541E+1	7.431899197E-3	7.2E+1	1E+0	8E+0	1.8E+0	8.0134E+0	8.0884E+0	8.66762E+1	6.8541E+1	1.6E+0	8E+0	2.313079312E-2	1.4649E+0	1.3E-3	1.5E+1	7E-2	7.01E-2
Filter:Points{I32}=1	0E+0	1.228163869E-3	1.56E-1	1.228163869E-3	3.371767975E-6	1.36029865E-6	-3.354E+0	1.358718125E-6	-8.113312095E-8	7.9859E+0	8.0715E+0	8.66404E+1	6.8541E+1	5.565210595E-4	7.3E+1	1E+0	8E+0	1.8E+0	8.0238E+0	8.0749E+0	8.66762E+1	6.8541E+1	1.6E+0	8E+0	7.431899197E-3	1.4649E+0	1.3E-3	1.6E+1	6E-2	6.01E-2
Filter:Type{U16}=1	0E+0	1.227995577E-3	1.56E-1	1.227995577E-3	3.371767975E-6	1.216995259E-6	-3.726E+0	1.214361144E-6	-8.007944699E-8	8.0181E+0	8.0901E+0	8.58524E+1	6.8541E+1	3.22232917E-2	7.4E+1	1E+0	8E+0	1.8E+0	7.9859E+0	8.0715E+0	8.66404E+1	6.8541E+1	1.6E+0	8E+0	5.565210595E-4	1.4649E+0	1.3E-3	1.7E+1	5E-2	5.01E-2
Filter:Type.__text__{String}=Repeat	0E+0	1.227995577E-3	1.56E-1	1.227995577E-3	3.371767975E-6	1.221210181E-6	-3.7152E+0	1.218575784E-6	-8.060629811E-8	8.0018E+0	8.0818E+0	8.58883E+1	6.8541E+1	1.622114703E-2	7.5E+1	1E+0	8E+0	1.8E+0	8.0181E+0	8.0901E+0	8.58524E+1	6.8541E+1	1.6E+0	8E+0	3.22232917E-2	1.4649E+0	1.3E-3	1.8E+1	5E-2	5E-2
Filter:Window{Double Float}=1.000000	0E+0	1.227995577E-3	1.56E-1	1.227995577E-3	3.338050296E-6	1.164311561E-6	-3.7104E+0	1.161677729E-6	-7.691842512E-8	7.9929E+0	8.0655E+0	8.57808E+1	6.8541E+1	-1.076467894E-2	7.6E+1	1E+0	8E+0	1.8E+0	8.0018E+0	8.0818E+0	8.58883E+1	6.8541E+1	1.6E+0	8E+0	1.622114703E-2	1.4649E+0	1.3E-3	1.9E+1	4.5E-2	4.49E-2
Iterator{I32}=0	0E+0	1.227827286E-3	1.56E-1	1.227827286E-3	3.304332616E-6	1.092662128E-6	-3.756E+0	1.090027731E-6	-7.270361616E-8	7.9846E+0	8.072E+0	8.58166E+1	6.8541E+1	-7.666810881E-3	7.7E+1	1E+0	8E+0	1.8E+0	7.9929E+0	8.0655E+0	8.57808E+1	6.8541E+1	1.6E+0	8E+0	-1.076467894E-2	1.4649E+0	1.3E-3	2E+1	4E-2	4E-2
Magnet: Control Mode{Boolean}=False	0E+0	1.227827286E-3	1.56E-1	1.227827286E-3	3.270614936E-6	1.017851644E-6	-4.7292E+0	1.013109786E-6	-8.587475275E-8	8.0391E+0	8.0961E+0	8.5745E+1	6.8541E+1	3.554435074E-2	7.8E+1	1E+0	8E+0	1.8E+0	7.9846E+0	8.072E+0	8.58166E+1	6.8541E+1	1.6E+0	8E+0	-7.666810881E-3	1.4649E+0	1.3E-3	2.1E+1	3.5E-2	3.5E-2
Magnet: Final Switch Heater{Enum U8 ((False,True,Mixed))}=	0E+0	1.227658995E-3	1.56E-1	1.227658995E-3	3.304332616E-6	9.562120149E-7	-4.6032E+0	9.530506819E-7	-7.84989502E-8	7.9902E+0	8.0575E+0	8.56734E+1	6.8541E+1	-2.906714007E-2	7.9E+1	1E+0	8E+0	1.8E+0	8.0391E+0	8.0961E+0	8.5745E+1	6.8541E+1	1.6E+0	8E+0	3.554435074E-2	1.4649E+0	1.3E-3	2.2E+1	3E-2	2.99E-2
Magnet: Power Supply{Enum U16 ((IPS120,LS625,PS110,Hg iPS,SMS Series,Cryomagnetics 4G,DMG Little CryoFree,DMG Big CryoFree))}=Hg iPS	0E+0	1.227490703E-3	1.56E-1	1.227490703E-3	3.338050296E-6	8.803473769E-7	-4.5696E+0	8.777129799E-7	-7.112311936E-8	8.0339E+0	8.0959E+0	8.56734E+1	6.8541E+1	3.256385401E-2	8E+1	1E+0	8E+0	1.8E+0	7.9902E+0	8.0575E+0	8.56734E+1	6.8541E+1	1.6E+0	8E+0	-2.906714007E-2	1.4649E+0	1.3E-3	2.3E+1	2.5E-2	2.5E-2
Magnet: Rate{Double Float}=0.500000	0E+0	1.227490703E-3	1.56E-1	1.227490703E-3	3.371767975E-6	8.108048392E-7	-4.9656E+0	8.076440719E-7	-7.112314765E-8	7.9961E+0	8.0643E+0	8.68195E+1	6.8541E+1	-1.296090614E-2	8.1E+1	1E+0	8E+0	1.8E+0	8.0339E+0	8.0959E+0	8.56734E+1	6.8541E+1	1.6E+0	8E+0	3.256385401E-2	1.4649E+0	1.3E-3	2.4E+1	2E-2	1.99E-2
Magnet: Setpoint{Double Float}=0.000000	0E+0	1.227320997E-3	1.56E-1	1.227320997E-3	3.304332616E-6	7.491652097E-7	-6.354E+0	7.449508533E-7	-8.429414282E-8	8.0028E+0	8.0837E+0	8.67837E+1	6.8541E+1	1.767585985E-2	8.2E+1	1E+0	8E+0	1.8E+0	7.9961E+0	8.0643E+0	8.68195E+1	6.8541E+1	1.6E+0	8E+0	-1.296090614E-2	1.4649E+0	1.3E-3	2.5E+1	1.5E-2	1.49E-2
Magnet: Units{Enum U16 ((Field,Current))}=Field	0E+0	1.227320997E-3	1.56E-1	1.227320997E-3	3.338050296E-6	6.938476805E-7	-6.18E+0	6.906863475E-7	-7.639160228E-8	8.0088E+0	8.0798E+0	8.67479E+1	6.8541E+1	8.125211112E-3	8.3E+1	1E+0	8E+0	1.8E+0	8.0028E+0	8.0837E+0	8.67837E+1	6.8541E+1	1.6E+0	8E+0	1.767585985E-2	1.4649E+0	1.3E-3	2.6E+1	1E-2	9.9E-3
Magnet: VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	0E+0	1.227320997E-3	1.56E-1	1.227320997E-3	3.236897256E-6	6.390542589E-7	-6.9216E+0	6.348396196E-7	-7.90258296E-8	8.006E+0	8.0852E+0	8.6712E+1	6.8541E+1	1.258543693E-2	8.4E+1	1E+0	8E+0	1.8E+0	8.0088E+0	8.0798E+0	8.67479E+1	6.8541E+1	1.6E+0	8E+0	8.125211112E-3	1.4649E+0	1.3E-3	2.7E+1	5E-3	5E-3
Main Screen Path{Path}=C:\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV\\\\1Code.vi	0E+0	1.227186364E-3	1.56E-1	1.227186364E-3	3.371767975E-6	5.568680862E-7	-8.454E+0	5.510726391E-7	-8.376740483E-8	8.0156E+0	8.0796E+0	8.66762E+1	6.8541E+1	8.273825049E-3	8.5E+1	1E+0	8E+0	1.8E+0	8.006E+0	8.0852E+0	8.6712E+1	6.8541E+1	1.6E+0	8E+0	1.258543693E-2	1.4649E+0	1.3E-3	2.8E+1	0E+0	-1E-4
Measurement Timestamp{Timestamp}=<19:44:34.961 17/05/2023>T	0E+0	1.227320997E-3	1.56E-1	1.227320997E-3	3.371767975E-6	4.852183703E-7	-8.214E+0	4.804767951E-7	-7.059635309E-8	8.0158E+0	8.0921E+0	8.66762E+1	6.8541E+1	2.112903632E-2	8.6E+1	1E+0	8E+0	1.8E+0	8.0156E+0	8.0796E+0	8.66762E+1	6.8541E+1	1.6E+0	8E+0	8.273825049E-3	1.4649E+0	1.3E-3	2.9E+1	-5E-3	-5.2E-3
Measurement Title{String}=	0E+0	1.227320997E-3	1.56E-1	1.227320997E-3	3.304332616E-6	4.356957226E-7	-1.34052E+1	4.246323299E-7	-1.022067415E-7	7.9983E+0	8.0791E+0	8.66404E+1	6.8541E+1	2.321919659E-3	8.7E+1	1E+0	8E+0	1.8E+0	8.0158E+0	8.0921E+0	8.66762E+1	6.8541E+1	1.6E+0	8E+0	2.112903632E-2	1.4649E+0	1.3E-3	3E+1	-1E-2	-1.01E-2
Measurment Select{U16}=4	0E+0	1.227320997E-3	1.56E-1	1.227320997E-3	3.338050296E-6	3.703678242E-7	-1.3428E+1	3.598313674E-7	-8.798210066E-8	8.0042E+0	8.0821E+0	8.66404E+1	6.8541E+1	2.42773979E-3	8.8E+1	1E+0	8E+0	1.8E+0	7.9983E+0	8.0791E+0	8.66404E+1	6.8541E+1	1.6E+0	8E+0	2.321919659E-3	1.4649E+0	1.3E-3	3.1E+1	-1.5E-2	-1.5E-2
Measurment Select.__text__{String}=6221-Lockin-DAQ	0E+0	1.227490703E-3	1.56E-1	1.227490703E-3	3.371767975E-6	2.945023376E-7	-1.7382E+1	2.797512416E-7	-8.956262574E-8	8.0038E+0	8.083E+0	8.66404E+1	6.8541E+1	6.30219141E-3	8.9E+1	1E+0	8E+0	1.8E+0	8.0042E+0	8.0821E+0	8.66404E+1	6.8541E+1	1.6E+0	8E+0	2.42773979E-3	1.4649E+0	1.3E-3	3.2E+1	-2E-2	-2.02E-2
Notes{String}=I+1A I-1E\\nrxx+1B Rxx-1C\\nRxy+1D Rxy-4A	0E+0	1.227490703E-3	1.56E-1	1.227490703E-3	3.371767975E-6	2.407650507E-7	-1.68708E+1	2.29701658E-7	-7.217684989E-8	7.9801E+0	8.0586E+0	8.66046E+1	6.8541E+1	-3.406509757E-2	9E+1	1E+0	8E+0	1.8E+0	8.0038E+0	8.083E+0	8.66404E+1	6.8541E+1	1.6E+0	8E+0	6.30219141E-3	1.4649E+0	1.3E-3	3.3E+1	-2.5E-2	-2.5E-2
Offset{Double Float}=0.000000	0E+0	1.227827286E-3	1.56E-1	1.227827286E-3	3.371767975E-6	1.849205855E-7	-2.75796E+1	1.633196047E-7	-8.692837014E-8	8.0007E+0	8.0845E+0	8.66046E+1	6.8541E+1	7.975922897E-3	9.1E+1	1E+0	8E+0	1.8E+0	7.9801E+0	8.0586E+0	8.66046E+1	6.8541E+1	1.6E+0	8E+0	-3.406509757E-2	1.4649E+0	1.3E-3	3.4E+1	-3E-2	-3.01E-2
Option: 2182 Autozero{Boolean}=True	0E+0	1.227827286E-3	1.56E-1	1.227827286E-3	3.304332616E-6	1.238070152E-7	-4.70532E+1	8.376740483E-8	-9.219682477E-8	8.0051E+0	8.0775E+0	8.66046E+1	6.8541E+1	-5.432801787E-3	9.2E+1	1E+0	8E+0	1.8E+0	8.0007E+0	8.0845E+0	8.66046E+1	6.8541E+1	1.6E+0	8E+0	7.975922897E-3	1.4649E+0	1.3E-3	3.5E+1	-3.5E-2	-3.51E-2
Option: 2182 Front Autozero{Boolean}=True	0E+0	1.227995577E-3	1.56E-1	1.227995577E-3	3.371767975E-6	8.903583119E-8	-7.167E+1	2.686876792E-8	-8.745524954E-8	8.0031E+0	8.0827E+0	8.66046E+1	6.8541E+1	6.40563108E-3	9.3E+1	1E+0	8E+0	1.8E+0	8.0051E+0	8.0775E+0	8.66046E+1	6.8541E+1	1.6E+0	8E+0	-5.432801787E-3	1.4649E+0	1.3E-3	3.6E+1	-4E-2	-4E-2
Option: 2182 Hold{Boolean}=False	0E+0	1.227995577E-3	1.56E-1	1.227995577E-3	3.304332616E-6	9.69384E-8	-1.216476E+2	-5.268386754E-8	-8.534790163E-8	8.0056E+0	8.085E+0	8.66046E+1	6.8541E+1	1.070914045E-2	9.4E+1	1E+0	8E+0	1.8E+0	8.0031E+0	8.0827E+0	8.66046E+1	6.8541E+1	1.6E+0	8E+0	6.40563108E-3	1.4649E+0	1.3E-3	3.7E+1	-4.5E-2	-4.51E-2
Option: 2182 Hold Count{I32}=10	0E+0	1.228062894E-3	1.56E-1	1.228062894E-3	3.371767975E-6	1.353975136E-7	-1.4664E+2	-1.137971267E-7	-7.533784347E-8	8.0283E+0	8.0982E+0	8.65688E+1	6.8541E+1	3.067913838E-2	9.5E+1	1E+0	8E+0	1.8E+0	8.0056E+0	8.085E+0	8.66046E+1	6.8541E+1	1.6E+0	8E+0	1.070914045E-2	1.4649E+0	1.3E-3	3.8E+1	-5E-2	-5.01E-2
Option: 2182 Hold Window{Double Float}=1.000000	0E+0	1.228029236E-3	1.56E-1	1.228029236E-3	3.270614936E-6	1.364511875E-7	-1.48524E+2	-1.185386454E-7	-7.375737496E-8	8.0059E+0	8.0929E+0	8.65688E+1	6.8541E+1	2.306172065E-2	9.6E+1	1E+0	8E+0	1.8E+0	8.0283E+0	8.0982E+0	8.65688E+1	6.8541E+1	1.6E+0	8E+0	3.067913838E-2	1.4649E+0	1.3E-3	3.9E+1	-5E-2	-5E-2
Option: 2182 Line Sync{Boolean}=False	0E+0	1.228163869E-3	1.56E-1	1.228163869E-3	3.371767975E-6	2.47087151E-7	-1.586292E+2	-2.333890784E-7	-9.219679649E-8	8.0025E+0	8.0823E+0	8.65688E+1	6.8541E+1	3.84680368E-3	9.7E+1	1E+0	8E+0	1.8E+0	8.0059E+0	8.0929E+0	8.65688E+1	6.8541E+1	1.6E+0	8E+0	2.306172065E-2	1.4649E+0	1.3E-3	4E+1	-6E-2	-6E-2
Option: 2182 Reference Reading{Double Float}=0.000000	0E+0	1.228333574E-3	1.56E-1	1.228333574E-3	3.304332616E-6	3.814312169E-7	-1.662708E+2	-3.740558103E-7	-9.325052701E-8	8.0001E+0	8.0802E+0	8.58883E+1	6.8541E+1	-1.424499322E-3	9.8E+1	1E+0	8E+0	1.8E+0	8.0025E+0	8.0823E+0	8.65688E+1	6.8541E+1	1.6E+0	8E+0	3.84680368E-3	1.4649E+0	1.3E-3	4.1E+1	-7E-2	-7E-2
Option: 2182 Relative Mode{Boolean}=False	0E+0	1.228468208E-3	1.56E-1	1.228468208E-3	3.371767975E-6	5.047113244E-7	-1.712568E+2	-5.010227726E-7	-7.797198594E-8	7.9924E+0	8.0746E+0	8.59241E+1	6.8541E+1	-1.257923804E-2	9.9E+1	1E+0	8E+0	1.8E+0	8.0001E+0	8.0802E+0	8.58883E+1	6.8541E+1	1.6E+0	8E+0	-1.424499322E-3	1.4649E+0	1.3E-3	4.2E+1	-8E-2	-7.99E-2
Option: 2182 Trigger Delay{Cluster (Boolean,Double Float)}={'Auto':True,'Time(s)':0.000000}	0E+0	1.228670157E-3	1.56E-1	1.228670157E-3	3.371767975E-6	6.358929259E-7	-1.730244E+2	-6.327324414E-7	-7.849886534E-8	8.0061E+0	8.0856E+0	8.58883E+1	6.8541E+1	3.178461688E-3	1E+2	1E+0	8E+0	1.8E+0	7.9924E+0	8.0746E+0	8.59241E+1	6.8541E+1	1.6E+0	8E+0	-1.257923804E-2	1.4649E+0	1.3E-3	4.3E+1	-9E-2	-9E-2
Option: 2182 Trigger Source{Enum U16 ((Immediate,Timer,Manual,Bus,Trigger link))}=Bus	0E+0	1.228670157E-3	1.56E-1	1.228670157E-3	3.371767975E-6	7.755072E-7	-1.73478E+2	-7.728730858E-7	-8.956262574E-8	8.0166E+0	8.0974E+0	8.58166E+1	6.74909E+1	2.045267634E-2	1.01E+2	1E+0	8E+0	1.8E+0	8.0061E+0	8.0856E+0	8.58883E+1	6.8541E+1	1.6E+0	8E+0	3.178461688E-3	1.4649E+0	1.3E-3	4.4E+1	-1E-1	-9.99E-2
Option: 2182 Trigger Timer{Double Float}=0.000000	0E+0	1.228670157E-3	1.56E-1	1.228670157E-3	3.371767975E-6	7.665512684E-7	-1.741128E+2	-7.654973964E-7	-7.955259587E-8	7.9957E+0	8.0854E+0	8.5745E+1	6.74909E+1	2.74606701E-3	1.02E+2	1E+0	8E+0	1.8E+0	8.0166E+0	8.0974E+0	8.58166E+1	6.74909E+1	1.6E+0	8E+0	2.045267634E-2	1.4649E+0	1.3E-3	4.5E+1	-1E-1	-1E-1
Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	0E+0	1.230187608E-3	1.56E-1	1.230187608E-3	3.371767975E-6	3.384411045E-6	-1.785492E+2	-3.385992135E-6	-8.745519297E-8	7.9932E+0	8.0812E+0	8.6712E+1	6.74909E+1	-5.123563576E-3	1.03E+2	1E+0	8E+0	1.8E+0	7.9957E+0	8.0854E+0	8.5745E+1	6.74909E+1	1.6E+0	8E+0	2.74606701E-3	1.4649E+0	1.3E-3	4.6E+1	-3E-1	-3E-1
Option: 560 Enabled{Boolean}=False	0E+0	1.231367062E-3	1.56E-1	1.231367062E-3	3.371767975E-6	6.002804828E-6	-1.790916E+2	-6.005438094E-6	-9.69384E-8	7.9863E+0	8.081E+0	8.65688E+1	6.74909E+1	-1.004985347E-2	1.04E+2	1E+0	8E+0	1.8E+0	7.9932E+0	8.0812E+0	8.6712E+1	6.74909E+1	1.6E+0	8E+0	-5.123563576E-3	1.4649E+0	1.3E-3	4.7E+1	-5E-1	-4.998E-1
Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	0E+0	1.232884514E-3	1.56E-1	1.232884514E-3	3.371767975E-6	8.603269212E-6	-1.79346E+2	-8.605899649E-6	-9.904574792E-8	8.0049E+0	8.076E+0	8.65688E+1	6.74909E+1	-2.140997909E-2	1.05E+2	1E+0	8E+0	1.8E+0	7.9863E+0	8.081E+0	8.65688E+1	6.74909E+1	1.6E+0	8E+0	-1.004985347E-2	1.4649E+0	1.3E-3	4.8E+1	-7E-1	-6.999E-1
Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	0E+0	1.234570256E-3	1.56E-1	1.234570256E-3	3.371767975E-6	1.123590413E-5	-1.794816E+2	-1.123853739E-5	-1.027335643E-7	8.1999E+0	8.2755E+0	8.64613E+1	6.74909E+1	2.397494316E-1	1.06E+2	1E+0	8E+0	1.8E+0	8.0049E+0	8.076E+0	8.65688E+1	6.74909E+1	1.6E+0	8E+0	-2.140997909E-2	1.4649E+0	1.3E-3	4.9E+1	-9E-1	-8.999E-1
Option: 6221 Adjust Mode{Enum U16 ((Offset,Frequency,Amplitude))}=Offset	0E+0	1.236255999E-3	1.56E-1	1.236255999E-3	3.371767975E-6	1.38558592E-5	-1.7955E+2	-1.385849247E-5	-1.106361614E-7	7.5601E+0	7.8099E+0	8.6139E+1	6.74909E+1	-6.048036814E-1	1.07E+2	1E+0	8E+0	1.8E+0	8.1999E+0	8.2755E+0	8.64613E+1	6.74909E+1	1.6E+0	8E+0	2.397494316E-1	1.4649E+0	1.3E-3	5E+1	-1.1E+0	-1.0999E+0
Option: 6221 Amplitude{Double Float}=1.000000E-6	0E+0	1.238616321E-3	1.56E-1	1.238616321E-3	3.371767975E-6	1.646950688E-5	-1.79586E+2	-1.647210904E-5	-1.206459933E-7	7.8815E+0	7.9715E+0	8.61748E+1	6.74909E+1	-3.010585904E-1	1.08E+2	1E+0	8E+0	1.8E+0	7.5601E+0	7.8099E+0	8.6139E+1	6.74909E+1	1.6E+0	8E+0	-6.048036814E-1	1.4649E+0	1.3E-3	5.1E+1	-1.3E+0	-1.3E+0
Option: 6221 Compliance{Double Float}=10.000000	0E+0	1.241146349E-3	1.56E-1	1.241146349E-3	3.371767975E-6	1.911422767E-5	-1.796532E+2	-1.911682982E-5	-1.174849715E-7	8.0201E+0	8.0658E+0	8.66046E+1	6.74909E+1	1.930922419E-1	1.09E+2	1E+0	8E+0	1.8E+0	7.8815E+0	7.9715E+0	8.61748E+1	6.74909E+1	1.6E+0	8E+0	-3.010585904E-1	1.4649E+0	1.3E-3	5.2E+1	-1.5E+0	-1.4999E+0
Option: 6221 Duty Cycle{Double Float}=50.000000	0E+0	1.241146349E-3	1.56E-1	1.241146349E-3	3.371767975E-6	1.910472415E-5	-1.796256E+2	-1.910735459E-5	-1.2591425E-7	8.0216E+0	8.0716E+0	8.66046E+1	6.74909E+1	1.7460908E-1	1.1E+2	1E+0	8E+0	1.8E+0	8.0201E+0	8.0658E+0	8.66046E+1	6.74909E+1	1.6E+0	8E+0	1.930922419E-1	1.4649E+0	1.3E-3	5.3E+1	-1.5E+0	-1.5E+0
Option: 6221 External Trigger{Boolean}=False	0E+0	1.235413127E-3	1.56E-1	1.235413127E-3	3.371767975E-6	1.252929011E-5	-1.794996E+2	-1.253192055E-5	-1.106361332E-7	8.0025E+0	8.0912E+0	8.64971E+1	6.74909E+1	2.345909737E-2	1.11E+2	1E+0	8E+0	1.8E+0	8.0216E+0	8.0716E+0	8.66046E+1	6.74909E+1	1.6E+0	8E+0	1.7460908E-1	1.4649E+0	1.3E-3	5.4E+1	-1E+0	-1.0001E+0
Option: 6221 External Trigger Ignore Multiple{Boolean}=False	0E+0	1.231367062E-3	1.56E-1	1.231367062E-3	3.371767975E-6	5.9985933E-6	-1.789788E+2	-6.001226566E-6	-1.080019341E-7	7.8264E+0	7.9712E+0	8.59957E+1	6.74909E+1	-2.681113183E-1	1.12E+2	1E+0	8E+0	1.8E+0	8.0025E+0	8.0912E+0	8.64971E+1	6.74909E+1	1.6E+0	8E+0	2.345909737E-2	1.4649E+0	1.3E-3	5.5E+1	-5E-1	-5.001E-1
Option: 6221 Frequency{Double Float}=119.770000	
Option: 6221 Function{U16}=1	
Option: 6221 Function.__text__{String}=Sine	
Option: 6221 Idle Level{Double Float}=0.000000	
Option: 6221 Input trigger Line{U8}=5	
Option: 6221 Offset{Double Float}=0.000000	
Option: 6221 Output Trigger Line{U8}=4	
Option: 6221 Pass Through{Boolean}=True	
Option: 6221 Phase Marker{Boolean}=True	
Option: 6221 Phase Marker Phase{Double Float}=0.000000	
Option: 6221 Range Level{Double Float}=2.000000E-12	
Option: 6221 Ranging{U16}=1	
Option: 6221 Ranging.__text__{String}=Best	
Option: 6221 Update Clock{Double Float}=0.000000	
Option: 6221 VISA{Visa Refnum (Void)}=GPIB0::13::INSTR	
Option: Confirm Config{Boolean}=False	
Option: Control Panel Ref{LVObjVI Refnum (Void)}=	
Option: DAQ Global Channel{Boolean}=False	
Option: DAQ Input Rate{Double Float}=10000.000000	
Option: DAQ Input Samples{I32}=200	
Option: DAQ Measurement Channels{1D Array (Cluster (UserDefinedRefnumTag Refnum (Void),\tkDAQmxPhysChanTagType Tag,\tkDAQmxScaleTagType Tag,Boolean,Double Float,String))}=[]	
Option: Differential{I32}=10106	
Option: Differential.__text__{String}=Differential	
Option: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values))}=Function Generator	
Option: Lockin Standoff Time{Double Float}=0.000000	
Option: Paranoid Save Data{Boolean}=True	
Option: Plot Autoback Path{Path}=C:\\\\TEMP\\\\XY Multiparam\\\\Backup.txt	
Option: SR830  Ref Phase{Double Float}=0.000000	
Option: SR830  Synch Filter{Boolean}=False	
Option: SR830  Time Constant{I16}=8	
Option: SR830  Time Constant.__text__{String}=100 ms	
Option: SR830 2x Line Filter{Boolean}=True	
Option: SR830 Adjust Gains{Boolean}=False	
Option: SR830 Auto Gain Lower.__text__{String}=2 nV/fA	
Option: SR830 Auto Gain Upper.__text__{String}=1 V/uA	
Option: SR830 Auto Offset 1{Boolean}=False	
Option: SR830 Auto Offset 2{Boolean}=False	
Option: SR830 Autophase{Boolean}=False	
Option: SR830 DC Coupling?{Boolean}=False	
Option: SR830 Display 1{U16}=0	
Option: SR830 Display 1.__text__{String}=X	
Option: SR830 Display 2{U16}=0	
Option: SR830 Display 2.__text__{String}=Y	
Option: SR830 Dynamic Reserve{I16}=1	
Option: SR830 Dynamic Reserve.__text__{String}=Normal	
Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Option: SR830 Filter Slope{I32}=1	
Option: SR830 Filter Slope.__text__{String}=12 dB/oct	
Option: SR830 Gain{I32}=-1	
Option: SR830 Gain.__text__{String}=Auto Gain	
Option: SR830 Ground Shield?{Boolean}=False	
Option: SR830 Harmonic{I32}=1	
Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A	
Option: SR830 Line Filter{Boolean}=True	
Option: SR830 No Reset{Boolean}=False	
Option: SR830 Offset 1{Double Float}=0.000000	
Option: SR830 Offset 2{Double Float}=0.000000	
Option: SR830 Output Channel 1{Boolean}=False	
Option: SR830 Output Channel 2{Boolean}=False	
Option: SR830 Ratio 1{U16}=0	
Option: SR830 Ratio 1.__text__{String}=None	
Option: SR830 Ratio 2{U16}=0	
Option: SR830 Ratio 2.__text__{String}=None	
Option: SR830 Ref Amplitude{Double Float}=0.100000	
Option: SR830 Ref Frequency{Double Float}=1013.000000	
Option: SR830 Ref Source{Boolean}=False	
Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta]	
Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Option: SR830 VISA{Visa Refnum (Void)}=	
Option: Sense Autorange{Boolean}=False	
Option: Sense Range Level{Double Float}=0.100000	
Option: Sense Rate{Double Float}=1.000000	
Option:560 Comport{Visa Refnum (Void)}=COM1	
Option:560 Filter High Pass{U16}=0	
Option:560 Filter High Pass.__text__{String}=0.03	
Option:560 Filter Lowpass{U16}=0	
Option:560 Filter Lowpass.__text__{String}=0.03	
Option:560 Filter Mode{U16}=0	
Option:560 Filter Mode.__text__{String}=6 dB high pass	
Option:560 Invert{Boolean}=False	
Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Option:570 Enabled{Boolean}=False	
Option:570 Filter High Pass{U16}=0	
Option:570 Filter High Pass.__text__{String}=0.03	
Option:570 Filter Lowpass{U16}=0	
Option:570 Filter Lowpass.__text__{String}=0.03	
Option:570 Filter Mode{U16}=0	
Option:570 Filter Mode.__text__{String}=6 dB high pass	
Option:570 Gain Mode{U16}=0	
Option:570 Gain Mode.__text__{String}=Low Noise	
Option:570 Input Offset{U16}=0	
Option:570 Input Offset On{Boolean}=False	
Option:570 Input Offset.__text__{String}=1pA	
Option:570 Sensitivity{U16}=0	
Option:570 Sensitivity.__text__{String}=1pA/V	
Option:Debug On{Boolean}=False	
Option:GPIB 2182{Visa Refnum (Void)}=	
Option:Parallel Config Voltage Measurers{Boolean}=True	
Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Option:SR830 Settle Time{Double Float}=5.000000	
Option:Sense Digits{I32}=8	
Output Names{1D Array (String)}=['Offset','Rxx::R','Rxx::Theta','Rxx::X','Rxx::Y','Rxy::R','Rxy::Theta','Rxy::X','Rxy::Y','temperature: T1','temperature: T2','temperature: T3','temperature: T4','temperature: dT/dt','iterator','multi[0]:iterator','multi[0]:y','multi[0]:temperature: setpoint','multi[0]:temperature: T1','multi[0]:temperature: T2','multi[0]:temperature: T3','multi[0]:temperature: T4','multi[0]:temperature: heater','multi[0]:temperature: gas','multi[0]:temperature: dT/dt','multi[0]:temperature: current temperature','multi[0]:temperature: error','multi[1]:iterator','multi[1]:y','multi[1]:Control:Magnet Output']	
Parameter Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Parameter Select{U16}=6	
Parameter Select.__text__{String}=Multi-Parameter	
Paths{U32}=0	
Plot: Column Renames{1D Array (Cluster (String,String))}=[]	
Plot: No dups{Boolean}=False	
Plot: StdDevs{Boolean}=False	
Plotting Class{String}=Parameter Plot	
Plotting Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	
Plotting Select{U16}=1	
Plotting Select.__text__{String}=Parameter Plot	
Project Code{String}=Topological_Insulators	
Ref: Temperature Window{LVObjVI Refnum (Void)}=	
Ref:Control Subpanel{LVObjUnknown Refnum (Void)}=	
Ref:Main Screen{LVObjVI Refnum (Void)}=	
Ref:Plotting Subpanel{LVObjUnknown Refnum (Void)}=	
Ref:Toolbar{LVObjUnknown Refnum (Void)}=	
Ref:XY Subpanel{LVObjUnknown Refnum (Void)}=	
Rxx::R{Double Float}=0.001231	
Rxx::Theta{Double Float}=0.156000	
Rxx::X{Double Float}=0.001231	
Rxx::Y{Double Float}=3.371768E-6	
Rxx:Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	
Rxx:Option: 560 Enabled{Boolean}=False	
Rxx:Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	
Rxx:Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	
Rxx:Option: Lockin Standoff Time{Double Float}=0.000000	
Rxx:Option: Lockin Type{Enum U16 ((SRS 830,EG&G 5302))}=SRS 830	
Rxx:Option: SR803 Full Scale Reading{Double Float}=0.000000	
Rxx:Option: SR830  Ref Phase{Double Float}=0.000000	
Rxx:Option: SR830  Synch Filter{Boolean}=False	
Rxx:Option: SR830  Time Constant{I16}=8	
Rxx:Option: SR830 2x Line Filter{Boolean}=False	
Rxx:Option: SR830 Adjust Gains{Boolean}=False	
Rxx:Option: SR830 Auto Gain Lower{I32}=0	
Rxx:Option: SR830 Auto Gain Upper{I32}=26	
Rxx:Option: SR830 Auto Offset 1{Boolean}=False	
Rxx:Option: SR830 Auto Offset 2{Boolean}=False	
Rxx:Option: SR830 Autophase{Boolean}=False	
Rxx:Option: SR830 DC Coupling?{Boolean}=False	
Rxx:Option: SR830 Display 1{U16}=0	
Rxx:Option: SR830 Display 2{U16}=0	
Rxx:Option: SR830 Dynamic Reserve{I16}=2	
Rxx:Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Rxx:Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Rxx:Option: SR830 Filter Slope{I32}=3	
Rxx:Option: SR830 Gain{I32}=18	
Rxx:Option: SR830 Ground Shield?{Boolean}=False	
Rxx:Option: SR830 Harmonic{I32}=1	
Rxx:Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A-B	
Rxx:Option: SR830 Line Filter{Boolean}=False	
Rxx:Option: SR830 No Reset{Boolean}=False	
Rxx:Option: SR830 Offset 1{Double Float}=0.000000	
Rxx:Option: SR830 Offset 2{Double Float}=0.000000	
Rxx:Option: SR830 Output Channel 1{Boolean}=False	
Rxx:Option: SR830 Output Channel 2{Boolean}=False	
Rxx:Option: SR830 Ratio 1{U16}=0	
Rxx:Option: SR830 Ratio 2{U16}=0	
Rxx:Option: SR830 Ref Amplitude{Double Float}=0.100000	
Rxx:Option: SR830 Ref Frequency{Double Float}=1013.000000	
Rxx:Option: SR830 Ref Source{Boolean}=False	
Rxx:Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta,X,Y]	
Rxx:Option: SR830 Time Constant value{Double Float}=0.000000	
Rxx:Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Rxx:Option: SR830 VISA{Visa Refnum (Void)}=GPIB0::5::INSTR	
Rxx:Option:560 Comport{Visa Refnum (Void)}=COM1	
Rxx:Option:560 Filter High Pass{U16}=0	
Rxx:Option:560 Filter Lowpass{U16}=0	
Rxx:Option:560 Filter Mode{U16}=0	
Rxx:Option:560 Invert{Boolean}=False	
Rxx:Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Rxx:Option:570 Enabled{Boolean}=False	
Rxx:Option:570 Filter High Pass{U16}=0	
Rxx:Option:570 Filter Lowpass{U16}=0	
Rxx:Option:570 Filter Mode{U16}=0	
Rxx:Option:570 Gain Mode{U16}=0	
Rxx:Option:570 Input Offset{U16}=0	
Rxx:Option:570 Input Offset On{Boolean}=False	
Rxx:Option:570 Sensitivity{U16}=0	
Rxx:Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Rxx:Option:SR830 Autogain Lower Threshold{Double Float}=0.100000	
Rxx:Option:SR830 Autogain Standoff{Double Float}=3.000000	
Rxx:Option:SR830 Autogain Upper Threshold{Double Float}=0.900000	
Rxx:Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Rxx:Option:SR830 Settle Time{Double Float}=0.000000	
Rxy::R{Double Float}=5.998593E-6	
Rxy::Theta{Double Float}=-178.978800	
Rxy::X{Double Float}=-6.001227E-6	
Rxy::Y{Double Float}=-1.080019E-7	
Rxy:Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	
Rxy:Option: 560 Enabled{Boolean}=False	
Rxy:Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	
Rxy:Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	
Rxy:Option: Lockin Standoff Time{Double Float}=0.000000	
Rxy:Option: Lockin Type{Enum U16 ((SRS 830,EG&G 5302))}=SRS 830	
Rxy:Option: SR803 Full Scale Reading{Double Float}=0.000000	
Rxy:Option: SR830  Ref Phase{Double Float}=0.000000	
Rxy:Option: SR830  Synch Filter{Boolean}=False	
Rxy:Option: SR830  Time Constant{I16}=8	
Rxy:Option: SR830 2x Line Filter{Boolean}=False	
Rxy:Option: SR830 Adjust Gains{Boolean}=False	
Rxy:Option: SR830 Auto Gain Lower{I32}=0	
Rxy:Option: SR830 Auto Gain Upper{I32}=26	
Rxy:Option: SR830 Auto Offset 1{Boolean}=False	
Rxy:Option: SR830 Auto Offset 2{Boolean}=False	
Rxy:Option: SR830 Autophase{Boolean}=False	
Rxy:Option: SR830 DC Coupling?{Boolean}=False	
Rxy:Option: SR830 Display 1{U16}=0	
Rxy:Option: SR830 Display 2{U16}=1	
Rxy:Option: SR830 Dynamic Reserve{I16}=2	
Rxy:Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Rxy:Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Rxy:Option: SR830 Filter Slope{I32}=3	
Rxy:Option: SR830 Gain{I32}=18	
Rxy:Option: SR830 Ground Shield?{Boolean}=False	
Rxy:Option: SR830 Harmonic{I32}=1	
Rxy:Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A-B	
Rxy:Option: SR830 Line Filter{Boolean}=False	
Rxy:Option: SR830 No Reset{Boolean}=False	
Rxy:Option: SR830 Offset 1{Double Float}=0.000000	
Rxy:Option: SR830 Offset 2{Double Float}=0.000000	
Rxy:Option: SR830 Output Channel 1{Boolean}=False	
Rxy:Option: SR830 Output Channel 2{Boolean}=False	
Rxy:Option: SR830 Ratio 1{U16}=0	
Rxy:Option: SR830 Ratio 2{U16}=0	
Rxy:Option: SR830 Ref Amplitude{Double Float}=0.100000	
Rxy:Option: SR830 Ref Frequency{Double Float}=1013.000000	
Rxy:Option: SR830 Ref Source{Boolean}=False	
Rxy:Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta,X,Y]	
Rxy:Option: SR830 Time Constant value{Double Float}=0.000000	
Rxy:Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Rxy:Option: SR830 VISA{Visa Refnum (Void)}=GPIB0::6::INSTR	
Rxy:Option:560 Comport{Visa Refnum (Void)}=COM1	
Rxy:Option:560 Filter High Pass{U16}=0	
Rxy:Option:560 Filter Lowpass{U16}=0	
Rxy:Option:560 Filter Mode{U16}=0	
Rxy:Option:560 Invert{Boolean}=False	
Rxy:Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Rxy:Option:570 Enabled{Boolean}=False	
Rxy:Option:570 Filter High Pass{U16}=0	
Rxy:Option:570 Filter Lowpass{U16}=0	
Rxy:Option:570 Filter Mode{U16}=0	
Rxy:Option:570 Gain Mode{U16}=0	
Rxy:Option:570 Input Offset{U16}=0	
Rxy:Option:570 Input Offset On{Boolean}=False	
Rxy:Option:570 Sensitivity{U16}=0	
Rxy:Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Rxy:Option:SR830 Autogain Lower Threshold{Double Float}=0.100000	
Rxy:Option:SR830 Autogain Standoff{Double Float}=3.000000	
Rxy:Option:SR830 Autogain Upper Threshold{Double Float}=0.900000	
Rxy:Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Rxy:Option:SR830 Settle Time{Double Float}=0.000000	
Sample ID{String}=MBE202221213_PA_D1 750C Cracker WAL	
Save:Filename{String}=${X-Y Class} ${2nd Parameter Class} ${iterator}{%04d} ${y}{%04.2g}.txt	
Save:Final Filename{String}=${X-Y Class} ${2nd Parameter Class} .txt	
Save:Final path{Path}=C:\\\\Data\\\\${Project Code}\\\\${User}\\\\${Sample ID}\\\\${Measurement Timestamp}{%Y%m%d}\\\\${X-Y Class}	
Save:Path{Path}=C:\\\\Data\\\\${Project Code}\\\\${User}\\\\${Sample ID}\\\\${Measurement Timestamp}{%Y%m%d}\\\\${X-Y Class}	
Startup path{Path}=C:\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV	
Sub Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Sweep Step{I32}=3	
T Control Measure.__text__{1D Array (String)}=['temperature: T1','temperature: T2','temperature: T3','temperature: T4','temperature: dT/dt']	
Timestamp{Timestamp}=<19:45:43.764 17/05/2023>T	
Toolbar{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Unaved Data{Boolean}=True	
Unsaved Data{Boolean}=False	
User{String}=Craig	
X-Y Class{String}=6221-Lockin-DAQ	
X-Y Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	
d(Offset){Double Float}=0.000000	
d(Rxx::R){Double Float}=0.000000	
d(Rxx::Theta){Double Float}=0.000000	
d(Rxx::X){Double Float}=0.000000	
d(Rxx::Y){Double Float}=4.735058E-22	
d(Rxy::R){Double Float}=7.770184E-9	
d(Rxy::Theta){Double Float}=0.097525	
d(Rxy::X){Double Float}=7.771141E-9	
d(Rxy::Y){Double Float}=1.037078E-8	
iterate result{U16}=5	
iterator{I32}=112	
multi[0]:Control: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values,Adaptive Step Ramp))}=List of Values	
multi[0]:Control: Monitor Update Timeout{Double Float}=0.010000	
multi[0]:Control: Open T Window{Boolean}=False	
multi[0]:Control: Reverse Temperature Sense{Boolean}=False	
multi[0]:Iterator{I32}=0	
multi[0]:Ref: Temperature Window{LVObjVI Refnum (Void)}=	
multi[0]:iterate result{U16}=0	
multi[0]:iterator{I32}=1	
multi[0]:temperature:  rate window{Double Float}=120.000000	
multi[0]:temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[0]:temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
multi[0]:temperature: T1{Double Float}=8.044800	
multi[0]:temperature: T2{Double Float}=8.093100	
multi[0]:temperature: T3{Double Float}=86.497100	
multi[0]:temperature: T4{Double Float}=67.490900	
multi[0]:temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
multi[0]:temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
multi[0]:temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
multi[0]:temperature: current temperature{Double Float}=1.464900	
multi[0]:temperature: current temperature 2{Double Float}=287.100000	
multi[0]:temperature: dT/dt{Double Float}=0.151055	
multi[0]:temperature: error{Double Float}=0.001300	
multi[0]:temperature: gas{Double Float}=8.000000	
multi[0]:temperature: gas control{Boolean}=False	
multi[0]:temperature: gas control 2{Boolean}=False	
multi[0]:temperature: gass boost{I8}=0	
multi[0]:temperature: gass boost 2{I8}=0	
multi[0]:temperature: gast flow{I16}=0	
multi[0]:temperature: gast flow 2{I16}=7	
multi[0]:temperature: heater{Double Float}=1.600000	
multi[0]:temperature: heater output{Double Float}=0.000000	
multi[0]:temperature: heater output 2{Double Float}=0.000000	
multi[0]:temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
multi[0]:temperature: monitor timeout{Double Float}=0.010000	
multi[0]:temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
multi[0]:temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
multi[0]:temperature: ramp rate{Double Float}=8.000000	
multi[0]:temperature: ramp rate 2{Double Float}=0.000000	
multi[0]:temperature: ramp target{Double Float}=20.000000	
multi[0]:temperature: ramp target 2{Double Float}=0.000000	
multi[0]:temperature: ramping{Boolean}=False	
multi[0]:temperature: setpoint{Double Float}=1.800000	
multi[0]:temperature: setpoint 2{Double Float}=287.100000	
multi[0]:temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
multi[0]:temperature: stability error{Extended Float}=0.040000	
multi[0]:temperature: stability script{String}=	
multi[0]:temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
multi[0]:temperature: temp control mode{U16}=2	
multi[0]:temperature: temp control mode 2{U16}=3	
multi[0]:temperature: temp control mode 2.__text__{String}=Open Loop	
multi[0]:temperature: temp control mode.__text__{String}=Zone	
multi[0]:temperature: temp control sensor{U16}=0	
multi[0]:temperature: temp control sensor 2{U16}=0	
multi[0]:temperature: temp control sensor 2.__text__{String}=Sensor 1	
multi[0]:temperature: temp control sensor.__text__{String}=Sensor A	
multi[0]:temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
multi[0]:temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
multi[0]:temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
multi[0]:temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
multi[0]:temperature: temp loop{U16}=0	
multi[0]:temperature: temp loop 2{U16}=0	
multi[0]:temperature: temp loop 2.__text__{String}=Heater	
multi[0]:temperature: temp loop.__text__{String}=Loop 1	
multi[0]:temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
multi[0]:temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[0]:temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[0]:temperature:error for gas boost{Double Float}=0.000000	
multi[0]:temperature:error for gas boost 2{Double Float}=0.000000	
multi[0]:temperature:heater range{U16}=2	
multi[0]:temperature:heater range 2{U16}=0	
multi[0]:temperature:heater range 2.__text__{String}=Off	
multi[0]:temperature:heater range.__text__{String}=40mW	
multi[0]:temperature:history window{Extended Float}=300.000000	
multi[0]:temperature:is stable?{Boolean}=False	
multi[0]:temperature:monitor{Boolean}=True	
multi[0]:temperature:ramping{Boolean}=False	
multi[0]:temperature:ramping on{Boolean}=False	
multi[0]:temperature:ramping on 2{Boolean}=False	
multi[0]:temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
multi[0]:temperature:stability code{U32}=6618880	
multi[0]:temperature:stability rate{Extended Float}=0.040000	
multi[0]:y{Double Float}=8.000000	
multi[1]:Control: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values,Adaptive Step Ramp))}=Multi-Segment Ramp	
multi[1]:Control: Gate delay{Double Float}=0.000000	
multi[1]:Control: Monitor Update Timeout{Double Float}=0.010000	
multi[1]:Control: Open T Window{Boolean}=False	
multi[1]:Control: Reverse Temperature Sense{Boolean}=False	
multi[1]:Control:Magnet Output{Double Float}=-0.000100	
multi[1]:Iterator{I32}=0	
multi[1]:Magnet: Final Switch Heater{Enum U8 ((False,True,Mixed))}=	
multi[1]:Magnet: Power Supply{Enum U16 ((IPS120,LS625,PS110,Hg iPS,SMS Series,Cryomagnetics 4G,DMG Little CryoFree,DMG Big CryoFree))}=Hg iPS	
multi[1]:Magnet: Rate{Double Float}=0.500000	
multi[1]:Magnet: Units{Enum U16 ((Field,Current))}=Field	
multi[1]:Magnet: VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[1]:Multi-segment_Stage{I32}=0	
multi[1]:Multi-segment_Stage_Changed{Boolean}=False	
multi[1]:Ref: Temperature Window{LVObjVI Refnum (Void)}=	
multi[1]:iterate result{U16}=4	
multi[1]:iterator{I32}=57	
multi[1]:measure point{Boolean}=False	
multi[1]:temperature:  rate window{Double Float}=120.000000	
multi[1]:temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[1]:temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
multi[1]:temperature: T1{Double Float}=1.842400	
multi[1]:temperature: T2{Double Float}=1.465600	
multi[1]:temperature: T3{Double Float}=86.318100	
multi[1]:temperature: T4{Double Float}=66.769200	
multi[1]:temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
multi[1]:temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
multi[1]:temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
multi[1]:temperature: current temperature{Double Float}=1.465600	
multi[1]:temperature: current temperature 2{Double Float}=287.100000	
multi[1]:temperature: dT/dt{Double Float}=-0.001864	
multi[1]:temperature: gas control{Boolean}=False	
multi[1]:temperature: gas control 2{Boolean}=False	
multi[1]:temperature: gass boost{I8}=0	
multi[1]:temperature: gass boost 2{I8}=0	
multi[1]:temperature: gast flow{I16}=0	
multi[1]:temperature: gast flow 2{I16}=7	
multi[1]:temperature: heater output{Double Float}=0.000000	
multi[1]:temperature: heater output 2{Double Float}=0.000000	
multi[1]:temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
multi[1]:temperature: monitor timeout{Double Float}=1.000000	
multi[1]:temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
multi[1]:temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
multi[1]:temperature: ramp rate{Double Float}=8.000000	
multi[1]:temperature: ramp rate 2{Double Float}=0.000000	
multi[1]:temperature: ramp target{Double Float}=20.000000	
multi[1]:temperature: ramp target 2{Double Float}=0.000000	
multi[1]:temperature: ramping{Boolean}=False	
multi[1]:temperature: setpoint{Double Float}=1.800000	
multi[1]:temperature: setpoint 2{Double Float}=287.100000	
multi[1]:temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
multi[1]:temperature: stability error{Extended Float}=0.040000	
multi[1]:temperature: stability script{String}=	
multi[1]:temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
multi[1]:temperature: temp control mode{U16}=2	
multi[1]:temperature: temp control mode 2{U16}=3	
multi[1]:temperature: temp control mode 2.__text__{String}=Open Loop	
multi[1]:temperature: temp control mode.__text__{String}=Zone	
multi[1]:temperature: temp control sensor{U16}=0	
multi[1]:temperature: temp control sensor 2{U16}=0	
multi[1]:temperature: temp control sensor 2.__text__{String}=Sensor 1	
multi[1]:temperature: temp control sensor.__text__{String}=Sensor A	
multi[1]:temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
multi[1]:temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
multi[1]:temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
multi[1]:temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
multi[1]:temperature: temp loop{U16}=0	
multi[1]:temperature: temp loop 2{U16}=0	
multi[1]:temperature: temp loop 2.__text__{String}=Heater	
multi[1]:temperature: temp loop.__text__{String}=Loop 1	
multi[1]:temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
multi[1]:temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[1]:temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[1]:temperature:error for gas boost{Double Float}=0.000000	
multi[1]:temperature:error for gas boost 2{Double Float}=0.000000	
multi[1]:temperature:heater range{U16}=2	
multi[1]:temperature:heater range 2{U16}=0	
multi[1]:temperature:heater range 2.__text__{String}=Off	
multi[1]:temperature:heater range.__text__{String}=40mW	
multi[1]:temperature:history window{Extended Float}=300.000000	
multi[1]:temperature:is stable?{Boolean}=True	
multi[1]:temperature:monitor{Boolean}=True	
multi[1]:temperature:ramping{Boolean}=False	
multi[1]:temperature:ramping on{Boolean}=False	
multi[1]:temperature:ramping on 2{Boolean}=False	
multi[1]:temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
multi[1]:temperature:stability code{U32}=6618880	
multi[1]:temperature:stability rate{Extended Float}=0.040000	
multi[1]:y{Double Float}=0.000000	
parameter: Termination{String}=False	
parameter: delta time{Double Float}=1.000000	
parameter: progress{Double Float}=100.000000	
temperature:  rate window{Double Float}=120.000000	
temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
temperature: T1{Double Float}=8.044800	
temperature: T2{Double Float}=8.093100	
temperature: T3{Double Float}=86.497100	
temperature: T4{Double Float}=67.490900	
temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
temperature: current temperature{Double Float}=1.464900	
temperature: current temperature 2{Double Float}=287.100000	
temperature: dT/dt{Double Float}=0.151055	
temperature: gas control{Boolean}=False	
temperature: gas control 2{Boolean}=False	
temperature: gass boost{I8}=0	
temperature: gass boost 2{I8}=0	
temperature: gast flow{I16}=0	
temperature: gast flow 2{I16}=7	
temperature: heater output{Double Float}=0.000000	
temperature: heater output 2{Double Float}=0.000000	
temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
temperature: monitor timeout{Double Float}=0.010000	
temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
temperature: ramp rate{Double Float}=8.000000	
temperature: ramp rate 2{Double Float}=0.000000	
temperature: ramp target{Double Float}=20.000000	
temperature: ramp target 2{Double Float}=0.000000	
temperature: ramping{Boolean}=False	
temperature: setpoint{Double Float}=1.800000	
temperature: setpoint 2{Double Float}=287.100000	
temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
temperature: stability error{Extended Float}=0.040000	
temperature: stability script{String}=	
temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
temperature: temp control mode{U16}=2	
temperature: temp control mode 2{U16}=3	
temperature: temp control mode 2.__text__{String}=Open Loop	
temperature: temp control mode.__text__{String}=Zone	
temperature: temp control sensor{U16}=0	
temperature: temp control sensor 2{U16}=0	
temperature: temp control sensor 2.__text__{String}=Sensor 1	
temperature: temp control sensor.__text__{String}=Sensor A	
temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
temperature: temp loop{U16}=0	
temperature: temp loop 2{U16}=0	
temperature: temp loop 2.__text__{String}=Heater	
temperature: temp loop.__text__{String}=Loop 1	
temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
temperature:error for gas boost{Double Float}=0.000000	
temperature:error for gas boost 2{Double Float}=0.000000	
temperature:heater range{U16}=2	
temperature:heater range 2{U16}=0	
temperature:heater range 2.__text__{String}=Off	
temperature:heater range.__text__{String}=40mW	
temperature:history window{Extended Float}=300.000000	
temperature:is stable?{Boolean}=False	
temperature:monitor{Boolean}=True	
temperature:ramping{Boolean}=False	
temperature:ramping on{Boolean}=False	
temperature:ramping on 2{Boolean}=False	
temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
temperature:stability code{U32}=6618880	
temperature:stability rate{Extended Float}=0.040000	
y{Double Float}=8.000000	
