TDI Format 1.5	Offset	Rxx::R	Rxx::Theta	Rxx::X	Rxx::Y	Rxy::R	Rxy::Theta	Rxy::X	Rxy::Y	temperature: T1	temperature: T2	temperature: T3	temperature: T4	temperature: dT/dt	iterator	multi[0]:iterator	multi[0]:y	multi[0]:temperature: setpoint	multi[0]:temperature: T1	multi[0]:temperature: T2	multi[0]:temperature: T3	multi[0]:temperature: T4	multi[0]:temperature: heater	multi[0]:temperature: gas	multi[0]:temperature: dT/dt	multi[0]:temperature: current temperature	multi[0]:temperature: error	multi[1]:iterator	multi[1]:y	multi[1]:Control:Magnet Output
2nd Parameter Class{String}=Multi-Parameter	0E+0	1.226309835E-3	1.56E-1	1.226309835E-3	3.338050296E-6	5.879510861E-7	-8.4696E+0	5.816289858E-7	-8.798210066E-8	3.0051E+0	3.0862E+0	8.59957E+1	6.43465E+1	-4.603137728E-3	3.37E+2	6E+0	3E+0	3E+0	3.0073E+0	3.0854E+0	8.60315E+1	6.43465E+1	2.8E+0	3E+0	-6.128051318E-3	3.0081E+0	-8.1E-3	0E+0	0E+0	0E+0
2nd Parameter Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	0E+0	1.232884514E-3	1.548E-1	1.232884514E-3	3.338050296E-6	7.193982769E-6	-4.848E-1	7.193982769E-6	-6.164008204E-8	2.9768E+0	3.0629E+0	8.59241E+1	6.43465E+1	-4.660173506E-2	3.38E+2	6E+0	3E+0	1.8E+0	3.0051E+0	3.0862E+0	8.59957E+1	6.43465E+1	2.8E+0	3E+0	-4.603137728E-3	1.4649E+0	-8.1E-3	1E+0	5E-1	4.999E-1
Analysis Class{String}=Basic Plot	0E+0	1.23709887E-3	1.56E-1	1.23709887E-3	3.371767975E-6	1.377788795E-5	-1.812E-1	1.377788795E-5	-4.583491611E-8	3.0052E+0	3.0912E+0	8.56017E+1	6.43465E+1	-4.604684073E-4	3.39E+2	6E+0	3E+0	1.8E+0	2.9768E+0	3.0629E+0	8.59241E+1	6.43465E+1	2.8E+0	3E+0	-4.660173506E-2	1.4649E+0	-8.1E-3	2E+0	1E+0	9.999E-1
Analysis Class Path{Path}=C\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV\\\\plugins\\\\Plotting\\\\Plotting_Base_class\\\\Plotting_Base.lvclass	0E+0	1.243168675E-3	1.56E-1	1.243168675E-3	3.371767975E-6	2.040653602E-5	-8.64E-2	2.040653602E-5	-3.161027527E-8	2.7224E+0	2.7917E+0	8.59957E+1	6.43465E+1	-1.353678823E+0	3.4E+2	6E+0	3E+0	1.8E+0	3.0052E+0	3.0912E+0	8.56017E+1	6.43465E+1	2.8E+0	3E+0	-4.604684073E-4	1.4649E+0	-8.1E-3	3E+0	1.5E+0	1.4998E+0
Analysis.# pre-routines{I32}=5	0E+0	1.243168675E-3	1.56E-1	1.243168675E-3	3.371767975E-6	2.042180953E-5	-8.52E-2	2.042180953E-5	-3.266394923E-8	2.7456E+0	2.8274E+0	8.59957E+1	6.43465E+1	-1.317221999E+0	3.41E+2	6E+0	3E+0	1.8E+0	2.7224E+0	2.7917E+0	8.59957E+1	6.43465E+1	2.8E+0	3E+0	-1.353678823E+0	1.4649E+0	-8.1E-3	4E+0	1.5E+0	1.5E+0
Analysis:Pre[0]:T Control Measure{1D Array (I32)}=[1,2,3,4,7]	0E+0	1.240302064E-3	1.56E-1	1.240302064E-3	3.371767975E-6	1.774600433E-5	-1.152E-1	1.774600433E-5	-3.687875819E-8	3.0005E+0	3.043E+0	8.59599E+1	6.43465E+1	3.406647444E-1	3.42E+2	6E+0	3E+0	1.8E+0	2.7456E+0	2.8274E+0	8.59957E+1	6.43465E+1	2.8E+0	3E+0	-1.317221999E+0	1.4649E+0	-8.1E-3	5E+0	1.3E+0	1.3002E+0
Autosave Tabs{Enum U32 ((XY Measurement Save,Parameter Plot Save 2))}=Parameter Plot Save 2	0E+0	1.238111447E-3	1.56E-1	1.238111447E-3	3.371767975E-6	1.509497615E-5	-1.368E-1	1.509497615E-5	-3.793240387E-8	2.9905E+0	3.0612E+0	8.59241E+1	6.43465E+1	7.20795542E-2	3.43E+2	6E+0	3E+0	1.8E+0	3.0005E+0	3.043E+0	8.59599E+1	6.43465E+1	2.8E+0	3E+0	3.406647444E-1	1.4649E+0	-8.1E-3	6E+0	1.1E+0	1.1001E+0
Control:Magnet Output{Double Float}=-0.007000	0E+0	1.236087707E-3	1.56E-1	1.236087707E-3	3.371767975E-6	1.246448802E-5	-2.16E-1	1.246448802E-5	-4.846914343E-8	3.0197E+0	3.0728E+0	8.59241E+1	6.43465E+1	-1.429367624E-2	3.44E+2	6E+0	3E+0	1.8E+0	2.9905E+0	3.0612E+0	8.59241E+1	6.43465E+1	2.8E+0	3E+0	7.20795542E-2	1.4649E+0	-8.1E-3	7E+0	9E-1	9.001E-1
Control:Magnet Rate{Double Float}=0.500000	0E+0	1.234401965E-3	1.56E-1	1.234401965E-3	3.371767975E-6	9.820256551E-6	-2.472E-1	9.820256551E-6	-4.372759649E-8	3.0377E+0	3.0679E+0	8.5745E+1	6.43465E+1	-4.032517597E-2	3.45E+2	6E+0	3E+0	1.8E+0	3.0197E+0	3.0728E+0	8.59241E+1	6.43465E+1	2.8E+0	3E+0	-1.429367624E-2	1.4649E+0	-8.1E-3	8E+0	7E-1	7.002E-1
Display Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	0E+0	1.232884514E-3	1.56E-1	1.232884514E-3	3.371767975E-6	7.186606231E-6	-4.728E-1	7.186606231E-6	-6.058640808E-8	2.9788E+0	3.1075E+0	8.61032E+1	6.43465E+1	2.123562805E-2	3.46E+2	6E+0	3E+0	1.8E+0	3.0377E+0	3.0679E+0	8.5745E+1	6.43465E+1	2.8E+0	3E+0	-4.032517597E-2	1.4649E+0	-8.1E-3	9E+0	5E-1	5.001E-1
Elapsed Time{Double Float}=12790.950867	0E+0	1.231671401E-3	1.56E-1	1.231671401E-3	3.371767975E-6	4.532913678E-6	-1.0368E+0	4.532913678E-6	-8.376740483E-8	2.9921E+0	3.1122E+0	8.59957E+1	6.43465E+1	3.595213965E-2	3.47E+2	6E+0	3E+0	1.8E+0	2.9788E+0	3.1075E+0	8.61032E+1	6.43465E+1	2.8E+0	3E+0	2.123562805E-2	1.4649E+0	-8.1E-3	1E+1	3E-1	3E-1
File:Autodel{Boolean}=True	0E+0	1.229849611E-3	1.56E-1	1.229849611E-3	3.371767975E-6	1.872384815E-6	-2.4948E+0	1.870803725E-6	-8.324044058E-8	2.9299E+0	3.049E+0	8.59599E+1	6.43465E+1	-6.543387473E-2	3.48E+2	6E+0	3E+0	1.8E+0	2.9921E+0	3.1122E+0	8.59957E+1	6.43465E+1	2.8E+0	3E+0	3.595213965E-2	1.4649E+0	-8.1E-3	1.1E+1	1E-1	1.001E-1
File:Autosave{Boolean}=False	0E+0	1.22968132E-3	1.56E-1	1.22968132E-3	3.371767975E-6	1.882394619E-6	-2.1516E+0	1.880816357E-6	-7.217684989E-8	3.0285E+0	3.0984E+0	8.59599E+1	6.43465E+1	9.250585921E-3	3.49E+2	6E+0	3E+0	1.8E+0	2.9299E+0	3.049E+0	8.59599E+1	6.43465E+1	2.8E+0	3E+0	-6.543387473E-2	1.4649E+0	-8.1E-3	1.2E+1	1E-1	1E-1
File:Export Config{Boolean}=True	0E+0	1.22968132E-3	1.56E-1	1.22968132E-3	3.270614936E-6	1.750686082E-6	-2.3436E+0	1.749102162E-6	-7.270364444E-8	2.9697E+0	3.0876E+0	8.59599E+1	6.43465E+1	8.40222463E-3	3.5E+2	6E+0	3E+0	1.8E+0	3.0285E+0	3.0984E+0	8.59599E+1	6.43465E+1	2.8E+0	3E+0	9.250585921E-3	1.4649E+0	-8.1E-3	1.3E+1	9E-2	9.01E-2
File:Final Autosave{Boolean}=True	0E+0	1.229513028E-3	1.56E-1	1.229513028E-3	3.371767975E-6	1.630568438E-6	-2.8476E+0	1.628990176E-6	-8.271367431E-8	2.9787E+0	3.0602E+0	8.59241E+1	6.43465E+1	-3.732184321E-2	3.51E+2	6E+0	3E+0	1.8E+0	2.9697E+0	3.0876E+0	8.59599E+1	6.43465E+1	2.8E+0	3E+0	8.40222463E-3	1.4649E+0	-8.1E-3	1.4E+1	8E-2	8E-2
Filter:Enable{Enum U16 ((None,Analog,Digital,Analog&Digitial))}=None	0E+0	1.229344737E-3	1.56E-1	1.229344737E-3	3.371767975E-6	1.485687916E-6	-2.8716E+0	1.484106825E-6	-7.586475116E-8	2.9814E+0	3.0745E+0	8.59599E+1	6.43465E+1	-1.901648566E-2	3.52E+2	6E+0	3E+0	1.8E+0	2.9787E+0	3.0602E+0	8.59241E+1	6.43465E+1	2.8E+0	3E+0	-3.732184321E-2	1.4649E+0	-8.1E-3	1.5E+1	7E-2	7E-2
Filter:Points{I32}=1	0E+0	1.22900674E-3	1.56E-1	1.22900674E-3	3.371767975E-6	1.370836521E-6	-3.8592E+0	1.367675471E-6	-9.377737813E-8	3.0595E+0	3.1132E+0	8.59599E+1	6.43465E+1	4.01285924E-2	3.53E+2	6E+0	3E+0	1.8E+0	2.9814E+0	3.0745E+0	8.59599E+1	6.43465E+1	2.8E+0	3E+0	-1.901648566E-2	1.4649E+0	-8.1E-3	1.6E+1	6E-2	6.01E-2
Filter:Type{U16}=1	0E+0	1.228838449E-3	1.56E-1	1.228838449E-3	3.304332616E-6	1.236488495E-6	-3.4932E+0	1.233854381E-6	-7.691836855E-8	3.0898E+0	3.1448E+0	8.57092E+1	6.43465E+1	8.988960832E-2	3.54E+2	6E+0	3E+0	1.8E+0	3.0595E+0	3.1132E+0	8.59599E+1	6.43465E+1	2.8E+0	3E+0	4.01285924E-2	1.4649E+0	-8.1E-3	1.7E+1	5E-2	5.01E-2
Filter:Type.__text__{String}=Repeat	0E+0	1.228838449E-3	1.56E-1	1.228838449E-3	3.371767975E-6	1.222790989E-6	-3.7524E+0	1.220156309E-6	-8.165994378E-8	3.0002E+0	3.0756E+0	8.56734E+1	6.43465E+1	-1.253194734E-2	3.55E+2	6E+0	3E+0	1.8E+0	3.0898E+0	3.1448E+0	8.57092E+1	6.43465E+1	2.8E+0	3E+0	8.988960832E-2	1.4649E+0	-8.1E-3	1.8E+1	5E-2	5.01E-2
Filter:Window{Double Float}=1.000000	0E+0	1.228670157E-3	1.56E-1	1.228670157E-3	3.371767975E-6	1.15746309E-6	-4.0332E+0	1.155355629E-6	-8.324049714E-8	3.0641E+0	3.1172E+0	8.56734E+1	6.43465E+1	5.113244429E-2	3.56E+2	6E+0	3E+0	1.8E+0	3.0002E+0	3.0756E+0	8.56734E+1	6.43465E+1	2.8E+0	3E+0	-1.253194734E-2	1.4649E+0	-8.1E-3	1.9E+1	4.5E-2	4.49E-2
Iterator{I32}=0	0E+0	1.228670157E-3	1.56E-1	1.228670157E-3	3.371767975E-6	1.09740342E-6	-4.0068E+0	1.095296525E-6	-7.849892191E-8	2.9909E+0	3.1051E+0	8.5745E+1	6.43465E+1	3.141041473E-2	3.57E+2	6E+0	3E+0	1.8E+0	3.0641E+0	3.1172E+0	8.56734E+1	6.43465E+1	2.8E+0	3E+0	5.113244429E-2	1.4649E+0	-8.1E-3	2E+1	4E-2	3.99E-2
Magnet: Control Mode{Boolean}=False	0E+0	1.228333574E-3	1.56E-1	1.228333574E-3	3.371767975E-6	1.031022781E-6	-3.588E+0	1.028915037E-6	-6.638157241E-8	2.9787E+0	3.0871E+0	8.57092E+1	6.43465E+1	-8.651314303E-3	3.58E+2	6E+0	3E+0	1.8E+0	2.9909E+0	3.1051E+0	8.5745E+1	6.43465E+1	2.8E+0	3E+0	3.141041473E-2	1.4649E+0	-8.1E-3	2.1E+1	3.5E-2	3.5E-2
Magnet: Final Switch Heater{Enum U8 ((False,True,Mixed))}=	0E+0	1.228163869E-3	1.56E-1	1.228163869E-3	3.371767975E-6	9.530509648E-7	-5.3532E+0	9.488360427E-7	-9.008944857E-8	2.9831E+0	3.0674E+0	8.57808E+1	6.43465E+1	-3.755613044E-2	3.59E+2	6E+0	3E+0	1.8E+0	2.9787E+0	3.0871E+0	8.57092E+1	6.43465E+1	2.8E+0	3E+0	-8.651314303E-3	1.4649E+0	-8.1E-3	2.2E+1	3E-2	3E-2
Magnet: Power Supply{Enum U16 ((IPS120,LS625,PS110,Hg iPS,SMS Series,Cryomagnetics 4G,DMG Little CryoFree,DMG Big CryoFree))}=Hg iPS	0E+0	1.227995577E-3	1.56E-1	1.227995577E-3	3.371767975E-6	8.887766554E-7	-4.98E+0	8.856156053E-7	-7.797201422E-8	3.0397E+0	3.1046E+0	8.58166E+1	6.43465E+1	1.495632529E-2	3.6E+2	6E+0	3E+0	1.8E+0	2.9831E+0	3.0674E+0	8.57808E+1	6.43465E+1	2.8E+0	3E+0	-3.755613044E-2	1.4649E+0	-8.1E-3	2.3E+1	2.5E-2	2.49E-2
Magnet: Rate{Double Float}=0.500000	0E+0	1.227658995E-3	1.56E-1	1.227658995E-3	3.338050296E-6	8.192344005E-7	-5.8356E+0	8.150197613E-7	-8.482105051E-8	3.0005E+0	3.0785E+0	8.61032E+1	6.43465E+1	-1.98552981E-2	3.61E+2	6E+0	3E+0	1.8E+0	3.0397E+0	3.1046E+0	8.58166E+1	6.43465E+1	2.8E+0	3E+0	1.495632529E-2	1.4649E+0	-8.1E-3	2.4E+1	2E-2	1.99E-2
Magnet: Setpoint{Double Float}=0.000000	0E+0	1.227320997E-3	1.56E-1	1.227320997E-3	3.304332616E-6	7.560145288E-7	-5.4672E+0	7.517998896E-7	-7.323049556E-8	2.9763E+0	3.0904E+0	8.61032E+1	6.43465E+1	5.710659549E-3	3.62E+2	6E+0	3E+0	1.8E+0	3.0005E+0	3.0785E+0	8.61032E+1	6.43465E+1	2.8E+0	3E+0	-1.98552981E-2	1.4649E+0	-8.1E-3	2.5E+1	1.5E-2	1.49E-2
Magnet: Units{Enum U16 ((Field,Current))}=Field	0E+0	1.226984415E-3	1.56E-1	1.226984415E-3	3.338050296E-6	6.896321927E-7	-6.0696E+0	6.859444894E-7	-7.428414123E-8	3.0818E+0	3.1355E+0	8.60315E+1	6.43465E+1	8.536680788E-2	3.63E+2	6E+0	3E+0	1.8E+0	2.9763E+0	3.0904E+0	8.61032E+1	6.43465E+1	2.8E+0	3E+0	5.710659549E-3	1.4649E+0	-8.1E-3	2.6E+1	1E-2	1E-2
Magnet: VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	0E+0	1.226647832E-3	1.56E-1	1.226647832E-3	3.338050296E-6	6.258831223E-7	-6.9456E+0	6.211415471E-7	-7.744521967E-8	2.9472E+0	3.045E+0	8.60315E+1	6.43465E+1	-5.67528829E-2	3.64E+2	6E+0	3E+0	1.8E+0	3.0818E+0	3.1355E+0	8.60315E+1	6.43465E+1	2.8E+0	3E+0	8.536680788E-2	1.4649E+0	-8.1E-3	2.7E+1	5E-3	5E-3
Main Screen Path{Path}=C:\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV\\\\1Code.vi	0E+0	1.226309835E-3	1.56E-1	1.226309835E-3	3.371767975E-6	5.579213925E-7	-8.3796E+0	5.52126511E-7	-8.324055371E-8	3.0176E+0	3.088E+0	8.59957E+1	6.43465E+1	5.274112336E-3	3.65E+2	6E+0	3E+0	1.8E+0	2.9472E+0	3.045E+0	8.60315E+1	6.43465E+1	2.8E+0	3E+0	-5.67528829E-2	1.4649E+0	-8.1E-3	2.8E+1	0E+0	-0E+0
Measurement Timestamp{Timestamp}=<22:33:51.840 17/05/2023>T	0E+0	1.226647832E-3	1.56E-1	1.226647832E-3	3.371767975E-6	4.894330096E-7	-9.4992E+0	4.820567545E-7	-8.218685147E-8	3.0569E+0	3.1183E+0	8.59599E+1	6.43465E+1	4.4842273E-2	3.66E+2	6E+0	3E+0	1.8E+0	3.0176E+0	3.088E+0	8.59957E+1	6.43465E+1	2.8E+0	3E+0	5.274112336E-3	1.4649E+0	-8.1E-3	2.9E+1	-5E-3	-5E-3
Measurement Title{String}=	0E+0	1.227152706E-3	1.56E-1	1.227152706E-3	3.371767975E-6	4.162027686E-7	-9.5688E+0	4.109345402E-7	-7.006944541E-8	3.002E+0	3.0817E+0	8.59599E+1	6.43465E+1	-1.272487175E-2	3.67E+2	6E+0	3E+0	1.8E+0	3.0569E+0	3.1183E+0	8.59599E+1	6.43465E+1	2.8E+0	3E+0	4.4842273E-2	1.4649E+0	-8.1E-3	3E+1	-1E-2	-1E-2
Measurment Select{U16}=4	0E+0	1.227490703E-3	1.56E-1	1.227490703E-3	3.371767975E-6	3.666804037E-7	-1.4298E+1	3.550895094E-7	-9.219682477E-8	3.0106E+0	3.0922E+0	8.59599E+1	6.43465E+1	-2.462676261E-3	3.68E+2	6E+0	3E+0	1.8E+0	3.002E+0	3.0817E+0	8.59599E+1	6.43465E+1	2.8E+0	3E+0	-1.272487175E-2	1.4649E+0	-8.1E-3	3.1E+1	-1.5E-2	-1.5E-2
Measurment Select.__text__{String}=6221-Lockin-DAQ	0E+0	1.227827286E-3	1.56E-1	1.227827286E-3	3.371767975E-6	2.966097987E-7	-1.29696E+1	2.892341092E-7	-6.796209749E-8	2.9701E+0	3.0552E+0	8.59599E+1	6.43465E+1	-5.223268643E-2	3.69E+2	6E+0	3E+0	1.8E+0	3.0106E+0	3.0922E+0	8.59599E+1	6.43465E+1	2.8E+0	3E+0	-2.462676261E-3	1.4649E+0	-8.1E-3	3.2E+1	-2E-2	-2E-2
Notes{String}=I+1A I-1E\\nrxx+1B Rxx-1C\\nRxy+1D Rxy-4A	0E+0	1.227995577E-3	1.56E-1	1.227995577E-3	3.371767975E-6	2.381309365E-7	-1.45332E+1	2.307552471E-7	-6.11132592E-8	3.0147E+0	3.0865E+0	8.59599E+1	6.43465E+1	6.051938981E-3	3.7E+2	6E+0	3E+0	1.8E+0	2.9701E+0	3.0552E+0	8.59599E+1	6.43465E+1	2.8E+0	3E+0	-5.223268643E-2	1.4649E+0	-8.1E-3	3.3E+1	-2.5E-2	-2.51E-2
Offset{Double Float}=0.000000	0E+0	1.228163869E-3	1.56E-1	1.228163869E-3	3.371767975E-6	1.754371522E-7	-2.57664E+1	1.580510935E-7	-7.797204251E-8	3.0547E+0	3.1173E+0	8.59599E+1	6.43465E+1	4.453050718E-2	3.71E+2	6E+0	3E+0	1.8E+0	3.0147E+0	3.0865E+0	8.59599E+1	6.43465E+1	2.8E+0	3E+0	6.051938981E-3	1.4649E+0	-8.1E-3	3.4E+1	-3E-2	-3E-2
Option: 2182 Autozero{Boolean}=True	0E+0	1.228333574E-3	1.56E-1	1.228333574E-3	3.371767975E-6	1.016799187E-7	-4.0002E+1	7.69182837E-8	-6.690845182E-8	3.0093E+0	3.1091E+0	8.59599E+1	6.43465E+1	3.350176662E-2	3.72E+2	6E+0	3E+0	1.8E+0	3.0547E+0	3.1173E+0	8.59599E+1	6.43465E+1	2.8E+0	3E+0	4.453050718E-2	1.4649E+0	-8.1E-3	3.5E+1	-3.5E-2	-3.51E-2
Option: 2182 Front Autozero{Boolean}=True	0E+0	1.228535524E-3	1.56E-1	1.228535524E-3	3.338050296E-6	8.218676662E-8	-7.6026E+1	1.896621042E-8	-8.21867949E-8	3.0118E+0	3.0943E+0	8.59599E+1	6.43465E+1	1.432675216E-2	3.73E+2	6E+0	3E+0	1.8E+0	3.0093E+0	3.1091E+0	8.59599E+1	6.43465E+1	2.8E+0	3E+0	3.350176662E-2	1.4649E+0	-8.1E-3	3.6E+1	-4E-2	-4.01E-2
Option: 2182 Hold{Boolean}=False	0E+0	1.228838449E-3	1.56E-1	1.228838449E-3	3.338050296E-6	8.534781677E-8	-1.161276E+2	-3.951290066E-8	-7.849892191E-8	2.972E+0	3.0648E+0	8.59241E+1	6.43465E+1	-2.830580808E-2	3.74E+2	6E+0	3E+0	1.8E+0	3.0118E+0	3.0943E+0	8.59599E+1	6.43465E+1	2.8E+0	3E+0	1.432675216E-2	1.4649E+0	-8.1E-3	3.7E+1	-4.5E-2	-4.51E-2
Option: 2182 Hold Count{I32}=10	0E+0	1.228838449E-3	1.56E-1	1.228838449E-3	3.371767975E-6	1.385585354E-7	-1.415112E+2	-1.111629843E-7	-8.850895178E-8	2.9585E+0	3.0495E+0	8.59241E+1	6.43465E+1	-4.935545102E-2	3.75E+2	6E+0	3E+0	1.8E+0	2.972E+0	3.0648E+0	8.59241E+1	6.43465E+1	2.8E+0	3E+0	-2.830580808E-2	1.4649E+0	-8.1E-3	3.8E+1	-5E-2	-5.01E-2
Option: 2182 Hold Window{Double Float}=1.000000	0E+0	1.228838449E-3	1.56E-1	1.228838449E-3	3.371767975E-6	1.348706059E-7	-1.412676E+2	-1.074751113E-7	-8.640157558E-8	2.9913E+0	3.0656E+0	8.59241E+1	6.43465E+1	-2.901116572E-2	3.76E+2	6E+0	3E+0	1.8E+0	2.9585E+0	3.0495E+0	8.59241E+1	6.43465E+1	2.8E+0	3E+0	-4.935545102E-2	1.4649E+0	-8.1E-3	3.9E+1	-5E-2	-5E-2
Option: 2182 Line Sync{Boolean}=False	0E+0	1.22900674E-3	1.56E-1	1.22900674E-3	3.371767975E-6	2.534092513E-7	-1.624332E+2	-2.444530368E-7	-7.797204251E-8	3.0204E+0	3.0937E+0	8.56734E+1	6.43465E+1	3.121782793E-3	3.77E+2	6E+0	3E+0	1.8E+0	2.9913E+0	3.0656E+0	8.59241E+1	6.43465E+1	2.8E+0	3E+0	-2.901116572E-2	1.4649E+0	-8.1E-3	4E+1	-6E-2	-6E-2
Option: 2182 Reference Reading{Double Float}=0.000000	0E+0	1.229344737E-3	1.56E-1	1.229344737E-3	3.304332616E-6	3.835386779E-7	-1.675356E+2	-3.772168604E-7	-8.429425595E-8	3.0283E+0	3.1035E+0	8.57092E+1	6.43465E+1	1.697861217E-2	3.78E+2	6E+0	3E+0	1.8E+0	3.0204E+0	3.0937E+0	8.56734E+1	6.43465E+1	2.8E+0	3E+0	3.121782793E-3	1.4649E+0	-8.1E-3	4.1E+1	-7E-2	-7E-2
Option: 2182 Relative Mode{Boolean}=False	0E+0	1.229513028E-3	1.56E-1	1.229513028E-3	3.371767975E-6	5.057646306E-7	-1.704816E+2	-5.020769273E-7	-8.534784506E-8	3.0064E+0	3.0918E+0	8.5745E+1	6.43465E+1	6.126260385E-3	3.79E+2	6E+0	3E+0	1.8E+0	3.0283E+0	3.1035E+0	8.57092E+1	6.43465E+1	2.8E+0	3E+0	1.697861217E-2	1.4649E+0	-8.1E-3	4.2E+1	-8E-2	-8E-2
Option: 2182 Trigger Delay{Cluster (Boolean,Double Float)}={'Auto':True,'Time(s)':0.000000}	0E+0	1.22968132E-3	1.56E-1	1.22968132E-3	3.304332616E-6	6.406350668E-7	-1.71594E+2	-6.353665556E-7	-9.483099552E-8	2.9845E+0	3.0654E+0	8.57808E+1	6.43465E+1	-2.687503584E-2	3.8E+2	6E+0	3E+0	1.8E+0	3.0064E+0	3.0918E+0	8.5745E+1	6.43465E+1	2.8E+0	3E+0	6.126260385E-3	1.4649E+0	-8.1E-3	4.3E+1	-9E-2	-9E-2
Option: 2182 Trigger Source{Enum U16 ((Immediate,Timer,Manual,Bus,Trigger link))}=Bus	0E+0	1.22968132E-3	1.56E-1	1.22968132E-3	3.371767975E-6	7.728730858E-7	-1.74414E+2	-7.723461499E-7	-7.691836855E-8	3.0101E+0	3.0922E+0	8.5745E+1	6.43465E+1	1.762703806E-2	3.81E+2	6E+0	3E+0	1.8E+0	2.9845E+0	3.0654E+0	8.57808E+1	6.43465E+1	2.8E+0	3E+0	-2.687503584E-2	1.4649E+0	-8.1E-3	4.4E+1	-1E-1	-9.99E-2
Option: 2182 Trigger Timer{Double Float}=0.000000	0E+0	1.229849611E-3	1.56E-1	1.229849611E-3	3.338050296E-6	7.72872803E-7	-1.743744E+2	-7.712925608E-7	-7.691842512E-8	2.9999E+0	3.0836E+0	8.58166E+1	6.43465E+1	1.085284748E-3	3.82E+2	6E+0	3E+0	1.8E+0	3.0101E+0	3.0922E+0	8.5745E+1	6.43465E+1	2.8E+0	3E+0	1.762703806E-2	1.4649E+0	-8.1E-3	4.5E+1	-1E-1	-9.99E-2
Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	0E+0	1.231536768E-3	1.56E-1	1.231536768E-3	3.371767975E-6	3.414966543E-6	-1.784748E+2	-3.416021546E-6	-9.219679649E-8	2.9938E+0	3.0648E+0	8.60673E+1	6.43465E+1	-3.638878837E-2	3.83E+2	6E+0	3E+0	1.8E+0	2.9999E+0	3.0836E+0	8.58166E+1	6.43465E+1	2.8E+0	3E+0	1.085284748E-3	1.4649E+0	-8.1E-3	4.6E+1	-3E-1	-2.998E-1
Option: 560 Enabled{Boolean}=False	0E+0	1.232884514E-3	1.56E-1	1.232884514E-3	3.371767975E-6	6.027570536E-6	-1.790496E+2	-6.030200973E-6	-1.011529827E-7	2.9818E+0	3.0672E+0	8.59599E+1	6.43465E+1	-3.12012285E-2	3.84E+2	6E+0	3E+0	1.8E+0	2.9938E+0	3.0648E+0	8.60673E+1	6.43465E+1	2.8E+0	3E+0	-3.638878837E-2	1.4649E+0	-8.1E-3	4.7E+1	-5E-1	-4.998E-1
Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	0E+0	1.234233673E-3	1.56E-1	1.234233673E-3	3.371767975E-6	8.65542258E-6	-1.792848E+2	-8.658055845E-6	-1.090556081E-7	2.9709E+0	3.0547E+0	8.59599E+1	6.43465E+1	-5.591969192E-2	3.85E+2	6E+0	3E+0	1.8E+0	2.9818E+0	3.0672E+0	8.59599E+1	6.43465E+1	2.8E+0	3E+0	-3.12012285E-2	1.4649E+0	-8.1E-3	4.8E+1	-7E-1	-6.999E-1
Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	0E+0	1.235919416E-3	1.56E-1	1.235919416E-3	3.371767975E-6	1.129649469E-5	-1.794696E+2	-1.129912513E-5	-1.058946145E-7	3.0173E+0	3.096E+0	8.59241E+1	6.43465E+1	8.483245969E-3	3.86E+2	6E+0	3E+0	1.8E+0	2.9709E+0	3.0547E+0	8.59599E+1	6.43465E+1	2.8E+0	3E+0	-5.591969192E-2	1.4649E+0	-8.1E-3	4.9E+1	-9E-1	-8.998E-1
Option: 6221 Adjust Mode{Enum U16 ((Offset,Frequency,Amplitude))}=Offset	0E+0	1.236930579E-3	1.56E-1	1.236930579E-3	3.371767975E-6	1.390959366E-5	-1.795344E+2	-1.391222975E-5	-1.143239779E-7	4.2528E+0	4.0287E+0	8.56734E+1	6.43465E+1	1.27304244E+0	3.87E+2	6E+0	3E+0	1.8E+0	3.0173E+0	3.096E+0	8.59241E+1	6.43465E+1	2.8E+0	3E+0	8.483245969E-3	1.4649E+0	-8.1E-3	5E+1	-1.1E+0	-1.0999E+0
Option: 6221 Amplitude{Double Float}=1.000000E-6	0E+0	1.240640061E-3	1.548E-1	1.240640061E-3	3.338050296E-6	1.657540319E-5	-1.795464E+2	-1.657800535E-5	-1.322362654E-7	2.3567E+0	2.5034E+0	8.5745E+1	6.43465E+1	-1.531698823E+0	3.88E+2	6E+0	3E+0	1.8E+0	4.2528E+0	4.0287E+0	8.56734E+1	6.43465E+1	2.8E+0	3E+0	1.27304244E+0	1.4649E+0	-8.1E-3	5.1E+1	-1.3E+0	-1.2999E+0
Option: 6221 Compliance{Double Float}=10.000000	0E+0	1.242662386E-3	1.56E-1	1.242662386E-3	3.371767975E-6	1.920530302E-5	-1.796304E+2	-1.920799003E-5	-1.259143631E-7	2.8978E+0	2.981E+0	8.60315E+1	6.43465E+1	-7.424862385E-1	3.89E+2	6E+0	3E+0	1.8E+0	2.3567E+0	2.5034E+0	8.5745E+1	6.43465E+1	2.8E+0	3E+0	-1.531698823E+0	1.4649E+0	-8.1E-3	5.2E+1	-1.5E+0	-1.4999E+0
Option: 6221 Duty Cycle{Double Float}=50.000000	0E+0	1.242662386E-3	1.56E-1	1.242662386E-3	3.371767975E-6	1.920903654E-5	-1.79604E+2	-1.92116387E-5	-1.353974287E-7	2.9053E+0	2.9903E+0	8.60315E+1	6.43465E+1	-4.583379328E-1	3.9E+2	6E+0	3E+0	1.8E+0	2.8978E+0	2.981E+0	8.60315E+1	6.43465E+1	2.8E+0	3E+0	-7.424862385E-1	1.4649E+0	-8.1E-3	5.3E+1	-1.5E+0	-1.5E+0
Option: 6221 External Trigger{Boolean}=False	0E+0	1.236795945E-3	1.56E-1	1.236795945E-3	3.371767975E-6	1.260093417E-5	-1.795524E+2	-1.260357309E-5	-1.000993936E-7	2.9767E+0	3.0562E+0	8.59241E+1	6.43465E+1	-2.630139887E-2	3.91E+2	6E+0	3E+0	1.8E+0	2.9053E+0	2.9903E+0	8.60315E+1	6.43465E+1	2.8E+0	3E+0	-4.583379328E-1	1.4649E+0	-8.1E-3	5.4E+1	-1E+0	-1.0001E+0
Option: 6221 External Trigger Ignore Multiple{Boolean}=False	0E+0	1.232884514E-3	1.56E-1	1.232884514E-3	3.371767975E-6	6.021249001E-6	-1.790772E+2	-6.023879438E-6	-9.851884023E-8	2.9867E+0	3.0678E+0	8.5745E+1	6.43465E+1	-4.471485317E-2	3.92E+2	6E+0	3E+0	1.8E+0	2.9767E+0	3.0562E+0	8.59241E+1	6.43465E+1	2.8E+0	3E+0	-2.630139887E-2	1.4649E+0	-8.1E-3	5.5E+1	-5E-1	-5E-1
Option: 6221 Frequency{Double Float}=119.770000	
Option: 6221 Function{U16}=1	
Option: 6221 Function.__text__{String}=Sine	
Option: 6221 Idle Level{Double Float}=0.000000	
Option: 6221 Input trigger Line{U8}=5	
Option: 6221 Offset{Double Float}=0.000000	
Option: 6221 Output Trigger Line{U8}=4	
Option: 6221 Pass Through{Boolean}=True	
Option: 6221 Phase Marker{Boolean}=True	
Option: 6221 Phase Marker Phase{Double Float}=0.000000	
Option: 6221 Range Level{Double Float}=2.000000E-12	
Option: 6221 Ranging{U16}=1	
Option: 6221 Ranging.__text__{String}=Best	
Option: 6221 Update Clock{Double Float}=0.000000	
Option: 6221 VISA{Visa Refnum (Void)}=GPIB0::13::INSTR	
Option: Confirm Config{Boolean}=False	
Option: Control Panel Ref{LVObjVI Refnum (Void)}=	
Option: DAQ Global Channel{Boolean}=False	
Option: DAQ Input Rate{Double Float}=10000.000000	
Option: DAQ Input Samples{I32}=200	
Option: DAQ Measurement Channels{1D Array (Cluster (UserDefinedRefnumTag Refnum (Void),\tkDAQmxPhysChanTagType Tag,\tkDAQmxScaleTagType Tag,Boolean,Double Float,String))}=[]	
Option: Differential{I32}=10106	
Option: Differential.__text__{String}=Differential	
Option: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values))}=Function Generator	
Option: Lockin Standoff Time{Double Float}=0.000000	
Option: Paranoid Save Data{Boolean}=True	
Option: Plot Autoback Path{Path}=C:\\\\TEMP\\\\XY Multiparam\\\\Backup.txt	
Option: SR830  Ref Phase{Double Float}=0.000000	
Option: SR830  Synch Filter{Boolean}=False	
Option: SR830  Time Constant{I16}=8	
Option: SR830  Time Constant.__text__{String}=100 ms	
Option: SR830 2x Line Filter{Boolean}=True	
Option: SR830 Adjust Gains{Boolean}=False	
Option: SR830 Auto Gain Lower.__text__{String}=2 nV/fA	
Option: SR830 Auto Gain Upper.__text__{String}=1 V/uA	
Option: SR830 Auto Offset 1{Boolean}=False	
Option: SR830 Auto Offset 2{Boolean}=False	
Option: SR830 Autophase{Boolean}=False	
Option: SR830 DC Coupling?{Boolean}=False	
Option: SR830 Display 1{U16}=0	
Option: SR830 Display 1.__text__{String}=X	
Option: SR830 Display 2{U16}=0	
Option: SR830 Display 2.__text__{String}=Y	
Option: SR830 Dynamic Reserve{I16}=1	
Option: SR830 Dynamic Reserve.__text__{String}=Normal	
Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Option: SR830 Filter Slope{I32}=1	
Option: SR830 Filter Slope.__text__{String}=12 dB/oct	
Option: SR830 Gain{I32}=-1	
Option: SR830 Gain.__text__{String}=Auto Gain	
Option: SR830 Ground Shield?{Boolean}=False	
Option: SR830 Harmonic{I32}=1	
Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A	
Option: SR830 Line Filter{Boolean}=True	
Option: SR830 No Reset{Boolean}=False	
Option: SR830 Offset 1{Double Float}=0.000000	
Option: SR830 Offset 2{Double Float}=0.000000	
Option: SR830 Output Channel 1{Boolean}=False	
Option: SR830 Output Channel 2{Boolean}=False	
Option: SR830 Ratio 1{U16}=0	
Option: SR830 Ratio 1.__text__{String}=None	
Option: SR830 Ratio 2{U16}=0	
Option: SR830 Ratio 2.__text__{String}=None	
Option: SR830 Ref Amplitude{Double Float}=0.100000	
Option: SR830 Ref Frequency{Double Float}=1013.000000	
Option: SR830 Ref Source{Boolean}=False	
Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta]	
Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Option: SR830 VISA{Visa Refnum (Void)}=	
Option: Sense Autorange{Boolean}=False	
Option: Sense Range Level{Double Float}=0.100000	
Option: Sense Rate{Double Float}=1.000000	
Option:560 Comport{Visa Refnum (Void)}=COM1	
Option:560 Filter High Pass{U16}=0	
Option:560 Filter High Pass.__text__{String}=0.03	
Option:560 Filter Lowpass{U16}=0	
Option:560 Filter Lowpass.__text__{String}=0.03	
Option:560 Filter Mode{U16}=0	
Option:560 Filter Mode.__text__{String}=6 dB high pass	
Option:560 Invert{Boolean}=False	
Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Option:570 Enabled{Boolean}=False	
Option:570 Filter High Pass{U16}=0	
Option:570 Filter High Pass.__text__{String}=0.03	
Option:570 Filter Lowpass{U16}=0	
Option:570 Filter Lowpass.__text__{String}=0.03	
Option:570 Filter Mode{U16}=0	
Option:570 Filter Mode.__text__{String}=6 dB high pass	
Option:570 Gain Mode{U16}=0	
Option:570 Gain Mode.__text__{String}=Low Noise	
Option:570 Input Offset{U16}=0	
Option:570 Input Offset On{Boolean}=False	
Option:570 Input Offset.__text__{String}=1pA	
Option:570 Sensitivity{U16}=0	
Option:570 Sensitivity.__text__{String}=1pA/V	
Option:Debug On{Boolean}=False	
Option:GPIB 2182{Visa Refnum (Void)}=	
Option:Parallel Config Voltage Measurers{Boolean}=True	
Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Option:SR830 Settle Time{Double Float}=5.000000	
Option:Sense Digits{I32}=8	
Output Names{1D Array (String)}=['Offset','Rxx::R','Rxx::Theta','Rxx::X','Rxx::Y','Rxy::R','Rxy::Theta','Rxy::X','Rxy::Y','temperature: T1','temperature: T2','temperature: T3','temperature: T4','temperature: dT/dt','iterator','multi[0]:iterator','multi[0]:y','multi[0]:temperature: setpoint','multi[0]:temperature: T1','multi[0]:temperature: T2','multi[0]:temperature: T3','multi[0]:temperature: T4','multi[0]:temperature: heater','multi[0]:temperature: gas','multi[0]:temperature: dT/dt','multi[0]:temperature: current temperature','multi[0]:temperature: error','multi[1]:iterator','multi[1]:y','multi[1]:Control:Magnet Output']	
Parameter Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Parameter Select{U16}=6	
Parameter Select.__text__{String}=Multi-Parameter	
Paths{U32}=0	
Plot: Column Renames{1D Array (Cluster (String,String))}=[]	
Plot: No dups{Boolean}=False	
Plot: StdDevs{Boolean}=False	
Plotting Class{String}=Parameter Plot	
Plotting Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	
Plotting Select{U16}=1	
Plotting Select.__text__{String}=Parameter Plot	
Project Code{String}=Topological_Insulators	
Ref: Temperature Window{LVObjVI Refnum (Void)}=	
Ref:Control Subpanel{LVObjUnknown Refnum (Void)}=	
Ref:Main Screen{LVObjVI Refnum (Void)}=	
Ref:Plotting Subpanel{LVObjUnknown Refnum (Void)}=	
Ref:Toolbar{LVObjUnknown Refnum (Void)}=	
Ref:XY Subpanel{LVObjUnknown Refnum (Void)}=	
Rxx::R{Double Float}=0.001233	
Rxx::Theta{Double Float}=0.156000	
Rxx::X{Double Float}=0.001233	
Rxx::Y{Double Float}=3.371768E-6	
Rxx:Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	
Rxx:Option: 560 Enabled{Boolean}=False	
Rxx:Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	
Rxx:Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	
Rxx:Option: Lockin Standoff Time{Double Float}=0.000000	
Rxx:Option: Lockin Type{Enum U16 ((SRS 830,EG&G 5302))}=SRS 830	
Rxx:Option: SR803 Full Scale Reading{Double Float}=0.000000	
Rxx:Option: SR830  Ref Phase{Double Float}=0.000000	
Rxx:Option: SR830  Synch Filter{Boolean}=False	
Rxx:Option: SR830  Time Constant{I16}=8	
Rxx:Option: SR830 2x Line Filter{Boolean}=False	
Rxx:Option: SR830 Adjust Gains{Boolean}=False	
Rxx:Option: SR830 Auto Gain Lower{I32}=0	
Rxx:Option: SR830 Auto Gain Upper{I32}=26	
Rxx:Option: SR830 Auto Offset 1{Boolean}=False	
Rxx:Option: SR830 Auto Offset 2{Boolean}=False	
Rxx:Option: SR830 Autophase{Boolean}=False	
Rxx:Option: SR830 DC Coupling?{Boolean}=False	
Rxx:Option: SR830 Display 1{U16}=0	
Rxx:Option: SR830 Display 2{U16}=0	
Rxx:Option: SR830 Dynamic Reserve{I16}=2	
Rxx:Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Rxx:Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Rxx:Option: SR830 Filter Slope{I32}=3	
Rxx:Option: SR830 Gain{I32}=18	
Rxx:Option: SR830 Ground Shield?{Boolean}=False	
Rxx:Option: SR830 Harmonic{I32}=1	
Rxx:Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A-B	
Rxx:Option: SR830 Line Filter{Boolean}=False	
Rxx:Option: SR830 No Reset{Boolean}=False	
Rxx:Option: SR830 Offset 1{Double Float}=0.000000	
Rxx:Option: SR830 Offset 2{Double Float}=0.000000	
Rxx:Option: SR830 Output Channel 1{Boolean}=False	
Rxx:Option: SR830 Output Channel 2{Boolean}=False	
Rxx:Option: SR830 Ratio 1{U16}=0	
Rxx:Option: SR830 Ratio 2{U16}=0	
Rxx:Option: SR830 Ref Amplitude{Double Float}=0.100000	
Rxx:Option: SR830 Ref Frequency{Double Float}=1013.000000	
Rxx:Option: SR830 Ref Source{Boolean}=False	
Rxx:Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta,X,Y]	
Rxx:Option: SR830 Time Constant value{Double Float}=0.000000	
Rxx:Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Rxx:Option: SR830 VISA{Visa Refnum (Void)}=GPIB0::5::INSTR	
Rxx:Option:560 Comport{Visa Refnum (Void)}=COM1	
Rxx:Option:560 Filter High Pass{U16}=0	
Rxx:Option:560 Filter Lowpass{U16}=0	
Rxx:Option:560 Filter Mode{U16}=0	
Rxx:Option:560 Invert{Boolean}=False	
Rxx:Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Rxx:Option:570 Enabled{Boolean}=False	
Rxx:Option:570 Filter High Pass{U16}=0	
Rxx:Option:570 Filter Lowpass{U16}=0	
Rxx:Option:570 Filter Mode{U16}=0	
Rxx:Option:570 Gain Mode{U16}=0	
Rxx:Option:570 Input Offset{U16}=0	
Rxx:Option:570 Input Offset On{Boolean}=False	
Rxx:Option:570 Sensitivity{U16}=0	
Rxx:Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Rxx:Option:SR830 Autogain Lower Threshold{Double Float}=0.100000	
Rxx:Option:SR830 Autogain Standoff{Double Float}=3.000000	
Rxx:Option:SR830 Autogain Upper Threshold{Double Float}=0.900000	
Rxx:Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Rxx:Option:SR830 Settle Time{Double Float}=0.000000	
Rxy::R{Double Float}=6.021249E-6	
Rxy::Theta{Double Float}=-179.077200	
Rxy::X{Double Float}=-6.023879E-6	
Rxy::Y{Double Float}=-9.851884E-8	
Rxy:Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	
Rxy:Option: 560 Enabled{Boolean}=False	
Rxy:Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	
Rxy:Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	
Rxy:Option: Lockin Standoff Time{Double Float}=0.000000	
Rxy:Option: Lockin Type{Enum U16 ((SRS 830,EG&G 5302))}=SRS 830	
Rxy:Option: SR803 Full Scale Reading{Double Float}=0.000000	
Rxy:Option: SR830  Ref Phase{Double Float}=0.000000	
Rxy:Option: SR830  Synch Filter{Boolean}=False	
Rxy:Option: SR830  Time Constant{I16}=8	
Rxy:Option: SR830 2x Line Filter{Boolean}=False	
Rxy:Option: SR830 Adjust Gains{Boolean}=False	
Rxy:Option: SR830 Auto Gain Lower{I32}=0	
Rxy:Option: SR830 Auto Gain Upper{I32}=26	
Rxy:Option: SR830 Auto Offset 1{Boolean}=False	
Rxy:Option: SR830 Auto Offset 2{Boolean}=False	
Rxy:Option: SR830 Autophase{Boolean}=False	
Rxy:Option: SR830 DC Coupling?{Boolean}=False	
Rxy:Option: SR830 Display 1{U16}=0	
Rxy:Option: SR830 Display 2{U16}=1	
Rxy:Option: SR830 Dynamic Reserve{I16}=2	
Rxy:Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Rxy:Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Rxy:Option: SR830 Filter Slope{I32}=3	
Rxy:Option: SR830 Gain{I32}=18	
Rxy:Option: SR830 Ground Shield?{Boolean}=False	
Rxy:Option: SR830 Harmonic{I32}=1	
Rxy:Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A-B	
Rxy:Option: SR830 Line Filter{Boolean}=False	
Rxy:Option: SR830 No Reset{Boolean}=False	
Rxy:Option: SR830 Offset 1{Double Float}=0.000000	
Rxy:Option: SR830 Offset 2{Double Float}=0.000000	
Rxy:Option: SR830 Output Channel 1{Boolean}=False	
Rxy:Option: SR830 Output Channel 2{Boolean}=False	
Rxy:Option: SR830 Ratio 1{U16}=0	
Rxy:Option: SR830 Ratio 2{U16}=0	
Rxy:Option: SR830 Ref Amplitude{Double Float}=0.100000	
Rxy:Option: SR830 Ref Frequency{Double Float}=1013.000000	
Rxy:Option: SR830 Ref Source{Boolean}=False	
Rxy:Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta,X,Y]	
Rxy:Option: SR830 Time Constant value{Double Float}=0.000000	
Rxy:Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Rxy:Option: SR830 VISA{Visa Refnum (Void)}=GPIB0::6::INSTR	
Rxy:Option:560 Comport{Visa Refnum (Void)}=COM1	
Rxy:Option:560 Filter High Pass{U16}=0	
Rxy:Option:560 Filter Lowpass{U16}=0	
Rxy:Option:560 Filter Mode{U16}=0	
Rxy:Option:560 Invert{Boolean}=False	
Rxy:Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Rxy:Option:570 Enabled{Boolean}=False	
Rxy:Option:570 Filter High Pass{U16}=0	
Rxy:Option:570 Filter Lowpass{U16}=0	
Rxy:Option:570 Filter Mode{U16}=0	
Rxy:Option:570 Gain Mode{U16}=0	
Rxy:Option:570 Input Offset{U16}=0	
Rxy:Option:570 Input Offset On{Boolean}=False	
Rxy:Option:570 Sensitivity{U16}=0	
Rxy:Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Rxy:Option:SR830 Autogain Lower Threshold{Double Float}=0.100000	
Rxy:Option:SR830 Autogain Standoff{Double Float}=3.000000	
Rxy:Option:SR830 Autogain Upper Threshold{Double Float}=0.900000	
Rxy:Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Rxy:Option:SR830 Settle Time{Double Float}=0.000000	
Sample ID{String}=MBE202221213_PA_D1 750C Cracker WAL	
Save:Filename{String}=${X-Y Class} ${2nd Parameter Class} ${iterator}{%04d} ${y}{%04.2g}.txt	
Save:Final Filename{String}=${X-Y Class} ${2nd Parameter Class} .txt	
Save:Final path{Path}=C:\\\\Data\\\\${Project Code}\\\\${User}\\\\${Sample ID}\\\\${Measurement Timestamp}{%Y%m%d}\\\\${X-Y Class}	
Save:Path{Path}=C:\\\\Data\\\\${Project Code}\\\\${User}\\\\${Sample ID}\\\\${Measurement Timestamp}{%Y%m%d}\\\\${X-Y Class}	
Startup path{Path}=C:\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV	
Sub Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Sweep Step{I32}=3	
T Control Measure.__text__{1D Array (String)}=['temperature: T1','temperature: T2','temperature: T3','temperature: T4','temperature: dT/dt']	
Timestamp{Timestamp}=<22:35:00.882 17/05/2023>T	
Toolbar{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Unaved Data{Boolean}=True	
Unsaved Data{Boolean}=False	
User{String}=Craig	
X-Y Class{String}=6221-Lockin-DAQ	
X-Y Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	
d(Offset){Double Float}=0.000000	
d(Rxx::R){Double Float}=0.000000	
d(Rxx::Theta){Double Float}=0.000000	
d(Rxx::X){Double Float}=0.000000	
d(Rxx::Y){Double Float}=4.735058E-22	
d(Rxy::R){Double Float}=7.989935E-9	
d(Rxy::Theta){Double Float}=0.135990	
d(Rxy::X){Double Float}=7.989935E-9	
d(Rxy::Y){Double Float}=1.401336E-8	
iterate result{U16}=5	
iterator{I32}=392	
multi[0]:Control: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values,Adaptive Step Ramp))}=List of Values	
multi[0]:Control: Monitor Update Timeout{Double Float}=0.010000	
multi[0]:Control: Open T Window{Boolean}=False	
multi[0]:Control: Reverse Temperature Sense{Boolean}=False	
multi[0]:Iterator{I32}=0	
multi[0]:Ref: Temperature Window{LVObjVI Refnum (Void)}=	
multi[0]:iterate result{U16}=0	
multi[0]:iterator{I32}=6	
multi[0]:temperature:  rate window{Double Float}=120.000000	
multi[0]:temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[0]:temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
multi[0]:temperature: T1{Double Float}=3.044900	
multi[0]:temperature: T2{Double Float}=3.135100	
multi[0]:temperature: T3{Double Float}=85.959900	
multi[0]:temperature: T4{Double Float}=64.346500	
multi[0]:temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
multi[0]:temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
multi[0]:temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
multi[0]:temperature: current temperature{Double Float}=1.464900	
multi[0]:temperature: current temperature 2{Double Float}=287.100000	
multi[0]:temperature: dT/dt{Double Float}=0.055846	
multi[0]:temperature: error{Double Float}=-0.008100	
multi[0]:temperature: gas{Double Float}=3.000000	
multi[0]:temperature: gas control{Boolean}=False	
multi[0]:temperature: gas control 2{Boolean}=False	
multi[0]:temperature: gass boost{I8}=0	
multi[0]:temperature: gass boost 2{I8}=0	
multi[0]:temperature: gast flow{I16}=0	
multi[0]:temperature: gast flow 2{I16}=7	
multi[0]:temperature: heater{Double Float}=2.800000	
multi[0]:temperature: heater output{Double Float}=0.000000	
multi[0]:temperature: heater output 2{Double Float}=0.000000	
multi[0]:temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
multi[0]:temperature: monitor timeout{Double Float}=0.010000	
multi[0]:temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
multi[0]:temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
multi[0]:temperature: ramp rate{Double Float}=8.000000	
multi[0]:temperature: ramp rate 2{Double Float}=0.000000	
multi[0]:temperature: ramp target{Double Float}=20.000000	
multi[0]:temperature: ramp target 2{Double Float}=0.000000	
multi[0]:temperature: ramping{Boolean}=False	
multi[0]:temperature: setpoint{Double Float}=1.800000	
multi[0]:temperature: setpoint 2{Double Float}=287.100000	
multi[0]:temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
multi[0]:temperature: stability error{Extended Float}=0.040000	
multi[0]:temperature: stability script{String}=	
multi[0]:temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
multi[0]:temperature: temp control mode{U16}=2	
multi[0]:temperature: temp control mode 2{U16}=3	
multi[0]:temperature: temp control mode 2.__text__{String}=Open Loop	
multi[0]:temperature: temp control mode.__text__{String}=Zone	
multi[0]:temperature: temp control sensor{U16}=0	
multi[0]:temperature: temp control sensor 2{U16}=0	
multi[0]:temperature: temp control sensor 2.__text__{String}=Sensor 1	
multi[0]:temperature: temp control sensor.__text__{String}=Sensor A	
multi[0]:temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
multi[0]:temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
multi[0]:temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
multi[0]:temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
multi[0]:temperature: temp loop{U16}=0	
multi[0]:temperature: temp loop 2{U16}=0	
multi[0]:temperature: temp loop 2.__text__{String}=Heater	
multi[0]:temperature: temp loop.__text__{String}=Loop 1	
multi[0]:temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
multi[0]:temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[0]:temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[0]:temperature:error for gas boost{Double Float}=0.000000	
multi[0]:temperature:error for gas boost 2{Double Float}=0.000000	
multi[0]:temperature:heater range{U16}=2	
multi[0]:temperature:heater range 2{U16}=0	
multi[0]:temperature:heater range 2.__text__{String}=Off	
multi[0]:temperature:heater range.__text__{String}=40mW	
multi[0]:temperature:history window{Extended Float}=300.000000	
multi[0]:temperature:is stable?{Boolean}=True	
multi[0]:temperature:monitor{Boolean}=True	
multi[0]:temperature:ramping{Boolean}=False	
multi[0]:temperature:ramping on{Boolean}=False	
multi[0]:temperature:ramping on 2{Boolean}=False	
multi[0]:temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
multi[0]:temperature:stability code{U32}=6618880	
multi[0]:temperature:stability rate{Extended Float}=0.040000	
multi[0]:y{Double Float}=3.000000	
multi[1]:Control: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values,Adaptive Step Ramp))}=Multi-Segment Ramp	
multi[1]:Control: Gate delay{Double Float}=0.000000	
multi[1]:Control: Monitor Update Timeout{Double Float}=0.010000	
multi[1]:Control: Open T Window{Boolean}=False	
multi[1]:Control: Reverse Temperature Sense{Boolean}=False	
multi[1]:Control:Magnet Output{Double Float}=-0.000100	
multi[1]:Iterator{I32}=0	
multi[1]:Magnet: Final Switch Heater{Enum U8 ((False,True,Mixed))}=	
multi[1]:Magnet: Power Supply{Enum U16 ((IPS120,LS625,PS110,Hg iPS,SMS Series,Cryomagnetics 4G,DMG Little CryoFree,DMG Big CryoFree))}=Hg iPS	
multi[1]:Magnet: Rate{Double Float}=0.500000	
multi[1]:Magnet: Units{Enum U16 ((Field,Current))}=Field	
multi[1]:Magnet: VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[1]:Multi-segment_Stage{I32}=0	
multi[1]:Multi-segment_Stage_Changed{Boolean}=False	
multi[1]:Ref: Temperature Window{LVObjVI Refnum (Void)}=	
multi[1]:iterate result{U16}=4	
multi[1]:iterator{I32}=57	
multi[1]:measure point{Boolean}=False	
multi[1]:temperature:  rate window{Double Float}=120.000000	
multi[1]:temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[1]:temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
multi[1]:temperature: T1{Double Float}=1.842400	
multi[1]:temperature: T2{Double Float}=1.465600	
multi[1]:temperature: T3{Double Float}=86.318100	
multi[1]:temperature: T4{Double Float}=66.769200	
multi[1]:temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
multi[1]:temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
multi[1]:temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
multi[1]:temperature: current temperature{Double Float}=1.465600	
multi[1]:temperature: current temperature 2{Double Float}=287.100000	
multi[1]:temperature: dT/dt{Double Float}=-0.001864	
multi[1]:temperature: gas control{Boolean}=False	
multi[1]:temperature: gas control 2{Boolean}=False	
multi[1]:temperature: gass boost{I8}=0	
multi[1]:temperature: gass boost 2{I8}=0	
multi[1]:temperature: gast flow{I16}=0	
multi[1]:temperature: gast flow 2{I16}=7	
multi[1]:temperature: heater output{Double Float}=0.000000	
multi[1]:temperature: heater output 2{Double Float}=0.000000	
multi[1]:temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
multi[1]:temperature: monitor timeout{Double Float}=1.000000	
multi[1]:temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
multi[1]:temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
multi[1]:temperature: ramp rate{Double Float}=8.000000	
multi[1]:temperature: ramp rate 2{Double Float}=0.000000	
multi[1]:temperature: ramp target{Double Float}=20.000000	
multi[1]:temperature: ramp target 2{Double Float}=0.000000	
multi[1]:temperature: ramping{Boolean}=False	
multi[1]:temperature: setpoint{Double Float}=1.800000	
multi[1]:temperature: setpoint 2{Double Float}=287.100000	
multi[1]:temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
multi[1]:temperature: stability error{Extended Float}=0.040000	
multi[1]:temperature: stability script{String}=	
multi[1]:temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
multi[1]:temperature: temp control mode{U16}=2	
multi[1]:temperature: temp control mode 2{U16}=3	
multi[1]:temperature: temp control mode 2.__text__{String}=Open Loop	
multi[1]:temperature: temp control mode.__text__{String}=Zone	
multi[1]:temperature: temp control sensor{U16}=0	
multi[1]:temperature: temp control sensor 2{U16}=0	
multi[1]:temperature: temp control sensor 2.__text__{String}=Sensor 1	
multi[1]:temperature: temp control sensor.__text__{String}=Sensor A	
multi[1]:temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
multi[1]:temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
multi[1]:temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
multi[1]:temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
multi[1]:temperature: temp loop{U16}=0	
multi[1]:temperature: temp loop 2{U16}=0	
multi[1]:temperature: temp loop 2.__text__{String}=Heater	
multi[1]:temperature: temp loop.__text__{String}=Loop 1	
multi[1]:temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
multi[1]:temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[1]:temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[1]:temperature:error for gas boost{Double Float}=0.000000	
multi[1]:temperature:error for gas boost 2{Double Float}=0.000000	
multi[1]:temperature:heater range{U16}=2	
multi[1]:temperature:heater range 2{U16}=0	
multi[1]:temperature:heater range 2.__text__{String}=Off	
multi[1]:temperature:heater range.__text__{String}=40mW	
multi[1]:temperature:history window{Extended Float}=300.000000	
multi[1]:temperature:is stable?{Boolean}=True	
multi[1]:temperature:monitor{Boolean}=True	
multi[1]:temperature:ramping{Boolean}=False	
multi[1]:temperature:ramping on{Boolean}=False	
multi[1]:temperature:ramping on 2{Boolean}=False	
multi[1]:temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
multi[1]:temperature:stability code{U32}=6618880	
multi[1]:temperature:stability rate{Extended Float}=0.040000	
multi[1]:y{Double Float}=0.000000	
parameter: Termination{String}=False	
parameter: delta time{Double Float}=1.000000	
parameter: progress{Double Float}=100.000000	
temperature:  rate window{Double Float}=120.000000	
temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':8.000000,'P':100.000000,'I':8.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':12.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':1,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':18.000000,'P':100.000000,'I':9.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':25.000000,'P':100.000000,'I':10.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':50.000000,'P':100.000000,'I':12.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':100.000000,'P':100.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':150.000000,'P':100.000000,'I':19.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':200.000000,'P':100.000000,'I':23.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000},{'Upper Temp':300.000000,'P':100.000000,'I':30.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':0.000000}]	
temperature: T1{Double Float}=3.044900	
temperature: T2{Double Float}=3.135100	
temperature: T3{Double Float}=85.959900	
temperature: T4{Double Float}=64.346500	
temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
temperature: current temperature{Double Float}=1.464900	
temperature: current temperature 2{Double Float}=287.100000	
temperature: dT/dt{Double Float}=0.055846	
temperature: gas control{Boolean}=False	
temperature: gas control 2{Boolean}=False	
temperature: gass boost{I8}=0	
temperature: gass boost 2{I8}=0	
temperature: gast flow{I16}=0	
temperature: gast flow 2{I16}=7	
temperature: heater output{Double Float}=0.000000	
temperature: heater output 2{Double Float}=0.000000	
temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
temperature: monitor timeout{Double Float}=0.010000	
temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
temperature: ramp rate{Double Float}=8.000000	
temperature: ramp rate 2{Double Float}=0.000000	
temperature: ramp target{Double Float}=20.000000	
temperature: ramp target 2{Double Float}=0.000000	
temperature: ramping{Boolean}=False	
temperature: setpoint{Double Float}=1.800000	
temperature: setpoint 2{Double Float}=287.100000	
temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
temperature: stability error{Extended Float}=0.040000	
temperature: stability script{String}=	
temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':0.500000,'temperature:stability rate':0.150000,'temperature:history window':120.000000}	
temperature: temp control mode{U16}=2	
temperature: temp control mode 2{U16}=3	
temperature: temp control mode 2.__text__{String}=Open Loop	
temperature: temp control mode.__text__{String}=Zone	
temperature: temp control sensor{U16}=0	
temperature: temp control sensor 2{U16}=0	
temperature: temp control sensor 2.__text__{String}=Sensor 1	
temperature: temp control sensor.__text__{String}=Sensor A	
temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
temperature: temp loop{U16}=0	
temperature: temp loop 2{U16}=0	
temperature: temp loop 2.__text__{String}=Heater	
temperature: temp loop.__text__{String}=Loop 1	
temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
temperature:error for gas boost{Double Float}=0.000000	
temperature:error for gas boost 2{Double Float}=0.000000	
temperature:heater range{U16}=2	
temperature:heater range 2{U16}=0	
temperature:heater range 2.__text__{String}=Off	
temperature:heater range.__text__{String}=40mW	
temperature:history window{Extended Float}=300.000000	
temperature:is stable?{Boolean}=True	
temperature:monitor{Boolean}=True	
temperature:ramping{Boolean}=False	
temperature:ramping on{Boolean}=False	
temperature:ramping on 2{Boolean}=False	
temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
temperature:stability code{U32}=6618880	
temperature:stability rate{Extended Float}=0.040000	
y{Double Float}=3.000000	
