TDI Format 1.5	Offset	Rxx::R	Rxx::Theta	Rxx::X	Rxx::Y	Rxy::R	Rxy::Theta	Rxy::X	Rxy::Y	temperature: T1	temperature: T2	temperature: T3	temperature: T4	temperature: dT/dt	iterator	multi[0]:iterator	multi[0]:y	multi[0]:temperature: setpoint	multi[0]:temperature: T1	multi[0]:temperature: T2	multi[0]:temperature: T3	multi[0]:temperature: T4	multi[0]:temperature: heater	multi[0]:temperature: gas	multi[0]:temperature: dT/dt	multi[0]:temperature: current temperature	multi[0]:temperature: error	multi[1]:iterator	multi[1]:y	multi[1]:Control:Magnet Output
2nd Parameter Class{String}=Multi-Parameter	0E+0	4.782856126E-4	1.992E-1	4.782856126E-4	1.618454285E-6	3.487674091E-7	1.66452E+1	3.313816332E-7	9.79918194E-8	8.0095E+1	7.9806E+1	9.13682E+1	8.31031E+1	8.517643064E-2	2.1E+1	1E+0	8E+1	8E+1	8.0096E+1	7.9805E+1	9.13682E+1	8.31031E+1	3.6E+0	8E+1	8.761053532E-2	8.0096E+1	-9.6E-2	0E+0	0E+0	-0E+0
2nd Parameter Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	0E+0	4.794480961E-4	2.016E-1	4.794480961E-4	1.652169136E-6	4.769463523E-6	2.1012E+0	4.765775254E-6	1.733301437E-7	8.0076E+1	7.9897E+1	9.11891E+1	8.31031E+1	7.509811968E-2	2.2E+1	1E+0	8E+1	6E+1	8.0095E+1	7.9806E+1	9.13682E+1	8.31031E+1	3.6E+0	8E+1	8.517643064E-2	6.1266E+1	-9.6E-2	1E+0	5E-1	4.998E-1
Analysis Class{String}=Basic Plot	0E+0	4.822468248E-4	2.04E-1	4.822468248E-4	1.685883988E-6	9.212815056E-6	7.68E-1	9.211760053E-6	1.222263204E-7	8.0076E+1	7.9985E+1	9.101E+1	8.31031E+1	7.518279552E-2	2.3E+1	1E+0	8E+1	6E+1	8.0076E+1	7.9897E+1	9.11891E+1	8.31031E+1	3.6E+0	8E+1	7.509811968E-2	6.1266E+1	-9.6E-2	2E+0	1E+0	9.998E-1
Analysis Class Path{Path}=C\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV\\\\plugins\\\\Plotting\\\\Plotting_Base_class\\\\Plotting_Base.lvclass	0E+0	4.866464432E-4	1.98E-1	4.866464432E-4	1.685883988E-6	1.374153418E-5	8.184E-1	1.374100526E-5	1.949299931E-7	8.0067E+1	8.0068E+1	9.1798E+1	8.31031E+1	7.517722249E-2	2.4E+1	1E+0	8E+1	6E+1	8.0076E+1	7.9985E+1	9.101E+1	8.31031E+1	3.6E+0	8E+1	7.518279552E-2	6.1266E+1	-9.6E-2	3E+0	1.5E+0	1.4999E+0
Analysis.# pre-routines{I32}=5	0E+0	4.867143254E-4	1.98E-1	4.867143254E-4	1.685883988E-6	1.373363438E-5	7.38E-1	1.373205329E-5	1.754374351E-7	8.0067E+1	8.0072E+1	9.1798E+1	8.31031E+1	7.342813164E-2	2.5E+1	1E+0	8E+1	6E+1	8.0067E+1	8.0068E+1	9.1798E+1	8.31031E+1	3.6E+0	8E+1	7.517722249E-2	6.1266E+1	-9.6E-2	4E+0	1.5E+0	1.5E+0
Analysis:Pre[0]:T Control Measure{1D Array (I32)}=[1,2,3,4,7]	0E+0	4.845222944E-4	1.98E-1	4.845222944E-4	1.685883988E-6	1.147930159E-5	7.416E-1	1.147824942E-5	1.475146368E-7	8.0058E+1	8.0111E+1	9.08309E+1	8.31031E+1	6.527028233E-2	2.6E+1	1E+0	8E+1	6E+1	8.0067E+1	8.0072E+1	9.1798E+1	8.31031E+1	3.6E+0	8E+1	7.342813164E-2	6.1266E+1	-9.6E-2	5E+0	1.25E+0	1.2502E+0
Autosave Tabs{Enum U32 ((XY Measurement Save,Parameter Plot Save 2))}=Parameter Plot Save 2	0E+0	4.827531132E-4	1.98E-1	4.827531132E-4	1.685883988E-6	9.221243769E-6	4.152E-1	9.221243769E-6	6.585486272E-8	8.0056E+1	8.0152E+1	9.08668E+1	8.31031E+1	6.624147296E-2	2.7E+1	1E+0	8E+1	6E+1	8.0058E+1	8.0111E+1	9.08309E+1	8.31031E+1	3.6E+0	8E+1	6.527028233E-2	6.1266E+1	-9.6E-2	6E+0	1E+0	1E+0
Control:Magnet Output{Double Float}=-0.007000	0E+0	4.814039535E-4	2.04E-1	4.814039535E-4	1.685883988E-6	6.961118364E-6	9.312E-1	6.961118364E-6	1.122166582E-7	8.0053E+1	8.0194E+1	9.09384E+1	8.31031E+1	6.61599189E-2	2.8E+1	1E+0	8E+1	6E+1	8.0056E+1	8.0152E+1	9.08668E+1	8.31031E+1	3.6E+0	8E+1	6.624147296E-2	6.1266E+1	-9.6E-2	7E+0	7.5E-1	7.502E-1
Control:Magnet Rate{Double Float}=0.500000	0E+0	4.803927908E-4	2.016E-1	4.803927908E-4	1.652169136E-6	4.744174556E-6	1.2228E+0	4.743116725E-6	1.006261033E-7	8.0048E+1	8.0226E+1	9.11175E+1	8.31031E+1	5.491350219E-2	2.9E+1	1E+0	8E+1	6E+1	8.0053E+1	8.0194E+1	9.09384E+1	8.31031E+1	3.6E+0	8E+1	6.61599189E-2	6.1266E+1	-9.6E-2	8E+0	5E-1	5.002E-1
Display Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	0E+0	4.798865023E-4	1.992E-1	4.798865023E-4	1.618454285E-6	2.482988492E-6	1.2084E+0	2.482459576E-6	5.11032859E-8	8.005E+1	8.0268E+1	9.16905E+1	8.31031E+1	6.054271013E-2	3E+1	1E+0	8E+1	6E+1	8.0048E+1	8.0226E+1	9.11175E+1	8.31031E+1	3.6E+0	8E+1	5.491350219E-2	6.1266E+1	-9.6E-2	9E+0	2.5E-1	2.501E-1
Elapsed Time{Double Float}=12790.950867	0E+0	4.798030637E-4	2.04E-1	4.798030637E-4	1.685883988E-6	3.002977848E-7	1.7484E+1	2.83965598E-7	8.850883864E-8	8.0042E+1	8.0303E+1	9.10817E+1	8.31031E+1	5.604319647E-2	3.1E+1	1E+0	8E+1	6E+1	8.005E+1	8.0268E+1	9.16905E+1	8.31031E+1	3.6E+0	8E+1	6.054271013E-2	6.1266E+1	-9.6E-2	1E+1	0E+0	1E-4
File:Autodel{Boolean}=True	0E+0	4.801396466E-4	2.016E-1	4.801396466E-4	1.652169136E-6	1.96036587E-6	1.781268E+2	-1.96194696E-6	6.374745823E-8	8.0042E+1	8.0341E+1	9.11533E+1	8.31031E+1	5.684027821E-2	3.2E+1	1E+0	8E+1	6E+1	8.0042E+1	8.0303E+1	9.10817E+1	8.31031E+1	3.6E+0	8E+1	5.604319647E-2	6.1266E+1	-9.6E-2	1.1E+1	-2.5E-1	-2.498E-1
File:Autosave{Boolean}=False	0E+0	4.809825178E-4	2.04E-1	4.809825178E-4	1.685883988E-6	4.190473177E-6	1.070472E+2	-4.192054268E-6	6.84889769E-8	8.0036E+1	8.0378E+1	9.10817E+1	8.31031E+1	5.571651459E-2	3.3E+1	1E+0	8E+1	6E+1	8.0042E+1	8.0341E+1	9.11533E+1	8.31031E+1	3.6E+0	8E+1	5.684027821E-2	6.1266E+1	-9.6E-2	1.2E+1	-5E-1	-4.999E-1
File:Export Config{Boolean}=True	0E+0	4.82161972E-4	2.04E-1	4.82161972E-4	1.685883988E-6	6.373699305E-6	1.792236E+2	-6.376332571E-6	8.482096565E-8	8.0041E+1	8.0412E+1	9.10817E+1	8.31031E+1	5.4753948E-2	3.4E+1	1E+0	8E+1	6E+1	8.0036E+1	8.0378E+1	9.10817E+1	8.31031E+1	3.6E+0	8E+1	5.571651459E-2	6.1266E+1	-9.6E-2	1.3E+1	-7.5E-1	-7.498E-1
File:Final Autosave{Boolean}=True	0E+0	4.837642759E-4	1.956E-1	4.837642759E-4	1.652169136E-6	8.697568972E-6	1.793544E+2	-8.700205066E-6	9.746516627E-8	8.0035E+1	8.0443E+1	9.16905E+1	8.31031E+1	4.953756556E-2	3.5E+1	1E+0	8E+1	6E+1	8.0041E+1	8.0412E+1	9.10817E+1	8.31031E+1	3.6E+0	8E+1	5.4753948E-2	6.1266E+1	-9.6E-2	1.4E+1	-1E+0	-9.999E-1
Filter:Enable{Enum U16 ((None,Analog,Digital,Analog&Digitial))}=None	0E+0	4.857699136E-4	1.98E-1	4.857699136E-4	1.685883988E-6	1.087923664E-5	1.076148E+2	-1.088187273E-5	7.165001008E-8	8.0029E+1	8.0479E+1	9.09026E+1	8.31031E+1	5.306238681E-2	3.6E+1	1E+0	8E+1	6E+1	8.0035E+1	8.0443E+1	9.16905E+1	8.31031E+1	3.6E+0	8E+1	4.953756556E-2	6.1266E+1	-9.6E-2	1.5E+1	-1.25E+0	-1.2498E+0
Filter:Points{I32}=1	0E+0	4.881469238E-4	1.98E-1	4.881469238E-4	1.685883988E-6	1.322260265E-5	1.078512E+2	-1.322523875E-5	3.266400014E-8	8.003E+1	8.0502E+1	9.07951E+1	8.21864E+1	3.88353169E-2	3.7E+1	1E+0	8E+1	6E+1	8.0029E+1	8.0479E+1	9.09026E+1	8.31031E+1	3.6E+0	8E+1	5.306238681E-2	6.1266E+1	-9.6E-2	1.6E+1	-1.5E+0	-1.4998E+0
Filter:Type{U16}=1	0E+0	4.881469238E-4	1.98E-1	4.881469238E-4	1.685883988E-6	1.317360298E-5	3.59316E+1	-1.31762419E-5	1.475147499E-8	8.0032E+1	8.0509E+1	9.07235E+1	8.21864E+1	4.400822148E-2	3.8E+1	1E+0	8E+1	6E+1	8.003E+1	8.0502E+1	9.07951E+1	8.21864E+1	3.6E+0	8E+1	3.88353169E-2	6.1266E+1	-9.6E-2	1.7E+1	-1.5E+0	-1.5E+0
Filter:Type.__text__{String}=Repeat	0E+0	4.841008587E-4	1.98E-1	4.841008587E-4	1.685883988E-6	8.693354616E-6	1.794456E+2	-8.69599071E-6	8.324049714E-8	8.0027E+1	8.0558E+1	9.08668E+1	8.21864E+1	3.912924975E-2	3.9E+1	1E+0	8E+1	6E+1	8.0032E+1	8.0509E+1	9.07235E+1	8.21864E+1	3.6E+0	8E+1	4.400822148E-2	6.1266E+1	-9.6E-2	1.8E+1	-1E+0	-1.0002E+0
Filter:Window{Double Float}=1.000000	0E+0	4.816231566E-4	2.04E-1	4.816231566E-4	1.685883988E-6	4.208911694E-6	1.791132E+2	-4.211544959E-6	6.427433764E-8	8.0025E+1	8.0606E+1	9.10458E+1	8.21864E+1	4.086156934E-2	4E+1	1E+0	8E+1	6E+1	8.0027E+1	8.0558E+1	9.08668E+1	8.21864E+1	3.6E+0	8E+1	3.912924975E-2	6.1266E+1	-9.6E-2	1.9E+1	-5E-1	-5E-1
Iterator{I32}=0	
Magnet: Control Mode{Boolean}=False	
Magnet: Final Switch Heater{Enum U8 ((False,True,Mixed))}=	
Magnet: Power Supply{Enum U16 ((IPS120,LS625,PS110,Hg iPS,SMS Series,Cryomagnetics 4G,DMG Little CryoFree,DMG Big CryoFree))}=Hg iPS	
Magnet: Rate{Double Float}=0.500000	
Magnet: Setpoint{Double Float}=0.000000	
Magnet: Units{Enum U16 ((Field,Current))}=Field	
Magnet: VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
Main Screen Path{Path}=C:\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV\\\\1Code.vi	
Measurement Timestamp{Timestamp}=<09:07:38.582 23/05/2023>T	
Measurement Title{String}=	
Measurment Select{U16}=4	
Measurment Select.__text__{String}=6221-Lockin-DAQ	
Notes{String}=I+3E I-3A\\nRxx+2B Rxx-2D\\nRxy+2A Rxy- 3D	
Offset{Double Float}=0.000000	
Option: 2182 Autozero{Boolean}=True	
Option: 2182 Front Autozero{Boolean}=True	
Option: 2182 Hold{Boolean}=False	
Option: 2182 Hold Count{I32}=10	
Option: 2182 Hold Window{Double Float}=1.000000	
Option: 2182 Line Sync{Boolean}=False	
Option: 2182 Reference Reading{Double Float}=0.000000	
Option: 2182 Relative Mode{Boolean}=False	
Option: 2182 Trigger Delay{Cluster (Boolean,Double Float)}={'Auto':True,'Time(s)':0.000000}	
Option: 2182 Trigger Source{Enum U16 ((Immediate,Timer,Manual,Bus,Trigger link))}=Bus	
Option: 2182 Trigger Timer{Double Float}=0.000000	
Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	
Option: 560 Enabled{Boolean}=False	
Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	
Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	
Option: 6221 Adjust Mode{Enum U16 ((Offset,Frequency,Amplitude))}=Offset	
Option: 6221 Amplitude{Double Float}=1.000000E-6	
Option: 6221 Compliance{Double Float}=10.000000	
Option: 6221 Duty Cycle{Double Float}=50.000000	
Option: 6221 External Trigger{Boolean}=False	
Option: 6221 External Trigger Ignore Multiple{Boolean}=False	
Option: 6221 Frequency{Double Float}=119.770000	
Option: 6221 Function{U16}=1	
Option: 6221 Function.__text__{String}=Sine	
Option: 6221 Idle Level{Double Float}=0.000000	
Option: 6221 Input trigger Line{U8}=5	
Option: 6221 Offset{Double Float}=0.000000	
Option: 6221 Output Trigger Line{U8}=4	
Option: 6221 Pass Through{Boolean}=True	
Option: 6221 Phase Marker{Boolean}=True	
Option: 6221 Phase Marker Phase{Double Float}=0.000000	
Option: 6221 Range Level{Double Float}=2.000000E-12	
Option: 6221 Ranging{U16}=1	
Option: 6221 Ranging.__text__{String}=Best	
Option: 6221 Update Clock{Double Float}=0.000000	
Option: 6221 VISA{Visa Refnum (Void)}=GPIB0::13::INSTR	
Option: Confirm Config{Boolean}=False	
Option: Control Panel Ref{LVObjVI Refnum (Void)}=	
Option: DAQ Global Channel{Boolean}=False	
Option: DAQ Input Rate{Double Float}=10000.000000	
Option: DAQ Input Samples{I32}=200	
Option: DAQ Measurement Channels{1D Array (Cluster (UserDefinedRefnumTag Refnum (Void),\tkDAQmxPhysChanTagType Tag,\tkDAQmxScaleTagType Tag,Boolean,Double Float,String))}=[]	
Option: Differential{I32}=10106	
Option: Differential.__text__{String}=Differential	
Option: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values))}=Function Generator	
Option: Lockin Standoff Time{Double Float}=0.000000	
Option: Paranoid Save Data{Boolean}=True	
Option: Plot Autoback Path{Path}=C:\\\\TEMP\\\\XY Multiparam\\\\Backup.txt	
Option: SR830  Ref Phase{Double Float}=0.000000	
Option: SR830  Synch Filter{Boolean}=False	
Option: SR830  Time Constant{I16}=8	
Option: SR830  Time Constant.__text__{String}=100 ms	
Option: SR830 2x Line Filter{Boolean}=True	
Option: SR830 Adjust Gains{Boolean}=False	
Option: SR830 Auto Gain Lower.__text__{String}=2 nV/fA	
Option: SR830 Auto Gain Upper.__text__{String}=1 V/uA	
Option: SR830 Auto Offset 1{Boolean}=False	
Option: SR830 Auto Offset 2{Boolean}=False	
Option: SR830 Autophase{Boolean}=False	
Option: SR830 DC Coupling?{Boolean}=False	
Option: SR830 Display 1{U16}=0	
Option: SR830 Display 1.__text__{String}=X	
Option: SR830 Display 2{U16}=0	
Option: SR830 Display 2.__text__{String}=Y	
Option: SR830 Dynamic Reserve{I16}=1	
Option: SR830 Dynamic Reserve.__text__{String}=Normal	
Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Option: SR830 Filter Slope{I32}=1	
Option: SR830 Filter Slope.__text__{String}=12 dB/oct	
Option: SR830 Gain{I32}=-1	
Option: SR830 Gain.__text__{String}=Auto Gain	
Option: SR830 Ground Shield?{Boolean}=False	
Option: SR830 Harmonic{I32}=1	
Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A	
Option: SR830 Line Filter{Boolean}=True	
Option: SR830 No Reset{Boolean}=False	
Option: SR830 Offset 1{Double Float}=0.000000	
Option: SR830 Offset 2{Double Float}=0.000000	
Option: SR830 Output Channel 1{Boolean}=False	
Option: SR830 Output Channel 2{Boolean}=False	
Option: SR830 Ratio 1{U16}=0	
Option: SR830 Ratio 1.__text__{String}=None	
Option: SR830 Ratio 2{U16}=0	
Option: SR830 Ratio 2.__text__{String}=None	
Option: SR830 Ref Amplitude{Double Float}=0.100000	
Option: SR830 Ref Frequency{Double Float}=1013.000000	
Option: SR830 Ref Source{Boolean}=False	
Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta]	
Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Option: SR830 VISA{Visa Refnum (Void)}=	
Option: Sense Autorange{Boolean}=False	
Option: Sense Range Level{Double Float}=0.100000	
Option: Sense Rate{Double Float}=1.000000	
Option:560 Comport{Visa Refnum (Void)}=COM1	
Option:560 Filter High Pass{U16}=0	
Option:560 Filter High Pass.__text__{String}=0.03	
Option:560 Filter Lowpass{U16}=0	
Option:560 Filter Lowpass.__text__{String}=0.03	
Option:560 Filter Mode{U16}=0	
Option:560 Filter Mode.__text__{String}=6 dB high pass	
Option:560 Invert{Boolean}=False	
Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Option:570 Enabled{Boolean}=False	
Option:570 Filter High Pass{U16}=0	
Option:570 Filter High Pass.__text__{String}=0.03	
Option:570 Filter Lowpass{U16}=0	
Option:570 Filter Lowpass.__text__{String}=0.03	
Option:570 Filter Mode{U16}=0	
Option:570 Filter Mode.__text__{String}=6 dB high pass	
Option:570 Gain Mode{U16}=0	
Option:570 Gain Mode.__text__{String}=Low Noise	
Option:570 Input Offset{U16}=0	
Option:570 Input Offset On{Boolean}=False	
Option:570 Input Offset.__text__{String}=1pA	
Option:570 Sensitivity{U16}=0	
Option:570 Sensitivity.__text__{String}=1pA/V	
Option:Debug On{Boolean}=False	
Option:GPIB 2182{Visa Refnum (Void)}=	
Option:Parallel Config Voltage Measurers{Boolean}=True	
Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Option:SR830 Settle Time{Double Float}=5.000000	
Option:Sense Digits{I32}=8	
Output Names{1D Array (String)}=['Offset','Rxx::R','Rxx::Theta','Rxx::X','Rxx::Y','Rxy::R','Rxy::Theta','Rxy::X','Rxy::Y','temperature: T1','temperature: T2','temperature: T3','temperature: T4','temperature: dT/dt','iterator','multi[0]:iterator','multi[0]:y','multi[0]:temperature: setpoint','multi[0]:temperature: T1','multi[0]:temperature: T2','multi[0]:temperature: T3','multi[0]:temperature: T4','multi[0]:temperature: heater','multi[0]:temperature: gas','multi[0]:temperature: dT/dt','multi[0]:temperature: current temperature','multi[0]:temperature: error','multi[1]:iterator','multi[1]:y','multi[1]:Control:Magnet Output']	
Parameter Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Parameter Select{U16}=6	
Parameter Select.__text__{String}=Multi-Parameter	
Paths{U32}=0	
Plot: Column Renames{1D Array (Cluster (String,String))}=[]	
Plot: No dups{Boolean}=False	
Plot: StdDevs{Boolean}=False	
Plotting Class{String}=Parameter Plot	
Plotting Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	
Plotting Select{U16}=1	
Plotting Select.__text__{String}=Parameter Plot	
Project Code{String}=Topological_Insulators	
Ref: Temperature Window{LVObjVI Refnum (Void)}=	
Ref:Control Subpanel{LVObjUnknown Refnum (Void)}=	
Ref:Main Screen{LVObjVI Refnum (Void)}=	
Ref:Plotting Subpanel{LVObjUnknown Refnum (Void)}=	
Ref:Toolbar{LVObjUnknown Refnum (Void)}=	
Ref:XY Subpanel{LVObjUnknown Refnum (Void)}=	
Rxx::R{Double Float}=0.000482	
Rxx::Theta{Double Float}=0.204000	
Rxx::X{Double Float}=0.000482	
Rxx::Y{Double Float}=1.685884E-6	
Rxx:Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	
Rxx:Option: 560 Enabled{Boolean}=False	
Rxx:Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	
Rxx:Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	
Rxx:Option: Lockin Standoff Time{Double Float}=0.000000	
Rxx:Option: Lockin Type{Enum U16 ((SRS 830,EG&G 5302))}=SRS 830	
Rxx:Option: SR803 Full Scale Reading{Double Float}=0.000000	
Rxx:Option: SR830  Ref Phase{Double Float}=0.000000	
Rxx:Option: SR830  Synch Filter{Boolean}=False	
Rxx:Option: SR830  Time Constant{I16}=8	
Rxx:Option: SR830 2x Line Filter{Boolean}=False	
Rxx:Option: SR830 Adjust Gains{Boolean}=False	
Rxx:Option: SR830 Auto Gain Lower{I32}=0	
Rxx:Option: SR830 Auto Gain Upper{I32}=26	
Rxx:Option: SR830 Auto Offset 1{Boolean}=False	
Rxx:Option: SR830 Auto Offset 2{Boolean}=False	
Rxx:Option: SR830 Autophase{Boolean}=False	
Rxx:Option: SR830 DC Coupling?{Boolean}=False	
Rxx:Option: SR830 Display 1{U16}=0	
Rxx:Option: SR830 Display 2{U16}=0	
Rxx:Option: SR830 Dynamic Reserve{I16}=2	
Rxx:Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Rxx:Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Rxx:Option: SR830 Filter Slope{I32}=3	
Rxx:Option: SR830 Gain{I32}=17	
Rxx:Option: SR830 Ground Shield?{Boolean}=False	
Rxx:Option: SR830 Harmonic{I32}=1	
Rxx:Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A-B	
Rxx:Option: SR830 Line Filter{Boolean}=False	
Rxx:Option: SR830 No Reset{Boolean}=False	
Rxx:Option: SR830 Offset 1{Double Float}=0.000000	
Rxx:Option: SR830 Offset 2{Double Float}=0.000000	
Rxx:Option: SR830 Output Channel 1{Boolean}=False	
Rxx:Option: SR830 Output Channel 2{Boolean}=False	
Rxx:Option: SR830 Ratio 1{U16}=0	
Rxx:Option: SR830 Ratio 2{U16}=0	
Rxx:Option: SR830 Ref Amplitude{Double Float}=0.100000	
Rxx:Option: SR830 Ref Frequency{Double Float}=1013.000000	
Rxx:Option: SR830 Ref Source{Boolean}=False	
Rxx:Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta,X,Y]	
Rxx:Option: SR830 Time Constant value{Double Float}=0.000000	
Rxx:Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Rxx:Option: SR830 VISA{Visa Refnum (Void)}=GPIB0::5::INSTR	
Rxx:Option:560 Comport{Visa Refnum (Void)}=COM1	
Rxx:Option:560 Filter High Pass{U16}=0	
Rxx:Option:560 Filter Lowpass{U16}=0	
Rxx:Option:560 Filter Mode{U16}=0	
Rxx:Option:560 Invert{Boolean}=False	
Rxx:Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Rxx:Option:570 Enabled{Boolean}=False	
Rxx:Option:570 Filter High Pass{U16}=0	
Rxx:Option:570 Filter Lowpass{U16}=0	
Rxx:Option:570 Filter Mode{U16}=0	
Rxx:Option:570 Gain Mode{U16}=0	
Rxx:Option:570 Input Offset{U16}=0	
Rxx:Option:570 Input Offset On{Boolean}=False	
Rxx:Option:570 Sensitivity{U16}=0	
Rxx:Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Rxx:Option:SR830 Autogain Lower Threshold{Double Float}=0.100000	
Rxx:Option:SR830 Autogain Standoff{Double Float}=3.000000	
Rxx:Option:SR830 Autogain Upper Threshold{Double Float}=0.900000	
Rxx:Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Rxx:Option:SR830 Settle Time{Double Float}=0.000000	
Rxy::R{Double Float}=4.208912E-6	
Rxy::Theta{Double Float}=179.113200	
Rxy::X{Double Float}=-4.211545E-6	
Rxy::Y{Double Float}=6.427434E-8	
Rxy:Option: 560 Coupling{Enum U16 ((ground,DC,AC))}=ground	
Rxy:Option: 560 Enabled{Boolean}=False	
Rxy:Option: 560 Gain{Enum U16 ((1,2,5,10,20,50,100,200,500,1000,2000,5000,10000,20000,50000))}=1	
Rxy:Option: 560 Input Source{Enum U16 ((A,A-B,B))}=A	
Rxy:Option: Lockin Standoff Time{Double Float}=0.000000	
Rxy:Option: Lockin Type{Enum U16 ((SRS 830,EG&G 5302))}=SRS 830	
Rxy:Option: SR803 Full Scale Reading{Double Float}=0.000000	
Rxy:Option: SR830  Ref Phase{Double Float}=0.000000	
Rxy:Option: SR830  Synch Filter{Boolean}=False	
Rxy:Option: SR830  Time Constant{I16}=8	
Rxy:Option: SR830 2x Line Filter{Boolean}=False	
Rxy:Option: SR830 Adjust Gains{Boolean}=False	
Rxy:Option: SR830 Auto Gain Lower{I32}=0	
Rxy:Option: SR830 Auto Gain Upper{I32}=26	
Rxy:Option: SR830 Auto Offset 1{Boolean}=False	
Rxy:Option: SR830 Auto Offset 2{Boolean}=False	
Rxy:Option: SR830 Autophase{Boolean}=False	
Rxy:Option: SR830 DC Coupling?{Boolean}=False	
Rxy:Option: SR830 Display 1{U16}=0	
Rxy:Option: SR830 Display 2{U16}=1	
Rxy:Option: SR830 Dynamic Reserve{I16}=1	
Rxy:Option: SR830 Expand 1{Enum U16 ((None,10x,100x))}=None	
Rxy:Option: SR830 Expand 2{Enum U16 ((None,10x,100x))}=None	
Rxy:Option: SR830 Filter Slope{I32}=3	
Rxy:Option: SR830 Gain{I32}=13	
Rxy:Option: SR830 Ground Shield?{Boolean}=False	
Rxy:Option: SR830 Harmonic{I32}=1	
Rxy:Option: SR830 Input{Enum U16 ((A,A-B,I 1MOhm,I 10MOhm))}=A-B	
Rxy:Option: SR830 Line Filter{Boolean}=False	
Rxy:Option: SR830 No Reset{Boolean}=False	
Rxy:Option: SR830 Offset 1{Double Float}=0.000000	
Rxy:Option: SR830 Offset 2{Double Float}=0.000000	
Rxy:Option: SR830 Output Channel 1{Boolean}=False	
Rxy:Option: SR830 Output Channel 2{Boolean}=False	
Rxy:Option: SR830 Ratio 1{U16}=0	
Rxy:Option: SR830 Ratio 2{U16}=0	
Rxy:Option: SR830 Ref Amplitude{Double Float}=0.100000	
Rxy:Option: SR830 Ref Frequency{Double Float}=1013.000000	
Rxy:Option: SR830 Ref Source{Boolean}=False	
Rxy:Option: SR830 Requested Parameters{1D Array (Enum U16 ((X,Y,R,Theta,Aux 1,Aux 2,Aux 3,Aux 4,Ref Freq,Channel 1,Channel 2)))}=[R,Theta,X,Y]	
Rxy:Option: SR830 Time Constant value{Double Float}=0.000000	
Rxy:Option: SR830 Trigger Edge{Enum U16 ((Zero Crossing,Rising Edge,Falling Edge))}=Falling Edge	
Rxy:Option: SR830 VISA{Visa Refnum (Void)}=GPIB0::6::INSTR	
Rxy:Option:560 Comport{Visa Refnum (Void)}=COM1	
Rxy:Option:560 Filter High Pass{U16}=0	
Rxy:Option:560 Filter Lowpass{U16}=0	
Rxy:Option:560 Filter Mode{U16}=0	
Rxy:Option:560 Invert{Boolean}=False	
Rxy:Option:560 dynamic reserve{Enum U16 ((low noise,high DR,calibration gains))}=calibration gains	
Rxy:Option:570 Enabled{Boolean}=False	
Rxy:Option:570 Filter High Pass{U16}=0	
Rxy:Option:570 Filter Lowpass{U16}=0	
Rxy:Option:570 Filter Mode{U16}=0	
Rxy:Option:570 Gain Mode{U16}=0	
Rxy:Option:570 Input Offset{U16}=0	
Rxy:Option:570 Input Offset On{Boolean}=False	
Rxy:Option:570 Sensitivity{U16}=0	
Rxy:Option:SR570 Comport{Visa Refnum (Void)}=COM1	
Rxy:Option:SR830 Autogain Lower Threshold{Double Float}=0.100000	
Rxy:Option:SR830 Autogain Standoff{Double Float}=3.000000	
Rxy:Option:SR830 Autogain Upper Threshold{Double Float}=0.900000	
Rxy:Option:SR830 Divide by 6221 Ampl{Boolean}=False	
Rxy:Option:SR830 Settle Time{Double Float}=0.000000	
Sample ID{String}=MBE202230105_PA_D1 900C Cracker MobvsT	
Save:Filename{String}=${X-Y Class} ${2nd Parameter Class} ${iterator}{%04d} ${y}{%04.2g}.txt	
Save:Final Filename{String}=${X-Y Class} ${2nd Parameter Class} .txt	
Save:Final path{Path}=C:\\\\Data\\\\${Project Code}\\\\${User}\\\\${Sample ID}\\\\${Measurement Timestamp}{%Y%m%d}\\\\${X-Y Class}	
Save:Path{Path}=C:\\\\Data\\\\${Project Code}\\\\${User}\\\\${Sample ID}\\\\${Measurement Timestamp}{%Y%m%d}\\\\${X-Y Class}	
Startup path{Path}=C:\\\\Program Files\\\\National Instruments\\\\LabVIEW 2018\\\\Stonerlab\\\\Programs\\\\Source Meter IV	
Sub Panel{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Sweep Step{I32}=3	
T Control Measure.__text__{1D Array (String)}=['temperature: T1','temperature: T2','temperature: T3','temperature: T4','temperature: dT/dt']	
Timestamp{Timestamp}=<09:08:47.711 23/05/2023>T	
Toolbar{Cluster (I32,Enum U16 ((Click,Latch,Unlatch)))}={'Index':5,'Type':Latch}	
Unaved Data{Boolean}=True	
Unsaved Data{Boolean}=False	
User{String}=Craig	
X-Y Class{String}=6221-Lockin-DAQ	
X-Y Class Path{Path}=..\\\\..\\\\..\\\\..\\\\..\\\\..\\\\..	
d(Offset){Double Float}=0.000000	
d(Rxx::R){Double Float}=4.647580E-8	
d(Rxx::Theta){Double Float}=3.103168E-17	
d(Rxx::X){Double Float}=4.647580E-8	
d(Rxx::Y){Double Float}=2.367529E-22	
d(Rxy::R){Double Float}=3.511606E-8	
d(Rxy::Theta){Double Float}=0.274017	
d(Rxy::X){Double Float}=3.511532E-8	
d(Rxy::Y){Double Float}=2.011322E-8	
iterate result{U16}=5	
iterator{I32}=40	
multi[0]:Control: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values,Adaptive Step Ramp))}=List of Values	
multi[0]:Control: Monitor Update Timeout{Double Float}=0.010000	
multi[0]:Control: Open T Window{Boolean}=False	
multi[0]:Control: Reverse Temperature Sense{Boolean}=False	
multi[0]:Iterator{I32}=0	
multi[0]:Ref: Temperature Window{LVObjVI Refnum (Void)}=	
multi[0]:iterate result{U16}=0	
multi[0]:iterator{I32}=1	
multi[0]:temperature:  rate window{Double Float}=120.000000	
multi[0]:temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[0]:temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':200.000000,'I':70.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':8.000000,'P':150.000000,'I':70.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':12.000000,'P':80.000000,'I':65.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':4,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':25.000000,'P':10.000000,'I':20.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':4,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':50.000000,'P':150.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':4,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':150.000000,'P':70.000000,'I':2.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':5,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':250.000000,'P':115.000000,'I':1.200000,'D':0.000000,'Manual Output':0.000000,'Heater Range':5,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':300.000000,'P':75.000000,'I':1.200000,'D':0.000000,'Manual Output':0.000000,'Heater Range':5,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':300.000000,'P':75.000000,'I':1.200000,'D':0.000000,'Manual Output':0.000000,'Heater Range':5,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':310.000000,'P':1.000000,'I':1.300000,'D':0.000000,'Manual Output':0.000000,'Heater Range':0,'Input Sensor':0,'Ramp Rate':8.000000}]	
multi[0]:temperature: T1{Double Float}=80.024000	
multi[0]:temperature: T2{Double Float}=80.653000	
multi[0]:temperature: T3{Double Float}=91.117500	
multi[0]:temperature: T4{Double Float}=82.186400	
multi[0]:temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
multi[0]:temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
multi[0]:temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
multi[0]:temperature: current temperature{Double Float}=61.266000	
multi[0]:temperature: current temperature 2{Double Float}=287.100000	
multi[0]:temperature: dT/dt{Double Float}=0.041359	
multi[0]:temperature: error{Double Float}=-0.096000	
multi[0]:temperature: gas{Double Float}=80.000000	
multi[0]:temperature: gas control{Boolean}=False	
multi[0]:temperature: gas control 2{Boolean}=False	
multi[0]:temperature: gass boost{I8}=0	
multi[0]:temperature: gass boost 2{I8}=0	
multi[0]:temperature: gast flow{I16}=0	
multi[0]:temperature: gast flow 2{I16}=13	
multi[0]:temperature: heater{Double Float}=3.600000	
multi[0]:temperature: heater output{Double Float}=100.000000	
multi[0]:temperature: heater output 2{Double Float}=0.000000	
multi[0]:temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
multi[0]:temperature: monitor timeout{Double Float}=0.010000	
multi[0]:temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':70.000000,'I':2.000000,'D':0.000000}	
multi[0]:temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
multi[0]:temperature: ramp rate{Double Float}=8.000000	
multi[0]:temperature: ramp rate 2{Double Float}=0.000000	
multi[0]:temperature: ramp target{Double Float}=60.000000	
multi[0]:temperature: ramp target 2{Double Float}=0.000000	
multi[0]:temperature: ramping{Boolean}=False	
multi[0]:temperature: setpoint{Double Float}=60.000000	
multi[0]:temperature: setpoint 2{Double Float}=287.100000	
multi[0]:temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
multi[0]:temperature: stability error{Extended Float}=0.040000	
multi[0]:temperature: stability script{String}=	
multi[0]:temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':1.000000,'temperature:stability rate':0.150000,'temperature:history window':300.000000}	
multi[0]:temperature: temp control mode{U16}=2	
multi[0]:temperature: temp control mode 2{U16}=3	
multi[0]:temperature: temp control mode 2.__text__{String}=Open Loop	
multi[0]:temperature: temp control mode.__text__{String}=Zone	
multi[0]:temperature: temp control sensor{U16}=0	
multi[0]:temperature: temp control sensor 2{U16}=0	
multi[0]:temperature: temp control sensor 2.__text__{String}=Sensor 1	
multi[0]:temperature: temp control sensor.__text__{String}=Sensor A	
multi[0]:temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
multi[0]:temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
multi[0]:temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
multi[0]:temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
multi[0]:temperature: temp loop{U16}=0	
multi[0]:temperature: temp loop 2{U16}=0	
multi[0]:temperature: temp loop 2.__text__{String}=Heater	
multi[0]:temperature: temp loop.__text__{String}=Loop 1	
multi[0]:temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
multi[0]:temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[0]:temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[0]:temperature:error for gas boost{Double Float}=0.000000	
multi[0]:temperature:error for gas boost 2{Double Float}=0.000000	
multi[0]:temperature:heater range{U16}=5	
multi[0]:temperature:heater range 2{U16}=0	
multi[0]:temperature:heater range 2.__text__{String}=Off	
multi[0]:temperature:heater range.__text__{String}=40W	
multi[0]:temperature:history window{Extended Float}=300.000000	
multi[0]:temperature:is stable?{Boolean}=True	
multi[0]:temperature:monitor{Boolean}=True	
multi[0]:temperature:ramping{Boolean}=False	
multi[0]:temperature:ramping on{Boolean}=False	
multi[0]:temperature:ramping on 2{Boolean}=False	
multi[0]:temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
multi[0]:temperature:stability code{U32}=6618880	
multi[0]:temperature:stability rate{Extended Float}=0.040000	
multi[0]:y{Double Float}=80.000000	
multi[1]:Control: Display{Enum U16 ((Function Generator,Multi-Segment Ramp,List of Values,Adaptive Step Ramp))}=Multi-Segment Ramp	
multi[1]:Control: Gate delay{Double Float}=0.000000	
multi[1]:Control: Monitor Update Timeout{Double Float}=0.010000	
multi[1]:Control: Open T Window{Boolean}=False	
multi[1]:Control: Reverse Temperature Sense{Boolean}=False	
multi[1]:Control:Magnet Output{Double Float}=-0.000100	
multi[1]:Iterator{I32}=0	
multi[1]:Magnet: Final Switch Heater{Enum U8 ((False,True,Mixed))}=	
multi[1]:Magnet: Power Supply{Enum U16 ((IPS120,LS625,PS110,Hg iPS,SMS Series,Cryomagnetics 4G,DMG Little CryoFree,DMG Big CryoFree))}=Hg iPS	
multi[1]:Magnet: Rate{Double Float}=0.500000	
multi[1]:Magnet: Units{Enum U16 ((Field,Current))}=Field	
multi[1]:Magnet: VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[1]:Multi-segment_Stage{I32}=0	
multi[1]:Multi-segment_Stage_Changed{Boolean}=False	
multi[1]:Ref: Temperature Window{LVObjVI Refnum (Void)}=	
multi[1]:iterate result{U16}=4	
multi[1]:iterator{I32}=21	
multi[1]:measure point{Boolean}=False	
multi[1]:temperature:  rate window{Double Float}=120.000000	
multi[1]:temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
multi[1]:temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':200.000000,'I':70.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':8.000000,'P':150.000000,'I':70.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':12.000000,'P':80.000000,'I':65.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':4,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':25.000000,'P':10.000000,'I':20.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':4,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':50.000000,'P':150.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':4,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':150.000000,'P':70.000000,'I':2.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':5,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':250.000000,'P':115.000000,'I':1.200000,'D':0.000000,'Manual Output':0.000000,'Heater Range':5,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':300.000000,'P':75.000000,'I':1.200000,'D':0.000000,'Manual Output':0.000000,'Heater Range':5,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':300.000000,'P':75.000000,'I':1.200000,'D':0.000000,'Manual Output':0.000000,'Heater Range':5,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':310.000000,'P':1.000000,'I':1.300000,'D':0.000000,'Manual Output':0.000000,'Heater Range':0,'Input Sensor':0,'Ramp Rate':8.000000}]	
multi[1]:temperature: T1{Double Float}=1.842400	
multi[1]:temperature: T2{Double Float}=1.465600	
multi[1]:temperature: T3{Double Float}=86.318100	
multi[1]:temperature: T4{Double Float}=66.769200	
multi[1]:temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
multi[1]:temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
multi[1]:temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
multi[1]:temperature: current temperature{Double Float}=1.520200	
multi[1]:temperature: current temperature 2{Double Float}=287.100000	
multi[1]:temperature: dT/dt{Double Float}=-0.001864	
multi[1]:temperature: error{Double Float}=0.002000	
multi[1]:temperature: gas{Double Float}=40.000000	
multi[1]:temperature: gas control{Boolean}=False	
multi[1]:temperature: gas control 2{Boolean}=False	
multi[1]:temperature: gass boost{I8}=0	
multi[1]:temperature: gass boost 2{I8}=0	
multi[1]:temperature: gast flow{I16}=0	
multi[1]:temperature: gast flow 2{I16}=13	
multi[1]:temperature: heater{Double Float}=22.900000	
multi[1]:temperature: heater output{Double Float}=0.000000	
multi[1]:temperature: heater output 2{Double Float}=0.000000	
multi[1]:temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
multi[1]:temperature: monitor timeout{Double Float}=1.000000	
multi[1]:temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':10.000000,'I':20.000000,'D':0.000000}	
multi[1]:temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
multi[1]:temperature: ramp rate{Double Float}=8.000000	
multi[1]:temperature: ramp rate 2{Double Float}=0.000000	
multi[1]:temperature: ramp target{Double Float}=20.000000	
multi[1]:temperature: ramp target 2{Double Float}=0.000000	
multi[1]:temperature: ramping{Boolean}=False	
multi[1]:temperature: setpoint{Double Float}=1.800000	
multi[1]:temperature: setpoint 2{Double Float}=287.100000	
multi[1]:temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
multi[1]:temperature: stability error{Extended Float}=0.040000	
multi[1]:temperature: stability script{String}=	
multi[1]:temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':1.000000,'temperature:stability rate':0.150000,'temperature:history window':300.000000}	
multi[1]:temperature: temp control mode{U16}=2	
multi[1]:temperature: temp control mode 2{U16}=3	
multi[1]:temperature: temp control mode 2.__text__{String}=Open Loop	
multi[1]:temperature: temp control mode.__text__{String}=Zone	
multi[1]:temperature: temp control sensor{U16}=0	
multi[1]:temperature: temp control sensor 2{U16}=0	
multi[1]:temperature: temp control sensor 2.__text__{String}=Sensor 1	
multi[1]:temperature: temp control sensor.__text__{String}=Sensor A	
multi[1]:temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
multi[1]:temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
multi[1]:temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
multi[1]:temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
multi[1]:temperature: temp loop{U16}=0	
multi[1]:temperature: temp loop 2{U16}=0	
multi[1]:temperature: temp loop 2.__text__{String}=Heater	
multi[1]:temperature: temp loop.__text__{String}=Loop 1	
multi[1]:temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
multi[1]:temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[1]:temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
multi[1]:temperature:error for gas boost{Double Float}=0.000000	
multi[1]:temperature:error for gas boost 2{Double Float}=0.000000	
multi[1]:temperature:heater range{U16}=3	
multi[1]:temperature:heater range 2{U16}=0	
multi[1]:temperature:heater range 2.__text__{String}=Off	
multi[1]:temperature:heater range.__text__{String}=400mW	
multi[1]:temperature:history window{Extended Float}=300.000000	
multi[1]:temperature:is stable?{Boolean}=True	
multi[1]:temperature:monitor{Boolean}=True	
multi[1]:temperature:ramping{Boolean}=False	
multi[1]:temperature:ramping on{Boolean}=False	
multi[1]:temperature:ramping on 2{Boolean}=False	
multi[1]:temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
multi[1]:temperature:stability code{U32}=6618880	
multi[1]:temperature:stability rate{Extended Float}=0.040000	
multi[1]:y{Double Float}=0.000000	
parameter: Termination{String}=False	
parameter: delta time{Double Float}=1.000000	
parameter: progress{Double Float}=100.000000	
temperature:  rate window{Double Float}=120.000000	
temperature: Level Meter VISA Ref{Visa Refnum (Void)}=GPIB0::25::1::INSTR	
temperature: PID Table{1D Array (Cluster (Double Float,Double Float,Double Float,Double Float,Double Float,U16,U16,Double Float))}=[{'Upper Temp':2.000000,'P':200.000000,'I':70.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':2,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':8.000000,'P':150.000000,'I':70.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':3,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':12.000000,'P':80.000000,'I':65.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':4,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':25.000000,'P':10.000000,'I':20.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':4,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':50.000000,'P':150.000000,'I':15.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':4,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':150.000000,'P':70.000000,'I':2.000000,'D':0.000000,'Manual Output':0.000000,'Heater Range':5,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':250.000000,'P':115.000000,'I':1.200000,'D':0.000000,'Manual Output':0.000000,'Heater Range':5,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':300.000000,'P':75.000000,'I':1.200000,'D':0.000000,'Manual Output':0.000000,'Heater Range':5,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':300.000000,'P':75.000000,'I':1.200000,'D':0.000000,'Manual Output':0.000000,'Heater Range':5,'Input Sensor':0,'Ramp Rate':8.000000},{'Upper Temp':310.000000,'P':1.000000,'I':1.300000,'D':0.000000,'Manual Output':0.000000,'Heater Range':0,'Input Sensor':0,'Ramp Rate':8.000000}]	
temperature: T1{Double Float}=80.024000	
temperature: T2{Double Float}=80.653000	
temperature: T3{Double Float}=91.117500	
temperature: T4{Double Float}=82.186400	
temperature: VISA Ref{Visa Refnum (Void)}=GPIB0::10::INSTR	
temperature: VISA Ref 2{Visa Refnum (Void)}=GPIB0::24::INSTR	
temperature: channels{Cluster (Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))),Cluster (Enum U16 ((Primary,Secondary,Level Meter)),U16,U16,Enum U16 ((Output %,Temp,Rate))))}={'0':{'Instrument':Primary,'Channel':0,'Units':0,'Scale':Temp},'1':{'Instrument':Primary,'Channel':1,'Units':0,'Scale':Temp},'2':{'Instrument':Level Meter,'Channel':1,'Units':0,'Scale':Output %},'3':{'Instrument':Level Meter,'Channel':0,'Units':0,'Scale':Output %}}	
temperature: current temperature{Double Float}=61.266000	
temperature: current temperature 2{Double Float}=287.100000	
temperature: dT/dt{Double Float}=0.041359	
temperature: gas control{Boolean}=False	
temperature: gas control 2{Boolean}=False	
temperature: gass boost{I8}=0	
temperature: gass boost 2{I8}=0	
temperature: gast flow{I16}=0	
temperature: gast flow 2{I16}=13	
temperature: heater output{Double Float}=100.000000	
temperature: heater output 2{Double Float}=0.000000	
temperature: level meter{Enum U16 ((None,Oxford ILM,Hg Level meter,Serial Level Meter))}=Hg Level meter	
temperature: monitor timeout{Double Float}=0.010000	
temperature: pid controls{Cluster (Double Float,Double Float,Double Float)}={'P':70.000000,'I':2.000000,'D':0.000000}	
temperature: pid controls 2{Cluster (Double Float,Double Float,Double Float)}={'P':40.000000,'I':1.000000,'D':0.000000}	
temperature: ramp rate{Double Float}=8.000000	
temperature: ramp rate 2{Double Float}=0.000000	
temperature: ramp target{Double Float}=60.000000	
temperature: ramp target 2{Double Float}=0.000000	
temperature: ramping{Boolean}=False	
temperature: setpoint{Double Float}=60.000000	
temperature: setpoint 2{Double Float}=287.100000	
temperature: signal on{1D Array (Boolean)}=[True,True,True,True,True,True,True,True,False,True]	
temperature: stability error{Extended Float}=0.040000	
temperature: stability script{String}=	
temperature: stability settings{Cluster (Double Float,Double Float,Double Float)}={'temperature: stability error':1.000000,'temperature:stability rate':0.150000,'temperature:history window':300.000000}	
temperature: temp control mode{U16}=2	
temperature: temp control mode 2{U16}=3	
temperature: temp control mode 2.__text__{String}=Open Loop	
temperature: temp control mode.__text__{String}=Zone	
temperature: temp control sensor{U16}=0	
temperature: temp control sensor 2{U16}=0	
temperature: temp control sensor 2.__text__{String}=Sensor 1	
temperature: temp control sensor.__text__{String}=Sensor A	
temperature: temp control units{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Kelvin	
temperature: temp control units 2{Enum U16 ((Keep,Kelvin,Celsius,Sensor))}=Sensor	
temperature: temp controller{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Lakeshore 340	
temperature: temp controller 2{Enum U16 ((None,Lakeshore 340,Oxford ITC 503,Oxford ITC 502,Lakeshore 335,Lakeshore 336,Mercury ITC,Lakeshore 350,Eurotherm 22xx,Lakeshore 370,Lakeshore 331/332))}=Oxford ITC 503	
temperature: temp loop{U16}=0	
temperature: temp loop 2{U16}=0	
temperature: temp loop 2.__text__{String}=Heater	
temperature: temp loop.__text__{String}=Loop 1	
temperature: values{1D Array (Double Float)}=[164.280000E+0,171.660000E+0,172.624000E+0,93.384600E+0,23.104700E+0,0.000000E+0,0.000000E+0,87.655327E-15,171.660000E+0,-7.380000E+0]	
temperature:Remote/Local Mode{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
temperature:Remote/Local Mode 2{Enum U16 ((Local,Remote,Local Unlocked,Remote Unlocked))}=Remote	
temperature:error for gas boost{Double Float}=0.000000	
temperature:error for gas boost 2{Double Float}=0.000000	
temperature:heater range{U16}=5	
temperature:heater range 2{U16}=0	
temperature:heater range 2.__text__{String}=Off	
temperature:heater range.__text__{String}=40W	
temperature:history window{Extended Float}=300.000000	
temperature:is stable?{Boolean}=True	
temperature:monitor{Boolean}=True	
temperature:ramping{Boolean}=False	
temperature:ramping on{Boolean}=False	
temperature:ramping on 2{Boolean}=False	
temperature:rate select{Enum U32 ((Radio Selection 1,Radio Selection 2,Radio Selection 3,Radio Selection 4))}=Radio Selection 2	
temperature:stability code{U32}=6618880	
temperature:stability rate{Extended Float}=0.040000	
y{Double Float}=80.000000	
