CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.2/conf/instr/spect/uxnmr.info
Date         : Wed Jan 29 13:15:42 2025
Release      : TOPSPIN Version 3.2-pl6
Installed in : /opt/topspin3.2
Host         : fbscpcu177
OS           : CentOS release 5.11 (Final)
CPU          : Intel(R) Xeon(R) CPU E5-1620 v2 @ 3.70GHz (8 cores at 1200 MHz with Hyperthreading)
User         : nmrsu (NMR Administrator (nmrsu))
Description  : CABINET 750 HD X TB
Location     : University of Leeds, Leeds
System       : Avance III NMR spectrometer
1H-frequency : 747.06 MHz
Order Number : 10187390
Configured in: /opt/topspin3.2/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.254
- Tctrl : 1
- Fctrls: 4
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU: AQS DRU-E Z102520/04712 ECL 07.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 140519
- DRU controls AQS-Rack and HPPR/2
DRU: AQS DRU-E Z102520/04713 ECL 07.00
- TCP/IP address = 149.236.99.88
- Firmware Version = 140519

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     0   0x24 0x33     0        S  1.3 SGU-1  AQS SGU/3 1200 (2CH) Z117130/00542 ECL 01.03 FPGA-Vs=20131031
     2   0x10 0x53   0x5    CD  R  0.3 REC-1  AQS RXAD/2 1000 Z130589/382 ECL 00.03
     3   0x34 0xda   0x1        X  2.2 REF-1  
     6   0x11 0x53   0x5    CD  R  0.3 REC-2  AQS RXAD/2 1000 Z130589/383 ECL 00.03
     7   0x26 0x33     0        S  1.3 SGU-2  AQS SGU/3 1200 (2CH) Z117130/00543 ECL 01.03 FPGA-Vs=20131031
    13   0xa0 0x93     0        V  0.1 PS-1   
    14   0xa1 0x91     0        V  1.2 PS-2   AQS PSM-D Power Supply Module
    --   0x20 0xd8     0        B  2.0 MASTER AQS/3+ Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345093_0818 W1345093/0818 ECL 12:
- TCP/IP address = 149.236.99.253
- Firmware VS    = 20120627
- Amplifier      = BLAX500 E 6-365MHZ INR: W1345093/0818 ECL 12
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/5075 ECL 21
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/010650 ECL 50
BLA_W1345097_0358 W1345097/0358 ECL 20:
- TCP/IP address = 149.236.99.252
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H500/100/250 E 700-900MHZ INR: W1345097/0358 ECL 20
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/5079 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/010363 ECL 50
LTRX Z109892/00202 ECL 02.01:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 750: Z109892/00202 ECL 02.01

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20150130
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 750: Z109892/00202 ECL 02.01
- Lock: on L-TRX board
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/02722 ECL 04.00
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/03099 ECL 01.05

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

Bruker Automatic Changer: device connected to 149.236.99.254:/dev/tty01
- Capacity: 24 holders
- Firmware: 970111
- use BACS air  = yes
- BACS sx delay = 1 s
- Sample Rail fast changer mode = no

Cryo Controller CRCO: device connected to 149.236.99.254:/dev/tty04

Preamplifiers :
HPPR: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Application firmware = c.
                no LED display for tuning and matching
    Module  1 : HPLNA 19F1H (virtual 50 Ohm reference: 100.2%/0.2deg, reflection meter)
                 PN=Z103207, SN=00202 from 20150216
    Module  2 : 2H
                 PN=Z003475, SN=00204 from 20150409
    Module  3 : XBB31P 2HS
                 PN=Z003508, SN=00204 from 20150529
    Module  4 : XBB31P 2HS
                 PN=Z003508, SN=00205 from 20150529
    Module  5 : 15N
                 PN=Z003532, SN=00201 from 20150519
    Module  6 : 13C
                 PN=Z003526, SN=00202 from 20150507


Frequency generation:
- F1: for SGU
- F2: for SGU
- F3: for SGU
- F4: for SGU



RF cable connections (detected by 'confamp')
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0358 at TCP/IP 149.236.99.252)
SGU1 AUX  output -> TUNE signal input of HPPR
SGU2 NORM output -> input 2 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0358 at TCP/IP 149.236.99.252)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 1 of transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0818 at TCP/IP 149.236.99.253)
SGU3 AUX  output -> input 3 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0358 at TCP/IP 149.236.99.252)
SGU4 NORM output -> input 2 of transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0818 at TCP/IP 149.236.99.253)
SGU4 AUX  output -> input 4 of transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0358 at TCP/IP 149.236.99.252)

Blanking cable connections (detected by 'confamp')
--------------------------------------------------------------------
transmitter 1 (BLAX500 E 6-365MHZ INR W1345093/0818 at TCP/IP 149.236.99.253) amplifier X-500W uses blanking 4
transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0358 at TCP/IP 149.236.99.252) amplifier 1H-100W uses blanking 2
transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0358 at TCP/IP 149.236.99.252) amplifier X-500W uses blanking 1
transmitter 2 (BLAXH2H500/100/250 E 700-900MHZ W1345097/0358 at TCP/IP 149.236.99.252) amplifier 2H-250W uses blanking 7
transmitter 3 (BSMS/2 LOCK TRANSCEIVER 750 Z109892/00202 at TCP/IP 149.236.99.20) amplifier 2H-5W needs no blanking

